(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "Net-(D1-K)")
  (net 4 "Net-(D2-A)")
  (net 5 "Net-(D3-A)")
  (net 6 "Net-(D4-A)")
  (net 7 "Net-(D5-A)")
  (net 8 "Net-(D6-A)")
  (net 9 "Net-(D7-A)")
  (net 10 "Net-(D8-A)")
  (net 11 "Net-(U11-Anode)")
  (net 12 "Net-(U11-Cathode)")
  (net 13 "Net-(U13-Anode)")
  (net 14 "Net-(U14-Anode)")
  (net 15 "Net-(U15-Anode)")
  (net 16 "Net-(U16-Anode)")
  (net 17 "Net-(U17-Anode)")
  (net 18 "Net-(U18-Anode)")
  (net 19 "Net-(U1-R_L)")
  (net 20 "unconnected-(U1-Pad5)")
  (net 21 "Net-(U2-R_L)")
  (net 22 "unconnected-(U2-Pad5)")
  (net 23 "Net-(U3-R_L)")
  (net 24 "unconnected-(U3-Pad5)")
  (net 25 "Net-(U4-R_L)")
  (net 26 "unconnected-(U4-Pad5)")
  (net 27 "Net-(U5-R_L)")
  (net 28 "unconnected-(U5-Pad5)")
  (net 29 "Net-(U6-R_L)")
  (net 30 "unconnected-(U6-Pad5)")
  (net 31 "Net-(U8-R_L)")
  (net 32 "unconnected-(U8-Pad5)")
  (net 33 "Net-(U9-R_L)")
  (net 34 "unconnected-(U9-Pad5)")
  (net 35 "unconnected-(U11-NC-Pad3)")
  (net 36 "unconnected-(U11-NC-Pad4)")
  (net 37 "unconnected-(U11-Pad5)")
  (net 38 "unconnected-(U12-NC-Pad3)")
  (net 39 "unconnected-(U12-NC-Pad4)")
  (net 40 "unconnected-(U12-Pad5)")
  (net 41 "unconnected-(U13-NC-Pad3)")
  (net 42 "unconnected-(U13-NC-Pad4)")
  (net 43 "unconnected-(U13-Pad5)")
  (net 44 "unconnected-(U14-NC-Pad3)")
  (net 45 "unconnected-(U14-NC-Pad4)")
  (net 46 "unconnected-(U14-Pad5)")
  (net 47 "unconnected-(U15-NC-Pad3)")
  (net 48 "unconnected-(U15-NC-Pad4)")
  (net 49 "unconnected-(U15-Pad5)")
  (net 50 "unconnected-(U16-NC-Pad3)")
  (net 51 "unconnected-(U16-NC-Pad4)")
  (net 52 "unconnected-(U16-Pad5)")
  (net 53 "unconnected-(U17-NC-Pad3)")
  (net 54 "unconnected-(U17-NC-Pad4)")
  (net 55 "unconnected-(U17-Pad5)")
  (net 56 "unconnected-(U18-NC-Pad3)")
  (net 57 "unconnected-(U18-NC-Pad4)")
  (net 58 "unconnected-(U18-Pad5)")
  (net 59 "Net-(D9-A)")
  (net 60 "Net-(U12-Cathode)")
  (net 61 "Net-(U13-Cathode)")
  (net 62 "Net-(U14-Cathode)")
  (net 63 "Net-(U15-Cathode)")
  (net 64 "Net-(U16-Cathode)")
  (net 65 "Net-(U17-Cathode)")
  (net 66 "Net-(U18-Cathode)")
  (net 67 "unconnected-(U20-I6-Pad6)")
  (net 68 "unconnected-(U20-O5-Pad12)")
  (net 69 "unconnected-(U20-O6-Pad11)")
  (net 70 "Net-(D1-A)")
  (net 71 "unconnected-(U20-I7-Pad7)")
  (net 72 "unconnected-(U20-O7-Pad10)")
  (net 73 "unconnected-(U19-O7-Pad10)")
  (net 74 "unconnected-(U19-O6-Pad11)")
  (net 75 "unconnected-(U19-O5-Pad12)")
  (net 76 "Net-(D10-K)")
  (net 77 "Net-(U12-Anode)")
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 58.42 84.194 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 13 "Net-(U13-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 95.112 87.978 180)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U17" (at 3.302 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(U17-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "Net-(U17-Cathode)") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(U17-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(U17-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(U17-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 74.696 37.3025)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -4.084 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U5-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U5-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(U5-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 96.012 52.832 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at -3.048 0 180) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 84.856 37.3025)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at 2.266 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U6-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U6-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(U6-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 93.98 84.071 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -2.8555 0 -180) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 17 "Net-(U17-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (at 100.253 80.836081)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at -5.003 -2.350081) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 64.556 37.3025)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at -4.104 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U4-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U4-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U4-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 105.272 87.978 180)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U18" (at 3.302 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(U18-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(U18-Cathode)") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(U18-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(U18-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(U18-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_Coaxial:BNC_TEConnectivity_1478204_Vertical" (layer "F.Cu")
    (at 104.648 69.788)
    (descr "BNC female PCB mount 4 pin straight chassis connector http://www.te.com/usa-en/product-1-1478204-0.html")
    (tags "BNC female PCB mount 4 pin straight chassis connector ")
    (property "Field4" "OUT")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J2" (at -0.25 -6.25) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 0 6.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.556 3.556) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 76 "Net-(D10-K)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.175 -3.175) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.175 3.175) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.175 -3.175) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.175 3.175) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_TEConnectivity_1478204_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 74.792 87.978 180)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U15" (at 3.302 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(U15-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "Net-(U15-Cathode)") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(U15-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(U15-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U15-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 40.132 52.819 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 76.454 60.39 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D6" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D6-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 32.258 39.829 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 44.236 37.3025)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -2.326 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U2-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U2-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(U2-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_DIP:DIP-14_W7.62mm_LongPads" (layer "F.Cu")
    (at 92.71 46.851 -90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad 2-Input NAND Schmitt Trigger, SOIC-14")
    (property "ki_keywords" "NAND2")
    (attr through_hole)
    (fp_text reference "U10" (at 1.917 -2.33 90) (layer "F.SilkS"))
    (fp_text value "SN74HCT00N" (at 3.81 17.57 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U6-R_L)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U6-R_L)") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D6-A)") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D4-A)") (pintype "output"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U5-R_L)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U5-R_L)") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(U8-R_L)") (pintype "input"))
    (pad "9" thru_hole oval (at 7.62 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(U8-R_L)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D7-A)") (pintype "output"))
    (pad "11" thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D8-A)") (pintype "output"))
    (pad "12" thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U9-R_L)") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U9-R_L)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 105.196 37.3025)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U9" (at 3.008 1.0515) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U9-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U9-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(U9-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 95.25 67.818 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D10" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(D10-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 55.118 67.31 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 64.77 62.0375 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 3 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (at 39.37 80.8305)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 5.588 -1.3285) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 53.594 39.829 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 1.778 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 88.893 84.071 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at -2.9865 -0.007) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 16 "Net-(U16-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 48.26 84.1355 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 77 "Net-(U12-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 34.172 87.978 180)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U11" (at 3.322 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U11-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U11-Cathode)") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "unconnected-(U11-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(U11-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(U11-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 81.788 39.878 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 108.458 84.194 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at -0.12 1.778 90) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 18 "Net-(U18-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (at 39.121581 43.174419)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 5.836419 0.259581) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 82.804 60.358 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D7" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D7-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 95.25 60.422 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D9" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(D9-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 63.246 39.829 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (at 100.076 43.174419)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at -5.842 0.513581) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 54.472 87.978 180)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U13" (at 3.048 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U13-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(U13-Cathode)") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(U13-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(U13-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(U13-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_DIP:DIP-14_W7.62mm_LongPads" (layer "F.Cu")
    (at 62.235 46.856 -90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad 2-Input NAND Schmitt Trigger, SOIC-14")
    (property "ki_keywords" "NAND2")
    (attr through_hole)
    (fp_text reference "U7" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "SN74HCT00N" (at 3.81 17.57 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U2-R_L)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U2-R_L)") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(D1-A)") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D5-A)") (pintype "output"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-R_L)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-R_L)") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U3-R_L)") (pintype "input"))
    (pad "9" thru_hole oval (at 7.62 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U3-R_L)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D2-A)") (pintype "output"))
    (pad "11" thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D3-A)") (pintype "output"))
    (pad "12" thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U4-R_L)") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U4-R_L)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 46.482 60.39 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D1" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 59.182 67.31 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 33.274 84.194 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.8555 0 -180) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 11 "Net-(U11-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 44.312 87.978 180)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U12" (at 3.302 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(U12-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(U12-Cathode)") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U12-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(U12-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(U12-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 84.952 87.978 180)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U16" (at 3.302 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(U16-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(U16-Cathode)") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(U16-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(U16-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(U16-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 67.31 52.975 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:BNC_TEConnectivity_1478204_Vertical" (layer "F.Cu")
    (at 104.648 54.802)
    (descr "BNC female PCB mount 4 pin straight chassis connector http://www.te.com/usa-en/product-1-1478204-0.html")
    (tags "BNC female PCB mount 4 pin straight chassis connector ")
    (property "Field4" "IN")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J1" (at -0.25 -6.25) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 0 6.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.556 3.556) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(D9-A)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.175 -3.175) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.175 3.175) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.175 -3.175) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.175 3.175) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_TEConnectivity_1478204_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm_LongPads" (layer "F.Cu")
    (at 50.19425 66.496 -90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16")
    (property "ki_keywords" "darlington transistor array")
    (attr through_hole)
    (fp_text reference "U19" (at 3.81 -2.33 -90) (layer "F.SilkS"))
    (fp_text value "ULN2003" (at 3.81 20.11 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I1") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I2") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I3") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I4") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I5") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I6") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I7") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval (at 7.62 17.78 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "COM") (pintype "passive"))
    (pad "10" thru_hole oval (at 7.62 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 73 "unconnected-(U19-O7-Pad10)") (pinfunction "O7") (pintype "open_collector"))
    (pad "11" thru_hole oval (at 7.62 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 74 "unconnected-(U19-O6-Pad11)") (pinfunction "O6") (pintype "open_collector"))
    (pad "12" thru_hole oval (at 7.62 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 75 "unconnected-(U19-O5-Pad12)") (pinfunction "O5") (pintype "open_collector"))
    (pad "13" thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U11-Cathode)") (pinfunction "O4") (pintype "open_collector"))
    (pad "14" thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(U12-Cathode)") (pinfunction "O3") (pintype "open_collector"))
    (pad "15" thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(U13-Cathode)") (pinfunction "O2") (pintype "open_collector"))
    (pad "16" thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(U14-Cathode)") (pinfunction "O1") (pintype "open_collector"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 54.396 37.3025)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -4.104 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U3-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U3-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(U3-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 64.632 87.978 180)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U14" (at 3.302 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U14-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(U14-Cathode)") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(U14-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U14-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(U14-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 73.152 39.829 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 108.204 41.353 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0.303 2.032 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 47.244 39.829 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 56.896 60.39 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D3" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 42.672 60.39 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D5" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 72.644 60.39 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D4" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 92.71 39.829 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm_LongPads" (layer "F.Cu")
    (at 80.66925 66.496 -90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16")
    (property "ki_keywords" "darlington transistor array")
    (attr through_hole)
    (fp_text reference "U20" (at 3.81 -2.33 -90) (layer "F.SilkS"))
    (fp_text value "ULN2003" (at 3.81 20.11 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I1") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I2") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I3") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I4") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "I5") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(U20-I6-Pad6)") (pinfunction "I6") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(U20-I7-Pad7)") (pinfunction "I7") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval (at 7.62 17.78 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "COM") (pintype "passive"))
    (pad "10" thru_hole oval (at 7.62 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 72 "unconnected-(U20-O7-Pad10)") (pinfunction "O7") (pintype "open_collector"))
    (pad "11" thru_hole oval (at 7.62 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(U20-O6-Pad11)") (pinfunction "O6") (pintype "open_collector"))
    (pad "12" thru_hole oval (at 7.62 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(U20-O5-Pad12)") (pinfunction "O5") (pintype "open_collector"))
    (pad "13" thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 63 "Net-(U15-Cathode)") (pinfunction "O4") (pintype "open_collector"))
    (pad "14" thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(U16-Cathode)") (pinfunction "O3") (pintype "open_collector"))
    (pad "15" thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 65 "Net-(U17-Cathode)") (pinfunction "O2") (pintype "open_collector"))
    (pad "16" thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(U18-Cathode)") (pinfunction "O1") (pintype "open_collector"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 86.614 60.358 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D8" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D8-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 53.086 60.39 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)")
    (property "ki_keywords" "Ultra Fast")
    (attr smd)
    (fp_text reference "D2" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "US1A" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 34.056 37.3025)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -4.084 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(U1-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 78.486 84.194 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 15 "Net-(U15-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 34.798 54.294 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at -2.54 -3.048 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 1.27 4.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.286 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.74 2.19) (drill 1.19) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.143678)
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.74 2.19) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 95.016 37.3025)
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U8" (at 2.012 0.7975) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(U8-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(U8-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(U8-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 68.326 84.194 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 14 "Net-(U14-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:WHAM_LOGO-oscar" (layer "B.Cu")
    (at 97.282 32.004 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at -2.54 1.905 90) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_line (start 110.236 100.33) (end 28.956 100.33)
    (layer "Edge.Cuts"))
  (gr_line (start 110.236 24.892) (end 110.236 100.33)
    (layer "Edge.Cuts"))
  (gr_line (start 28.956 24.892) (end 110.236 24.892)
    (layer "Edge.Cuts"))
  (gr_line (start 28.956 100.33) (end 28.956 24.892)
    (layer "Edge.Cuts"))
  (gr_text "eat your heart \nout oscar" (at 88.646 73.152 90) (layer "F.Cu"))
  (gr_text "do you know what happens to \nyour body without fiber?" (at 85.852 86.36) (layer "B.Cu"))
  (gr_text "Beacon Fiber Repeater\nVersion: Alpha\nEverett Penne Jan 18, 2024" (at 52.07 32.766) (layer "B.SilkS"))
  (gr_text "BNC OUT" (at 98.806 75.438 90) (layer "F.SilkS"))
  (gr_text "<-- FIBER OUT" (at 30.734 86.36 90) (layer "F.SilkS"))
  (gr_text "FIBER IN -->" (at 30.734 50.292 90) (layer "F.SilkS"))
  (gr_text "GND" (at 32.512 49.976) (layer "F.SilkS"))
  (gr_text "+5V" (at 31.496 58.866) (layer "F.SilkS"))
  (gr_text "BNC IN" (at 98.806 60.198 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "B.SilkS")
    (pts (xy 39.37 80.8305) (xy 100.253 80.836081))
    (height -3.346467)
    (gr_text "2.4 in" (at 69.811807 77.486824 359.9947469) (layer "B.SilkS"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 1))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "B.SilkS")
    (pts (xy 39.121581 43.174419) (xy 100.076 43.174419))
    (height 2.79958)
    (gr_text "2.4 in" (at 69.598791 45.973999) (layer "B.SilkS"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 1))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "B.SilkS")
    (pts (xy 100.076 43.174419) (xy 100.253 80.836081))
    (height 4.81833)
    (gr_text "1.5 in" (at 95.346223 62.027895 270.2692733) (layer "B.SilkS"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 1))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 28.956 28.956)
        (xy 29.21 100.33)
        (xy 110.236 100.33)
        (xy 110.236 24.892)
        (xy 28.956 24.892)
      )
    )
  )
)
