(kicad_pcb (version 20171130) (host pcbnew 5.1.6)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 27)
    (zones 0)
    (modules 4)
    (nets 36)
  )
  (page A4)
  (title_block
    (date 2020-06-23)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J5-Pad10)")
  (net 3 "Net-(J5-Pad9)")
  (net 4 "Net-(J5-Pad7)")
  (net 5 "Net-(J5-Pad6)")
  (net 6 "Net-(J6-Pad10)")
  (net 7 "Net-(J6-Pad9)")
  (net 8 "Net-(J6-Pad2)")
  (net 9 "Net-(J6-Pad1)")
  (net 10 "Net-(J1-Pad12)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad13)")
  (net 13 "Net-(J1-Pad11)")
  (net 14 "Net-(J1-Pad1)")
  (net 15 "Net-(J8-Pad8)")
  (net 16 "Net-(J8-Pad4)")
  (net 17 "Net-(J8-Pad2)")
  (net 18 "Net-(J8-Pad7)")
  (net 19 "Net-(J8-Pad5)")
  (net 20 "Net-(J8-Pad3)")
  (net 21 "Net-(J8-Pad1)")
  (net 22 "Net-(J1-Pad10)")
  (net 23 "Net-(J1-Pad9)")
  (net 24 /COL_5_R)
  (net 25 /ROW_9_R)
  (net 26 /ROW_7_R)
  (net 27 /COL_6_R)
  (net 28 /ROW_8_R)
  (net 29 /ROW_6_R)
  (net 30 /ROW_3_L)
  (net 31 /COL_5_L)
  (net 32 /COL_6_L)
  (net 33 /ROW_5_L)
  (net 34 /ROW_2_L)
  (net 35 /ROW_4_L)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /COL_5_L)
    (add_net /COL_5_R)
    (add_net /COL_6_L)
    (add_net /COL_6_R)
    (add_net /ROW_2_L)
    (add_net /ROW_3_L)
    (add_net /ROW_4_L)
    (add_net /ROW_5_L)
    (add_net /ROW_6_R)
    (add_net /ROW_7_R)
    (add_net /ROW_8_R)
    (add_net /ROW_9_R)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad9)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad10)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad9)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J8-Pad5)")
    (add_net "Net-(J8-Pad7)")
    (add_net "Net-(J8-Pad8)")
  )
  (module kinx:39-53-2135 (layer F.Cu) (tedit 5EE5D146)
    (at 112.395 130.81 180)
    (descr "\"1.25 FPC CONN ASSY ZF 13\"")
    (fp_text reference J8 (at -12.827 -0.254 180) (layer F.SilkS) hide)
    (fp_text value THUMB_LEFT_BAK_KB600 (at -10.16 -3.81 180) (layer F.Fab) hide)
    (pad 12 thru_hole circle (at 6.25 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /ROW_2_L) (solder_mask_margin 0.0635))
    (pad 10 thru_hole circle (at 3.75 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /COL_6_L) (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.25 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J8-Pad8)") (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -1.25 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /ROW_3_L) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at -3.75 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J8-Pad4)") (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -6.25 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J8-Pad2)") (solder_mask_margin 0.0635))
    (pad 13 thru_hole circle (at 7.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /ROW_4_L) (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at 5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /ROW_5_L) (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /COL_5_L) (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at 0 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J8-Pad7)") (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -2.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J8-Pad5)") (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J8-Pad3)") (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -7.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J8-Pad1)") (solder_mask_margin 0.0635))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 98.171 135.509 270)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J5 (at -2.54 -22.987 180) (layer B.SilkS) hide)
    (fp_text value "THUMB\nLEFT\nBAK" (at -4.572 -0.127 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -11.43 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J5-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J5-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /ROW_3_L))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J5-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J5-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /COL_5_L))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /COL_6_L))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /ROW_5_L))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /ROW_2_L))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /ROW_4_L))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kinx:39-53-2135 (layer F.Cu) (tedit 5EE5D146)
    (at 137.795 130.81 180)
    (descr "\"1.25 FPC CONN ASSY ZF 13\"")
    (fp_text reference J1 (at 11.557 -0.254 180) (layer F.SilkS) hide)
    (fp_text value THUMB_RIGHT_SPC_KB600 (at -10.16 -3.81 180) (layer F.Fab) hide)
    (pad 12 thru_hole circle (at 6.25 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad12)") (solder_mask_margin 0.0635))
    (pad 10 thru_hole circle (at 3.75 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad10)") (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.25 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /COL_5_R) (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -1.25 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /ROW_9_R) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at -3.75 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /ROW_7_R) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -6.25 1.65 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (solder_mask_margin 0.0635))
    (pad 13 thru_hole circle (at 7.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad13)") (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at 5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad11)") (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad9)") (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at 0 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /COL_6_R) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -2.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /ROW_8_R) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /ROW_6_R) (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -7.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad1)") (solder_mask_margin 0.0635))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 151.13 135.509 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J6 (at 2.794 -23.749 180) (layer B.SilkS) hide)
    (fp_text value "THUMB\nRIGHT\nSPC" (at 4.699 0.127 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -11.43 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J6-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J6-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /COL_5_R))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /COL_6_R))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /ROW_9_R))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /ROW_8_R))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /ROW_7_R))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /ROW_6_R))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "kinx\nu6w5\nv2020-07-20" (at 148.209 131.318) (layer B.SilkS))
  (gr_line (start 154.305 138.176) (end 125.349 138.176) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.305 127) (end 125.349 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.206 138.176) (end 124.206 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.349 138.176) (end 125.349 127) (layer Edge.Cuts) (width 0.05))
  (gr_text "kinx\nu6w5\nv2020-07-20" (at 100.965 131.064) (layer B.SilkS))
  (gr_line (start 95.25 138.176) (end 124.206 138.176) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.305 138.176) (end 154.305 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.206 127) (end 95.25 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95.25 127) (end 95.25 138.176) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 123.952 138.049) (xy 95.377 138.049) (xy 95.377 127.127) (xy 123.952 127.127)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 123.952 138.049) (xy 95.377 138.049) (xy 95.377 127.127) (xy 123.952 127.127)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 154.051 138.049) (xy 125.476 138.049) (xy 125.476 127.127) (xy 154.051 127.127)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 154.051 138.049) (xy 125.476 138.049) (xy 125.476 127.127) (xy 154.051 127.127)
      )
    )
  )
)
