(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 70)
    (no_connects 0)
    (area 72.795001 43.655 159.444 95.012382)
    (thickness 1.6)
    (drawings 13)
    (tracks 140)
    (zones 0)
    (modules 5)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 104.14 73.025)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 D0)
  (net 2 D1)
  (net 3 D2)
  (net 4 D3)
  (net 5 D4)
  (net 6 D5)
  (net 7 D6)
  (net 8 D7)
  (net 9 DP)
  (net 10 "Net-(J1-Pad25)")
  (net 11 ATN)
  (net 12 BSY)
  (net 13 ACK)
  (net 14 MSG)
  (net 15 SEL)
  (net 16 CD)
  (net 17 REQ)
  (net 18 IO)
  (net 19 RST)
  (net 20 "Net-(J1-Pad26)")
  (net 21 "Net-(D1-Pad1)")
  (net 22 "Net-(U1-Pad5)")
  (net 23 GND)
  (net 24 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ACK)
    (add_net ATN)
    (add_net BSY)
    (add_net CD)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net DP)
    (add_net GND)
    (add_net IO)
    (add_net MSG)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(U1-Pad5)")
    (add_net REQ)
    (add_net RST)
    (add_net SEL)
    (add_net VCC)
  )
  (module Connectors_IDC:IDC-Header_2x25_Pitch2.54mm_Straight (layer F.Cu) (tedit 59DE12FA)
    (at 90.805 87.63 90)
    (descr "50 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J1 (at 1.27 -6.604 90) (layer F.SilkS))
    (fp_text value Conn_02x25_Odd_Even (at 1.27 67.564 90) (layer F.Fab))
    (fp_text user %R (at 1.27 30.48 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 D0))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 D1))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 D2))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 D3))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 D4))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 D5))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 D6))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 D7))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 DP))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 ATN))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 BSY))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 ACK))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 RST))
    (pad 41 thru_hole oval (at 0 50.8 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 42 thru_hole oval (at 2.54 50.8 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 MSG))
    (pad 43 thru_hole oval (at 0 53.34 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 44 thru_hole oval (at 2.54 53.34 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 SEL))
    (pad 45 thru_hole oval (at 0 55.88 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 46 thru_hole oval (at 2.54 55.88 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 CD))
    (pad 47 thru_hole oval (at 0 58.42 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 48 thru_hole oval (at 2.54 58.42 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 REQ))
    (pad 49 thru_hole oval (at 0 60.96 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 50 thru_hole oval (at 2.54 60.96 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 IO))
    (model ${KISYS3DMOD}/Connectors_IDC.3dshapes/IDC-Header_2x25_Pitch2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_DSub:DSUB-25_Female_Horizontal_Pitch2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm (layer F.Cu) (tedit 59F2C3AB)
    (at 104.14 68.58 180)
    (descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm")
    (fp_text reference J2 (at -16.62 -2.8 180) (layer F.SilkS))
    (fp_text value DB25_Female_MountingHoles (at -16.62 18.61 180) (layer F.Fab))
    (fp_text user %R (at -16.62 14.025 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 D0))
    (pad 2 thru_hole circle (at -2.77 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 D1))
    (pad 3 thru_hole circle (at -5.54 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 D2))
    (pad 4 thru_hole circle (at -8.31 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 D3))
    (pad 5 thru_hole circle (at -11.08 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 D4))
    (pad 6 thru_hole circle (at -13.85 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 D5))
    (pad 7 thru_hole circle (at -16.62 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 D6))
    (pad 8 thru_hole circle (at -19.39 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 D7))
    (pad 9 thru_hole circle (at -22.16 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 DP))
    (pad 10 thru_hole circle (at -24.93 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 11 thru_hole circle (at -27.7 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 12 thru_hole circle (at -30.47 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 13 thru_hole circle (at -33.24 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 14 thru_hole circle (at -1.385 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 15 thru_hole circle (at -4.155 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 16 thru_hole circle (at -6.925 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 VCC))
    (pad 17 thru_hole circle (at -9.695 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 IO))
    (pad 18 thru_hole circle (at -12.465 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 REQ))
    (pad 19 thru_hole circle (at -15.235 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 CD))
    (pad 20 thru_hole circle (at -18.005 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 SEL))
    (pad 21 thru_hole circle (at -20.775 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 MSG))
    (pad 22 thru_hole circle (at -23.545 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 RST))
    (pad 23 thru_hole circle (at -26.315 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 ACK))
    (pad 24 thru_hole circle (at -29.085 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 BSY))
    (pad 25 thru_hole circle (at -31.855 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 ATN))
    (pad 0 thru_hole circle (at -40.17 1.42 180) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 0 thru_hole circle (at 6.93 1.42 180) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 23 GND))
    (model ${KISYS3DMOD}/Connectors_DSub.3dshapes/DSUB-25_Female_Horizontal_Pitch2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 118.6815 76.3905)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 3.81 -2.41) (layer F.SilkS))
    (fp_text value D (at 3.81 2.41) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 DP))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 106.045 72.39 270)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33 270) (layer F.SilkS))
    (fp_text value 74LS280 (at 3.81 17.57 270) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 D6))
    (pad 8 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 D0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 D7))
    (pad 9 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 D1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 D2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 11 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 D3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 D4))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 D5))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A98260A)
    (at 111.125 78.105 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 1.778 2.667 90) (layer F.SilkS))
    (fp_text value C (at 1.25 2.56 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Quartermaster\nParity Generator\nFor Lt. Kernal" (at 88.9 65.405 90) (layer F.Mask))
  (gr_text "SCSI Device" (at 139.7 79.375) (layer F.SilkS))
  (gr_text "Lt. Kernal" (at 139.7 73.025) (layer F.SilkS))
  (gr_text "(c) 2018 David Wood" (at 154.94 69.85 90) (layer F.Mask))
  (gr_text "Lieutenant Kernal\nDB25 only!" (at 104.902 61.849) (layer B.Mask))
  (gr_line (start 157.48 91.44) (end 157.48 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 91.44) (end 157.48 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 89.535) (end 85.09 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 33.02 (width 0.3) (layer Dwgs.User)
    (gr_text "33.020 mm" (at 79.295 74.93 270) (layer Dwgs.User))
    (feature1 (pts (xy 84.455 91.44) (xy 77.945 91.44)))
    (feature2 (pts (xy 84.455 58.42) (xy 77.945 58.42)))
    (crossbar (pts (xy 80.645 58.42) (xy 80.645 91.44)))
    (arrow1a (pts (xy 80.645 91.44) (xy 80.058579 90.313496)))
    (arrow1b (pts (xy 80.645 91.44) (xy 81.231421 90.313496)))
    (arrow2a (pts (xy 80.645 58.42) (xy 80.058579 59.546504)))
    (arrow2b (pts (xy 80.645 58.42) (xy 81.231421 59.546504)))
  )
  (dimension 72.39 (width 0.3) (layer Dwgs.User)
    (gr_text "72.390 mm" (at 121.285 45.005) (layer Dwgs.User))
    (feature1 (pts (xy 157.48 49.53) (xy 157.48 43.655)))
    (feature2 (pts (xy 85.09 49.53) (xy 85.09 43.655)))
    (crossbar (pts (xy 85.09 46.355) (xy 157.48 46.355)))
    (arrow1a (pts (xy 157.48 46.355) (xy 156.353496 46.941421)))
    (arrow1b (pts (xy 157.48 46.355) (xy 156.353496 45.768579)))
    (arrow2a (pts (xy 85.09 46.355) (xy 86.216504 46.941421)))
    (arrow2b (pts (xy 85.09 46.355) (xy 86.216504 45.768579)))
  )
  (gr_line (start 157.48 58.42) (end 157.48 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 58.42) (end 157.48 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 89.535) (end 85.09 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 23) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 91.44) (xy 85.09 91.44) (xy 85.09 58.42) (xy 157.48 58.42)
      )
    )
  )
  (zone (net 23) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 91.44) (xy 85.09 91.44) (xy 85.09 58.42) (xy 157.48 58.42)
      )
    )
  )
)
