<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="54.9148" y1="61.214" x2="14.7215125" y2="61.278784375" width="0.4064" layer="20"/>
<wire x1="14.7215125" y1="61.278784375" x2="13.84445625" y2="60.402271875" width="0.4064" layer="20" curve="90.103392"/>
<wire x1="13.84445625" y1="60.402271875" x2="13.91725625" y2="16.513425" width="0.4064" layer="20"/>
<wire x1="13.91725625" y1="16.513425" x2="15.0908875" y2="15.3416" width="0.4064" layer="20" curve="89.905107"/>
<wire x1="15.0908875" y1="15.3416" x2="67.599421875" y2="15.3416" width="0.4064" layer="20"/>
<wire x1="67.599421875" y1="15.3416" x2="68.50099375" y2="16.246284375" width="0.4064" layer="20" curve="90.197404"/>
<wire x1="68.50099375" y1="16.246284375" x2="68.354559375" y2="60.313421875" width="0.4064" layer="20"/>
<wire x1="68.354559375" y1="60.313421875" x2="67.461075" y2="61.204" width="0.4064" layer="20" curve="89.809626"/>
<wire x1="67.461075" y1="61.204" x2="57.4648" y2="61.204" width="0.4064" layer="20"/>
<wire x1="57.4648" y1="61.204" x2="54.9148" y2="61.214" width="0.4064" layer="20"/>
<text>Heartbeat</text>
<text>Error</text>
<text>Programming</text>
<text>GND</text>
<text>MOSI</text>
<text>VCC</text>
<text>Reset</text>
<text>SCK</text>
<text>MISO</text>
<text>  ATTiny 
13-45-85</text>
<text>   ATTiny 
24-44-84</text>
<text>   ATTiny 
2313-4313</text>
<text>ATTiny Programming Shield</text>
<text>Rev A</text>
<text>ISP</text>
<wire x1="54.59489375" y1="51.4107" x2="54.6081375" y2="57.5558" width="0.4064" layer="20"/>
<wire x1="54.6081375" y1="57.5558" x2="53.745784375" y2="58.42" width="0.4064" layer="20" curve="90.123539"/>
<wire x1="53.745784375" y1="58.42" x2="45.22334375" y2="58.42" width="0.4064" layer="20"/>
<wire x1="45.22334375" y1="58.42" x2="44.448334375" y2="57.64715" width="0.4064" layer="20" curve="89.840129"/>
<wire x1="44.448334375" y1="57.64715" x2="44.43460625" y2="51.2773" width="0.4064" layer="20"/>
<wire x1="44.43460625" y1="51.2773" x2="49.09350625" y2="47.371" width="0.4064" layer="20" curve="90.123501"/>
<wire x1="49.09350625" y1="47.371" x2="49.83438125" y2="47.371" width="0.4064" layer="20"/>
<wire x1="49.83438125" y1="47.371" x2="54.59489375" y2="51.4107" width="0.4064" layer="20" curve="89.884809"/>
<text>RX  TX</text>
<text>CutOut</text>
<wire x1="45.72" y1="58.7756" x2="45.72" y2="60.0964" width="0.254" layer="20"/>
<wire x1="45.72" y1="60.0964" x2="46.6852" y2="60.0964" width="0.254" layer="20"/>
<wire x1="45.72" y1="58.7502" x2="45.3644" y2="59.6138" width="0.254" layer="20"/>
<wire x1="45.72" y1="58.7248" x2="46.0502" y2="59.5884" width="0.254" layer="20"/>
<wire x1="52.578" y1="60.0964" x2="53.3654" y2="60.0964" width="0.254" layer="20"/>
<wire x1="53.3654" y1="60.0964" x2="53.3654" y2="58.7756" width="0.254" layer="20"/>
<wire x1="53.3654" y1="58.7756" x2="53.6956" y2="59.6392" width="0.254" layer="20"/>
<wire x1="53.6956" y1="59.6392" x2="53.3908" y2="58.7756" width="0.254" layer="20"/>
<wire x1="53.3654" y1="58.7756" x2="53.0352" y2="59.6392" width="0.254" layer="20"/>
<text>RV-Project.Com</text>
<text>1. Connect shield to Arduino UNO.
2. Set "Arduino as ISP" on IDE.
3. Set ATTiny MCU, as well as speed.
4. Set port for Arduino UNO.</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="1206-CAP">
</package>
<package name="SMD_ELECTROLYTIC_3.5MMDIA">
</package>
<package name="LED3MM-NS">
<description>&lt;h3&gt;LED 3MM - No Silk&lt;/h3&gt;
3 mm, round</description>
</package>
<package name="1206-RES">
</package>
<package name="DIL14">
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="DIL20">
</package>
<package name="ART_CHEROKEE_LARGE">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_ROUND">
</package>
<package name="1X06_NO_SILK">
</package>
<package name="2X3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="a-lib" package="1206-CAP" value=".1uF"/>
<element name="C2" library="a-lib" package="SMD_ELECTROLYTIC_3.5MMDIA" value="SMD_ELECTROLYTIC10UF_16V"/>
<element name="JP1" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="a-lib" package="LED3MM-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="a-lib" package="LED3MM-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="a-lib" package="LED3MM-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="1K"/>
<element name="R2" library="a-lib" package="1206-RES" value="1K"/>
<element name="R3" library="a-lib" package="1206-RES" value="1K"/>
<element name="U1" library="a-lib" package="DIL14" value="ATTINY84"/>
<element name="U2" library="a-lib" package="DIP08" value="TINY85-20-DIP">
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="U3" library="a-lib" package="DIL20" value="ATTINY4313"/>
<element name="LOGO1" library="a-lib" package="ART_CHEROKEE_LARGE" value="Cherokee Large"/>
<element name="C3" library="a-lib" package="1206-CAP" value=".1uF"/>
<element name="C4" library="a-lib" package="1206-CAP" value=".1uF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U3" pad="1"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="U3" pad="20"/>
<contactref element="JP3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="9"/>
<contactref element="U2" pad="7"/>
<contactref element="U3" pad="19"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="5"/>
<contactref element="U3" pad="17"/>
<contactref element="U1" pad="7"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="6"/>
<contactref element="U3" pad="18"/>
<contactref element="U1" pad="8"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="U3" pad="10"/>
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="14"/>
<contactref element="JP3" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="4"/>
<contactref element="C2" pad="P$1"/>
<contactref element="JP2" pad="5"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED1" pad="K"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="1"/>
<contactref element="C2" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="LED3" pad="A"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="JP1" pad="8"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="JP1" pad="7"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP4" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$6">
</signal>
</signals>
</board>
</drawing>
</eagle>
