(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 16)
    (no_connects 0)
    (area 153.594999 95.174999 179.145001 115.645001)
    (thickness 1.6)
    (drawings 21)
    (tracks 36)
    (zones 0)
    (modules 3)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad4)")
  (net 5 "Net-(P1-Pad5)")
  (net 6 "Net-(P1-Pad6)")
  (net 7 "Net-(P1-Pad7)")
  (net 8 /VCC)
  (net 9 "Net-(P2-Pad1)")
  (net 10 "Net-(P2-Pad2)")
  (net 11 "Net-(P2-Pad3)")
  (net 12 "Net-(P2-Pad4)")
  (net 13 "Net-(P2-Pad5)")
  (net 14 "Net-(P2-Pad6)")
  (net 15 "Net-(P2-Pad7)")
  (net 16 /GND)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /GND)
    (add_net /VCC)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
  )
  (module esp-12s:ESP-12 (layer F.Cu) (tedit 592B6773)
    (at 159.482 100.267)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference ESP-12 (at 6.9 7.3) (layer F.SilkS))
    (fp_text value ESP-12 (at 6.992 1) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.CrtYd))
    (pad 1 smd rect (at 0 0) (size 2.6 1.1) (drill (offset -1 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 0 2) (size 2.6 1.1) (drill (offset -1 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 0 4) (size 2.6 1.1) (drill (offset -1 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 0 6) (size 2.6 1.1) (drill (offset -1 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 0 8) (size 2.6 1.1) (drill (offset -1 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (pad 6 smd rect (at 0 10) (size 2.6 1.1) (drill (offset -1 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad6)"))
    (pad 7 smd rect (at 0 12) (size 2.6 1.1) (drill (offset -1 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (pad 8 smd rect (at 0 14) (size 2.6 1.1) (drill (offset -1 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 /VCC))
    (pad 9 smd rect (at 14 14) (size 2.6 1.1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask)
      (net 16 /GND))
    (pad 10 smd rect (at 14 12) (size 2.6 1.1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P2-Pad7)"))
    (pad 11 smd rect (at 14 10) (size 2.6 1.1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P2-Pad6)"))
    (pad 12 smd rect (at 14 8) (size 2.6 1.1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P2-Pad5)"))
    (pad 13 smd rect (at 14 6) (size 2.6 1.1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P2-Pad4)"))
    (pad 14 smd rect (at 14 4) (size 2.6 1.1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P2-Pad3)"))
    (pad 15 smd rect (at 14 2) (size 2.6 1.1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 16 smd rect (at 14 0) (size 2.6 1.1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P2-Pad1)"))
    (model ${KIPRJMOD}/libraries/esp8266/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
  )
  (module headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 592B5CD0)
    (at 177.8 96.52)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 592B5CD0)
    (at 154.94 96.52)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text GND (at 176.403 114.3 90) (layer F.SilkS))
  (gr_text 15 (at 176.403 111.76 90) (layer F.SilkS))
  (gr_text 2 (at 176.403 109.22 90) (layer F.SilkS))
  (gr_text 0 (at 176.403 106.68 90) (layer F.SilkS))
  (gr_text 4 (at 176.403 104.14 90) (layer F.SilkS))
  (gr_text 5 (at 176.403 101.6 90) (layer F.SilkS))
  (gr_text RX (at 176.403 99.06 90) (layer F.SilkS))
  (gr_text TX (at 176.403 96.52 90) (layer F.SilkS))
  (gr_text VCC (at 156.464 114.3 270) (layer F.SilkS))
  (gr_text 13 (at 156.464 111.76 270) (layer F.SilkS))
  (gr_text 12 (at 156.464 109.22 270) (layer F.SilkS))
  (gr_text 14 (at 156.464 106.68 270) (layer F.SilkS))
  (gr_text 16 (at 156.464 104.14 270) (layer F.SilkS))
  (gr_text EN (at 156.464 101.6 270) (layer F.SilkS))
  (gr_text A (at 156.464 99.06 270) (layer F.SilkS))
  (gr_text RST (at 156.464 96.52 270) (layer F.SilkS))
  (dimension 22.86 (width 0.3) (layer Margin)
    (gr_text "0.9000 in" (at 166.37 120.73) (layer Margin))
    (feature1 (pts (xy 177.8 114.3) (xy 177.8 122.08)))
    (feature2 (pts (xy 154.94 114.3) (xy 154.94 122.08)))
    (crossbar (pts (xy 154.94 119.38) (xy 177.8 119.38)))
    (arrow1a (pts (xy 177.8 119.38) (xy 176.673496 119.966421)))
    (arrow1b (pts (xy 177.8 119.38) (xy 176.673496 118.793579)))
    (arrow2a (pts (xy 154.94 119.38) (xy 156.066504 119.966421)))
    (arrow2b (pts (xy 154.94 119.38) (xy 156.066504 118.793579)))
  )
  (gr_line (start 153.67 115.57) (end 153.67 95.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.07 115.57) (end 153.67 115.57) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.07 95.25) (end 179.07 115.57) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 95.25) (end 179.07 95.25) (layer Edge.Cuts) (width 0.15))
)
