(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 62)
    (no_connects 1)
    (area 137.084999 79.680999 169.239001 115.391001)
    (thickness 1.6)
    (drawings 26)
    (tracks 410)
    (zones 0)
    (modules 18)
    (nets 41)
  )
  (page A4)
  (title_block
    (title gbReROM)
    (date 2016-12-17)
    (rev 0.01)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 SERIAL_IN)
  (net 4 SHIFT_REG_CLK)
  (net 5 ~MASTER_RESET)
  (net 6 STO_REG_CLK)
  (net 7 ~OUTPUT_EN)
  (net 8 "Net-(U1-Pad9)")
  (net 9 "Net-(U2-Pad9)")
  (net 10 WE#)
  (net 11 OE#)
  (net 12 CE#)
  (net 13 Q0)
  (net 14 Q1)
  (net 15 Q2)
  (net 16 Q3)
  (net 17 Q4)
  (net 18 Q5)
  (net 19 Q6)
  (net 20 Q7)
  (net 21 A1)
  (net 22 A2)
  (net 23 A3)
  (net 24 A4)
  (net 25 A5)
  (net 26 A6)
  (net 27 A7)
  (net 28 A0)
  (net 29 A9)
  (net 30 A10)
  (net 31 A11)
  (net 32 A12)
  (net 33 A13)
  (net 34 A14)
  (net 35 A15)
  (net 36 A8)
  (net 37 A17)
  (net 38 A18)
  (net 39 A16)
  (net 40 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A16)
    (add_net A17)
    (add_net A18)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net CE#)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad9)")
    (add_net OE#)
    (add_net Q0)
    (add_net Q1)
    (add_net Q2)
    (add_net Q3)
    (add_net Q4)
    (add_net Q5)
    (add_net Q6)
    (add_net Q7)
    (add_net SERIAL_IN)
    (add_net SHIFT_REG_CLK)
    (add_net STO_REG_CLK)
    (add_net WE#)
    (add_net ~MASTER_RESET)
    (add_net ~OUTPUT_EN)
  )
  (net_class PWR ""
    (clearance 0.3)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module 3M3221B1CT-ND (layer F.Cu) (tedit 5855E0E3)
    (at 150.622 97.79 270)
    (fp_text reference U4 (at 5.4356 -6.6802 360) (layer F.SilkS))
    (fp_text value MX29F040C (at 0.508 1.4605 270) (layer F.Fab) hide)
    (pad 5 smd rect (at -5.334 -5.08) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 27 A7))
    (pad 7 smd rect (at -5.334 -2.54) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 25 A5))
    (pad 6 smd rect (at -5.334 -3.81) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 26 A6))
    (pad 8 smd rect (at -5.334 -1.27) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 24 A4))
    (pad 11 smd rect (at -5.334 2.54) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 21 A1))
    (pad 9 smd rect (at -5.334 0) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 23 A3))
    (pad 10 smd rect (at -5.334 1.27) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 22 A2))
    (pad 12 smd rect (at -5.334 3.81) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 28 A0))
    (pad 13 smd rect (at -5.334 5.08) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 13 Q0))
    (pad 15 smd rect (at -2.54 6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 15 Q2))
    (pad 16 smd rect (at -1.27 6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -3.81 6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 14 Q1))
    (pad 17 smd rect (at 0 6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 16 Q3))
    (pad 19 smd rect (at 2.54 6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 18 Q5))
    (pad 18 smd rect (at 1.27 6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 17 Q4))
    (pad 20 smd rect (at 3.81 6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 19 Q6))
    (pad 21 smd rect (at 5.334 5.08) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 20 Q7))
    (pad 22 smd rect (at 5.334 3.81) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 12 CE#))
    (pad 24 smd rect (at 5.334 1.27) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 11 OE#))
    (pad 25 smd rect (at 5.334 0) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 31 A11))
    (pad 23 smd rect (at 5.334 2.54) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 30 A10))
    (pad 26 smd rect (at 5.334 -1.27) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 29 A9))
    (pad 28 smd rect (at 5.334 -3.81) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 33 A13))
    (pad 27 smd rect (at 5.334 -2.54) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 36 A8))
    (pad 29 smd rect (at 5.334 -5.08) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 34 A14))
    (pad 30 smd rect (at 3.81 -6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 37 A17))
    (pad 32 smd rect (at 1.27 -6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 31 smd rect (at 2.54 -6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 10 WE#))
    (pad 1 smd rect (at 0 -6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 38 A18))
    (pad 4 smd rect (at -3.81 -6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 32 A12))
    (pad 2 smd rect (at -1.27 -6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 39 A16))
    (pad 3 smd rect (at -2.54 -6.604 270) (size 0.7 1.91) (layers F.Cu F.Paste F.Mask)
      (net 35 A15))
  )
  (module w_pin_strip:pin_socket_3 (layer F.Cu) (tedit 58558B62)
    (at 138.684 109.22 90)
    (descr "Pin socket 3pin")
    (tags "CONN DEV")
    (fp_text reference K1 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_3 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 WE#))
    (pad 2 thru_hole oval (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 OE#))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 CE#))
    (model walter/pin_strip/pin_socket_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_8 (layer F.Cu) (tedit 58558B65)
    (at 138.684 95.25 90)
    (descr "Pin socket 8pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at 0 -2.159 180) (layer F.SilkS) hide)
    (fp_text value CONN_8 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -8.89 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 20 Q7))
    (pad 2 thru_hole oval (at -6.35 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 19 Q6))
    (pad 3 thru_hole oval (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 18 Q5))
    (pad 4 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 17 Q4))
    (pad 5 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 Q3))
    (pad 6 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 Q2))
    (pad 7 thru_hole oval (at 6.35 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 Q1))
    (pad 8 thru_hole oval (at 8.89 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 Q0))
    (model walter/pin_strip/pin_socket_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 58557A6E)
    (at 138.684 81.28 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P2 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 58557A70)
    (at 138.684 83.82 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P3 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 58558B75)
    (at 167.64 91.44 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P4 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 SERIAL_IN))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 58558B6B)
    (at 167.64 83.82 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P5 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 SHIFT_REG_CLK))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 58558B67)
    (at 167.64 81.28 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P6 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 ~MASTER_RESET))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 58558B6D)
    (at 167.64 86.36 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P7 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 STO_REG_CLK))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 58558B71)
    (at 167.64 88.9 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P8 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 ~OUTPUT_EN))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:so-16 (layer F.Cu) (tedit 58558B1C)
    (at 154.305 84.455)
    (descr SO-16)
    (fp_text reference U1 (at 5.715 -0.254 90) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 0.254) (layer F.SilkS))
    (pad 1 smd rect (at -4.445 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 21 A1))
    (pad 2 smd rect (at -3.175 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 22 A2))
    (pad 3 smd rect (at -1.905 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 23 A3))
    (pad 4 smd rect (at -0.635 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 24 A4))
    (pad 5 smd rect (at 0.635 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 25 A5))
    (pad 6 smd rect (at 1.905 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 26 A6))
    (pad 7 smd rect (at 3.175 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 27 A7))
    (pad 8 smd rect (at 4.445 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 4.445 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 3.175 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 5 ~MASTER_RESET))
    (pad 11 smd rect (at 1.905 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 4 SHIFT_REG_CLK))
    (pad 12 smd rect (at 0.635 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 6 STO_REG_CLK))
    (pad 13 smd rect (at -0.635 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 7 ~OUTPUT_EN))
    (pad 14 smd rect (at -1.905 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 3 SERIAL_IN))
    (pad 15 smd rect (at -3.175 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 28 A0))
    (pad 16 smd rect (at -4.445 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model walter/smd_dil/so-16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:so-16 (layer F.Cu) (tedit 58558B23)
    (at 165.1 99.06 270)
    (descr SO-16)
    (fp_text reference U2 (at 5.715 0 360) (layer F.SilkS))
    (fp_text value 74HC595 (at 0.9525 0.0635 270) (layer F.SilkS))
    (pad 1 smd rect (at -4.445 2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 35 A15))
    (pad 2 smd rect (at -3.175 2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 39 A16))
    (pad 3 smd rect (at -1.905 2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 38 A18))
    (pad 4 smd rect (at -0.635 2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 37 A17))
    (pad 5 smd rect (at 0.635 2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 34 A14))
    (pad 6 smd rect (at 1.905 2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 36 A8))
    (pad 7 smd rect (at 3.175 2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 33 A13))
    (pad 8 smd rect (at 4.445 2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 4.445 -2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 3.175 -2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 5 ~MASTER_RESET))
    (pad 11 smd rect (at 1.905 -2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 4 SHIFT_REG_CLK))
    (pad 12 smd rect (at 0.635 -2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 6 STO_REG_CLK))
    (pad 13 smd rect (at -0.635 -2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 7 ~OUTPUT_EN))
    (pad 14 smd rect (at -1.905 -2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad9)"))
    (pad 15 smd rect (at -3.175 -2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 32 A12))
    (pad 16 smd rect (at -4.445 -2.794 270) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model walter/smd_dil/so-16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:so-16 (layer F.Cu) (tedit 58558B92)
    (at 154.686 110.998)
    (descr SO-16)
    (fp_text reference U3 (at 5.6388 0.1524 90) (layer F.SilkS))
    (fp_text value 74HC595 (at 0.1524 0.3556) (layer F.SilkS))
    (pad 1 smd rect (at -4.445 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 31 A11))
    (pad 2 smd rect (at -3.175 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 30 A10))
    (pad 3 smd rect (at -1.905 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.635 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0.635 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.905 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.175 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 4.445 2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 4.445 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 3.175 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 5 ~MASTER_RESET))
    (pad 11 smd rect (at 1.905 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 4 SHIFT_REG_CLK))
    (pad 12 smd rect (at 0.635 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 6 STO_REG_CLK))
    (pad 13 smd rect (at -0.635 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 7 ~OUTPUT_EN))
    (pad 14 smd rect (at -1.905 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U2-Pad9)"))
    (pad 15 smd rect (at -3.175 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 29 A9))
    (pad 16 smd rect (at -4.445 -2.794) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model walter/smd_dil/so-16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 5855E0AD)
    (at 147.955 82.55 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C1 (at -0.254 -1.651 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0.9906 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 5855DFF9)
    (at 162.433 91.313 270)
    (descr "SMT capacitor, 0805")
    (fp_text reference C2 (at -2.413 -0.127 360) (layer F.SilkS))
    (fp_text value 100n (at 0 0.9906 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 270) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -0.9525 0 270) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 58558BE1)
    (at 147.828 110.49 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C3 (at -2.4638 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0.9906 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0805 (layer F.Cu) (tedit 58558BC3)
    (at 166.116 109.982 180)
    (descr "SMD LED, 0805")
    (fp_text reference D1 (at 0 1.524 360) (layer F.SilkS))
    (fp_text value LED (at 0.1016 1.6256 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_leds/led_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0805 (layer F.Cu) (tedit 5855E0BD)
    (at 166.116 112.014 180)
    (descr "SMT resistor, 0805")
    (fp_text reference R1 (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value 330R (at 0 0.9906 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad1)"))
    (model walter/smd_resistors/r_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 169.164 115.316) (end 169.164 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 115.316) (end 169.164 115.316) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 113.284) (end 137.16 115.316) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 79.756) (end 137.16 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.716 79.756) (end 137.16 79.756) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text DS (at 165.354 91.44) (layer F.SilkS))
  (gr_text ~OE (at 165.227 88.9) (layer F.SilkS))
  (gr_text STCP (at 164.719 86.36) (layer F.SilkS))
  (gr_text SHCP (at 164.592 83.947) (layer F.SilkS))
  (gr_text ~MR (at 165.1 81.407) (layer F.SilkS))
  (gr_text VCC (at 141.478 81.28) (layer F.SilkS))
  (gr_text GND (at 141.478 83.82) (layer F.SilkS))
  (gr_text Q0 (at 141.224 86.36) (layer F.SilkS))
  (gr_text Q7 (at 144.272 107.95) (layer F.SilkS))
  (gr_text ~WE (at 141.224 112.014) (layer F.SilkS))
  (gr_text "~OE\n" (at 141.224 109.982) (layer F.SilkS))
  (gr_text ~CE (at 141.224 107.95) (layer F.SilkS))
  (gr_text ROM (at 150.622 97.79) (layer F.SilkS))
  (gr_text "gbReROM\nrel/2016-12\nrev0.01" (at 152.4 91.694 90) (layer B.SilkS))
  (gr_line (start 169.164 79.756) (end 169.164 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.716 79.756) (end 169.164 79.756) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.164 115.316) (xy 137.16 115.316) (xy 137.16 79.756) (xy 169.164 79.756)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.164 115.316) (xy 137.16 115.316) (xy 137.16 79.756) (xy 169.164 79.756)
      )
    )
  )
)
