(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 230 130)
		(grid_origin 230 130)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "./gerbers")
		)
	)
	(net 0 "")
	(net 1 "+BATT")
	(net 2 "Net-(an1--)")
	(net 3 "Net-(an1-+)")
	(net 4 "-BATT")
	(net 5 "anodes")
	(net 6 "Net-(cath1-+)")
	(net 7 "Net-(R2-Pad1)")
	(net 8 "Net-(R1-Pad2)")
	(net 9 "Net-(cath1--)")
	(net 10 "cathodes")
	(net 11 "GND")
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 231.2 140.7 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0.05 1.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "47nF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.862501 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.862501 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 234.025 140.7 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RF2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "560"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(cath1--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "cathodes")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:LED_D5.0mm-T1_34"
		(layer "F.Cu")
		(at 235.334 126.9266 30)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
		(tags "LED diameter 5.0mm 2 pins")
		(property "Reference" "D3"
			(at 0 -3.96 30)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3"
			(at -2.0734 3.166 120)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.02 0 30)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -1.27 0 30)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "cathodes")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 30)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "anodes")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:LED_D5.0mm-T1_34"
		(layer "F.Cu")
		(at 224.666 126.9266 150)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
		(tags "LED diameter 5.0mm 2 pins")
		(property "Reference" "D7"
			(at 0 -3.96 150)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "7"
			(at -2.1734 -3.165999 60)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 150)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.02 0 150)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -1.27 0 150)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "cathodes")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 150)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "anodes")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 227.575 119.325 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at -0.425 1.425 90)
			(layer "F.SilkS")
		)
		(property "Value" "47nF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.862501 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "-BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.862501 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 226.75 140.75)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -2.25 0.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "560"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "-BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 225.75 138 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0.75 -1.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "560"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(R2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:PostHole_4.05mm"
		(layer "F.Cu")
		(at 238 122)
		(descr "Mounting Hole 2.7mm, M2.5")
		(tags "mounting hole 2.7mm m2.5")
		(property "Reference" "H2"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 4.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 231.25 118.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "47nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.862501 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.862501 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 240.25 133.75 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RA1"
			(at 3.5 -1 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "Net-(an1-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 11 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 236.75 141.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RG2"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "560"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(cath1--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:LED_D5.0mm-T1_34"
		(layer "F.Cu")
		(at 230 123.8532 90)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
		(tags "LED diameter 5.0mm 2 pins")
		(property "Reference" "D2"
			(at 0 -3.96 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2"
			(at 3.8532 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.02 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -1.27 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "cathodes")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "anodes")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:PostHole_4.05mm"
		(layer "F.Cu")
		(at 238 138)
		(descr "Mounting Hole 2.7mm, M2.5")
		(tags "mounting hole 2.7mm m2.5")
		(property "Reference" "H4"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 4.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 226 121.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RF1"
			(at 1 9.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "560"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(an1--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "anodes")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:LED_D5.0mm-T1_34"
		(layer "F.Cu")
		(at 230 136.1468 -90)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
		(tags "LED diameter 5.0mm 2 pins")
		(property "Reference" "D5"
			(at 0 -3.96 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5"
			(at -1.7532 3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.02 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -1.27 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "cathodes")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "anodes")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:LED_D5.0mm-T1_34"
		(layer "F.Cu")
		(at 230 130 90)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
		(tags "LED diameter 5.0mm 2 pins")
		(property "Reference" "D1"
			(at 0 -3.96 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1"
			(at 0 3.96 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.02 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -1.27 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "cathodes")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "anodes")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 224.25 118.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RG1"
			(at -3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "560"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(an1--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:PostHole_4.05mm"
		(layer "F.Cu")
		(at 222 122)
		(descr "Mounting Hole 2.7mm, M2.5")
		(tags "mounting hole 2.7mm m2.5")
		(property "Reference" "H1"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 4.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "kicad-mza:LED_D5.0mm-T1_34"
		(layer "F.Cu")
		(at 224.666 133.0734 -150)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
		(tags "LED diameter 5.0mm 2 pins")
		(property "Reference" "D6"
			(at 0 -3.96 30)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6"
			(at 1.8734 -3.175 120)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.02 0 210)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -1.27 0 210)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "cathodes")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 210)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "anodes")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:LED_D5.0mm-T1_34"
		(layer "F.Cu")
		(at 235.334 133.0734 -30)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
		(tags "LED diameter 5.0mm 2 pins")
		(property "Reference" "D4"
			(at 0 -3.96 150)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4"
			(at 1.8234 3.166001 60)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 150)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.02 0 330)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -1.27 0 330)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "cathodes")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 330)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "anodes")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:PostHole_4.05mm"
		(layer "F.Cu")
		(at 222 138)
		(descr "Mounting Hole 2.7mm, M2.5")
		(tags "mounting hole 2.7mm m2.5")
		(property "Reference" "H3"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 4.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 221.5 132 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "Ca1"
			(at -2 6.668084 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "6.8uF"
			(at 0 -1.679999 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 11 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "-BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:MMCX_Molex_73415-1471_Vertical"
		(layer "B.Cu")
		(at 240.15 130.05)
		(descr "http://www.molex.com/pdm_docs/sd/734151471_sd.pdf")
		(tags "Molex MMCX Coaxial Connector 50 ohms Female Jack Vertical THT")
		(property "Reference" "in1"
			(at 0 3.0368 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 -2.794 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "F&B.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(an1-+)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1.27 -1.27)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "F&B.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1.27 1.27)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "F&B.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 -1.27)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "F&B.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 1.27)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "F&B.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/MMCX_Molex_73415-1471_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "B.Cu")
		(at 234.25 136.25 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.25 90)
			(layer "B.SilkS")
		)
		(property "Value" "47nF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.862501 0 90)
			(size 1.075 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "-BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.862501 0 90)
			(size 1.075 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "B.Cu")
		(at 227.75 120.5 90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "an1"
			(at 0.5 2.25 90)
			(layer "B.SilkS")
		)
		(property "Value" "LMH6702MF"
			(at 0 -2.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6702.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "anodes")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "-BATT")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(an1-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(an1--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+BATT")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 221.5 128 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "Ca2"
			(at 1 6.418084 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "6.8uF"
			(at 0 -1.679999 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 11 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:molex-mini-fit-jr-3pos-right-angle-or-16AWG"
		(layer "B.Cu")
		(at 219.55 130 90)
		(property "Reference" "pow1"
			(at 9.2456 -8.7417 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x03_Male"
			(at 0 -15 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at -4.2 -7.3 90)
			(size 1.524 1.524)
			(drill 3.05)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 4.2 -7.3 90)
			(size 1.524 1.524)
			(drill 3.05)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at 4.058999 -0.141 90)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -0.141 90)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4.058999 -0.141 90)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "-BATT")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "B.Cu")
		(at 233.25 140.25 -90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "cath1"
			(at 0 2.5 90)
			(layer "B.SilkS")
		)
		(property "Value" "LMH6702MF"
			(at 0 -2.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6702.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "cathodes")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "-BATT")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(cath1-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(cath1--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+BATT")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:Potentiometer_Bourns_3224G_Horizontal"
		(layer "B.Cu")
		(at 226.75 138.75 90)
		(descr "Potentiometer, horizontal, Bourns 3224G, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
		(tags "Potentiometer horizontal Bourns 3224G")
		(property "Reference" "cat1"
			(at 0.610001 -5.455 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "2k"
			(at 0 -3.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/")
		(sheetfile "shichi-16mm.revC.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 2.6 1.15 90)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "Net-(R1-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.600001 0 90)
			(size 1.3 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "Net-(cath1-+)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.6 -1.15 90)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "Net-(R2-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224G_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 241 117.5) (xy 242.5 119) (xy 242.5 141) (xy 241 142.5) (xy 219 142.5) (xy 217.5 141) (xy 217.5 119)
			(xy 219 117.5)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "shichi"
		(at 241.5 125.25 90)
		(layer "F.SilkS")
	)
	(gr_text "revC"
		(at 241.5 120.5 90)
		(layer "F.SilkS")
	)
	(gr_text "mza"
		(at 241.25 137.5 90)
		(layer "F.SilkS")
	)
	(gr_text "2025-09-22"
		(at 232 126.25 90)
		(layer "B.SilkS")
	)
	(gr_text "IDL_25_008"
		(at 227.75 128 90)
		(layer "B.SilkS")
	)
	(zone
		(net 11)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2032)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 216 116) (xy 244 116) (xy 244 144) (xy 216 144)
			)
		)
	)
	(zone
		(net 10)
		(net_name "cathodes")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2032)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 235.25 127) (xy 235.25 133) (xy 230 136) (xy 224.75 133) (xy 224.75 127) (xy 230 124)
			)
		)
	)
	(zone
		(net 5)
		(net_name "anodes")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2032)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 230 120) (xy 221.75 125) (xy 221.75 134.75) (xy 230 140) (xy 238.5 135.25) (xy 238.75 125)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+BATT")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2032)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 217 116.75) (xy 243.25 116.75) (xy 243.25 143.25) (xy 217 143.25)
			)
		)
	)
	(zone
		(net 4)
		(net_name "-BATT")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads thru_hole_only
			(clearance 0.2)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 215 115) (xy 245 115) (xy 245 145) (xy 215 145)
			)
		)
	)
	(embedded_fonts no)
)
