(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Beetje 32U4 Blok")
    (date "2018-08-10")
    (rev "0.0")
    (company "www.MakersBox.us")
    (comment 1 "648.ken@gmail.com")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0000080_7ffffffe)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "/10")
  (net 2 "/04")
  (net 3 "/05")
  (net 4 "/06")
  (net 5 "/07")
  (net 6 "/08")
  (net 7 "/09")
  (net 8 "/11")
  (net 9 "/12")
  (net 10 "/18")
  (net 11 "/19")
  (net 12 "/20")
  (net 13 "/03")
  (net 14 "GND")
  (net 15 "+5V")
  (net 16 "Net-(R1-Pad1)")
  (net 17 "/A")
  (net 18 "unconnected-(U1-Pad7)")
  (net 19 "Net-(D3-Pad2)")
  (net 20 "Net-(J3-Pad2)")
  (net 21 "/INT")
  (net 22 "/01")
  (net 23 "/02")
  (net 24 "/13")
  (net 25 "/14")
  (net 26 "/15")
  (net 27 "/16")
  (net 28 "/17")
  (net 29 "Net-(D3-Pad1)")
  (net 30 "/SCL")
  (net 31 "/SDA")
  (net 32 "/L1_A")
  (net 33 "/PWR1")
  (net 34 "/GND1")
  (net 35 "/GND2")
  (net 36 "/L1_B")
  (net 37 "Net-(D1-Pad1)")
  (net 38 "Net-(J11-Pad1)")
  (net 39 "/L2_A")
  (net 40 "/L2_B")
  (net 41 "/T1_A")
  (net 42 "/T1_B")
  (net 43 "/T2_A")
  (net 44 "/T2_B")
  (net 45 "/STO2")
  (net 46 "/STO1")
  (net 47 "Net-(J2-Pad2)")
  (net 48 "Net-(J7-Pad1)")
  (net 49 "Net-(J10-Pad1)")
  (net 50 "/STO2RET")
  (net 51 "/STO1RET")
  (net 52 "/UDPI2")
  (net 53 "/UDPI1")
  (net 54 "Net-(J8-Pad1)")
  (net 55 "Net-(J9-Pad1)")
  (net 56 "Net-(J12-Pad1)")
  (net 57 "Net-(J13-Pad1)")
  (net 58 "Net-(J14-Pad1)")
  (footprint "footprints:MEC8-113-CARD_2" locked (layer "F.Cu")
    (tedit 637EA67F)
    (at 115.062 114.454 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X0" (at 4.375 -1.25 90) (layer "F.Fab"))
    (fp_text value "Card Edge" (at 10.9 -1 90) (layer "F.Fab"))
    (fp_line (start 8.4 0.5) (end 8.4 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 1 6.5) (end 1.5 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 8.5 51.5) (end 1 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 17.5 0.5) (end 17.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 19 51.5) (end 20 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 2.5 0.5) (end 2.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 19 6.5) (end 20 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 17 0) (end 11.3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 3 0) (end 7.9 0) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 10.8 5.5) (end 10.8 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 21 50.5) (end 21 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 0 6.5) (end 1 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start -1 47.5) (end -1 7.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start -1 50.5) (end -1 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 0 51.5) (end 1 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 9.4 6.5) (end 9.8 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 11.5 51.5) (end 19 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 18.5 6.5) (end 19 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 21 7.5) (end 21 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 18.5 6.5) (mid 17.792893 6.207107) (end 17.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 2.5 0.5) (mid 2.646447 0.146447) (end 3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 7.9 0) (mid 8.253553 0.146447) (end 8.4 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 17 0) (mid 17.353553 0.146447) (end 17.5 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start -1 7.5) (mid -0.707107 6.792893) (end 0 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 8.5 51.5) (mid 10 50) (end 11.5 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 10.8 0.5) (mid 10.946447 0.146447) (end 11.3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 21 50.5) (mid 20.707107 51.207107) (end 20 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 10.8 5.5) (mid 10.507107 6.207107) (end 9.8 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 20 6.5) (mid 20.707107 6.792893) (end 21 7.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 9.4 6.5) (mid 8.692893 6.207107) (end 8.4 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 2.5 5.5) (mid 2.207107 6.207107) (end 1.5 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 0 51.5) (mid -0.707107 51.207107) (end -1 50.5) (layer "Edge.Cuts") (width 0.12))
    (pad "1" smd rect locked (at 3.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at 5.2 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at 6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect locked (at 6.8 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at 7.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect locked (at 11.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect locked (at 12.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect locked (at 13.2 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect locked (at 14 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect locked (at 14.8 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/INT") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect locked (at 15.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "/A") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect locked (at 16.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "+5V") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect locked (at 3.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/11") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect locked (at 4.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/12") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect locked (at 5.2 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/13") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect locked (at 6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/14") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect locked (at 6.8 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/15") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect locked (at 7.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/16") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect locked (at 11.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/17") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect locked (at 12.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/18") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect locked (at 13.2 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/19") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect locked (at 14 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/20") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect locked (at 14.8 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SCL") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect locked (at 15.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/SDA") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect locked (at 16.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "Pin_26") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.127 104.254 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -2.225 0) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -0.114 1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636E7B24)
    (at 128.612 100.184 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "LED" (at -2.706 -0.146 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 126.492 109.836 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "10K" (at 0 1.25 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(J3-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 131.752 104.394 90)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -2.8 90) (layer "F.SilkS") hide)
    (fp_text value "ATtiny816" (at 0.127 -2.75 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect locked (at -0.425 -0.425 90) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.425 0.425 90) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.425 0.425 90) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.425 -0.425 90) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd custom locked (at -1.45 -0.8 90) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(J7-Pad1)") (pinfunction "PA2") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.35 -0.05)
            (xy 0.299289 -0.05)
            (xy 0.35 0.000711)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "2" smd roundrect locked (at -1.45 -0.4 90) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(J9-Pad1)") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -1.45 0 90) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect locked (at -1.45 0.4 90) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd custom locked (at -1.45 0.8 90) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/STO2") (pinfunction "PA4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
            (xy 0.35 -0.000711)
            (xy 0.299289 0.05)
            (xy -0.35 0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "6" smd custom locked (at -0.8 1.45 90) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/STO2RET") (pinfunction "PA5") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.05 -0.299289)
            (xy 0.000711 -0.35)
            (xy 0.05 -0.35)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "7" smd roundrect locked (at -0.4 1.45 90) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/L1_A") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at 0 1.45 90) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/L1_B") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect locked (at 0.4 1.45 90) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/L2_A") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "10" smd custom locked (at 0.8 1.45 90) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/L2_B") (pinfunction "PB4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.05 -0.35)
            (xy -0.000711 -0.35)
            (xy 0.05 -0.299289)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "11" smd custom locked (at 1.45 0.8 90) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/08") (pinfunction "PB3") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
            (xy 0.35 0.05)
            (xy -0.299289 0.05)
            (xy -0.35 -0.000711)
          ) (width 0.1) (fill yes))
      ))
    (pad "12" smd roundrect locked (at 1.45 0.4 90) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J10-Pad1)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at 1.45 0 90) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd roundrect locked (at 1.45 -0.4 90) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd custom locked (at 1.45 -0.8 90) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(D3-Pad1)") (pinfunction "PC0") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.35 0.000711)
            (xy -0.299289 -0.05)
            (xy 0.35 -0.05)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "16" smd custom locked (at 0.8 -1.45 90) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(J8-Pad1)") (pinfunction "PC1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
            (xy 0.05 0.299289)
            (xy -0.000711 0.35)
            (xy -0.05 0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "17" smd roundrect locked (at 0.4 -1.45 90) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "18" smd roundrect locked (at 0 -1.45 90) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "19" smd roundrect locked (at -0.4 -1.45 90) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/UDPI1") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "20" smd custom locked (at -0.8 -1.45 90) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/GND2") (pinfunction "PA1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
            (xy 0.05 0.35)
            (xy 0.000711 0.35)
            (xy -0.05 0.299289)
          ) (width 0.1) (fill yes))
      ))
    (pad "21" smd rect locked (at 0 0 90) (size 1.7 1.7) (layers "F.Cu" "F.Mask")
      (net 14 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 130.556 109.836 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "100" (at 0 1.25 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/UDPI1") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(J3-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 130.556 96.012 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.778 0) (layer "F.Fab"))
    (fp_text value "10K" (at -0.127 1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/A") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 125.222 100.184 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "1K" (at 0 -1.25) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D3-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:DFN-8-1EP_3x2mm" (layer "F.Cu")
    (tedit 638826C0)
    (at 127.287 96.073 180)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
    (tags "DFN 0.5")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.55) (layer "F.SilkS") hide)
    (fp_text value "24LC32" (at 0.056 -2.153) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -1.5 0 90) (layer "F.Fab"))
    (pad "" smd rect locked (at 0.325 0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at 0.325 -0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.325 0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.325 -0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "1" smd rect locked (at -1.45 -0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(R1-Pad1)") (pinfunction "A0") (pintype "input"))
    (pad "2" smd rect locked (at -1.45 -0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" smd rect locked (at -1.45 0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" smd rect locked (at -1.45 0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect locked (at 1.45 0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd rect locked (at 1.45 0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd rect locked (at 1.45 -0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(U1-Pad7)") (pinfunction "WP") (pintype "input+no_connect"))
    (pad "8" smd rect locked (at 1.45 -0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "VCC") (pintype "power_in") (clearance -0.1016))
    (pad "9" smd rect locked (at 0 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Mask"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.892 103.363 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 2.555 -0.381 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -0.142 1.143 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:HARWIN_M80-5000000M1-02-PM1-00-000" (layer "F.Cu")
    (tedit 68A4C4E2)
    (at 157.48 104.362 -90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -6.075 -4.66 90) (layer "F.SilkS") hide)
    (fp_text value "M80" (at 12.34 5.16 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 2 0 270) (size 3.216 3.216) (drill 2.2) (layers *.Cu *.Mask)
      (net 37 "Net-(D1-Pad1)") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle locked (at -2 0 270) (size 3.216 3.216) (drill 2.2) (layers *.Cu *.Mask)
      (net 34 "/GND1") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (model "${KIPRJMOD}/3D/M80-5000000M1-02-PM1-00-000_asm.stp"
      (offset (xyz 0 0 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.65mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 129.794 102.108)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J8" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "11" (at 0.762 -0.635) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 0.65 0.65) (layers "F.Cu" "F.Mask")
      (net 54 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "footprints:TestPoint_Pad_D0.65mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 130.048 106.934)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J7" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "15" (at -0.508 0.762) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 0.65 0.65) (layers "F.Cu" "F.Mask")
      (net 48 "Net-(J7-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "footprints:TestPoint_Pad_D0.65mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 149.606 105.664)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J11" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "10" (at -0.762 0.635) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 0.65 0.65) (layers "F.Cu" "F.Mask")
      (net 38 "Net-(J11-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 151.168 108.78 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "100" (at 0.165 1.338) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/UDPI2") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(J2-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.65mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 148.336 100.838)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J13" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "16" (at 0.889 -0.254) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 0.65 0.65) (layers "F.Cu" "F.Mask")
      (net 57 "Net-(J13-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "footprints:TestPoint_Pad_D0.65mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 150.368 105.283)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J12" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "11" (at 0.254 0.762) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 0.65 0.65) (layers "F.Cu" "F.Mask")
      (net 56 "Net-(J12-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x06_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 143.002 107.823 180)
    (descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.27mm single row")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J15" (at 0 -1.695) (layer "F.SilkS") hide)
    (fp_text value "TPs" (at 0 8.045) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.175 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 41 "/T1_A") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 42 "/T1_B") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 46 "/STO1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 51 "/STO1RET") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 43 "/T2_A") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 44 "/T2_B") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x06_P1.27mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 146.558 108.78 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at 0 1.338) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(J2-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:HARWIN_G125-MV11205L1P" (layer "F.Cu")
    (tedit 68715183)
    (at 139.309 104.571 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J16" (at -1.95 -4.135 90) (layer "F.Fab"))
    (fp_text value "GECKO 12P" (at 9.095 4.115 90) (layer "F.Fab"))
    (fp_line (start -3.85 -0.45) (end -3.85 0.45) (layer "Edge.Cuts") (width 0.01))
    (fp_line (start -4.9 0.45) (end -4.9 -0.45) (layer "Edge.Cuts") (width 0.01))
    (fp_line (start 3.85 0.45) (end 3.85 -0.45) (layer "Edge.Cuts") (width 0.01))
    (fp_line (start 4.9 -0.45) (end 4.9 0.45) (layer "Edge.Cuts") (width 0.01))
    (fp_arc (start 4.9 0.45) (mid 4.746231 0.821231) (end 4.375 0.975) (layer "Edge.Cuts") (width 0.01))
    (fp_arc (start -4.375 0.975) (mid -4.746231 0.821231) (end -4.9 0.45) (layer "Edge.Cuts") (width 0.01))
    (fp_arc (start -4.375 -0.975) (mid -4.003769 -0.821231) (end -3.85 -0.45) (layer "Edge.Cuts") (width 0.01))
    (fp_arc (start -4.9 -0.45) (mid -4.746231 -0.821231) (end -4.375 -0.975) (layer "Edge.Cuts") (width 0.01))
    (fp_arc (start 4.375 0.975) (mid 4.003769 0.821231) (end 3.85 0.45) (layer "Edge.Cuts") (width 0.01))
    (fp_arc (start 4.375 -0.975) (mid 4.746231 -0.821231) (end 4.9 -0.45) (layer "Edge.Cuts") (width 0.01))
    (fp_arc (start 3.85 -0.45) (mid 4.003769 -0.821231) (end 4.375 -0.975) (layer "Edge.Cuts") (width 0.01))
    (fp_arc (start -3.85 0.45) (mid -4.003769 0.821231) (end -4.375 0.975) (layer "Edge.Cuts") (width 0.01))
    (pad "" np_thru_hole circle locked (at -4.375 0 90) (size 1.05 1.05) (drill 1.05) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 4.375 0 90) (size 1.05 1.05) (drill 1.05) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at -3.125 0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 41 "/T1_A") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle locked (at -1.875 0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 42 "/T1_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle locked (at -0.625 0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 46 "/STO1") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle locked (at 0.625 0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 51 "/STO1RET") (pinfunction "Pin_4") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle locked (at 1.875 0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 43 "/T2_A") (pinfunction "Pin_5") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle locked (at 3.125 0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 44 "/T2_B") (pinfunction "Pin_6") (pintype "passive") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle locked (at -3.125 -0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 45 "/STO2") (pinfunction "Pin_7") (pintype "passive") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle locked (at -1.875 -0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 50 "/STO2RET") (pinfunction "Pin_8") (pintype "passive") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle locked (at -0.625 -0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 "/L1_A") (pinfunction "Pin_9") (pintype "passive") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle locked (at 0.625 -0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 36 "/L1_B") (pinfunction "Pin_10") (pintype "passive") (solder_mask_margin 0.102))
    (pad "11" thru_hole circle locked (at 1.875 -0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 39 "/L2_A") (pinfunction "Pin_11") (pintype "passive") (solder_mask_margin 0.102))
    (pad "12" thru_hole circle locked (at 3.125 -0.625 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 40 "/L2_B") (pinfunction "Pin_12") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 148.082 103.378 -90)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.8 90) (layer "F.SilkS") hide)
    (fp_text value "ATtiny816" (at 0 2.8 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd custom (at -1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/PWR1") (pinfunction "PA2") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.000711)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.299289 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "2" smd roundrect (at -1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(J13-Pad1)") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd custom (at -1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/T2_B") (pinfunction "PA4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 -0.000711)
            (xy 0.299289 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "6" smd custom (at -0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/T2_A") (pinfunction "PA5") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.299289)
            (xy 0.000711 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "7" smd roundrect (at -0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/STO1RET") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 0 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/STO1") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/T1_B") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "10" smd custom (at 0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/T1_A") (pinfunction "PB4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 -0.299289)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy -0.000711 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "11" smd custom (at 1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/09") (pinfunction "PB3") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.299289 0.05)
            (xy -0.35 -0.000711)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "12" smd roundrect (at 1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(J14-Pad1)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd custom (at 1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(J11-Pad1)") (pinfunction "PC0") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 0.000711)
            (xy -0.299289 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "16" smd custom (at 0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(J12-Pad1)") (pinfunction "PC1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.299289)
            (xy -0.000711 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "17" smd roundrect (at 0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "18" smd roundrect (at 0 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/UDPI2") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "20" smd custom (at -0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/GND1") (pinfunction "PA1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy 0.000711 0.35)
            (xy -0.05 0.299289)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "21" smd rect (at 0 0 270) (size 1.7 1.7) (layers "F.Cu" "F.Mask")
      (net 14 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.65mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 130.81 107.442)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J9" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "16" (at 0.762 -0.508) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 0.65 0.65) (layers "F.Cu" "F.Mask")
      (net 55 "Net-(J9-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x06_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 135.636 107.823 180)
    (descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.27mm single row")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J18" (at 0 -1.695) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06" (at 0 8.045) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.175 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 45 "/STO2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 50 "/STO2RET") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 32 "/L1_A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 36 "/L1_B") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 39 "/L2_A") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 40 "/L2_B") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x06_P1.27mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.65mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 132.588 101.346)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J10" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "7" (at 0.508 -0.381) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 0.65 0.65) (layers "F.Cu" "F.Mask")
      (net 49 "Net-(J10-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "footprints:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 147.542 96.266 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SS14" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/PWR1") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.65mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 147.574 106.426)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J14" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "7" (at -0.508 -0.254) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 0.65 0.65) (layers "F.Cu" "F.Mask")
      (net 58 "Net-(J14-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "B.Cu")
    (tedit 59FED667)
    (at 126.81 112.776 -90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -2 1) (layer "B.SilkS") hide)
    (fp_text value "+UDPI1-" (at -2 -2) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "B.Cu")
    (tedit 59FED667)
    (at 154.21 113.03 -90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.06 90) (layer "B.SilkS") hide)
    (fp_text value "+UDPI2-" (at -2 -2.095) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ken.olsen@agilityrobotics.com" (at 142.24 113.792) (layer "B.SilkS"))
  (gr_text "ECAT TESTER" (at 142.494 96.52) (layer "B.SilkS"))
  (gr_text "Rev 0.2\nAug 2025" (at 165.862 112.776) (layer "B.SilkS"))
  (gr_text "Rapid Prototyping Card" (at 142.494 112.014) (layer "B.SilkS"))
  (gr_text "Molex Ulta-Fit\n1722981104" (at 157.734 98.806) (layer "B.SilkS"))
  (gr_text "\nG125-MV11205L1P" (at 139.192 98.298) (layer "B.SilkS"))
  (gr_text "ECAT Tester" (at 143.637 112.522) (layer "F.SilkS"))
)
