(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6002)
    (drawings 6)
    (tracks 83)
    (zones 0)
    (modules 18)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.127)
    (segment_width 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(R1-Pad2)")
  (net 4 "Net-(R2-Pad2)")
  (net 5 "Net-(D1-PadA)")
  (net 6 "Net-(Cc1-Pad2)")
  (net 7 "Net-(Cc1-Pad1)")
  (net 8 "Net-(Rf1-Pad2)")
  (net 9 "Net-(Q1-Pad4)")
  (net 10 "Net-(C1-Pad1)")
  (net 11 "Net-(C3-Pad1)")
  (net 12 "Net-(J1-Pad2)")
  (net 13 "Net-(J2-Pad2)")
  (net 14 "Net-(R4-Pad1)")
  (net 15 "Net-(L1-Pad1)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(Cc1-Pad1)")
    (add_net "Net-(Cc1-Pad2)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(Rf1-Pad2)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 186.375 94.72504 90)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0 -2.25 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 191.15 85.82504 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.57504 0.1 90) (layer B.SilkS))
    (fp_text value 0.01uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 187.225 87.70004 180)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3 (at -0.025 -2.29996 180) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 180) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 193.75 85.97504)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference Cc1 (at 0 1.5) (layer B.SilkS))
    (fp_text value 22nF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(Cc1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Cc1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-DO-219AB (layer F.Cu) (tedit 5BC00A4B)
    (at 193 87.77504)
    (attr smd)
    (fp_text reference D1 (at 0 1.72496) (layer F.SilkS))
    (fp_text value "ES1FL R3G" (at 0 1.524) (layer F.SilkS) hide)
    (pad A smd rect (at 1.5494 0 180) (size 1.1938 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-PadA)"))
    (pad C smd rect (at -1.5494 0) (size 1.1938 1.397) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C3-Pad1)"))
  )
  (module nixiemisc:nixiemisc-SO08 (layer B.Cu) (tedit 5BC009D5)
    (at 187.198 90.424 270)
    (descr "SOIC, 0.15 INCH WIDTH")
    (tags "SOIC, 0.15 INCH WIDTH")
    (attr smd)
    (fp_text reference Q1 (at 0.1 -0.025 180) (layer B.SilkS))
    (fp_text value DMT6010LSS (at 3.5052 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.905 -2.79908 270) (size 0.59944 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -0.635 -2.79908 270) (size 0.59944 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 0.635 -2.79908 270) (size 0.59944 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 1.905 -2.79908 270) (size 0.59944 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(Q1-Pad4)"))
    (pad 5 smd rect (at 1.905 2.79908 270) (size 0.59944 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(L1-Pad1)"))
    (pad 6 smd rect (at 0.635 2.79908 270) (size 0.59944 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(L1-Pad1)"))
    (pad 7 smd rect (at -0.635 2.79908 270) (size 0.59944 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(L1-Pad1)"))
    (pad 8 smd rect (at -1.905 2.79908 270) (size 0.59944 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(L1-Pad1)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 191.25 84.55004 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.30004 0 270) (layer F.SilkS))
    (fp_text value 360K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R2-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 193.8 85.25004)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 5.9K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 193.725 84.70004 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Rc1 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Cc1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 194.025 95.60004 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Rf1 (at -0.05 -1.35 180) (layer B.SilkS))
    (fp_text value 47k (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(Rf1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 188.775 85.77504 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Rsen1 (at 0.35 -1.6 90) (layer B.SilkS))
    (fp_text value 0.1 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:VSSOP-8_3.0x3.0mm_Pitch0.65mm (layer B.Cu) (tedit 59E7C95B)
    (at 194.056 91.40004 270)
    (descr "VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf")
    (tags "VSSOP-8 3.0 x 3.0")
    (attr smd)
    (fp_text reference U1 (at 0.025 -0.1 270) (layer B.SilkS))
    (fp_text value LM3478SOIC8 (at 0.02 -2.73 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 2.2 0.975) (size 0.45 1.45) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 2.2 0.325) (size 0.45 1.45) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(Rf1-Pad2)"))
    (pad 6 smd rect (at 2.2 -0.325) (size 0.45 1.45) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R4-Pad1)"))
    (pad 5 smd rect (at 2.2 -0.975) (size 0.45 1.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.2 -0.975) (size 0.45 1.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.2 -0.325) (size 0.45 1.45) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -2.2 0.325) (size 0.45 1.45) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(Cc1-Pad1)"))
    (pad 1 smd rect (at -2.2 0.975) (size 0.45 1.45) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/VSSOP-8_3.0x3.0mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 189.1 84.55004 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.30004 0.15 90) (layer F.SilkS))
    (fp_text value 360K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 186.5 95.00004 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.75 0.00004 180) (layer B.SilkS))
    (fp_text value Si2319CDS (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 5BC008B5)
    (at 197.5 89.00004 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 5BC008A8)
    (at 182.5 89.00004 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 191.516 91.694 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.286 0 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(Q1-Pad4)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coilcraft:LPR6235 (layer F.Cu) (tedit 5DC44873)
    (at 191.65 93.50004)
    (descr "Flyback transformer")
    (tags "flyback transformer")
    (attr smd)
    (fp_text reference L1 (at 0 0) (layer F.SilkS))
    (fp_text value LPR6235-253LMR (at 0 4.43484) (layer F.SilkS) hide)
    (fp_text user 1 (at -0.79248 -1.2446) (layer Dwgs.User))
    (fp_text user 2 (at 0.79248 -1.35382) (layer Dwgs.User))
    (fp_text user 3 (at 1.51384 0.5334) (layer Dwgs.User))
    (fp_text user 4 (at -0.82296 0.635) (layer Dwgs.User))
    (pad 1 smd rect (at -2.49936 -1.99898 90) (size 1.29794 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(L1-Pad1)"))
    (pad 4 smd rect (at 1.99898 -2.49936 180) (size 1.29794 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-PadA)"))
    (pad 3 smd rect (at 2.49936 1.99898 270) (size 1.29794 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.99898 2.49936) (size 1.29794 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C1-Pad1)"))
  )
  (gr_text Ven (at 197.5 93.5) (layer B.SilkS))
  (gr_text HV (at 197.5 87) (layer B.SilkS))
  (gr_text VIN (at 182.5 93.5) (layer B.SilkS))
  (gr_text GND (at 182.5 87) (layer B.SilkS))
  (gr_circle (center 190 90.00004) (end 190 81.00004) (layer Edge.Cuts) (width 0.127))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189 96.00004) (xy 194.5 96.00004) (xy 194.5 91.00004) (xy 189 91.00004)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180 100.00004) (xy 200 100.00004) (xy 200 80.00004) (xy 180 80.00004)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180 100.00004) (xy 200 100.00004) (xy 200 80.00004) (xy 180 80.00004)
      )
    )
  )
)
