(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu16.04.1-stable)
  (general
    (links 23)
    (no_connects 0)
    (area 143.0676 93.08548 179.756615 139.750001)
    (thickness 1.6002)
    (drawings 28)
    (tracks 208)
    (zones 0)
    (modules 9)
    (nets 23)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.50622 3.01498)
    (pad_drill 0.99822)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 GPIO2)
  (net 3 EN)
  (net 4 GPIO0)
  (net 5 GPIO4)
  (net 6 GPIO5)
  (net 7 GPIO9)
  (net 8 GPIO10)
  (net 9 GPIO12)
  (net 10 GPIO13)
  (net 11 GPIO14)
  (net 12 GPIO15)
  (net 13 GPIO16)
  (net 14 TXD0)
  (net 15 RXD0)
  (net 16 +5V)
  (net 17 "Net-(U2-Pad9)")
  (net 18 "Net-(U2-Pad10)")
  (net 19 "Net-(U2-Pad13)")
  (net 20 "Net-(U2-Pad14)")
  (net 21 RST)
  (net 22 ADC)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net ADC)
    (add_net EN)
    (add_net GND)
    (add_net GPIO0)
    (add_net GPIO10)
    (add_net GPIO12)
    (add_net GPIO13)
    (add_net GPIO14)
    (add_net GPIO15)
    (add_net GPIO16)
    (add_net GPIO2)
    (add_net GPIO4)
    (add_net GPIO5)
    (add_net GPIO9)
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad9)")
    (add_net RST)
    (add_net RXD0)
    (add_net TXD0)
  )
  (module ESP8266:ESP-12E (layer Top) (tedit 5782F033)
    (at 148.5011 105.0036)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference ESP-12 (at 8.4709 7.2644) (layer F.SilkS))
    (fp_text value ESP-12E (at 8 1) (layer F.Fab))
    (fp_text user "No Copper" (at 7.9 -5.4) (layer F.CrtYd))
    (pad 9 smd oval (at 2.99 15.75 90) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 17 "Net-(U2-Pad9)"))
    (pad 10 smd oval (at 4.99 15.75 90) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 18 "Net-(U2-Pad10)"))
    (pad 11 smd oval (at 6.99 15.75 90) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 7 GPIO9))
    (pad 12 smd oval (at 8.99 15.75 90) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 8 GPIO10))
    (pad 13 smd oval (at 10.99 15.75 90) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 19 "Net-(U2-Pad13)"))
    (pad 14 smd oval (at 12.99 15.75 90) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 20 "Net-(U2-Pad14)"))
    (pad 1 smd rect (at 0 0) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 21 RST))
    (pad 2 smd oval (at 0 2) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 22 ADC))
    (pad 3 smd oval (at 0 4) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 3 EN))
    (pad 4 smd oval (at 0 6) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 13 GPIO16))
    (pad 5 smd oval (at 0 8) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 11 GPIO14))
    (pad 6 smd oval (at 0 10) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 9 GPIO12))
    (pad 7 smd oval (at 0 12) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 10 GPIO13))
    (pad 8 smd oval (at 0 14) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 3 EN))
    (pad 15 smd oval (at 16 14) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd oval (at 16 12) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 12 GPIO15))
    (pad 17 smd oval (at 16 10) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 2 GPIO2))
    (pad 18 smd oval (at 16 8) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 4 GPIO0))
    (pad 19 smd oval (at 16 6) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 5 GPIO4))
    (pad 20 smd oval (at 16 4) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 6 GPIO5))
    (pad 21 smd oval (at 16 2) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 15 RXD0))
    (pad 22 smd oval (at 16 0) (size 2.4 1.1) (layers Top F.Paste F.Mask)
      (net 14 TXD0))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x12 (layer Top) (tedit 57830447)
    (at 168.402 109.22)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.508 -2.286) (layer F.SilkS) hide)
    (fp_text value CONN_01X12 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GPIO0))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GPIO2))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GPIO4))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GPIO5))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GPIO9))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 GPIO10))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 GPIO12))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 GPIO13))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 GPIO14))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 GPIO15))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GPIO16))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes:DIODE_DO214AB-SMC (layer Top) (tedit 5782EF99)
    (at 152.4 133.35 180)
    (fp_text reference D2 (at 0 0.254 270) (layer F.SilkS))
    (fp_text value D (at -4 0 270) (layer F.Fab) hide)
    (pad C smd rect (at 0 -3.2 180) (size 3.5 2.5) (layers Top F.Paste F.Mask))
    (pad A smd rect (at 0 3.2 180) (size 3.5 2.5) (layers Top F.Paste F.Mask))
  )
  (module Diodes:DIODE_DO214AB-SMC (layer Top) (tedit 5782EF9B)
    (at 147.955 133.35 180)
    (fp_text reference D1 (at 0.127 0.254 270) (layer F.SilkS))
    (fp_text value D (at -4 0 270) (layer F.Fab) hide)
    (pad C smd rect (at 0 -3.2 180) (size 3.5 2.5) (layers Top F.Paste F.Mask))
    (pad A smd rect (at 0 3.2 180) (size 3.5 2.5) (layers Top F.Paste F.Mask))
  )
  (module Connect:PINHEAD1-2 (layer Top) (tedit 578304EA)
    (at 153.543 125.095 270)
    (attr virtual)
    (fp_text reference F1 (at -0.127 -1.778 270) (layer F.SilkS) hide)
    (fp_text value JUMPER (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -1.27 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 GPIO0))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connect:PINHEAD1-2 (layer Top) (tedit 5783043E)
    (at 147.955 125.095 270)
    (attr virtual)
    (fp_text reference F2 (at 0.127 2.159 270) (layer F.SilkS) hide)
    (fp_text value JUMPER (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -1.27 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 2 GPIO2))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 3 EN))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer Top) (tedit 57830437)
    (at 156.845 125.095 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 1.905 4.953 180) (layer F.SilkS) hide)
    (fp_text value UART (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 TXD0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 RXD0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 +5V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer Top) (tedit 57830429)
    (at 161.29 133.35 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -0.762 180) (layer F.SilkS) hide)
    (fp_text value LD1117S33TR (at 0 0.762 180) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302 180) (size 3.6576 2.032) (layers Top F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302 180) (size 1.016 2.032) (layers Top F.Paste F.Mask)
      (net 3 EN))
    (pad 3 smd rect (at 2.286 3.302 180) (size 1.016 2.032) (layers Top F.Paste F.Mask)
      (net 16 +5V))
    (pad 1 smd rect (at -2.286 3.302 180) (size 1.016 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer Top) (tedit 0)
    (at 167.386 98.552)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912) (layer F.SilkS))
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab))
  )
  (gr_text "GND	" (at 166.624 136.906 90) (layer F.SilkS))
  (gr_text 16 (at 166.624 134.62 90) (layer F.SilkS))
  (gr_text "15	" (at 166.624 131.826 90) (layer F.SilkS))
  (gr_text "14	" (at 166.624 129.286 90) (layer F.SilkS))
  (gr_text "13	" (at 166.624 126.746 90) (layer F.SilkS))
  (gr_text "12	" (at 166.624 124.206 90) (layer F.SilkS))
  (gr_text "10	" (at 166.624 121.666 90) (layer F.SilkS))
  (gr_text 9 (at 166.624 119.38 90) (layer F.SilkS))
  (gr_text 5 (at 166.624 116.84 90) (layer F.SilkS))
  (gr_text 4 (at 166.624 114.3 90) (layer F.SilkS))
  (gr_text 2 (at 166.497 111.76 90) (layer F.SilkS))
  (gr_text "0\n" (at 166.497 109.347 90) (layer F.SilkS))
  (gr_text "GPIO\n" (at 168.529 106.934) (layer F.SilkS))
  (gr_text TX (at 157.48 122.936) (layer F.SilkS))
  (gr_text RX (at 159.385 122.936) (layer F.SilkS))
  (gr_text +5V (at 161.798 122.936) (layer F.SilkS))
  (gr_text GND (at 164.465 122.936) (layer F.SilkS))
  (gr_text "Sisuware\nRevision 0.1" (at 157.734 99.314) (layer B.SilkS))
  (gr_arc (start 147.32 137.16) (end 147.32 139.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 168.91 137.16) (end 171.45 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.78 137.16) (end 144.78 125.73) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.91 139.7) (end 147.32 139.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.45 125.73) (end 171.45 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 147.32 97.79) (end 144.78 97.79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 168.91 97.79) (end 168.91 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.78 97.79) (end 144.78 125.73) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.91 95.25) (end 147.32 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.45 125.73) (end 171.45 97.79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name EN) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.815 103.632) (xy 171.196 103.632) (xy 171.196 137.922) (xy 169.418 139.7) (xy 147.066 139.7)
        (xy 144.78 137.414) (xy 144.78 103.632) (xy 145.415 103.632) (xy 145.415 103.505) (xy 170.815 103.505)
        (xy 170.815 103.632)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.815 137.795) (xy 169.545 139.065) (xy 146.685 139.065) (xy 145.415 137.795) (xy 145.415 103.505)
        (xy 170.815 103.505) (xy 170.815 137.795)
      )
    )
  )
)
