(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 2.67)
    (drawings 85)
    (tracks 485)
    (zones 0)
    (modules 48)
    (nets 46)
  )
  (page B)
  (title_block
    (title "Aspera HVPS Board")
    (date 2022-11-05)
    (rev 1.0)
    (comment 2 ASPERA-UA-DWG-00004)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 50 50)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x30000_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers1a"))
  )
  (net 0 "")
  (net 1 "Net-(D2-Pad2)")
  (net 2 "/PCB_top_level/HVPS 2/+5Vref")
  (net 3 "/PCB_top_level/HVPS 1/+5Vref")
  (net 4 "/PCB_top_level/HVPS 1/-HV_OUT")
  (net 5 "/PCB_top_level/HVPS 2/-HV_OUT")
  (net 6 /PCB_top_level/+12V_IN)
  (net 7 "Net-(D6-Pad1)")
  (net 8 "Net-(D5-Pad1)")
  (net 9 CHASSIS)
  (net 10 /PCB_top_level/-HV)
  (net 11 /PCB_top_level/HVPS2_Imon)
  (net 12 /PCB_top_level/HVPS2_ON_OUT_5V)
  (net 13 /PCB_top_level/HVPS2_Vset)
  (net 14 /PCB_top_level/HVPS2_Vmon)
  (net 15 /PCB_top_level/HVPS1_Vmon)
  (net 16 /PCB_top_level/HVPS1_Vset)
  (net 17 /PCB_top_level/HVPS1_ON_OUT_5V)
  (net 18 /PCB_top_level/HVPS1_Imon)
  (net 19 /PCB_top_level/HVPS_TEMP1-)
  (net 20 /PCB_top_level/HVPS_TEMP+)
  (net 21 /PCB_top_level/HVPS_TEMP2-)
  (net 22 "Net-(J6-Pad11)")
  (net 23 "Net-(J6-Pad12)")
  (net 24 "Net-(J6-Pad13)")
  (net 25 "Net-(J6-Pad18)")
  (net 26 /PCB_top_level/-RF)
  (net 27 /PCB_top_level/HVPS2.RTN)
  (net 28 "/PCB_top_level/HVPS 2/V_BUS")
  (net 29 "/PCB_top_level/HVPS 2/-RF_OUT")
  (net 30 "/PCB_top_level/HVPS 1/-RF_OUT")
  (net 31 /PCB_top_level/HVPS1.RTN)
  (net 32 "Net-(C1-Pad1)")
  (net 33 "Net-(C3-Pad1)")
  (net 34 /PCB_top_level/HVPS1.PWR)
  (net 35 /PCB_top_level/HVPS2.PWR)
  (net 36 "Net-(C6-Pad2)")
  (net 37 "Net-(C7-Pad2)")
  (net 38 "Net-(C8-Pad2)")
  (net 39 "Net-(C9-Pad2)")
  (net 40 "Net-(U2-Pad11)")
  (net 41 "Net-(U1-Pad11)")
  (net 42 "Net-(U2-Pad12)")
  (net 43 "Net-(U1-Pad12)")
  (net 44 "Net-(J6-Pad14)")
  (net 45 "Net-(D4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/PCB_top_level/HVPS 1/+5Vref")
    (add_net "/PCB_top_level/HVPS 2/+5Vref")
    (add_net /PCB_top_level/HVPS1_Imon)
    (add_net /PCB_top_level/HVPS1_ON_OUT_5V)
    (add_net /PCB_top_level/HVPS1_Vmon)
    (add_net /PCB_top_level/HVPS1_Vset)
    (add_net /PCB_top_level/HVPS2_Imon)
    (add_net /PCB_top_level/HVPS2_ON_OUT_5V)
    (add_net /PCB_top_level/HVPS2_Vmon)
    (add_net /PCB_top_level/HVPS2_Vset)
    (add_net /PCB_top_level/HVPS_TEMP+)
    (add_net /PCB_top_level/HVPS_TEMP1-)
    (add_net /PCB_top_level/HVPS_TEMP2-)
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J6-Pad11)")
    (add_net "Net-(J6-Pad12)")
    (add_net "Net-(J6-Pad13)")
    (add_net "Net-(J6-Pad14)")
    (add_net "Net-(J6-Pad18)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
  )
  (net_class HV ""
    (clearance 1)
    (trace_width 1)
    (via_dia 1.2)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PCB_top_level/-HV)
    (add_net /PCB_top_level/-RF)
    (add_net "/PCB_top_level/HVPS 1/-HV_OUT")
    (add_net "/PCB_top_level/HVPS 1/-RF_OUT")
    (add_net "/PCB_top_level/HVPS 2/-HV_OUT")
    (add_net "/PCB_top_level/HVPS 2/-RF_OUT")
    (add_net CHASSIS)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
  )
  (net_class pwr ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PCB_top_level/+12V_IN)
    (add_net "/PCB_top_level/HVPS 2/V_BUS")
    (add_net /PCB_top_level/HVPS1.PWR)
    (add_net /PCB_top_level/HVPS1.RTN)
    (add_net /PCB_top_level/HVPS2.PWR)
    (add_net /PCB_top_level/HVPS2.RTN)
  )
  (module Aspera_footprints:hole_9mm (layer F.Cu) (tedit 594FDCDD)
    (at 103 75.5)
    (fp_text reference X9 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value HOLE_NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 9 9) (drill 9) (layers *.Cu *.Mask))
  )
  (module Aspera_footprints:hole_9mm (layer F.Cu) (tedit 594FDCDD)
    (at 102 127.9)
    (fp_text reference X10 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value HOLE_NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 9 9) (drill 9) (layers *.Cu *.Mask))
  )
  (module Aspera_footprints:AD590MF (layer B.Cu) (tedit 6365523E)
    (at 89.8 80.8 180)
    (fp_text reference U3 (at 2.7 3.9 270) (layer B.SilkS))
    (fp_text value AD590 (at 0.635 3.556 180) (layer B.SilkS) hide)
    (fp_text user %R (at 0.8 3.75 -90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.4826 2) (drill (offset 0 -0.5)) (layers B.Cu B.Paste B.Mask)
      (net 20 /PCB_top_level/HVPS_TEMP+))
    (pad 2 smd rect (at 1.27 0 180) (size 0.4826 2) (drill (offset 0 -0.5)) (layers B.Cu B.Paste B.Mask)
      (net 19 /PCB_top_level/HVPS_TEMP1-))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/AD590xF.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:AD590MF (layer B.Cu) (tedit 6365523E)
    (at 90.1 120.7 180)
    (fp_text reference U4 (at 1.6 7.4 180) (layer B.SilkS))
    (fp_text value AD590 (at 0.635 3.556 180) (layer B.SilkS) hide)
    (fp_text user %R (at 0.8 3.75 -90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.4826 2) (drill (offset 0 -0.5)) (layers B.Cu B.Paste B.Mask)
      (net 20 /PCB_top_level/HVPS_TEMP+))
    (pad 2 smd rect (at 1.27 0 180) (size 0.4826 2) (drill (offset 0 -0.5)) (layers B.Cu B.Paste B.Mask)
      (net 21 /PCB_top_level/HVPS_TEMP2-))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/AD590xF.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:Ultravolt-6AA-I-fixed-nosilk (layer F.Cu) (tedit 63653BC8)
    (at 62 134)
    (fp_text reference U2 (at 8.8 5.8) (layer F.SilkS))
    (fp_text value Ultravolt-AA-I (at 36.703 -15.24) (layer F.Fab) hide)
    (fp_text user %R (at 36.65 -16.8) (layer F.Fab))
    (pad 15 thru_hole circle (at 62.23 -30.48) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (pad 16 thru_hole circle (at 62.23 -27.94) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (pad 17 thru_hole circle (at 62.23 -8.255) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "/PCB_top_level/HVPS 2/-RF_OUT"))
    (pad 18 thru_hole circle (at 62.23 -5.715) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "/PCB_top_level/HVPS 2/-RF_OUT"))
    (pad 8 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 /PCB_top_level/HVPS2.RTN))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 /PCB_top_level/HVPS2.RTN))
    (pad 9 thru_hole circle (at 2.54 -5.08) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "/PCB_top_level/HVPS 2/V_BUS"))
    (pad 2 thru_hole circle (at 0 -5.08) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "/PCB_top_level/HVPS 2/V_BUS"))
    (pad 10 thru_hole circle (at 2.54 -10.16) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -10.16) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /PCB_top_level/HVPS2_Imon))
    (pad 11 thru_hole circle (at 2.54 -15.24) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(U2-Pad11)"))
    (pad 4 thru_hole circle (at 0 -15.24) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /PCB_top_level/HVPS2_ON_OUT_5V))
    (pad 12 thru_hole circle (at 2.54 -20.32) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 "Net-(U2-Pad12)"))
    (pad 5 thru_hole circle (at 0 -20.32) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 /PCB_top_level/HVPS2.RTN))
    (pad 13 thru_hole circle (at 2.54 -25.4) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "/PCB_top_level/HVPS 2/+5Vref"))
    (pad 6 thru_hole circle (at 0 -25.4) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 /PCB_top_level/HVPS2_Vset))
    (pad 14 thru_hole circle (at 2.54 -30.48) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 /PCB_top_level/HVPS2_Vmon))
    (pad 19 thru_hole circle (at 16.51 -29.21) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (solder_mask_margin 1) (zone_connect 2))
    (pad 20 thru_hole circle (at 16.51 -1.27) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (solder_mask_margin 1) (zone_connect 2))
    (pad 7 thru_hole circle (at 0 -30.48) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "/PCB_top_level/HVPS 2/+5Vref"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/Ultravolt_AA-I.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:Ultravolt-6AA-I-fixed-nosilk (layer F.Cu) (tedit 63653BC8)
    (at 62 92.2)
    (fp_text reference U1 (at 8.8 5.8) (layer F.SilkS))
    (fp_text value Ultravolt-AA-I (at 36.703 -15.24) (layer F.Fab) hide)
    (fp_text user %R (at 36.65 -16.8) (layer F.Fab))
    (pad 15 thru_hole circle (at 62.23 -30.48) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (pad 16 thru_hole circle (at 62.23 -27.94) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (pad 17 thru_hole circle (at 62.23 -8.255) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "/PCB_top_level/HVPS 1/-RF_OUT"))
    (pad 18 thru_hole circle (at 62.23 -5.715) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "/PCB_top_level/HVPS 1/-RF_OUT"))
    (pad 8 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 /PCB_top_level/HVPS1.RTN))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 /PCB_top_level/HVPS1.RTN))
    (pad 9 thru_hole circle (at 2.54 -5.08) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /PCB_top_level/+12V_IN))
    (pad 2 thru_hole circle (at 0 -5.08) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /PCB_top_level/+12V_IN))
    (pad 10 thru_hole circle (at 2.54 -10.16) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -10.16) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 /PCB_top_level/HVPS1_Imon))
    (pad 11 thru_hole circle (at 2.54 -15.24) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad11)"))
    (pad 4 thru_hole circle (at 0 -15.24) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 /PCB_top_level/HVPS1_ON_OUT_5V))
    (pad 12 thru_hole circle (at 2.54 -20.32) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad12)"))
    (pad 5 thru_hole circle (at 0 -20.32) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 /PCB_top_level/HVPS1.RTN))
    (pad 13 thru_hole circle (at 2.54 -25.4) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "/PCB_top_level/HVPS 1/+5Vref"))
    (pad 6 thru_hole circle (at 0 -25.4) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 /PCB_top_level/HVPS1_Vset))
    (pad 14 thru_hole circle (at 2.54 -30.48) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 /PCB_top_level/HVPS1_Vmon))
    (pad 19 thru_hole circle (at 16.51 -29.21) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (solder_mask_margin 1) (zone_connect 2))
    (pad 20 thru_hole circle (at 16.51 -1.27) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (solder_mask_margin 1) (zone_connect 2))
    (pad 7 thru_hole circle (at 0 -30.48) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "/PCB_top_level/HVPS 1/+5Vref"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/Ultravolt_AA-I.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:C1808 (layer B.Cu) (tedit 63653A93)
    (at 135 141.5 180)
    (fp_text reference C2 (at 0 0 180) (layer B.Fab))
    (fp_text value 100pF (at -0.01 -0.03 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -2.3 0 180) (size 1.75 2.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 26 /PCB_top_level/-RF))
    (pad 2 smd roundrect (at 2.3 0 180) (size 1.75 2.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 9 CHASSIS))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/Kemet_C1808C.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:1N4989 (layer B.Cu) (tedit 63653A23)
    (at 152.2 143.6 165)
    (fp_text reference D5 (at 0.141421 0.141421 165) (layer B.Fab))
    (fp_text value JANTX1N4989 (at 0 0.499999 165) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at -5.079999 0 165) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 8 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 5.079999 0 165) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 26 /PCB_top_level/-RF))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/1N4989.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:1N4989 (layer B.Cu) (tedit 636539E3)
    (at 158.8 135.1 250)
    (fp_text reference D6 (at 0.199545 0.034378 250) (layer B.Fab))
    (fp_text value JANTX1N4989 (at -0.000001 0.499999 250) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at -5.079999 0 250) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 5.079999 0 250) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 8 "Net-(D5-Pad1)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/1N4989.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:1N4989 (layer B.Cu) (tedit 636539A2)
    (at 164.8 134.5 90)
    (fp_text reference D7 (at 0.4 0.7 90) (layer B.Fab))
    (fp_text value JANTX1N4989 (at 0 0.5 90) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at -5.079999 0 90) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (pad 2 thru_hole circle (at 5.079999 0 90) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/1N4989.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:SlimMox10403_TH_vert (layer F.Cu) (tedit 63653946)
    (at 144.5 132 60)
    (fp_text reference R2 (at 0 0 60) (layer F.Fab))
    (fp_text value 200M (at 0.28 -0.04 60) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -11.43 0.8535 60) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 /PCB_top_level/-RF))
    (pad 2 thru_hole circle (at 11.43 0.8535 60) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "Net-(D4-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/SlimMox10403.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:DD1000_mod (layer B.Cu) (tedit 63653907)
    (at 134.1 125 12)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 6.5mm")
    (fp_text reference D4 (at -0.1 2.3 12) (layer B.SilkS) hide)
    (fp_text value DD1000 (at 0 -2.4 12) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 12) (layer B.Fab))
    (pad 1 smd circle (at -10 0 12) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 29 "/PCB_top_level/HVPS 2/-RF_OUT"))
    (pad 2 thru_hole oval (at 10 0 12) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(D4-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/DD1000.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:R_2010_HV (layer B.Cu) (tedit 636538E1)
    (at 125.8 118.4 225)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R3 (at 0 2.25 225) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -2.35 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd roundrect (at 2.93 0 225) (size 2.4 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15)
      (net 29 "/PCB_top_level/HVPS 2/-RF_OUT"))
    (pad 1 smd roundrect (at -2.93 0 225) (size 2.4 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15)
      (net 33 "Net-(C3-Pad1)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_2010_HV.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:HVCC103Y6P202M (layer F.Cu) (tedit 636538CB)
    (at 143 108 90)
    (fp_text reference C3 (at 0 0 90) (layer F.Fab))
    (fp_text value 2000pF (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 4.8 4 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at -4.8 -4 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/HVCC103Y6P202M.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:DD1000 (layer F.Cu) (tedit 636538A0)
    (at 150.5 106 90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 6.5mm")
    (fp_text reference D3 (at 7.1 1 90) (layer F.SilkS) hide)
    (fp_text value DD1000 (at 0.3 -0.1 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -10 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/PCB_top_level/HVPS 2/-HV_OUT"))
    (pad 2 thru_hole oval (at 10 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /PCB_top_level/-HV))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/DD1000.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:R_2010_HV (layer B.Cu) (tedit 6365388B)
    (at 149 110 90)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R5 (at 0 2.25 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -2.35 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 2.93 0 90) (size 2.4 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15)
      (net 33 "Net-(C3-Pad1)"))
    (pad 1 smd roundrect (at -2.93 0 90) (size 2.4 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15)
      (net 5 "/PCB_top_level/HVPS 2/-HV_OUT"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_2010_HV.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:HVCC103Y6P202M (layer F.Cu) (tedit 63653871)
    (at 157.5 106.5 270)
    (fp_text reference C5 (at 0 0 270) (layer F.Fab))
    (fp_text value 2000pF (at 0 -0.5 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at -4.8 -4 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (pad 1 thru_hole circle (at 4.8 4 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/PCB_top_level/HVPS 2/-HV_OUT"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/HVCC103Y6P202M.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:DD1000_mod (layer B.Cu) (tedit 636537EC)
    (at 133.9 89.1 345)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 6.5mm")
    (fp_text reference D2 (at -0.1 2.299999 345) (layer B.SilkS) hide)
    (fp_text value DD1000 (at 0 -2.4 345) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 345) (layer B.Fab))
    (pad 1 smd circle (at -10 0 345) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 30 "/PCB_top_level/HVPS 1/-RF_OUT"))
    (pad 2 thru_hole oval (at 10 0 345) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D2-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/DD1000.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:DD1000 (layer F.Cu) (tedit 636537BE)
    (at 152.5 84.5 270)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 6.5mm")
    (fp_text reference D1 (at -4.8 2.3 270) (layer F.SilkS) hide)
    (fp_text value DD1000 (at 0.3 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -10 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/PCB_top_level/HVPS 1/-HV_OUT"))
    (pad 2 thru_hole oval (at 10 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /PCB_top_level/-HV))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/DD1000.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:HVCC103Y6P202M (layer F.Cu) (tedit 63653796)
    (at 159 72 270)
    (fp_text reference C4 (at 0 -0.1 270) (layer F.Fab))
    (fp_text value 2000pF (at 0 -0.5 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 4.8 4 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/PCB_top_level/HVPS 1/-HV_OUT"))
    (pad 2 thru_hole circle (at -4.8 -4 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/HVCC103Y6P202M.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:HVCC103Y6P202M (layer F.Cu) (tedit 63653764)
    (at 142.9 72 90)
    (fp_text reference C1 (at 0 0 90) (layer F.Fab))
    (fp_text value 2000pF (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at -4.8 -4 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
    (pad 1 thru_hole circle (at 4.8 4 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/HVCC103Y6P202M.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:R_2010_HV (layer B.Cu) (tedit 63653724)
    (at 149 74 90)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R4 (at 0 2.25 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -2.35 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -2.93 0 90) (size 2.4 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15)
      (net 4 "/PCB_top_level/HVPS 1/-HV_OUT"))
    (pad 2 smd roundrect (at 2.93 0 90) (size 2.4 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15)
      (net 32 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_2010_HV.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:R_2010_HV (layer B.Cu) (tedit 63653709)
    (at 124.1 77.5 225)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R1 (at 0 2.25 225) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -2.35 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 1 smd roundrect (at -2.93 0 225) (size 2.4 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15)
      (net 32 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 2.93 0 225) (size 2.4 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15)
      (net 30 "/PCB_top_level/HVPS 1/-RF_OUT"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_2010_HV.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:HOLE_3.5mm_connected_smaller (layer F.Cu) (tedit 63652890)
    (at 53.5 53.5)
    (fp_text reference X1 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (zone_connect 2))
  )
  (module Aspera_footprints:HOLE_3.5mm_connected_smaller (layer F.Cu) (tedit 6364C217)
    (at 166.5 53.5)
    (fp_text reference X3 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
  )
  (module Aspera_footprints:HOLE_3.5mm_connected_smaller (layer F.Cu) (tedit 6364C217)
    (at 166.5 100)
    (fp_text reference X4 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
  )
  (module Aspera_footprints:HOLE_3.5mm_connected_smaller (layer F.Cu) (tedit 6364C217)
    (at 166.5 146.5)
    (fp_text reference X5 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
  )
  (module Aspera_footprints:HOLE_3.5mm_connected_smaller (layer F.Cu) (tedit 6364C217)
    (at 110 146.5)
    (fp_text reference X6 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
  )
  (module Aspera_footprints:HOLE_3.5mm_connected_smaller (layer F.Cu) (tedit 636528B3)
    (at 53.5 146.5)
    (fp_text reference X7 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (zone_connect 2))
  )
  (module Aspera_footprints:HOLE_3.5mm_connected_smaller (layer F.Cu) (tedit 636528A8)
    (at 53.5 100)
    (fp_text reference X8 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (zone_connect 2))
  )
  (module Aspera_footprints:HOLE_3.5mm_connected_smaller (layer F.Cu) (tedit 6364C217)
    (at 110 53.5)
    (fp_text reference X2 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 -4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 9 CHASSIS))
  )
  (module Aspera_footprints:SPM7054 (layer B.Cu) (tedit 6364BF39)
    (at 62.2 143.7 270)
    (fp_text reference L2 (at -3.2 -4.2 270) (layer B.SilkS))
    (fp_text value 100uH (at 0 -3.1 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 3.05 0 270) (size 3 3.3) (layers B.Cu B.Paste B.Mask)
      (net 35 /PCB_top_level/HVPS2.PWR))
    (pad 1 smd rect (at -3.05 0 270) (size 3 3.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "/PCB_top_level/HVPS 2/V_BUS"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/SPM7054.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:wire_22_Round_HV (layer B.Cu) (tedit 6364C426)
    (at 144.5 93.5)
    (descr "Mesurement Point, Round, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point Round Trough Hole 3mm 1.5mm")
    (attr virtual)
    (fp_text reference JP1 (at 0 3) (layer B.SilkS) hide)
    (fp_text value "20KV Wire Jumper" (at 3.5 18 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(D2-Pad2)"))
  )
  (module Aspera_footprints:wire_22_Round_HV (layer B.Cu) (tedit 6364C409)
    (at 153 122.5)
    (descr "Mesurement Point, Round, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point Round Trough Hole 3mm 1.5mm")
    (attr virtual)
    (fp_text reference JP2 (at 0 3) (layer B.SilkS) hide)
    (fp_text value "Wire Jumper" (at 0 -3) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "Net-(D4-Pad2)"))
  )
  (module Aspera_footprints:SPM7054 (layer B.Cu) (tedit 6364C07F)
    (at 81.4 98)
    (fp_text reference L1 (at 2.6 -4.2) (layer B.SilkS))
    (fp_text value 100uH (at 0 -3.1) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.05 0) (size 3 3.3) (layers B.Cu B.Paste B.Mask)
      (net 6 /PCB_top_level/+12V_IN))
    (pad 2 smd rect (at 3.05 0) (size 3 3.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /PCB_top_level/HVPS1.PWR))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/SPM7054.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:C_2220_HandSoldering (layer B.Cu) (tedit 6364C08C)
    (at 70.924999 97.779311 180)
    (descr "Capacitor SMD 2220, hand soldering")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C6 (at -0.075001 -3.520689 180) (layer B.SilkS))
    (fp_text value 22uF (at 0 -3.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0.024999 -0.120689 180) (layer B.Fab))
    (pad 2 smd rect (at 3.5 0 180) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -3.5 0 180) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 6 /PCB_top_level/+12V_IN))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_2220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:C_2220_HandSoldering (layer B.Cu) (tedit 6364C091)
    (at 68.9 89.7 270)
    (descr "Capacitor SMD 2220, hand soldering")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C7 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value 22uF (at 0 -3.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0.024999 -0.200689 270) (layer B.Fab))
    (pad 1 smd rect (at -3.5 0 270) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 6 /PCB_top_level/+12V_IN))
    (pad 2 smd rect (at 3.5 0 270) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(C7-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_2220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:C_2220_HandSoldering (layer B.Cu) (tedit 6364BED9)
    (at 69 131.4 270)
    (descr "Capacitor SMD 2220, hand soldering")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C8 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value 22uF (at 0 -3.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 3.5 0 270) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -3.5 0 270) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 28 "/PCB_top_level/HVPS 2/V_BUS"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_2220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:C_2220_HandSoldering (layer B.Cu) (tedit 6364BF51)
    (at 70.8 123.4)
    (descr "Capacitor SMD 2220, hand soldering")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C9 (at 0.1 -3.5 180) (layer B.SilkS))
    (fp_text value 22uF (at 0 -3.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.5 0) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 28 "/PCB_top_level/HVPS 2/V_BUS"))
    (pad 2 smd rect (at 3.5 0) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(C9-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_2220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0805_HandSoldering (layer B.Cu) (tedit 63653D5B)
    (at 73.3 136.3 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 /PCB_top_level/HVPS2.RTN))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(C9-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0805_HandSoldering (layer B.Cu) (tedit 63653D61)
    (at 69.1 137.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 3.3 0.1) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 /PCB_top_level/HVPS2.RTN))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0805_HandSoldering (layer B.Cu) (tedit 63653D43)
    (at 63.2 94.9)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -3.3 0.1) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 /PCB_top_level/HVPS1.RTN))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(C7-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0805_HandSoldering (layer B.Cu) (tedit 63653D48)
    (at 63.2 97)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -3.3 0.1) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 /PCB_top_level/HVPS1.RTN))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:M80-5412022 (layer F.Cu) (tedit 62DC716C)
    (at 92 142)
    (descr M80-54120YY)
    (tags Connector)
    (fp_text reference J6 (at -25.5 2.5 90) (layer F.SilkS))
    (fp_text value "Harwin M80, 2x10" (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 /PCB_top_level/HVPS_TEMP+))
    (pad 2 thru_hole circle (at -2 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 /PCB_top_level/HVPS_TEMP2-))
    (pad 3 thru_hole circle (at -4 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 /PCB_top_level/HVPS_TEMP1-))
    (pad 4 thru_hole circle (at -6 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 /PCB_top_level/HVPS1_Vmon))
    (pad 5 thru_hole circle (at -8 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 /PCB_top_level/HVPS1_ON_OUT_5V))
    (pad 6 thru_hole circle (at -10 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 34 /PCB_top_level/HVPS1.PWR))
    (pad 7 thru_hole circle (at -12 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 31 /PCB_top_level/HVPS1.RTN))
    (pad 8 thru_hole circle (at -14 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /PCB_top_level/HVPS2_Vmon))
    (pad 9 thru_hole circle (at -16 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /PCB_top_level/HVPS2_Vset))
    (pad 10 thru_hole circle (at -18 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /PCB_top_level/HVPS2_Imon))
    (pad 11 thru_hole circle (at 0 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad11)"))
    (pad 12 thru_hole circle (at -2 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 "Net-(J6-Pad12)"))
    (pad 13 thru_hole circle (at -4 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 "Net-(J6-Pad13)"))
    (pad 14 thru_hole circle (at -6 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 44 "Net-(J6-Pad14)"))
    (pad 15 thru_hole circle (at -8 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 /PCB_top_level/HVPS1_Vset))
    (pad 16 thru_hole circle (at -10 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /PCB_top_level/HVPS1_Imon))
    (pad 17 thru_hole circle (at -12 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 35 /PCB_top_level/HVPS2.PWR))
    (pad 18 thru_hole circle (at -14 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 "Net-(J6-Pad18)"))
    (pad 19 thru_hole circle (at -16 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /PCB_top_level/HVPS2_ON_OUT_5V))
    (pad 20 thru_hole circle (at -18 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 /PCB_top_level/HVPS2.RTN))
    (pad 21 np_thru_hole circle (at 3.5 1) (size 2.2 0) (drill 2.2) (layers *.Cu *.Mask))
    (pad 22 np_thru_hole circle (at -21.5 1) (size 2.2 0) (drill 2.2) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/M80_5412022_ASM_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Aspera_footprints:Measurement_Point_Round-SMD-Pad_Big (layer F.Cu) (tedit 6364C4A3)
    (at 157.5 89.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference J7 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CON-HV (at 0 3) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers F.Cu F.Mask)
      (net 10 /PCB_top_level/-HV))
  )
  (module Aspera_footprints:Measurement_Point_Round-SMD-Pad_Big (layer F.Cu) (tedit 6364BCA9)
    (at 142.8 143.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference J8 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CON-RF (at 3.36 -0.24 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers F.Cu F.Mask)
      (net 26 /PCB_top_level/-RF))
  )
  (module Aspera_footprints:Steward_Logo (layer B.Cu) (tedit 5F2C1ACD)
    (at 97 122.7 90)
    (fp_text reference G1 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value STEWARD_LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Aspera_footprints:high_voltage (layer B.Cu) (tedit 0)
    (at 90 62.5 180)
    (fp_text reference G2 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "HV WARNING" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "100K on top\n2000pF cap on bottom" (at 191.2 133.1) (layer Dwgs.User))
  (gr_text "to\nReynolds 600" (at 176.4 123) (layer Dwgs.User))
  (gr_text 100K (at 139.4 130.7 60) (layer Dwgs.User))
  (gr_text "Full PCB fab instructions are in README_Aspera-UA-DWG-00004_HVPS.txt" (at 338.5 85.5) (layer B.Fab))
  (gr_text "Serial numbers on the delivered boards do NOT need to be contiguous" (at 338.5 70.5) (layer B.Fab))
  (gr_text "Characters shall be 2mm x 2mm" (at 338.5 65.5) (layer B.Fab))
  (gr_text "Serialize beginning with \"001\" in space provided" (at 338.5 60.7) (layer B.Fab))
  (gr_text 1 (at 345.4 60.7) (layer B.Fab))
  (gr_text 1 (at 60.9 42.5) (layer B.Fab))
  (gr_text "Build 1   S/N" (at 88.8 101.2 270) (layer B.Fab))
  (gr_text "ASPERA-UA-DWG-00004\nVersion 1.0\n2022/11/4   D. Hamara" (at 93.4 98.2 270) (layer B.Fab))
  (gr_text "Aspera HVPS Board" (at 97.4 98.8 270) (layer B.Fab))
  (gr_text "STEWARD OBSERVATORY" (at 99.9 98.8 270) (layer B.Fab))
  (gr_arc (start 165.9 54.1) (end 170 54.1) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 165.9 145.9) (end 165.9 150) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 54.1 145.9) (end 50 145.9) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 54.1 54.1) (end 54.1 50) (angle -90) (layer Edge.Cuts) (width 0.1))
  (dimension 120 (width 0.3) (layer F.Fab)
    (gr_text "120.000 mm" (at 110 157.6) (layer F.Fab))
    (feature1 (pts (xy 170 143.5) (xy 170 156.086421)))
    (feature2 (pts (xy 50 143.5) (xy 50 156.086421)))
    (crossbar (pts (xy 50 155.5) (xy 170 155.5)))
    (arrow1a (pts (xy 170 155.5) (xy 168.873496 156.086421)))
    (arrow1b (pts (xy 170 155.5) (xy 168.873496 154.913579)))
    (arrow2a (pts (xy 50 155.5) (xy 51.126504 156.086421)))
    (arrow2b (pts (xy 50 155.5) (xy 51.126504 154.913579)))
  )
  (dimension 100 (width 0.3) (layer F.Fab)
    (gr_text "100.000 mm" (at 40.9 100 270) (layer F.Fab))
    (feature1 (pts (xy 54 150) (xy 42.413579 150)))
    (feature2 (pts (xy 54 50) (xy 42.413579 50)))
    (crossbar (pts (xy 43 50) (xy 43 150)))
    (arrow1a (pts (xy 43 150) (xy 42.413579 148.873496)))
    (arrow1b (pts (xy 43 150) (xy 43.586421 148.873496)))
    (arrow2a (pts (xy 43 50) (xy 42.413579 51.126504)))
    (arrow2b (pts (xy 43 50) (xy 43.586421 51.126504)))
  )
  (gr_text "Build 1   S/N" (at 88.8 101.2 270) (layer B.SilkS))
  (gr_text "Aspera HVPS Board" (at 97.4 98.8 270) (layer B.SilkS))
  (gr_text "ASPERA-UA-DWG-00004\nVersion 1.0\n2022/11/4   D. Hamara" (at 93.4 98.2 270) (layer B.SilkS))
  (gr_text "STEWARD OBSERVATORY" (at 99.9 98.8 270) (layer B.SilkS))
  (gr_text "BOARD INSTALLATION:\n#4 x 3/8\" BUTTON HEAD HEX SCREW (MCMASTER # 98164A063)\nWITH NAS620C4 WASHER (MCMASTER # 90945A711) 9PL" (at 197.8 31.1) (layer Dwgs.User))
  (target plus (at 172 48) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 48.5 151.5) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_text "HIGH VOLTAGE" (at 90.7 71.7) (layer B.SilkS))
  (gr_text DANGER (at 90.5 52.5) (layer B.SilkS))
  (gr_line (start 128.35 50) (end 165.9 50) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170 79.25) (end 170 117.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170 127.9) (end 170 145.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3 150) (end 54.1 150) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132.95 150) (end 137.6 150) (angle -180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 170 122.55) (end 170 117.2) (angle -180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 170 73.9) (end 170 68.55) (angle -180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 123 50) (end 117.65 50) (angle -180) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50 145.9) (end 50 54.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.9 150) (end 137.6 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170 54.1) (end 170 68.55) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.1 50) (end 117.65 50) (layer Edge.Cuts) (width 0.1))
  (zone (net 9) (net_name CHASSIS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.3 50.3) (xy 101.3 50.3) (xy 101.3 149.4) (xy 50.2 149.4)
      )
    )
  )
  (zone (net 9) (net_name CHASSIS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.3 50.3) (xy 101.3 50.3) (xy 101.3 149.4) (xy 50.2 149.4)
      )
    )
  )
  (zone (net 4) (net_name "/PCB_top_level/HVPS 1/-HV_OUT") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 147.5 78.14) (xy 156.18 78.14) (xy 156.18 75.87) (xy 153.72 73.5) (xy 151.69 73.46)
        (xy 151.28 74.96) (xy 150.96 75.72) (xy 147.51 75.72)
      )
    )
  )
  (zone (net 10) (net_name /PCB_top_level/-HV) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 153.83 92.69) (xy 152.24 93.59) (xy 149.24 95.89) (xy 150.35 97.2) (xy 153.65 94.68)
        (xy 154.26 93.23)
      )
    )
  )
  (zone (net 29) (net_name "/PCB_top_level/HVPS 2/-RF_OUT") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 123.52 118.54) (xy 125.62 120.64) (xy 125.6 129.4) (xy 123 129.4) (xy 123.23 121.7)
        (xy 121.81 120.28)
      )
    )
  )
  (zone (net 32) (net_name "Net-(C1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 150.5 72.3) (xy 150.49 69.41) (xy 147.3 65.99) (xy 142.43 66.86) (xy 141.43 66.9)
        (xy 141.42 67.91) (xy 142.44 67.84) (xy 146.58 68.22) (xy 147.5 69.86) (xy 147.5 72.31)
      )
    )
  )
  (zone (net 5) (net_name "/PCB_top_level/HVPS 2/-HV_OUT") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 147.49 111.75) (xy 151 111.76) (xy 153.62 109.92) (xy 154.86 111.16) (xy 150.77 117.58)
        (xy 147.48 114.69)
      )
    )
  )
  (zone (net 45) (net_name "Net-(D4-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 154.59 123.83) (xy 143.02 123.94) (xy 142.86 122.04) (xy 154.5 120.89)
      )
    )
  )
  (zone (net 33) (net_name "Net-(C3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 125.92 116.17) (xy 128.81 113.21) (xy 129.97 111.58) (xy 131.61 108.8) (xy 133.36 105.96)
        (xy 143.52 105.83) (xy 146.93 101.61) (xy 150.51 105.55) (xy 150.51 108.27) (xy 147.1 108.28)
        (xy 143.55 106.97) (xy 134.31 106.95) (xy 130.93 112.37) (xy 129.9 114.94) (xy 129.8 116.53)
        (xy 128.02 118.27)
      )
    )
  )
  (zone (net 32) (net_name "Net-(C1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.75))
    (polygon
      (pts
        (xy 124.27 75.22) (xy 125.92 73.56) (xy 128.9 71.91) (xy 129.82 70.97) (xy 130.59 71.61)
        (xy 129.67 72.54) (xy 128.1 75.63) (xy 126.39 77.33)
      )
    )
  )
  (zone (net 1) (net_name "Net-(D2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 142.42 91.09) (xy 143.66 90.42) (xy 146.775 93.805) (xy 143.625 95.775)
      )
    )
  )
  (zone (net 30) (net_name "/PCB_top_level/HVPS 1/-RF_OUT") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.75))
    (polygon
      (pts
        (xy 121.85 77.69) (xy 125.56 81.4) (xy 125.46 88.01) (xy 122.96 88.15) (xy 122.54 81.73)
        (xy 120.1 79.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.9 101.1) (xy 73.1 101.1) (xy 73.05 95.1) (xy 68.55 95.1) (xy 68.6 101.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.897864 91.570018) (xy 71.897865 87.370018) (xy 65.897864 87.420018) (xy 65.897864 91.920018) (xy 71.897864 91.870018)
      )
    )
  )
  (zone (net 26) (net_name /PCB_top_level/-RF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 138.7 141.1) (xy 144.6 141.9) (xy 146.7 140.2) (xy 149.2 140.4) (xy 149.2 143.9)
        (xy 142.7 145.3) (xy 138.2 142.9)
      )
    )
  )
)
