(kicad_pcb (version 20171130) (host pcbnew "(5.1.0-0)")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 666)
    (zones 0)
    (modules 48)
    (nets 47)
  )
  (page A4)
  (layers
    (0 F.Cu jumper)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.1524)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.254)
    (segment_width 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 49.47 165.795)
    (grid_origin 49.47 165.795)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U5-Pad9)")
  (net 2 "Net-(U5-Pad8)")
  (net 3 +3V3)
  (net 4 "Net-(U5-Pad7)")
  (net 5 "Net-(U5-Pad12)")
  (net 6 "Net-(U5-Pad6)")
  (net 7 "Net-(U5-Pad5)")
  (net 8 "Net-(U5-Pad10)")
  (net 9 "Net-(U5-Pad11)")
  (net 10 GND)
  (net 11 +5V)
  (net 12 +12V)
  (net 13 /LED_IN_B)
  (net 14 /LED_IN_A)
  (net 15 "Net-(R5-Pad2)")
  (net 16 "Net-(R4-Pad2)")
  (net 17 "Net-(Q1-Pad1)")
  (net 18 "Net-(Q2-Pad1)")
  (net 19 "Net-(R11-Pad1)")
  (net 20 "Net-(Q1-Pad2)")
  (net 21 "Net-(Q2-Pad2)")
  (net 22 "Net-(U2-Pad4)")
  (net 23 "Net-(U2-Pad12)")
  (net 24 "Net-(U3-Pad12)")
  (net 25 "Net-(U3-Pad4)")
  (net 26 /BUZZER_DAC)
  (net 27 "/AUTON_EN_LED_(10_D10)")
  (net 28 /AUTON_EN_MOS_A)
  (net 29 /AUTON_EN_MOS_B)
  (net 30 "/RS485_TX_EN_(2_D2)")
  (net 31 "/7S_LED_(11_MOSI)")
  (net 32 "/7S_LED_(13_SCK)")
  (net 33 "/7S_LED_LAT_(12_D12)")
  (net 34 "/I_SEN_B_(A2)")
  (net 35 "/I_SEN_A_(A3)")
  (net 36 "/RS485_RX_(0_RX)")
  (net 37 "/RS485_TX_(1_TX)")
  (net 38 /CAN_EN_SW_B)
  (net 39 "/AUTON_EN_LED_FBK_(A0)")
  (net 40 /CAN_EN_SW_A)
  (net 41 "/CAN_EN_LED_(9_D9)")
  (net 42 /RS485+)
  (net 43 /RS485-)
  (net 44 "Net-(D4-Pad1)")
  (net 45 "Net-(D5-Pad1)")
  (net 46 "Net-(C7-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.381)
    (diff_pair_gap 0.635)
    (add_net "/7S_LED_(11_MOSI)")
    (add_net "/7S_LED_(13_SCK)")
    (add_net "/7S_LED_LAT_(12_D12)")
    (add_net "/AUTON_EN_LED_(10_D10)")
    (add_net "/AUTON_EN_LED_FBK_(A0)")
    (add_net /AUTON_EN_MOS_A)
    (add_net /AUTON_EN_MOS_B)
    (add_net /BUZZER_DAC)
    (add_net "/CAN_EN_LED_(9_D9)")
    (add_net /CAN_EN_SW_A)
    (add_net /CAN_EN_SW_B)
    (add_net "/I_SEN_A_(A3)")
    (add_net "/I_SEN_B_(A2)")
    (add_net /LED_IN_A)
    (add_net /LED_IN_B)
    (add_net /RS485+)
    (add_net /RS485-)
    (add_net "/RS485_RX_(0_RX)")
    (add_net "/RS485_TX_(1_TX)")
    (add_net "/RS485_TX_EN_(2_D2)")
    (add_net GND)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U5-Pad9)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 3.81)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.381)
    (diff_pair_gap 0.635)
    (add_net +12V)
  )
  (net_class board_power ""
    (clearance 0.1524)
    (trace_width 0.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.381)
    (diff_pair_gap 0.635)
    (add_net +3V3)
    (add_net +5V)
  )
  (module soar_lib:canvas_soar_logo (layer B.Cu) (tedit 0)
    (at 124.273 108.391 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 115.129 61.909)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 91.253 98.612)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 118.05 116.011)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 109.668 89.341)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D6 (at 0 2.5) (layer B.SilkS))
    (fp_text value D_TVS_x2 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 43 /RS485-))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 42 /RS485+))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 113.351 98.104 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at -2.921 0.127 90) (layer B.SilkS))
    (fp_text value FB (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C7-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 124.273 100.0875 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module soar_lib:Display_7Segment_DSM7TA39101T (layer F.Cu) (tedit 5CAE646B)
    (at 119.32 97.342)
    (fp_text reference U6 (at 0 -16.51) (layer F.SilkS))
    (fp_text value DSM7TA39101T (at 6.35 1.27) (layer F.Fab))
    (pad 5 smd rect (at 8.713 -0.508 90) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U5-Pad12)"))
    (pad 4 smd rect (at 6.833 -0.508 270) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U5-Pad7)"))
    (pad 3 smd rect (at 4.953 -0.508 90) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 3.073 -0.508 270) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U5-Pad8)"))
    (pad 1 smd rect (at 1.193 -0.508 270) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U5-Pad9)"))
    (pad 10 smd rect (at 1.193 -14.478 270) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U5-Pad11)"))
    (pad 9 smd rect (at 3.073 -14.478 270) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U5-Pad10)"))
    (pad 8 smd rect (at 4.953 -14.478 270) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at 6.833 -14.478 270) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U5-Pad5)"))
    (pad 6 smd rect (at 8.713 -14.478 270) (size 1.2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U5-Pad6)"))
  )
  (module soar_lib:SF_SAMD21_MINI (layer B.Cu) (tedit 5CAE45CB)
    (at 119.447 97.977)
    (fp_text reference U7 (at 15.113 6.858) (layer B.SilkS))
    (fp_text value SF_SAMD21_MINI (at 5 -27.2) (layer B.Fab))
    (pad 24 thru_hole circle (at 12.44 3.8) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 12.44 1.26) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 22 thru_hole circle (at 12.44 -1.28) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 12.44 -3.82) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 20 thru_hole circle (at 12.44 -6.36) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "/I_SEN_A_(A3)"))
    (pad 19 thru_hole circle (at 12.44 -8.9) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "/I_SEN_B_(A2)"))
    (pad 18 thru_hole circle (at 12.44 -11.44) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "/AUTON_EN_LED_FBK_(A0)"))
    (pad 17 thru_hole circle (at 12.44 -13.98) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "/AUTON_EN_LED_FBK_(A0)"))
    (pad 16 thru_hole circle (at 12.44 -16.52) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "/7S_LED_(13_SCK)"))
    (pad 15 thru_hole circle (at 12.44 -19.06) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "/7S_LED_LAT_(12_D12)"))
    (pad 14 thru_hole circle (at 12.44 -21.6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "/7S_LED_(11_MOSI)"))
    (pad 13 thru_hole circle (at 12.44 -24.14) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "/AUTON_EN_LED_(10_D10)"))
    (pad 12 thru_hole circle (at -2.8 -24.14) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "/CAN_EN_LED_(9_D9)"))
    (pad 11 thru_hole circle (at -2.8 -21.6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 /CAN_EN_SW_B))
    (pad 10 thru_hole circle (at -2.8 -19.06) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 /CAN_EN_SW_A))
    (pad 9 thru_hole circle (at -2.8 -16.52) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "/CAN_EN_LED_(9_D9)"))
    (pad 8 thru_hole circle (at -2.8 -13.98) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 /AUTON_EN_MOS_B))
    (pad 7 thru_hole circle (at -2.8 -11.44) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 /AUTON_EN_MOS_A))
    (pad 6 thru_hole circle (at -2.8 -8.9) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 /BUZZER_DAC))
    (pad 5 thru_hole circle (at -2.8 -6.36) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "/RS485_TX_EN_(2_D2)"))
    (pad 4 thru_hole circle (at -2.8 -3.82) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 3 thru_hole circle (at -2.8 -1.28) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.8 1.26) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "/RS485_RX_(0_RX)"))
    (pad 1 thru_hole circle (at -2.8 3.8) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "/RS485_TX_(1_TX)"))
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.94 73.339 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value TVS (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "/AUTON_EN_LED_FBK_(A0)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.129 67.243 90)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at 0 -1.651 90) (layer F.SilkS))
    (fp_text value TVS (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /CAN_EN_SW_B))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.416 64.703 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at 0.508 1.397 180) (layer F.SilkS))
    (fp_text value TVS (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.2655 64.703 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D5 (at 2.6925 0 180) (layer F.SilkS))
    (fp_text value TVS (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.844 73.339 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value TVS (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /CAN_EN_SW_A))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5CAE0FFF)
    (at 97.095 71.942 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -2.54 -0.381 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Dsub:DSUB-9_Female_Vertical_P2.77x2.84mm_MountingHoles (layer B.Cu) (tedit 59FEDEE2)
    (at 99.762 94.929 270)
    (descr "9-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 25mm")
    (fp_text reference J1 (at -5.54 5.89 270) (layer B.SilkS))
    (fp_text value DB9_Male_MountingHoles (at -5.54 -8.73 270) (layer B.Fab))
    (fp_text user %R (at -5.54 -1.42 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole circle (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 3 thru_hole circle (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 43 /RS485-))
    (pad 4 thru_hole circle (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 +12V))
    (pad 5 thru_hole circle (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 +12V))
    (pad 6 thru_hole circle (at -1.385 -2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 7 thru_hole circle (at -4.155 -2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 8 thru_hole circle (at -6.925 -2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 42 /RS485+))
    (pad 9 thru_hole circle (at -9.695 -2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 0 thru_hole circle (at -18.04 -1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 0 thru_hole circle (at 6.96 -1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Female_Vertical_P2.77x2.84mm_MountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 92.65 79.308 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 0 -5.461 270) (layer B.SilkS))
    (fp_text value "5V Connector Terminal" (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module soar_lib:Connector_Phoenix_TerminalBlock_2P_5mm_90D (layer B.Cu) (tedit 5C9625CD)
    (at 83.506 81.34 270)
    (descr 1729018)
    (tags Connector)
    (fp_text reference J5 (at -3.937 3.302) (layer B.SilkS))
    (fp_text value LED_IN_CABIN (at -5.969 14.478 270) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask B.SilkS)
      (net 13 /LED_IN_B))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask B.SilkS)
      (net 12 +12V))
  )
  (module soar_lib:Connector_Phoenix_TerminalBlock_2P_5mm_90D (layer B.Cu) (tedit 5C9625CD)
    (at 83.506 98.358 90)
    (descr 1729018)
    (tags Connector)
    (fp_text reference J2 (at -3.937 -3.175 180) (layer B.SilkS))
    (fp_text value LED_IN_ROOF (at -8.89 -14.351 90) (layer B.SilkS) hide)
    (pad 2 thru_hole circle (at 5 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask B.SilkS)
      (net 12 +12V))
    (pad 1 thru_hole rect (at 0 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask B.SilkS)
      (net 14 /LED_IN_A))
  )
  (module soar_lib:Buzzer_SMD_CPT_9019S (layer F.Cu) (tedit 5C87A7EC)
    (at 93.285 89.595)
    (attr smd)
    (fp_text reference BZ1 (at -5.461 0 90) (layer F.SilkS))
    (fp_text value Buzzer (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 4.064) (size 4.2 2) (layers F.Cu F.Paste F.Mask)
      (net 26 /BUZZER_DAC))
    (pad 2 smd rect (at 0 -4.064) (size 4.2 2) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 131.131 70.291 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -0.762 1.778 90) (layer F.SilkS))
    (fp_text value 180 (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "/AUTON_EN_LED_(10_D10)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 110.415 82.991 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 4.826 0.142 90) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at -2.727243 3.908015 -90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 /RS485-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 112.3985 82.991 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 /RS485+))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 111.3825 85.785 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.7305 0 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 /RS485-))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 /RS485+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 119.066 62.163 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0.889 1.778 180) (layer F.SilkS))
    (fp_text value 180 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "/CAN_EN_LED_(9_D9)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5CAE1004)
    (at 101.032 118.678)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 2.921 0) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.65) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /AUTON_EN_MOS_A))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 96.968 117.027 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 2.921 0.127 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(Q1-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 112.97 70.799 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.794 0 -90) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 29 /AUTON_EN_MOS_B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 119.32 89.214 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 3.175 0 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 115.129 70.799 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 2.794 0 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 "/RS485_TX_EN_(2_D2)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-3_TabPin2 (layer B.Cu) (tedit 5A70FB8C)
    (at 103.445 111.693)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference Q1 (at 9.398 0.127 90) (layer B.SilkS))
    (fp_text value NMOS (at 0 -6.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -5.775 0) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 20 "Net-(Q1-Pad2)"))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-3_TabPin2 (layer B.Cu) (tedit 5A70FB8C)
    (at 103.445 67.243)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference Q2 (at 9.525 -1.524 90) (layer B.SilkS))
    (fp_text value NMOS (at 0 -6.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -5.775 0) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 21 "Net-(Q2-Pad2)"))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 110.303 94.675)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 2.794 0 90) (layer B.SilkS))
    (fp_text value TLV75533PDBV (at 0 -2.54) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 11 +5V))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 11 +5V))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-16_4.4x5mm_P0.65mm (layer B.Cu) (tedit 5A02F25C)
    (at 89.475 107.121 135)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 3.81 135) (layer B.SilkS))
    (fp_text value INA250-Q1 (at 0 -3.55 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 1 smd rect (at -2.95 2.275 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at -2.95 1.625001 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at -2.95 0.975 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(Q1-Pad2)"))
    (pad 4 smd rect (at -2.95 0.325 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -2.95 -0.325 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U2-Pad4)"))
    (pad 6 smd rect (at -2.95 -0.975 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 7 smd rect (at -2.95 -1.625001 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 8 smd rect (at -2.95 -2.275 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 9 smd rect (at 2.95 -2.275 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 35 "/I_SEN_A_(A3)"))
    (pad 10 smd rect (at 2.95 -1.625001 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 11 smd rect (at 2.95 -0.975 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 12 smd rect (at 2.95 -0.325 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 2.95 0.325 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(U2-Pad12)"))
    (pad 14 smd rect (at 2.95 0.975 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 /LED_IN_A))
    (pad 15 smd rect (at 2.95 1.625001 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 /LED_IN_A))
    (pad 16 smd rect (at 2.95 2.275 135) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 /LED_IN_A))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-16_4.4x5mm_P0.65mm (layer B.Cu) (tedit 5A02F25C)
    (at 89.475 72.831 225)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at -0.127 3.81 225) (layer B.SilkS))
    (fp_text value INA250-Q1 (at 0 -3.55 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 1 smd rect (at -2.95 2.275 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at -2.95 1.625 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at -2.95 0.975 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(Q2-Pad2)"))
    (pad 4 smd rect (at -2.95 0.325 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -2.95 -0.325 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U3-Pad4)"))
    (pad 6 smd rect (at -2.95 -0.975 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 7 smd rect (at -2.95 -1.625 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 8 smd rect (at -2.95 -2.275 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 9 smd rect (at 2.95 -2.275 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 "/I_SEN_B_(A2)"))
    (pad 10 smd rect (at 2.95 -1.625 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 11 smd rect (at 2.95 -0.975 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 12 smd rect (at 2.95 -0.325 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U3-Pad12)"))
    (pad 13 smd rect (at 2.95 0.325 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U3-Pad12)"))
    (pad 14 smd rect (at 2.95 0.975 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 /LED_IN_B))
    (pad 15 smd rect (at 2.95 1.625 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 /LED_IN_B))
    (pad 16 smd rect (at 2.95 2.275 225) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 /LED_IN_B))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-16_4.4x5mm_P0.65mm (layer B.Cu) (tedit 5A02F25C)
    (at 124.527 89.849 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U5 (at 0 3.55 180) (layer B.SilkS))
    (fp_text value MAX6968AUE+ (at 0 -3.55 180) (layer B.Fab))
    (fp_text user %R (at -0.225001 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2.95 2.275 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at -2.95 1.625 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 31 "/7S_LED_(11_MOSI)"))
    (pad 3 smd rect (at -2.95 0.975 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 32 "/7S_LED_(13_SCK)"))
    (pad 4 smd rect (at -2.95 0.325 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 "/7S_LED_LAT_(12_D12)"))
    (pad 5 smd rect (at -2.95 -0.325 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(U5-Pad5)"))
    (pad 6 smd rect (at -2.95 -0.975 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U5-Pad6)"))
    (pad 7 smd rect (at -2.95 -1.625 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U5-Pad7)"))
    (pad 8 smd rect (at -2.95 -2.275 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(U5-Pad8)"))
    (pad 9 smd rect (at 2.95 -2.275 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(U5-Pad9)"))
    (pad 10 smd rect (at 2.95 -1.625 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(U5-Pad10)"))
    (pad 11 smd rect (at 2.95 -0.975 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(U5-Pad11)"))
    (pad 12 smd rect (at 2.95 -0.325 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(U5-Pad12)"))
    (pad 13 smd rect (at 2.95 0.325 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 14 smd rect (at 2.95 0.975 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 2.95 1.625 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(R11-Pad1)"))
    (pad 16 smd rect (at 2.95 2.275 180) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5A02F2D3)
    (at 111.3825 77.53 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -3.429 270) (layer B.SilkS))
    (fp_text value SN65HVD72DR (at 0 -3.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 36 "/RS485_RX_(0_RX)"))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 "/RS485_TX_EN_(2_D2)"))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 "/RS485_TX_EN_(2_D2)"))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 37 "/RS485_TX_(1_TX)"))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(R4-Pad2)"))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(R5-Pad2)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 119.066 70.164)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J4 (at 3.429 -7.62) (layer B.SilkS))
    (fp_text value "CAN Tx Enable" (at 1.27 -7.41) (layer B.Fab))
    (fp_text user %R (at 1.27 -2.54 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /CAN_EN_SW_A))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /CAN_EN_SW_B))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(D5-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 125.162 70.164)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J3 (at 5.334 -2.54) (layer B.SilkS))
    (fp_text value "Autonomous Enable" (at 1.27 -4.87) (layer B.Fab))
    (fp_text user %R (at 1.27 -1.27 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/AUTON_EN_LED_FBK_(A0)"))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 124.273 80.197 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at -7.830205 9.957667 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 120.59 85.785)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.651) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 -6.604) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 111.446 98.231 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.667 0 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C7-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 92.142 75.625 45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 1.65 45) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 45) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.9375 0 45) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5C9CCCE3)
    (at 89.856 79.689 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.54 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 109.287 98.231 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.667 0 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 84.014 103.565 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 1.65 135) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 2 smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 1 smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 82.49 105.089 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.796051 135) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 1 smd roundrect (at -0.937501 0 135) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.937501 0 135) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 108.525 82.991 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.54 -0.254 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text HIB-V1.0 (at 120.717 112.709) (layer B.SilkS))
  (gr_text LED- (at 78.299 98.358 270) (layer B.SilkS))
  (gr_text LED- (at 78.299 81.34 270) (layer B.SilkS))
  (gr_text LED+ (at 78.299 93.278 270) (layer B.SilkS))
  (gr_text LED+ (at 78.299 86.293 270) (layer B.SilkS))
  (gr_arc (start 108.271 90.103) (end 139.258999 79.689001) (angle 360) (layer Edge.Cuts) (width 0.254))
  (gr_text "Approximate size of cupholders in the car" (at 111.446 46.923) (layer Eco1.User))
  (dimension 25.4 (width 0.3) (layer Eco1.User)
    (gr_text "1.0000 in" (at 219.591 89.959195 90) (layer Eco1.User))
    (feature1 (pts (xy 144.464468 77.259195) (xy 218.077421 77.259195)))
    (feature2 (pts (xy 144.464468 102.659195) (xy 218.077421 102.659195)))
    (crossbar (pts (xy 217.491 102.659195) (xy 217.491 77.259195)))
    (arrow1a (pts (xy 217.491 77.259195) (xy 218.077421 78.385699)))
    (arrow1b (pts (xy 217.491 77.259195) (xy 216.904579 78.385699)))
    (arrow2a (pts (xy 217.491 102.659195) (xy 218.077421 101.532691)))
    (arrow2b (pts (xy 217.491 102.659195) (xy 216.904579 101.532691)))
  )
  (dimension 19.05 (width 0.3) (layer Eco1.User)
    (gr_text "0.7500 in" (at 155.859525 131.688208) (layer Eco1.User))
    (feature1 (pts (xy 165.384525 77.089341) (xy 165.384525 130.174629)))
    (feature2 (pts (xy 146.334525 77.089341) (xy 146.334525 130.174629)))
    (crossbar (pts (xy 146.334525 129.588208) (xy 165.384525 129.588208)))
    (arrow1a (pts (xy 165.384525 129.588208) (xy 164.258021 130.174629)))
    (arrow1b (pts (xy 165.384525 129.588208) (xy 164.258021 129.001787)))
    (arrow2a (pts (xy 146.334525 129.588208) (xy 147.461029 130.174629)))
    (arrow2b (pts (xy 146.334525 129.588208) (xy 147.461029 129.001787)))
  )
  (zone (net 14) (net_name /LED_IN_A) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 88.459 105.216) (xy 90.237 103.438) (xy 84.268 96.834) (xy 81.982 96.834) (xy 81.982 99.628)
        (xy 83.252 101.025) (xy 84.268 101.025)
      )
    )
  )
  (zone (net 23) (net_name "Net-(U2-Pad12)") (layer B.Cu) (hatch edge 0.508)
    (priority 9)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 86.3 104.835) (xy 87.189 103.946) (xy 88.459 105.216) (xy 87.57 106.105)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 86.681 106.994) (xy 87.062 106.613) (xy 85.792 105.343) (xy 85.792 104.073) (xy 84.776 103.057)
        (xy 81.855 105.851) (xy 82.998 106.994) (xy 84.395 105.597) (xy 85.284 105.597)
      )
    )
  )
  (zone (net 22) (net_name "Net-(U2-Pad4)") (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 90.491 109.026) (xy 91.761 110.296) (xy 92.65 109.407) (xy 91.38 108.137)
      )
    )
  )
  (zone (net 20) (net_name "Net-(Q1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 91.38 108.137) (xy 92.777 109.534) (xy 92.777 113.09) (xy 100.524 113.09) (xy 101.921 117.281)
        (xy 111.7 117.281) (xy 111.7 106.105) (xy 102.048 106.105) (xy 100.524 110.423) (xy 95.19 110.423)
        (xy 94.809 110.042) (xy 94.809 108.264) (xy 93.031 106.486)
      )
    )
  )
  (zone (net 12) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 81.982 95.437) (xy 81.982 83.88) (xy 93.793 83.88) (xy 95.317 82.483) (xy 101.286 82.483)
        (xy 101.286 88.071) (xy 98.492 88.071) (xy 91.126 95.437)
      )
    )
  )
  (zone (net 13) (net_name /LED_IN_B) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 82.363 83.245) (xy 86.3 83.245) (xy 86.3 74.99) (xy 87.697 73.593) (xy 85.157 71.053)
        (xy 82.363 73.847)
      )
    )
  )
  (zone (net 24) (net_name "Net-(U3-Pad12)") (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 86.427 75.117) (xy 87.189 75.879) (xy 88.332 74.736) (xy 87.57 73.974)
      )
    )
  )
  (zone (net 25) (net_name "Net-(U3-Pad4)") (layer B.Cu) (hatch edge 0.508)
    (priority 15)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 90.491 70.926) (xy 91.38 71.815) (xy 92.65 70.545) (xy 91.761 69.656)
      )
    )
  )
  (zone (net 21) (net_name "Net-(Q2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 90.491 70.799) (xy 92.777 68.513) (xy 102.048 68.513) (xy 102.048 72.704) (xy 111.573 72.704)
        (xy 111.573 61.655) (xy 102.048 61.655) (xy 102.048 65.973) (xy 90.491 65.973) (xy 88.078 68.386)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 141.545 123.631) (xy 74.87 123.631) (xy 74.87 56.575) (xy 141.545 56.575)
      )
    )
  )
  (zone (net 11) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 14)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 110.176 95.183) (xy 110.176 96.199) (xy 103.445 96.199) (xy 101.286 94.04) (xy 101.286 92.389)
        (xy 107.128 92.389) (xy 108.398 93.278) (xy 110.176 93.278) (xy 110.176 94.167) (xy 106.747 94.167)
        (xy 106.747 95.183)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 74.87 123.631) (xy 141.672 123.631) (xy 141.672 56.575) (xy 74.87 56.575)
      )
    )
  )
)
