(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 59)
    (zones 0)
    (modules 7)
    (nets 53)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom jumper)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 T5)
  (net 2 T23)
  (net 3 T18)
  (net 4 T0)
  (net 5 T4)
  (net 6 T22)
  (net 7 T19)
  (net 8 T1)
  (net 9 T3)
  (net 10 T21)
  (net 11 T20)
  (net 12 T2)
  (net 13 T9)
  (net 14 T17)
  (net 15 T6)
  (net 16 T8)
  (net 17 T7)
  (net 18 "Net-(U1-Pad17)")
  (net 19 "Net-(U1-Pad18)")
  (net 20 "Net-(U1-Pad19)")
  (net 21 "Net-(U1-Pad20)")
  (net 22 "Net-(U1-Pad16)")
  (net 23 "Net-(U1-Pad15)")
  (net 24 "Net-(U1-Pad14)")
  (net 25 "Net-(U1-Pad31)")
  (net 26 "Net-(U1-Pad32)")
  (net 27 "Net-(U1-Pad33)")
  (net 28 "Net-(U1-Pad34)")
  (net 29 "Net-(U1-Pad35)")
  (net 30 "Net-(U1-Pad36)")
  (net 31 "Net-(U1-Pad37)")
  (net 32 "Net-(U1-Pad13)")
  (net 33 "Net-(U1-Pad12)")
  (net 34 "Net-(U1-Pad1)")
  (net 35 "Net-(U1-Pad38)")
  (net 36 "Net-(U1-Pad39)")
  (net 37 "Net-(U1-Pad42)")
  (net 38 "Net-(U1-Pad43)")
  (net 39 "Net-(U1-Pad44)")
  (net 40 "Net-(U1-Pad45)")
  (net 41 "Net-(U1-Pad46)")
  (net 42 "Net-(U1-Pad47)")
  (net 43 "Net-(U1-Pad48)")
  (net 44 "Net-(U1-Pad50)")
  (net 45 "Net-(U1-Pad51)")
  (net 46 "Net-(U1-Pad52)")
  (net 47 T14)
  (net 48 T15)
  (net 49 T16)
  (net 50 "Net-(U1-Pad40)")
  (net 51 "Net-(U1-Pad41)")
  (net 52 "Net-(U1-Pad49)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad52)")
    (add_net T0)
    (add_net T1)
    (add_net T14)
    (add_net T15)
    (add_net T16)
    (add_net T17)
    (add_net T18)
    (add_net T19)
    (add_net T2)
    (add_net T20)
    (add_net T21)
    (add_net T22)
    (add_net T23)
    (add_net T3)
    (add_net T4)
    (add_net T5)
    (add_net T6)
    (add_net T7)
    (add_net T8)
    (add_net T9)
  )
  (module teensy:Teensy30_31_32_LC (layer Top) (tedit 5C4E3CB6)
    (at 151.13 97.155)
    (fp_text reference U1 (at 0 -10.16) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 0 10.16) (layer F.Fab))
    (fp_text user T3.2 (at -10.16 -2.54 90) (layer F.SilkS))
    (pad 17 thru_hole circle (at 16.51 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at 16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-Pad20)"))
    (pad 16 thru_hole circle (at 16.51 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U1-Pad16)"))
    (pad 15 thru_hole circle (at 16.51 5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-Pad15)"))
    (pad 14 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-Pad14)"))
    (pad 21 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 T14))
    (pad 22 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 T15))
    (pad 23 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 49 T16))
    (pad 24 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 T17))
    (pad 25 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 T18))
    (pad 26 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 T19))
    (pad 27 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 T20))
    (pad 28 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 T21))
    (pad 29 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 T22))
    (pad 30 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 T23))
    (pad 31 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U1-Pad32)"))
    (pad 33 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U1-Pad33)"))
    (pad 34 thru_hole circle (at -13.97 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U1-Pad34)"))
    (pad 35 thru_hole circle (at -8.89 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U1-Pad35)"))
    (pad 36 thru_hole circle (at -6.35 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U1-Pad36)"))
    (pad 37 thru_hole circle (at -3.81 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U1-Pad37)"))
    (pad 13 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U1-Pad13)"))
    (pad 12 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad12)"))
    (pad 11 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 T9))
    (pad 10 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 16 T8))
    (pad 9 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 T7))
    (pad 8 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 T6))
    (pad 7 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 T5))
    (pad 6 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 T4))
    (pad 5 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 T3))
    (pad 4 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 T2))
    (pad 3 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 T1))
    (pad 2 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 T0))
    (pad 1 thru_hole rect (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad1)"))
    (pad 38 thru_hole circle (at -1.27 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad38)"))
    (pad 39 thru_hole circle (at 1.27 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad39)"))
    (pad 40 thru_hole circle (at 3.81 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad40)"))
    (pad 41 thru_hole circle (at 6.35 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(U1-Pad41)"))
    (pad 42 thru_hole circle (at 8.89 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad42)"))
    (pad 43 thru_hole circle (at 11.43 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad43)"))
    (pad 44 thru_hole circle (at 13.97 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad44)"))
    (pad 45 thru_hole circle (at 13.97 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad45)"))
    (pad 46 thru_hole circle (at 11.43 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad46)"))
    (pad 47 thru_hole circle (at 8.89 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad47)"))
    (pad 48 thru_hole circle (at 6.35 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad48)"))
    (pad 49 thru_hole circle (at 3.81 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(U1-Pad49)"))
    (pad 50 thru_hole circle (at 1.27 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad50)"))
    (pad 51 thru_hole circle (at -1.27 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad51)"))
    (pad 52 thru_hole circle (at -10.16 0) (size 1.9 1.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U1-Pad52)"))
  )
  (module Keyboard_Scanner:STAGGERED_8_PIN_THT (layer Top) (tedit 5C4E2309)
    (at 144.78 109.855)
    (fp_text reference J2 (at -8.95 0 90) (layer F.SilkS))
    (fp_text value Conn_01x08_Female (at -2 0) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 T3))
    (pad 7 thru_hole oval (at 1.27 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 T20))
    (pad 6 thru_hole oval (at 0 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 T2))
    (pad 5 thru_hole oval (at -1.27 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 T21))
    (pad 4 thru_hole oval (at -2.54 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 T1))
    (pad 3 thru_hole oval (at -3.81 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 T22))
    (pad 2 thru_hole oval (at -5.08 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 T0))
    (pad 1 thru_hole oval (at -6.35 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 T23))
  )
  (module Keyboard_Scanner:STAGGERED_12_PIN_THT (layer Top) (tedit 5C4E2194)
    (at 160.02 109.855)
    (fp_text reference J1 (at -8.95 0 90) (layer F.SilkS))
    (fp_text value Conn_01x12_Female (at 0 0) (layer F.Fab))
    (pad 1 thru_hole oval (at -6.35 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 T19))
    (pad 2 thru_hole oval (at -5.08 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 T4))
    (pad 3 thru_hole oval (at -3.81 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 T18))
    (pad 4 thru_hole oval (at -2.54 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 T5))
    (pad 5 thru_hole oval (at -1.27 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 T17))
    (pad 6 thru_hole oval (at 0 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 T6))
    (pad 7 thru_hole oval (at 1.27 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 T16))
    (pad 8 thru_hole oval (at 2.54 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 T7))
    (pad 9 thru_hole oval (at 3.81 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 T15))
    (pad 10 thru_hole oval (at 5.08 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 T8))
    (pad 11 thru_hole oval (at 6.35 -1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 T14))
    (pad 12 thru_hole oval (at 7.62 1.1) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 T9))
  )
  (module "" (layer Top) (tedit 0)
    (at 168.91 114.935)
    (fp_text reference @HOLE0 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 168.8211 84.9376)
    (fp_text reference @HOLE1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 133.35 84.9376)
    (fp_text reference @HOLE2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 133.35 114.935)
    (fp_text reference @HOLE3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )
  (gr_text "RLC 27-Jan-2019\nToshiba T2000sxe Adapter" (at 150.495 114.935) (layer B.SilkS))
  (gr_line (start 129.54 118.745) (end 129.54 81.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 81.28) (end 172.72 81.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 81.28) (end 172.72 118.745) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 118.745) (end 129.54 118.745) (layer Edge.Cuts) (width 0.15))
  (gr_text "3.2 Keyboard Scanner" (at 137.16 84.455) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2024) (thermal_bridge_width 0.2024))
    (polygon
      (pts
        (xy 130.175 81.915) (xy 130.175 118.11) (xy 172.085 118.11) (xy 172.085 81.915)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2024) (thermal_bridge_width 0.2024))
    (polygon
      (pts
        (xy 130.175 81.915) (xy 130.175 118.11) (xy 172.085 118.11) (xy 172.085 81.915)
      )
    )
  )
)
