(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 59)
    (zones 0)
    (modules 16)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 /+5V)
  (net 10 GND)
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(J3-Pad4)")
  (net 13 "Net-(J3-Pad3)")
  (net 14 "Net-(J3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /+5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
  )
  (module Potentiometer_THT:Potentiometer_ACP_CA9-H2,5_Horizontal (layer F.Cu) (tedit 5A3D4994)
    (at 126.365 90.17 90)
    (descr "Potentiometer, horizontal, ACP CA9-H2,5, http://www.acptechnologies.com/wp-content/uploads/2017/05/02-ACP-CA9-CE9.pdf")
    (tags "Potentiometer horizontal ACP CA9-H2,5")
    (fp_text reference RV2 (at 0 -3.65 90) (layer F.SilkS))
    (fp_text value "0-100 ohm" (at 0 8.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.4 2.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 2.5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (pad 3 thru_hole circle (at 0 5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_ACP_CA9-H2,5_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_ACP_CA9-H2,5_Horizontal (layer F.Cu) (tedit 5A3D4994)
    (at 150.495 90.17 90)
    (descr "Potentiometer, horizontal, ACP CA9-H2,5, http://www.acptechnologies.com/wp-content/uploads/2017/05/02-ACP-CA9-CE9.pdf")
    (tags "Potentiometer horizontal ACP CA9-H2,5")
    (fp_text reference RV1 (at 0 -3.65 90) (layer F.SilkS))
    (fp_text value "0-100 ohm" (at 0 8.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.4 2.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 2.5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at 0 5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_ACP_CA9-H2,5_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 123.825 121.92 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.175 2.54 90) (layer F.SilkS))
    (fp_text value "10 ohm" (at 5.08 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad4)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 137.795 95.885 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value "0-100 ohm" (at 5.08 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 143.51 95.885 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value "0-100 ohm " (at 5.08 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 147.32 107.95)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value "75 ohm" (at 5.08 2.37) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 157.48 100.965 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 2.54) (layer F.SilkS))
    (fp_text value "75 ohm" (at 5.08 2.37) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 128.905 113.03 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value S8050 (at 1.27 2.79 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 /+5V))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 152.4 113.03 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value S8050 (at 1.27 2.79 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 /+5V))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x04_P3.81mm_Drill1mm (layer F.Cu) (tedit 5AEE60B2)
    (at 135.255 77.47 180)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J3 (at 5.715 -3.175) (layer F.Fab) hide)
    (fp_text value Conn_01x04 (at 5.715 3.175) (layer F.Fab) hide)
    (fp_text user %R (at 5.715 0) (layer F.Fab))
    (pad 4 thru_hole circle (at 11.43 0 180) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at 7.62 0 180) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module Connector_Wire:SolderWirePad_1x03_P3.175mm_Drill1mm (layer F.Cu) (tedit 5AEE5F67)
    (at 123.825 129.985)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J2 (at 3.175 -3.81) (layer F.Fab) hide)
    (fp_text value Conn_01x03 (at 3.175 3.175) (layer F.Fab) hide)
    (fp_text user %R (at 3.175 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 6.35 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill1mm (layer F.Cu) (tedit 5AEE5F04)
    (at 157.48 130.175 180)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J1 (at 1.905 -3.81) (layer F.Fab) hide)
    (fp_text value Conn_01x02 (at 1.905 3.81) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 /+5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 137.795 114.3 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 3.81 -2.12 90) (layer F.SilkS))
    (fp_text value 1n4148 (at 3.81 2.12 90) (layer F.Fab) hide)
    (fp_text user K (at 0 -1.8 90) (layer F.SilkS))
    (fp_text user K (at 0 -1.8 90) (layer F.Fab))
    (fp_text user %R (at 4.11 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 144.145 114.3 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 3.81 -2.12 90) (layer F.SilkS))
    (fp_text value 1n4148 (at 3.81 2.12 90) (layer F.Fab) hide)
    (fp_text user K (at 0 -1.905 90) (layer F.SilkS))
    (fp_text user K (at 0 -1.8 90) (layer F.Fab))
    (fp_text user %R (at 4.11 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 128.905 104.775 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.25 -4.4 90) (layer F.SilkS))
    (fp_text value "220 uF" (at 1.25 4.4 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 139.7 104.775 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -4.4 90) (layer F.SilkS))
    (fp_text value "220 uF" (at 1.25 4.4 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Jumper R4 and R3 and leave\nRV1 and RV2 unpopulated\nif using transistors." (at 141.605 126.365) (layer B.SilkS))
  (gr_text "S-ENC-YUV v1.0\nKPackLabs 2023-02" (at 149.86 77.47) (layer F.SilkS))
  (gr_line (start 160.655 73.66) (end 160.655 133.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 73.66) (end 160.655 73.66) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 133.35) (end 120.65 73.66) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.655 133.35) (end 120.65 133.35) (layer Edge.Cuts) (width 0.1))
  (gr_text OUTPUT (at 129.54 82.55) (layer F.SilkS))
  (gr_text GND (at 135.255 80.645) (layer F.SilkS))
  (gr_text Pr (at 131.445 80.645) (layer F.SilkS))
  (gr_text Pb (at 127.635 80.645) (layer F.SilkS))
  (gr_text Y (at 123.825 80.645) (layer F.SilkS))
  (gr_text GND (at 157.48 127) (layer F.SilkS))
  (gr_text 5V (at 153.67 127) (layer F.SilkS))
  (gr_text INPUT (at 127 125.095) (layer F.SilkS))
  (gr_text Pr (at 130.175 127) (layer F.SilkS))
  (gr_text Pb (at 127 127) (layer F.SilkS))
  (gr_text Y (at 123.825 127) (layer F.SilkS))
)
