<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0.381" y1="35.59" x2="0.381" y2="24.012025" width="0" layer="20"/>
<wire x1="0.381" y1="24.012025" x2="0.8209875" y2="23.3090125" width="0" layer="20" curve="45"/>
<wire x1="0.8209875" y1="23.3090125" x2="1.2110125" y2="22.7919875" width="0" layer="20"/>
<wire x1="1.2110125" y1="22.7919875" x2="1.27" y2="22.596975" width="0" layer="20" curve="-45"/>
<wire x1="1.27" y1="22.596975" x2="1.27" y2="15.376025" width="0" layer="20"/>
<wire x1="1.27" y1="15.376025" x2="1.0840125" y2="15.0540125" width="0" layer="20" curve="-45"/>
<wire x1="1.0840125" y1="15.0540125" x2="0.5669875" y2="14.4099875" width="0" layer="20"/>
<wire x1="0.5669875" y1="14.4099875" x2="0.381" y2="13.960975" width="0" layer="20" curve="45"/>
<wire x1="0.381" y1="13.960975" x2="0.381" y2="2.5" width="0" layer="20"/>
<wire x1="0.381" y1="2.5" x2="2.881" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.881" y1="0" x2="41.62" y2="0" width="0" layer="20"/>
<wire x1="41.62" y1="0" x2="44.12" y2="2.5" width="0" layer="20" curve="90"/>
<wire x1="44.12" y1="2.5" x2="44.07030625" y2="13.70875" width="0" layer="20"/>
<wire x1="44.07030625" y1="13.70875" x2="43.884328125" y2="14.154671875" width="0" layer="20" curve="44.718902"/>
<wire x1="43.884328125" y1="14.154671875" x2="43.3659875" y2="14.6730125" width="0" layer="20"/>
<wire x1="43.3659875" y1="14.6730125" x2="43.18" y2="15.122025" width="0" layer="20" curve="-45"/>
<wire x1="43.18" y1="15.122025" x2="43.18" y2="22.596975" width="0" layer="20"/>
<wire x1="43.18" y1="22.596975" x2="43.3659875" y2="23.0459875" width="0" layer="20" curve="-45"/>
<wire x1="43.3659875" y1="23.0459875" x2="43.9340125" y2="23.6140125" width="0" layer="20"/>
<wire x1="43.9340125" y1="23.6140125" x2="44.12" y2="24.063025" width="0" layer="20" curve="45"/>
<wire x1="44.12" y1="24.063025" x2="44.12" y2="35.59" width="0" layer="20"/>
<wire x1="44.12" y1="35.59" x2="41.62" y2="38.09" width="0" layer="20" curve="90"/>
<wire x1="41.62" y1="38.09" x2="2.881" y2="38.09" width="0" layer="20"/>
<wire x1="2.881" y1="38.09" x2="0.381" y2="35.59" width="0" layer="20" curve="90"/>
<text>2019</text>
<text>+</text>
<text>+</text>
<text>MIDI F-to-MIDI F
rev 0.2</text>
<text>Type A KORG</text>
<text>Type B 1010
Arturia</text>
<text>Type A KORG</text>
<text>Type B 1010
Arturia</text>
<hole x="41.275" y="19.177" drill="2.794"/>
<hole x="3.302" y="19.177" drill="2.794"/>
<text>MIDI F-to-MIDI F
DIN-5 / TRS
Type A or B</text>
<text>/Users/JEP/Dropbox (Personal)/Adafruit_Industries/john_park_logo_forPCB_300dpi.bmp</text>
<text>/Users/JEP/Dropbox (Personal)/Adafruit_Industries/john_park_logo_forPCB_300dpi.bmp</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="CP-2350">
<description>Female &lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
5 pins 90 deg. with shield, horizontal (DIN 41524)</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="STX3100">
<description>&lt;b&gt;MIC/HEADPHONE JACK&lt;/b&gt;&lt;p&gt;
KS-S stereo microphone/headphone jack&lt;p&gt;
 PG203JN (Schukat)</description>
</package>
<package name="RGBLED5050">
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH_DPDT_SMD_JS202011JCQN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="adafruit" package="CP-2350" value="DIN_MIDI">
<attribute name="4POS" value=""/>
<attribute name="5NEG" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="adafruit" package="CP-2350" value="MIDIJACK">
<attribute name="4POS" value=""/>
<attribute name="5NEG" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="adafruit" package="STX3100" value="TRS_MIDI">
<attribute name="NAME"/>
<attribute name="RING" value=""/>
<attribute name="SHIELD" value=""/>
<attribute name="TIP" value=""/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="adafruit" package="STX3100" value="TRS_MIDI">
<attribute name="NAME"/>
<attribute name="RING" value=""/>
<attribute name="SHIELD" value=""/>
<attribute name="TIP" value=""/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="SWITCH_DPDT_SMD_JS202011JCQN" value="TRS_MIDI_TYPE">
<attribute name="PROD_ID" value="SWCH-14133"/>
<attribute name="TYPE-A" value=""/>
<attribute name="TYPE-B" value=""/>
</element>
<element name="S2" library="SparkFun-Switches" package="SWITCH_DPDT_SMD_JS202011JCQN" value="TRS_MIDI_TYPE">
<attribute name="PROD_ID" value="SWCH-14133"/>
<attribute name="TYPE-A" value=""/>
<attribute name="TYPE_B" value=""/>
</element>
<element name="LED_RGB" library="adafruit" package="RGBLED5050" value="RGBLED5050">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="4"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="4"/>
<contactref element="S1" pad="6"/>
<contactref element="S1" pad="3"/>
<contactref element="J2" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="6"/>
<contactref element="LED_RGB" pad="1"/>
<contactref element="LED_RGB" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="S1" pad="2"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="J4" pad="2"/>
<contactref element="S2" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="J4" pad="5"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="J3" pad="2"/>
<contactref element="S1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="J3" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LED_RGB" pad="5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED_RGB" pad="6"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
