<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="14.859" x2="0" y2="2.921" width="0" layer="20"/>
<wire x1="0" y1="14.859" x2="8.763" y2="14.859" width="0" layer="20"/>
<wire x1="8.763" y1="14.859" x2="8.9580125" y2="15.0540125" width="0" layer="20"/>
<wire x1="8.9580125" y1="15.0540125" x2="9.407025" y2="15.24" width="0" layer="20" curve="-45"/>
<wire x1="9.407025" y1="15.24" x2="19.05" y2="15.24" width="0" layer="20"/>
<wire x1="19.05" y1="15.24" x2="19.685" y2="15.875" width="0" layer="20" curve="90"/>
<wire x1="19.685" y1="15.875" x2="19.685" y2="17.145" width="0" layer="20"/>
<wire x1="19.685" y1="17.145" x2="20.32" y2="17.78" width="0" layer="20" curve="-90"/>
<wire x1="20.32" y1="17.78" x2="32.385" y2="17.78" width="0" layer="20"/>
<wire x1="32.385" y1="17.78" x2="33.02" y2="17.145" width="0" layer="20" curve="-90"/>
<wire x1="33.02" y1="17.145" x2="33.02" y2="0.635" width="0" layer="20"/>
<wire x1="33.02" y1="0.635" x2="32.385" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="32.385" y1="0" x2="20.32" y2="0" width="0" layer="20"/>
<wire x1="20.32" y1="0" x2="19.685" y2="0.635" width="0" layer="20" curve="-90"/>
<wire x1="19.685" y1="0.635" x2="19.685" y2="1.905" width="0" layer="20"/>
<wire x1="19.685" y1="1.905" x2="19.05" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="19.05" y1="2.54" x2="9.482665625" y2="2.54" width="0" layer="20"/>
<wire x1="9.482665625" y1="2.54" x2="9.101665625" y2="2.667" width="0" layer="20" curve="-36.869898"/>
<wire x1="9.101665625" y1="2.667" x2="8.763" y2="2.921" width="0" layer="20"/>
<wire x1="8.763" y1="2.921" x2="0" y2="2.921" width="0" layer="20"/>
</plain>
<libraries>
<library name="OPL_Capacitor">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service
&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;
&lt;br&gt;&lt;/b&gt;</description>
<packages>
<package name="C0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-PCB-NOPASTE">
</package>
</packages>
</library>
<library name="OPL_Resistor">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service
&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;
&lt;br&gt;&lt;/b&gt;</description>
<packages>
<package name="R0402">
</package>
</packages>
</library>
<library name="CP2102N-A01-GQFN20R">
<packages>
<package name="SILABS_QFN20">
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
</packages>
</library>
<library name="littlefuse">
<packages>
<package name="SOT143">
</package>
</packages>
</library>
<library name="RJHSE-5081">
<packages>
<package name="RJHSE-5081">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="OPL_Capacitor" package="C0402" value="4.7uf">
<attribute name="MPN" value="CC0402MRX5R5BB475"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="OPL_Capacitor" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="OPL_Capacitor" package="C0402" value="4.7uf">
<attribute name="MPN" value="CC0402MRX5R5BB475"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="OPL_Capacitor" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="RJHSE-5081" package="RJHSE-5081" value="RJHSE-5081">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" connector, mod jack, rt angle pcb, shielded, led1-g, led2-y, single port, rj-45 8 cont "/>
<attribute name="MF" value="Amphenol ICC"/>
<attribute name="MP" value="RJHSE-5381"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="USB-A-PCB-NOPASTE" value="USBPCB_NOPASTE"/>
<element name="R1" library="OPL_Resistor" package="R0402" value="1K">
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="OPL_Resistor" package="R0402" value="330R">
<attribute name="MPN" value="RC0402FR-07330RL"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="OPL_Resistor" package="R0402" value="330R">
<attribute name="MPN" value="RC0402FR-07330RL"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="CP2102N-A01-GQFN20R" package="SILABS_QFN20" value="CP2102N-A01-GQFN20R">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Ic Bridge Usb To Uart 20qfn "/>
<attribute name="MF" value="Silicon Labs"/>
<attribute name="MP" value="CP2102N-A01-GQFN20R"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="QFN-20 Silicon Labs"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="U2" library="maxim" package="SO16L" value="MAX202ECWE">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MAX202ECWE+T"/>
<attribute name="OC_FARNELL" value="9724419"/>
<attribute name="OC_NEWARK" value="67K4364"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="C5" library="OPL_Capacitor" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="OPL_Capacitor" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="OPL_Capacitor" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="OPL_Capacitor" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="littlefuse" package="SOT143" value="SP0503BAHTG"/>
<element name="R4" library="OPL_Resistor" package="R0402" value="22K">
<attribute name="MPN" value="RC0402FR-0722RL"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="OPL_Resistor" package="R0402" value="47K">
<attribute name="MPN" value="RC0402JR-0747KL"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="21"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="J2" pad="GND"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="U2" pad="15"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="J1" pad="3"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="DSR">
<contactref element="J1" pad="2"/>
</signal>
<signal name="CTS">
<contactref element="J1" pad="1"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="TXD">
<contactref element="J1" pad="6"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="DTR">
<contactref element="J1" pad="7"/>
</signal>
<signal name="RTS">
<contactref element="J1" pad="8"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="UART_TXD">
<contactref element="U1" pad="18"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="UART_RXD">
<contactref element="U1" pad="17"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="9"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="UART_RTS">
<contactref element="U1" pad="16"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="UART_CTS">
<contactref element="U1" pad="15"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="USBDP">
<contactref element="U1" pad="4"/>
<contactref element="J2" pad="USB_P"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="USBDN">
<contactref element="U1" pad="5"/>
<contactref element="J2" pad="USB_M"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="J2" pad="5V"/>
<contactref element="U3" pad="2"/>
<contactref element="U2" pad="16"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="1"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="4"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="6"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="RXT_LED">
<contactref element="U1" pad="19"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="TXT_LED">
<contactref element="U1" pad="20"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="VBUS">
<contactref element="U1" pad="8"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
