(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GNDREF")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(U2-IN+)")
  (net 5 "Net-(D1-K)")
  (net 6 "Net-(D1-A)")
  (net 7 "Net-(D2-DOUT)")
  (net 8 "Net-(D2-DIN)")
  (net 9 "Net-(D3-DOUT)")
  (net 10 "Net-(J1-Pin_2)")
  (net 11 "/scl")
  (net 12 "/sda")
  (net 13 "Net-(J3-Pin_1)")
  (net 14 "Net-(J3-Pin_2)")
  (net 15 "/updi")
  (net 16 "/mosi")
  (net 17 "/miso")
  (net 18 "/sck")
  (net 19 "/trig")
  (net 20 "Net-(Q1-B)")
  (net 21 "Net-(U1-PA4)")
  (net 22 "unconnected-(SW1-A-Pad1)")
  (net 23 "/dac")
  (net 24 "Net-(U1-PA7)")
  (net 25 "/rx")
  (net 26 "unconnected-(U2-NC-Pad2)")
  (net 27 "Net-(U2-IN-)")
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 227.65 125.25 180)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, SOIC-14")
    (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR")
    (attr smd)
    (fp_text reference "U1" (at 0 -5.28) (layer "F.SilkS") hide)
    (fp_text value "ATtiny1614-SS" (at 0 5.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 -3.81 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.55 -2.54 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U1-PA4)") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.55 -1.27 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D2-DIN)") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.55 0 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/dac") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.55 1.27 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1-PA7)") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.55 2.54 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/rx") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.55 3.81 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/trig") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.55 3.81 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/sda") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 2.55 2.54 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/scl") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 2.55 1.27 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/updi") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 2.55 0 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/mosi") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 2.55 -1.27 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/miso") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 2.55 -2.54 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/sck") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 2.55 -3.81 180) (size 1.95 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 245 112.3 -90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D1" (at 1.27 -3.96 90) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 1.27 3.96 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "F.Cu")
    (at 232.1 135.75 90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.06 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03_Pin" (at 0 6.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/scl") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "/sda") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/rx") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:D_SO-8" (layer "F.Cu")
    (at 230.235 115.062 90)
    (descr "8-Lead Plastic SO, Exposed Die Pad (see https://www.diodes.com/assets/Package-Files/SO-8EP.pdf)")
    (tags "SO exposed pad")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "2.5W Filterless Class-D Mono Audio Amplifier, SOIC-8")
    (property "ki_keywords" "audio amplifier class d")
    (attr smd)
    (fp_text reference "U2" (at 0 -3.3 90) (layer "F.SilkS") hide)
    (fp_text value "PAM8302AAD" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.53 -1.905 90) (size 1.605 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(U1-PA7)") (pinfunction "~{SD}") (pintype "input"))
    (pad "2" smd rect (at -2.53 -0.635 90) (size 1.605 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "unconnected-(U2-NC-Pad2)") (pinfunction "NC") (pintype "no_connect"))
    (pad "3" smd rect (at -2.53 0.635 90) (size 1.605 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U2-IN+)") (pinfunction "IN+") (pintype "input"))
    (pad "4" smd rect (at -2.53 1.905 90) (size 1.605 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(U2-IN-)") (pinfunction "IN-") (pintype "input"))
    (pad "5" smd rect (at 2.53 1.905 90) (size 1.605 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(J3-Pin_1)") (pinfunction "OUT+") (pintype "output"))
    (pad "6" smd rect (at 2.53 0.635 90) (size 1.605 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (pad "7" smd rect (at 2.53 -0.635 90) (size 1.605 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect (at 2.53 -1.905 90) (size 1.605 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J3-Pin_2)") (pinfunction "OUT-") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/Diodes_SO-8EP.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:Potentiometer_Bourns_TC33X_Vertical_handsolder" (layer "F.Cu")
    (at 225.55 117.65 90)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "VOL1" (at 0 -2.5 90) (layer "F.SilkS") hide)
    (fp_text value "10K" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 -0.8 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.9 -1 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDREF") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.55 0 90) (size 1.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C3-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -1.9 1 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/dac") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 225.725 131.275 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value ".1" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (at 238.125 120.125)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23")
    (property "ki_keywords" "NPN Transistor")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.5) (layer "F.SilkS") hide)
    (fp_text value "MMBT3904" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(Q1-B)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDREF") (pinfunction "E") (pintype "passive"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 233.9 125.95 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rbase1" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 21 "Net-(U1-PA4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 20 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x01_P2.00mm_Vertical" (layer "F.Cu")
    (at 228.1 137.75)
    (descr "Through hole straight pin header, 1x01, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.00mm single row")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J10" (at 0 -2.06) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 2.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "/sck") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x01_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 229.6 133.65)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 237.4 124.9125 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "0.1" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:PinHeader_1x03_P2.54mm_Vertical_smd" (layer "F.Cu")
    (at 233.42 129.75 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03" (at 0 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.54) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 90) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 1 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd circle (at 0 2.54 90) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd circle (at 0 5.08 90) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 15 "/updi") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (at 224.8 135.4)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.06) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02" (at 0 4.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 0 2) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2962962963)
      (net 10 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 234.2 116.1 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.85 -90) (layer "F.SilkS") hide)
    (fp_text value "1" (at 0 1.85 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 229.85 119.65)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value ".1" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Net-(U2-IN+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:LED_neopixel_regular_or_MINI_PLCC4_3.5x3.5mm_P1.75mm_handsolder" (layer "F.Cu")
    (at 242.95 123.175 180)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D2" (at 0 -2.75 180) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 3.25 180) (layer "F.Fab"))
    (fp_text user "1" (at -3.3 -1.45 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.95 -1.05 180) (size 2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect (at -1.95 1.05 180) (size 2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D2-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at 1.95 1.05 180) (size 2 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.2) (chamfer bottom_right)
      (net 2 "GNDREF") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect (at 1.95 -1.05 180) (size 2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D2-DIN)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 235.45 112 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -3.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03_Pin" (at 0 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D3-DOUT)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDREF") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (at 224.75 111.7)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.06) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02" (at 0 4.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J3-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 235.9 132.8 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 3-pole, pins 1+2 closed/bridged")
    (property "ki_keywords" "Jumper SPDT")
    (attr exclude_from_pos_files)
    (net_tie_pad_groups "1, 2, 3")
    (fp_text reference "JP1" (at 0 -1.8) (layer "F.SilkS") hide)
    (fp_text value "Jumper_3_Bridged12" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -1.3 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 19 "/trig") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GNDREF") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(J1-Pin_2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 233.9 121.4 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value ".1" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GNDREF") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 27 "Net-(U2-IN-)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 238.85 115.9)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (at 236.1 137.75 -90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.06 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2962962963)
      (net 2 "GNDREF") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole rect (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/mosi") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/miso") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 243.7 118.2 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.82) (layer "F.SilkS") hide)
    (fp_text value "18" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(D1-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:spdt switch-f" (layer "F.Cu")
    (at 243.931852 132.3 -105)
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr smd)
    (fp_text reference "SW1" (at 0 -0.5 -105 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SW_SPDT" (at 0 1 -105 unlocked) (layer "F.Fab"))
    (fp_text user "NO" (at 0.45 -1.45 -15 unlocked) (layer "Dwgs.User"))
    (fp_text user "C" (at 5.55 -0.85 -15 unlocked) (layer "Dwgs.User"))
    (fp_text user "NC" (at -4.55 -0.85 -15 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -105 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.08 1.8 255) (size 1.6 4.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.35) (chamfer top_right)
      (net 22 "unconnected-(SW1-A-Pad1)") (pinfunction "A") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 5.08 1.8 255) (size 1.6 4.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.35) (chamfer top_left)
      (net 10 "Net-(J1-Pin_2)") (pinfunction "B") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 1.8 255) (size 1.6 4.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/trig") (pinfunction "C") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "attinyspeaker:speakersymbol" (layer "B.Cu")
    (at 226.80121 114.583 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 5.334 unlocked) (layer "B.SilkS") hide)
    (fp_text value "speakersymbol" (at 0 -1 unlocked) (layer "B.Fab"))
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "B.Cu")
    (at 242.6 122.2)
    (descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
    (tags "MesurementPoint Square SMDPad 1mmx2mm ")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J7" (at 0 2.54 180) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 -2.54 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 0.6 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0) (chamfer top_left bottom_left)
      (net 8 "Net-(D2-DIN)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "attinyspeaker:LED_neopixel_regular_or_MINI_PLCC4_3.5x3.5mm_P1.75mm_handsolder" (layer "B.Cu")
    (at 242.95 123.175)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D3" (at 0 2.75 180) (layer "B.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -3.25 180) (layer "B.Fab"))
    (fp_text user "1" (at -3.3 1.45 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect (at -1.95 1.05) (size 2 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect (at -1.95 -1.05) (size 2 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "Net-(D3-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at 1.95 -1.05) (size 2 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.2) (chamfer top_right)
      (net 2 "GNDREF") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect (at 1.95 1.05) (size 2 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "Net-(D2-DOUT)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (at 237.425 123.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "newblaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 1.68 90) (layer "B.SilkS") hide)
    (fp_text value ".1" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 242.575 138.65) (end 243.039134 136.939884)
    (layer "Edge.Cuts"))
  (gr_line (start 246.4 126.28) (end 245.925 126.15)
    (layer "Edge.Cuts"))
  (gr_line (start 244.682068 130.709674) (end 244.375 130.3)
    (layer "Edge.Cuts"))
  (gr_line (start 245.45 127.875) (end 245.925 126.15)
    (layer "Edge.Cuts"))
  (gr_line (start 242.575 138.65) (end 242.7 138.7)
    (layer "Edge.Cuts"))
  (gr_line (start 244.975 128.075) (end 245.45 127.875)
    (layer "Edge.Cuts"))
  (gr_line (start 242.739134 136.514884) (end 243.305256 134.291039)
    (layer "Edge.Cuts"))
  (gr_line (start 243.780256 134.091039) (end 244.682068 130.709674)
    (layer "Edge.Cuts"))
  (gr_line (start 223.4 110.5) (end 246.4 110.5)
    (layer "Edge.Cuts"))
  (gr_line (start 242.7 138.9) (end 223.4 138.9)
    (layer "Edge.Cuts"))
  (gr_line (start 244.375 130.3) (end 244.975 128.075)
    (layer "Edge.Cuts"))
  (gr_line (start 223.4 138.9) (end 223.4 110.5)
    (layer "Edge.Cuts"))
  (gr_line (start 243.039134 136.939884) (end 242.739134 136.514884)
    (layer "Edge.Cuts"))
  (gr_line (start 243.305256 134.291039) (end 243.780256 134.091039)
    (layer "Edge.Cuts"))
  (gr_line (start 246.4 110.5) (end 246.4 126.28)
    (layer "Edge.Cuts"))
  (gr_line (start 242.7 138.9) (end 242.7 138.7)
    (layer "Edge.Cuts"))
  (gr_text "+    -" (at 226.35 110.8 -270) (layer "B.SilkS"))
  (gr_text "N3+" (at 239 114) (layer "B.SilkS"))
  (gr_text "PA5" (at 243.825 121.125) (layer "B.SilkS"))
  (gr_text "N2" (at 238.925 124 -90) (layer "B.SilkS"))
  (gr_text "POWER" (at 225.9 138.8 -90) (layer "B.SilkS"))
  (gr_text "ATTINY1614\n+PAM8302\nIR BLASTER\nPROJECT BOARD" (at 229.7 125.475 -90) (layer "B.SilkS"))
  (gr_text "EXTRA\nI/O" (at 237.4 136.65 270) (layer "B.SilkS"))
  (gr_text "0.1uF" (at 238.825 121.175) (layer "B.SilkS"))
  (gr_text "C" (at 241.8 135.9 345) (layer "F.SilkS"))
  (gr_text "NO" (at 242.6 130.7 345) (layer "F.SilkS"))
  (gr_text "PB0" (at 231 134.9) (layer "F.SilkS"))
  (gr_text "GND" (at 234.85 128.875) (layer "F.SilkS"))
  (gr_text "0.1uF" (at 224.2 133.25) (layer "F.SilkS"))
  (gr_text "1uF" (at 236.25 117.05 90) (layer "F.SilkS"))
  (gr_text "3V" (at 235.1 113.95) (layer "F.SilkS"))
  (gr_text "VCC" (at 232.375 128.825) (layer "F.SilkS"))
  (gr_text "vol" (at 226.6 114.15 -90) (layer "F.SilkS"))
  (gr_text "0.1uF" (at 236.1 123.05) (layer "F.SilkS"))
  (gr_text "always\non" (at 233.5 133.5) (layer "F.SilkS"))
  (gr_text "N1" (at 239.025 123.325 270) (layer "F.SilkS"))
  (gr_text "+SPKR-" (at 225.7 110.55 270) (layer "F.SilkS"))
  (gr_text "NEO" (at 236.9 114) (layer "F.SilkS"))
  (gr_text "PB1" (at 233.1 134.9) (layer "F.SilkS"))
  (gr_text "AT1614" (at 228.6 127.3 90) (layer "F.SilkS"))
  (gr_text "NC" (at 243.95 126.05 345) (layer "F.SilkS"))
  (gr_text "PA2" (at 228.9 136.8) (layer "F.SilkS"))
  (gr_text "3V" (at 237.4 136.6) (layer "F.SilkS"))
  (gr_text "0" (at 232.45 121.25 90) (layer "F.SilkS"))
  (gr_text "GND" (at 226.6 138.7 90) (layer "F.SilkS"))
  (gr_text ".1uF" (at 233 119.6) (layer "F.SilkS"))
  (gr_text "PA1" (at 229.3 135.8) (layer "F.SilkS"))
  (gr_text "1KΩ" (at 232.75 124.2) (layer "F.SilkS"))
  (gr_text "GND" (at 239.4 113.95) (layer "F.SilkS"))
  (gr_text "on\ntrigger" (at 238.15 133.65) (layer "F.SilkS"))
  (gr_text "+3V" (at 226.5 136.3 90) (layer "F.SilkS"))
  (gr_text "GND" (at 237.05 138.4) (layer "F.SilkS"))
  (gr_text "P8302" (at 228.3 115.1) (layer "F.SilkS"))
  (gr_text "10K" (at 224.5 118.6) (layer "F.SilkS"))
  (gr_text "NPN" (at 237.7 119.1 -90) (layer "F.SilkS"))
  (gr_text "UPDI" (at 237.225 128.925) (layer "F.SilkS"))
  (gr_text "0" (at 232.6 119.6) (layer "F.SilkS"))
  (gr_text "10-27Ω" (at 241.5 120.3) (layer "F.SilkS"))
  (gr_text "PA3" (at 226.8 136.8) (layer "F.SilkS"))
  (gr_text "PB3" (at 235.35 134.9) (layer "F.SilkS"))
  (gr_text ".1uF" (at 232.45 120.85 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GNDREF") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.3))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.4) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 223.8 110.75)
        (xy 246 110.8)
        (xy 246 125.2)
        (xy 245 125.8)
        (xy 241.6 138.6)
        (xy 223.7 138.6)
      )
    )
  )
  (zone (net 1) (net_name "VCC") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.3))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.4) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 223.8 110.75)
        (xy 239.2 111)
        (xy 242.8 116.8)
        (xy 242.775 124.175)
        (xy 239.55 128.05)
        (xy 239.825 130.75)
        (xy 236.8 136.2)
        (xy 227.4 138.6)
        (xy 223.7 138.6)
      )
    )
  )
)
