(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 0.8)
    (drawings 12)
    (tracks 48)
    (zones 0)
    (modules 10)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.25)
    (user_trace_width 0.28)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 110 89)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(U1-Pad1)")
  (net 4 "Net-(U1-Pad5)")
  (net 5 "Net-(U1-Pad8)")
  (net 6 "Net-(R5-Pad2)")
  (net 7 "Net-(J13-Pad1)")
  (net 8 "Net-(J15-Pad1)")
  (net 9 "Net-(J11-Pad1)")
  (net 10 -in)
  (net 11 out)
  (net 12 +in)
  (net 13 +V)
  (net 14 -V)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class SMD ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class grounds ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
  )
  (net_class power ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net +V)
    (add_net +in)
    (add_net -V)
    (add_net -in)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
    (add_net out)
  )
  (net_class soic ""
    (clearance 0.1524)
    (trace_width 0.4)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module "Duallys:R_0805(1206)combo" (layer F.Cu) (tedit 5FE133FD)
    (at 111.2 78.3 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0.04 -0.01 180) (layer F.SilkS))
    (fp_text value 21R5 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 10 -in))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 -in))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Duallys:PinHeader_1x05_P2mm_With (layer B.Cu) (tedit 5FDE3665)
    (at 112.5 82.15 270)
    (descr "Through hole straight pin header, 1x05, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.00mm single row")
    (fp_text reference J1 (at 0 2.06 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 -10.06 270) (layer B.Fab))
    (fp_text user %R (at 0 -4) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 out))
    (pad 4 thru_hole oval (at 0 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +V))
    (pad 3 thru_hole oval (at 0 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 -V))
    (pad 2 thru_hole oval (at 0 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 +in))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 -in))
    (model ${KIPRJMOD}/lib/3d/tmm-105-03-l-s.stp
      (offset (xyz 0 1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 -90))
    )
  )
  (module Duallys:Kemet-33nF (layer F.Cu) (tedit 5FDD33E3)
    (at 114 70.1)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C1 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 33n (at 2.5 -3.5) (layer F.SilkS) hide)
    (pad 2 smd roundrect (at 3.9 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at 1.1 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/Kem-PHE-33n.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 116.5 77.9)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0.1 -1.5) (layer F.SilkS))
    (fp_text value OPA1611 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +in))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 -V))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(U1-Pad5)"))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(R5-Pad2)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 +V))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(U1-Pad8)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 112.6 73.6 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -0.05 270) (layer F.SilkS))
    (fp_text value 2k26 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.8 78.3 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 0 180) (layer F.SilkS))
    (fp_text value 3k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 out))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.4 73.6 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 0 270) (layer F.SilkS))
    (fp_text value 75 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Duallys:Combo-4P-Preci-A (layer F.Cu) (tedit 5FD78565)
    (at 112.68 84.5)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 3.86 -1.67) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 4.14 8.96) (layer F.Fab))
    (fp_text user %R (at 3.82 5.94) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 -V))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 +in))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 -in))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)"))
    (pad 4 thru_hole rect (at 7.62 3 270) (size 3 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 -V))
    (pad 3 thru_hole rect (at 5.08 3 270) (size 3 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 +in))
    (pad 2 thru_hole rect (at 2.54 3 270) (size 3 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 -in))
    (pad 1 thru_hole rect (at 0 3 270) (size 3 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)"))
    (model ${KIPRJMOD}/lib/3d/preci-dip_399.stp
      (offset (xyz 3.81 -1.55 1.27))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (module Duallys:ThruPin-3325 (layer F.Cu) (tedit 5FD4F26B)
    (at 111.3 70.1)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (fp_text reference J13 (at 0 -1.648) (layer F.Fab))
    (fp_text value Tie (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(J13-Pad1)"))
    (model ${KIPRJMOD}/lib/3d/MillMax-3325-0.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Duallys:ThruPin-3325 (layer F.Cu) (tedit 5FD4F26B)
    (at 121.7 70.1)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (fp_text reference J15 (at 0 -1.648) (layer F.Fab))
    (fp_text value Tie (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J15-Pad1)"))
    (model ${KIPRJMOD}/lib/3d/MillMax-3325-0.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text A (at 116.5 73.5) (layer B.SilkS))
  (gr_text 4 (at 122.3 85.3) (layer F.SilkS))
  (gr_text 1 (at 110.7 85.3) (layer F.SilkS))
  (gr_line (start 123 89) (end 110 89) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123 68) (end 123 89) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110 68) (end 123 68) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110 68) (end 110 89) (layer Edge.Cuts) (width 0.05))
  (zone (net 10) (net_name -in) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110 68) (xy 110 85.8) (xy 123 85.8) (xy 123 68)
      )
    )
  )
)
