(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 625)
    (zones 0)
    (modules 8)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 A17)
  (net 3 A14)
  (net 4 A13)
  (net 5 A8)
  (net 6 A9)
  (net 7 A11)
  (net 8 OEn)
  (net 9 A10)
  (net 10 CEn)
  (net 11 D7)
  (net 12 D6)
  (net 13 D5)
  (net 14 D4)
  (net 15 D3)
  (net 16 GND)
  (net 17 D2)
  (net 18 D1)
  (net 19 D0)
  (net 20 A0)
  (net 21 A1)
  (net 22 A2)
  (net 23 A3)
  (net 24 A4)
  (net 25 A5)
  (net 26 A6)
  (net 27 A7)
  (net 28 A12)
  (net 29 A15)
  (net 30 A16)
  (net 31 A18)
  (net 32 D15)
  (net 33 D14)
  (net 34 D13)
  (net 35 D12)
  (net 36 D11)
  (net 37 D10)
  (net 38 D9)
  (net 39 D8)
  (net 40 "Net-(JP1-Pad2)")
  (net 41 "Net-(JP2-Pad2)")
  (net 42 "Net-(TP1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A16)
    (add_net A17)
    (add_net A18)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net CEn)
    (add_net D0)
    (add_net D1)
    (add_net D10)
    (add_net D11)
    (add_net D12)
    (add_net D13)
    (add_net D14)
    (add_net D15)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(TP1-Pad1)")
    (add_net OEn)
  )
  (net_class PWR ""
    (clearance 0.254)
    (trace_width 0.762)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net GND)
    (add_net VCC)
  )
  (module plcc_rom_adapter:DIP-42_W15.24mm_flipped (layer F.Cu) (tedit 60CD3A4B)
    (at 124.27712 62.72784)
    (descr "42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference ZX1 (at 0.01524 -26.26868) (layer F.Fab) hide)
    (fp_text value 27C800 (at 0.03 27.73) (layer F.Fab))
    (fp_text user %R (at 0.03 0) (layer F.Fab))
    (pad 42 thru_hole oval (at -7.59 -25.4) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 7.65 25.4) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 36 D11))
    (pad 41 thru_hole oval (at -7.59 -22.86) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 5 A8))
    (pad 20 thru_hole oval (at 7.65 22.86) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 15 D3))
    (pad 40 thru_hole oval (at -7.59 -20.32) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 6 A9))
    (pad 19 thru_hole oval (at 7.65 20.32) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 37 D10))
    (pad 39 thru_hole oval (at -7.59 -17.78) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 9 A10))
    (pad 18 thru_hole oval (at 7.65 17.78) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 17 D2))
    (pad 38 thru_hole oval (at -7.59 -15.24) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 7 A11))
    (pad 17 thru_hole oval (at 7.65 15.24) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 38 D9))
    (pad 37 thru_hole oval (at -7.59 -12.7) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 28 A12))
    (pad 16 thru_hole oval (at 7.65 12.7) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 18 D1))
    (pad 36 thru_hole oval (at -7.59 -10.16) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 4 A13))
    (pad 15 thru_hole oval (at 7.65 10.16) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 39 D8))
    (pad 35 thru_hole oval (at -7.59 -7.62) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 3 A14))
    (pad 14 thru_hole oval (at 7.65 7.62) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 19 D0))
    (pad 34 thru_hole oval (at -7.59 -5.08) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 29 A15))
    (pad 13 thru_hole oval (at 7.65 5.08) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 8 OEn))
    (pad 33 thru_hole oval (at -7.59 -2.54) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 30 A16))
    (pad 12 thru_hole oval (at 7.65 2.54) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 32 thru_hole oval (at -7.59 0) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 42 "Net-(TP1-Pad1)"))
    (pad 11 thru_hole oval (at 7.65 0) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 10 CEn))
    (pad 31 thru_hole oval (at -7.59 2.54) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 10 thru_hole oval (at 7.65 -2.54) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 20 A0))
    (pad 30 thru_hole oval (at -7.59 5.08) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 32 D15))
    (pad 9 thru_hole oval (at 7.65 -5.08) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 21 A1))
    (pad 29 thru_hole oval (at -7.59 7.62) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 11 D7))
    (pad 8 thru_hole oval (at 7.65 -7.62) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 22 A2))
    (pad 28 thru_hole oval (at -7.59 10.16) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 33 D14))
    (pad 7 thru_hole oval (at 7.65 -10.16) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 23 A3))
    (pad 27 thru_hole oval (at -7.59 12.7) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 12 D6))
    (pad 6 thru_hole oval (at 7.65 -12.7) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 24 A4))
    (pad 26 thru_hole oval (at -7.59 15.24) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 34 D13))
    (pad 5 thru_hole oval (at 7.65 -15.24) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 25 A5))
    (pad 25 thru_hole oval (at -7.59 17.78) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 4 thru_hole oval (at 7.65 -17.78) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 26 A6))
    (pad 24 thru_hole oval (at -7.59 20.32) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 35 D12))
    (pad 3 thru_hole oval (at 7.65 -20.32) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 27 A7))
    (pad 23 thru_hole oval (at -7.59 22.86) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 14 D4))
    (pad 2 thru_hole oval (at 7.65 -22.86) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 2 A17))
    (pad 22 thru_hole oval (at -7.59 25.4) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 1 thru_hole rect (at 7.65 -25.4) (size 1.6 1.6) (drill 1.07) (layers *.Cu *.Mask)
      (net 31 A18))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 125.65634 44.82846)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -2.8067 0.0381) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 124.5108 68.59524 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 118.8974 62.7253)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 2.25044 0.02032) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 42 "Net-(TP1-Pad1)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 122.20194 41.36136 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.89484) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 41 "Net-(JP2-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 121.68632 69.2658)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 40 "Net-(JP1-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Package_LCC:PLCC-32_11.4x14.0mm_P1.27mm (layer B.Cu) (tedit 5B298677)
    (at 124.31268 48.5189 180)
    (descr "PLCC, 32 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc0015.pdf), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py")
    (tags "PLCC LCC")
    (attr smd)
    (fp_text reference U2 (at 0 8.52) (layer B.SilkS))
    (fp_text value SST39SF040 (at 0 -8.52) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 32 smd roundrect (at 1.27 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 31 smd roundrect (at 2.54 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(JP2-Pad2)"))
    (pad 30 smd roundrect (at 3.81 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 A17))
    (pad 29 smd roundrect (at 5.5625 5.08 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 A14))
    (pad 28 smd roundrect (at 5.5625 3.81 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 A13))
    (pad 27 smd roundrect (at 5.5625 2.54 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 A8))
    (pad 26 smd roundrect (at 5.5625 1.27 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 A9))
    (pad 25 smd roundrect (at 5.5625 0 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 A11))
    (pad 24 smd roundrect (at 5.5625 -1.27 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 OEn))
    (pad 23 smd roundrect (at 5.5625 -2.54 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 A10))
    (pad 22 smd roundrect (at 5.5625 -3.81 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 CEn))
    (pad 21 smd roundrect (at 5.5625 -5.08 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 D15))
    (pad 20 smd roundrect (at 3.81 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 D14))
    (pad 19 smd roundrect (at 2.54 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 D13))
    (pad 18 smd roundrect (at 1.27 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 D12))
    (pad 17 smd roundrect (at 0 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 D11))
    (pad 16 smd roundrect (at -1.27 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 GND))
    (pad 15 smd roundrect (at -2.54 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 D10))
    (pad 14 smd roundrect (at -3.81 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 D9))
    (pad 13 smd roundrect (at -5.5625 -5.08 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 D8))
    (pad 12 smd roundrect (at -5.5625 -3.81 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 A0))
    (pad 11 smd roundrect (at -5.5625 -2.54 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 A1))
    (pad 10 smd roundrect (at -5.5625 -1.27 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 A2))
    (pad 9 smd roundrect (at -5.5625 0 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 A3))
    (pad 8 smd roundrect (at -5.5625 1.27 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 A4))
    (pad 7 smd roundrect (at -5.5625 2.54 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 A5))
    (pad 6 smd roundrect (at -5.5625 3.81 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 A6))
    (pad 5 smd roundrect (at -5.5625 5.08 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 A7))
    (pad 4 smd roundrect (at -3.81 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 A12))
    (pad 3 smd roundrect (at -2.54 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 29 A15))
    (pad 2 smd roundrect (at -1.27 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 A16))
    (pad 1 smd roundrect (at 0 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 A18))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-32_11.4x14.0mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LCC:PLCC-32_11.4x14.0mm_P1.27mm (layer B.Cu) (tedit 5B298677)
    (at 124.30252 76.2254 180)
    (descr "PLCC, 32 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc0015.pdf), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py")
    (tags "PLCC LCC")
    (attr smd)
    (fp_text reference U1 (at 0 8.52) (layer B.SilkS))
    (fp_text value SST39SF040 (at 0 -8.52) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 32 smd roundrect (at 1.27 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 31 smd roundrect (at 2.54 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(JP1-Pad2)"))
    (pad 30 smd roundrect (at 3.81 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 A17))
    (pad 29 smd roundrect (at 5.5625 5.08 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 A14))
    (pad 28 smd roundrect (at 5.5625 3.81 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 A13))
    (pad 27 smd roundrect (at 5.5625 2.54 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 A8))
    (pad 26 smd roundrect (at 5.5625 1.27 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 A9))
    (pad 25 smd roundrect (at 5.5625 0 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 A11))
    (pad 24 smd roundrect (at 5.5625 -1.27 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 OEn))
    (pad 23 smd roundrect (at 5.5625 -2.54 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 A10))
    (pad 22 smd roundrect (at 5.5625 -3.81 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 CEn))
    (pad 21 smd roundrect (at 5.5625 -5.08 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 D7))
    (pad 20 smd roundrect (at 3.81 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 D6))
    (pad 19 smd roundrect (at 2.54 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 D5))
    (pad 18 smd roundrect (at 1.27 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 D4))
    (pad 17 smd roundrect (at 0 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 D3))
    (pad 16 smd roundrect (at -1.27 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 GND))
    (pad 15 smd roundrect (at -2.54 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 D2))
    (pad 14 smd roundrect (at -3.81 -6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 D1))
    (pad 13 smd roundrect (at -5.5625 -5.08 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 D0))
    (pad 12 smd roundrect (at -5.5625 -3.81 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 A0))
    (pad 11 smd roundrect (at -5.5625 -2.54 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 A1))
    (pad 10 smd roundrect (at -5.5625 -1.27 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 A2))
    (pad 9 smd roundrect (at -5.5625 0 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 A3))
    (pad 8 smd roundrect (at -5.5625 1.27 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 A4))
    (pad 7 smd roundrect (at -5.5625 2.54 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 A5))
    (pad 6 smd roundrect (at -5.5625 3.81 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 A6))
    (pad 5 smd roundrect (at -5.5625 5.08 180) (size 1.475 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 A7))
    (pad 4 smd roundrect (at -3.81 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 A12))
    (pad 3 smd roundrect (at -2.54 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 29 A15))
    (pad 2 smd roundrect (at -1.27 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 A16))
    (pad 1 smd roundrect (at 0 6.8375 180) (size 0.6 1.475) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 A18))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-32_11.4x14.0mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 128.44018 37.1475 270) (layer B.SilkS))
  (gr_text "LO BYTE" (at 124.36856 63.95212) (layer B.SilkS))
  (gr_text "HI BYTE" (at 124.16028 61.33846) (layer B.SilkS))
  (gr_line (start 115.316 89.916) (end 115.316 35.56) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.096 89.91092) (end 115.316 89.916) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.096 35.56) (end 133.096 89.91092) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.316 35.56) (end 133.096 35.56) (layer Edge.Cuts) (width 0.05))
  (zone (net 16) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 110.75924 31.63824) (xy 142.71752 30.83052) (xy 141.30528 102.67696) (xy 106.1974 99.85248)
      )
    )
  )
  (zone (net 16) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 107.93984 27.80284) (xy 146.45132 27.06624) (xy 147.86356 104.75976) (xy 100.0506 102.53472)
      )
    )
  )
  (zone (net 16) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 106.39552 26.07564) (xy 150.63724 24.03348) (xy 153.8732 112.00892) (xy 94.31528 107.58424)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.2286))
    (polygon
      (pts
        (xy 122.43562 38.3921) (xy 124.56668 38.3921) (xy 124.57684 39.36746) (xy 122.43308 39.36746)
      )
    )
  )
  (zone (net 16) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 138.49604 32.87776) (xy 136.94156 98.61804) (xy 111.9632 95.86468) (xy 112.31372 32.75584) (xy 112.3188 32.75584)
      )
    )
    (polygon
      (pts
        (xy 120.68048 68.21424) (xy 123.68022 68.21678) (xy 123.6726 66.32956) (xy 120.68048 66.32194)
      )
    )
    (polygon
      (pts
        (xy 121.93778 39.9415) (xy 125.04928 39.94658) (xy 125.03912 37.82314) (xy 121.92 37.81806)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.2286))
    (polygon
      (pts
        (xy 121.1707 66.76898) (xy 123.14682 66.76644) (xy 123.14428 67.7672) (xy 121.1707 67.7672)
      )
    )
  )
)
