<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.78" y2="0" width="0" layer="20"/>
<wire x1="17.78" y1="0" x2="17.78" y2="17.78" width="0" layer="20"/>
<wire x1="17.78" y1="17.78" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<text>iCEStamp1K</text>
<text>Designed in Thailand
By TinLethax</text>
<text>rev2.1</text>
<text>iCE40LP1K-CM36</text>
<text>E2</text>
<text>GND</text>
<text>Vcc</text>
<text>F2</text>
<text>E3</text>
<text>F3</text>
<text>RST</text>
<text>SO</text>
<text>SI</text>
<text>CK</text>
<text>E6</text>
<text>SS</text>
<text>D6</text>
<text>C5</text>
<text>C6</text>
<text>B5</text>
<text>B6</text>
<text>B4</text>
<text>DONE</text>
<text>A3</text>
<text>B3</text>
<text>A2</text>
<text>GND</text>
<text>Vcc</text>
<text>A1</text>
<text>B1</text>
<text>C2</text>
<text>C1</text>
<text>C3</text>
<text>D1</text>
<text>E1</text>
<text>2mil
2.5mil
3mil</text>
<text>Design w/ caution</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="Headers">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Headers&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="62000811121">
</package>
</packages>
</library>
<library name="XC6206P122MR-G">
<description>&lt;LDO Voltage Regulators 1uA Low Quiescent 3 Terminal, Low ESR Cap. Compatible, Voltage Regulator&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT95P280X130-3N">
<description>&lt;b&gt;SOT-23&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="ICE40LP1K-CM36A">
<description>&lt;iCE40 LP/HX/LM - Low-power, high-performance FPGA&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="BGA36C40P6X6_250X250X100">
<description>&lt;b&gt;36-BALL UCBGA&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="ICE40LP1K-CM36A" package="BGA36C40P6X6_250X250X100" value="ICE40LP1K-CM36A">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="iCE40 LP/HX/LM - Low-power, high-performance FPGA"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Lattice Semiconductor"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ICE40LP1K-CM36A"/>
<attribute name="MOUSER_PART_NUMBER" value="842-ICE40LP1K-CM36A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Lattice/ICE40LP1K-CM36A?qs=w%2Fv1CP2dgqpOjceq4EogWg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Headers" package="62000811121" value="62000811121">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="MANUFACTURER" value="Würth Elektronik "/>
<attribute name="MPN" value="62000811121"/>
</element>
<element name="J2" library="Headers" package="62000811121" value="62000811121">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="MANUFACTURER" value="Würth Elektronik "/>
<attribute name="MPN" value="62000811121"/>
</element>
<element name="J3" library="Headers" package="62000811121" value="62000811121">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="MANUFACTURER" value="Würth Elektronik "/>
<attribute name="MPN" value="62000811121"/>
</element>
<element name="J4" library="Headers" package="62000811121" value="62000811121">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="MANUFACTURER" value="Würth Elektronik "/>
<attribute name="MPN" value="62000811121"/>
</element>
<element name="C3" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="XC6206P122MR-G" package="SOT95P280X130-3N" value="XC6206P122MR-G">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="LDO Voltage Regulators 1uA Low Quiescent 3 Terminal, Low ESR Cap. Compatible, Voltage Regulator"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="MANUFACTURER_NAME" value="Torex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="XC6206P122MR-G"/>
<attribute name="MOUSER_PART_NUMBER" value="865-XC6206P122MR-G"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Torex-Semiconductor/XC6206P122MR-G?qs=AsjdqWjXhJ%2F35%2FU%2FZk2JYg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCORE">
<contactref element="IC1" pad="B2"/>
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="IC1" pad="A6"/>
<contactref element="IC1" pad="A4"/>
<contactref element="IC1" pad="F1"/>
<contactref element="IC1" pad="F6"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J4" pad="1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="D2"/>
<contactref element="IC1" pad="D4"/>
<contactref element="IC1" pad="D3"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J3" pad="8"/>
<contactref element="J3" pad="7"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="A1"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="A2"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="A3"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="B1">
<contactref element="IC1" pad="B1"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="B3">
<contactref element="IC1" pad="B3"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="B4">
<contactref element="IC1" pad="B4"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="B5">
<contactref element="IC1" pad="B5"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="B6">
<contactref element="IC1" pad="B6"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="C1">
<contactref element="IC1" pad="C1"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="C2">
<contactref element="IC1" pad="C2"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="C3">
<contactref element="IC1" pad="C3"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="CDONE">
<contactref element="IC1" pad="C4"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="C5">
<contactref element="IC1" pad="C5"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="C6">
<contactref element="IC1" pad="C6"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="SPI_SDI">
<contactref element="IC1" pad="F5"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="CRESET">
<contactref element="IC1" pad="F4"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="F3">
<contactref element="IC1" pad="F3"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="F2">
<contactref element="IC1" pad="F2"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="E6">
<contactref element="IC1" pad="E6"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="SPI_SCK">
<contactref element="IC1" pad="E5"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="SPI_SDO">
<contactref element="IC1" pad="E4"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="E3">
<contactref element="IC1" pad="E3"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="E2">
<contactref element="IC1" pad="E2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="E1">
<contactref element="IC1" pad="E1"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="D6"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="SPI_SS">
<contactref element="IC1" pad="D5"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="D1">
<contactref element="IC1" pad="D1"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
