(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 133)
    (no_connects 0)
    (area 64.8726 29.8726 153.277401 174.000001)
    (thickness 1.6)
    (drawings 42)
    (tracks 751)
    (zones 0)
    (modules 44)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.18)
    (user_trace_width 0.18)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.8 0.5)
    (user_via 1 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C2-Pad1)")
  (net 2 /VBL-)
  (net 3 GND)
  (net 4 "Net-(D1-Pad2)")
  (net 5 +3V3)
  (net 6 /IF0)
  (net 7 /~RESET)
  (net 8 /IF1)
  (net 9 /IF2)
  (net 10 /DEN)
  (net 11 /DCLK)
  (net 12 /VSYNC)
  (net 13 /HSYNC)
  (net 14 /DX0)
  (net 15 /DX2)
  (net 16 /DX3)
  (net 17 /DX4)
  (net 18 /DX5)
  (net 19 /DX6)
  (net 20 /DX7)
  (net 21 /VBL+)
  (net 22 "Net-(BATTERY1-Pad2)")
  (net 23 /PMOD0)
  (net 24 /PMOD1)
  (net 25 /PMOD2)
  (net 26 /PMOD3)
  (net 27 /PMOD4)
  (net 28 /PMOD5)
  (net 29 /PMOD6)
  (net 30 /PMOD7)
  (net 31 /AUDIO)
  (net 32 "Net-(LCD1-Pad11)")
  (net 33 "Net-(LCD1-Pad10)")
  (net 34 "Net-(LCD1-Pad9)")
  (net 35 /TPS_CTRL)
  (net 36 /BUTTON_5)
  (net 37 /BUTTON_4)
  (net 38 /BUTTON_3)
  (net 39 /BUTTON_2)
  (net 40 /BUTTON_1)
  (net 41 /BUTTON_0)
  (net 42 /OSC_OUT)
  (net 43 /DX1)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /AUDIO)
    (add_net /BUTTON_0)
    (add_net /BUTTON_1)
    (add_net /BUTTON_2)
    (add_net /BUTTON_3)
    (add_net /BUTTON_4)
    (add_net /BUTTON_5)
    (add_net /DCLK)
    (add_net /DEN)
    (add_net /DX0)
    (add_net /DX1)
    (add_net /DX2)
    (add_net /DX3)
    (add_net /DX4)
    (add_net /DX5)
    (add_net /DX6)
    (add_net /DX7)
    (add_net /HSYNC)
    (add_net /IF0)
    (add_net /IF1)
    (add_net /IF2)
    (add_net /OSC_OUT)
    (add_net /PMOD0)
    (add_net /PMOD1)
    (add_net /PMOD2)
    (add_net /PMOD3)
    (add_net /PMOD4)
    (add_net /PMOD5)
    (add_net /PMOD6)
    (add_net /PMOD7)
    (add_net /TPS_CTRL)
    (add_net /VBL+)
    (add_net /VBL-)
    (add_net /VSYNC)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(BATTERY1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(LCD1-Pad10)")
    (add_net "Net-(LCD1-Pad11)")
    (add_net "Net-(LCD1-Pad9)")
  )
  (module "Custom Parts:MOLEX_51296-5494_54pin_0.5mm_BTM" locked (layer F.Cu) (tedit 5A802025)
    (at 100.25 103.5 180)
    (fp_text reference LCD1 (at 2.5 -2 360) (layer F.SilkS))
    (fp_text value LQ035NC111 (at 0 1.85 180) (layer F.Fab))
    (pad M smd rect (at 14.8 2.65 180) (size 1.4 1.5) (layers F.Cu F.Paste F.Mask))
    (pad M smd rect (at -14.8 2.65 180) (size 1.4 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 54 smd rect (at 13.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 53 smd rect (at 12.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 52 smd rect (at 12.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /DEN))
    (pad 51 smd rect (at 11.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 50 smd rect (at 11.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /IF0))
    (pad 49 smd rect (at 10.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /IF1))
    (pad 48 smd rect (at 10.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /IF2))
    (pad 47 smd rect (at 9.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 46 smd rect (at 9.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 45 smd rect (at 8.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd rect (at 8.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 43 smd rect (at 7.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 7.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 41 smd rect (at 6.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 40 smd rect (at 6.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 5.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 5.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /DCLK))
    (pad 37 smd rect (at 4.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /VSYNC))
    (pad 36 smd rect (at 4.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /HSYNC))
    (pad 35 smd rect (at 3.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /DX7))
    (pad 34 smd rect (at 3.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /DX6))
    (pad 33 smd rect (at 2.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /DX5))
    (pad 32 smd rect (at 2.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /DX4))
    (pad 31 smd rect (at 1.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /DX3))
    (pad 30 smd rect (at 1.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /DX2))
    (pad 29 smd rect (at 0.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 43 /DX1))
    (pad 28 smd rect (at 0.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /DX0))
    (pad 27 smd rect (at -0.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 26 smd rect (at -0.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 25 smd rect (at -1.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 24 smd rect (at -1.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 23 smd rect (at -2.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 22 smd rect (at -2.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 21 smd rect (at -3.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 20 smd rect (at -3.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 19 smd rect (at -4.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 18 smd rect (at -4.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 17 smd rect (at -5.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 16 smd rect (at -5.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 15 smd rect (at -6.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 14 smd rect (at -6.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at -7.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 12 smd rect (at -7.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 11 smd rect (at -8.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(LCD1-Pad11)"))
    (pad 10 smd rect (at -8.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(LCD1-Pad10)"))
    (pad 9 smd rect (at -9.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(LCD1-Pad9)"))
    (pad 8 smd rect (at -9.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /~RESET))
    (pad 7 smd rect (at -10.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -10.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -11.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -11.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /VBL+))
    (pad 3 smd rect (at -12.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /VBL+))
    (pad 2 smd rect (at -12.75 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBL-))
    (pad 1 smd rect (at -13.25 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBL-))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A801F57)
    (at 73 150.5 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference BATTERY1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(BATTERY1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A801F9C)
    (at 125.43 110.3 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.45 -3.18 90) (layer F.SilkS))
    (fp_text value 10µ (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0.05 0.07 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A801FBA)
    (at 128.5 105.71 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.04 -3 90) (layer F.SilkS))
    (fp_text value 220n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A801FB4)
    (at 132.5 105.71 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -0.04 2 90) (layer F.SilkS))
    (fp_text value 1µ/50V (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at -0.04 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /VBL+))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 93 106 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 10µ (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5A801FD8)
    (at 132.5 110.21 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0.04 -2 270) (layer F.SilkS))
    (fp_text value MBR0540 (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 1.54 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /VBL+))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Parts:Pin_Header_Angled_2x06_Pitch2.54mm_PMOD" (layer F.Cu) (tedit 5A801F7F)
    (at 140 106)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference J1 (at 4.5 -2.25) (layer F.SilkS))
    (fp_text value PMOD (at 5.655 14.97) (layer F.Fab))
    (fp_text user %R (at 5.31 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /PMOD0))
    (pad 7 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /PMOD1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /PMOD2))
    (pad 8 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /PMOD3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /PMOD4))
    (pad 9 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /PMOD5))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /PMOD6))
    (pad 10 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /PMOD7))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Parts:AUDIO_JACK_3.5mm" (layer F.Cu) (tedit 5A801F84)
    (at 142 131 180)
    (fp_text reference J2 (at -2.5 7 180) (layer F.SilkS))
    (fp_text value Audio-Jack-3 (at 8.5 0 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 5 -2.5 180) (size 2 2) (drill 1.25) (layers *.Cu *.Mask)
      (net 31 /AUDIO))
    (pad 2 thru_hole circle (at 5 -5 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 /AUDIO))
    (pad 1 thru_hole circle (at 5 2.5 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 /AUDIO))
    (pad 1 thru_hole circle (at 5 5 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 /AUDIO))
    (pad "" np_thru_hole circle (at 0 -5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.5 -5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.5 5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5 0 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module "Custom Parts:muRata_L_2020" (layer F.Cu) (tedit 5A4A97CA)
    (at 128.44 115.01)
    (fp_text reference L1 (at 0 3.7) (layer F.SilkS))
    (fp_text value 10µH/A915AY-100M (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2.6 0) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2.6 0) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801F9E)
    (at 123.65 110.24 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.51 -2.65 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 /TPS_CTRL))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801FB8)
    (at 127 105.71 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.04 -3 90) (layer F.SilkS))
    (fp_text value 10 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBL-))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A802015)
    (at 79.5 107 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.25 4.75 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /IF2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A802015)
    (at 81 107 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.25 4.75 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /IF1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801FE2)
    (at 111.5 106.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /~RESET))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801FED)
    (at 110 106.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(LCD1-Pad9)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801FEB)
    (at 108.5 106.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(LCD1-Pad10)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801FE7)
    (at 107 106.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(LCD1-Pad11)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A802014)
    (at 82.5 107 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.25 4.75 270) (layer F.SilkS))
    (fp_text value DNP (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /IF0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 124.5 148 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /BUTTON_5))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 124.5 165 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 /BUTTON_4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801F42)
    (at 85.5 166 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -0.25 3.5 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 /BUTTON_3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 114.5 148 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /BUTTON_2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801F4E)
    (at 88 135 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /BUTTON_1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A801F45)
    (at 83.5 166 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at -0.25 3 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 /BUTTON_0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer F.Cu) (tedit 592546E6)
    (at 141 147.5 180)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW1 (at 6.08 -4.66 180) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 180) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0 180) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 /BUTTON_5))
    (pad 2 thru_hole oval (at 12.5 5 180) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 1 thru_hole oval (at 0 0 180) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 /BUTTON_5))
    (pad 2 thru_hole oval (at 0 5 180) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0.248 -0.1 0))
      (scale (xyz 3.93701 3.93701 3.93701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer F.Cu) (tedit 592546E6)
    (at 141 164.5 180)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW2 (at 6.08 -4.66 180) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 180) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0 180) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 37 /BUTTON_4))
    (pad 2 thru_hole oval (at 12.5 5 180) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 1 thru_hole oval (at 0 0 180) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 37 /BUTTON_4))
    (pad 2 thru_hole oval (at 0 5 180) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0.248 -0.1 0))
      (scale (xyz 3.93701 3.93701 3.93701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5A801EED)
    (at 97 169 135)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW3 (at -1.06066 2.474874 225) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 135) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 135) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0 135) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 38 /BUTTON_3))
    (pad 2 thru_hole oval (at 12.5 5 135) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 1 thru_hole oval (at 0 0 135) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 38 /BUTTON_3))
    (pad 2 thru_hole oval (at 0 5 135) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0.248 -0.1 0))
      (scale (xyz 3.93701 3.93701 3.93701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer F.Cu) (tedit 592546E6)
    (at 111 150 225)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW4 (at 6.08 -4.66 225) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 225) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 225) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0 225) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 /BUTTON_2))
    (pad 2 thru_hole oval (at 12.5 5 225) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 1 thru_hole oval (at 0 0 225) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 /BUTTON_2))
    (pad 2 thru_hole oval (at 0 5 225) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0.248 -0.1 0))
      (scale (xyz 3.93701 3.93701 3.93701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5A801F0D)
    (at 92 136 315)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW5 (at 13.435029 2.474874 405) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 315) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 315) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0 315) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 /BUTTON_1))
    (pad 2 thru_hole oval (at 12.5 5 315) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 1 thru_hole oval (at 0 0 315) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 /BUTTON_1))
    (pad 2 thru_hole oval (at 0 5 315) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0.248 -0.1 0))
      (scale (xyz 3.93701 3.93701 3.93701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5A801F13)
    (at 90 150 225)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW6 (at 6.010408 -4.949747 225) (layer F.SilkS))
    (fp_text value SW_Push (at 5.303301 -1.06066 225) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 225) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0 225) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 41 /BUTTON_0))
    (pad 2 thru_hole oval (at 12.5 5 225) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 1 thru_hole oval (at 0 0 225) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 41 /BUTTON_0))
    (pad 2 thru_hole oval (at 0 5 225) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0.248 -0.1 0))
      (scale (xyz 3.93701 3.93701 3.93701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_CuK_OS102011MA1QN1_SPDT_Angled (layer F.Cu) (tedit 5A801F52)
    (at 73.5 138 270)
    (descr "CuK miniature slide switch, OS series, SPDT, right angle, http://www.ckswitches.com/media/1428/os.pdf")
    (tags "switch SPDT")
    (fp_text reference SW7 (at -1 -3.25 270) (layer F.SilkS))
    (fp_text value SW_SPDT (at 1.7 7.7 270) (layer F.Fab))
    (fp_text user %R (at 2.3 1.7 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(BATTERY1-Pad2)"))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -2.1 0 270) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 6.1 0 270) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_CuK_OS102011MA1QN1_SPDT_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A801FCF)
    (at 128.5 110.21 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 2.46 -0.25 180) (layer F.SilkS))
    (fp_text value TPS61165 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 35 /TPS_CTRL))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBL-))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 5A801FA7)
    (at 117.32 129.78 270)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference UPDUINO2_DOWN1 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x16 (at 0 40.43 270) (layer F.Fab))
    (fp_text user %R (at 0 19.05 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /PMOD7))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /PMOD6))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /PMOD5))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /PMOD4))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /PMOD3))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /PMOD2))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /AUDIO))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /PMOD1))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /OSC_OUT))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /PMOD0))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /BUTTON_3))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /BUTTON_2))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /BUTTON_1))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /BUTTON_0))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 5A801FA4)
    (at 117.32 112 270)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference UPDUINO2_UP1 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x18 (at 0 45.51 270) (layer F.Fab))
    (fp_text user %R (at 0 21.59 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /~RESET))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /DX0))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /DX1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /DX2))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /DX3))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /DX4))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /DX5))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /DX6))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /DX7))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HSYNC))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /VSYNC))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /DCLK))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /DEN))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /TPS_CTRL))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /BUTTON_4))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /BUTTON_5))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /OSC_OUT))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x18_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A802011)
    (at 79.5 104.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0.25 -4.75 90) (layer F.SilkS))
    (fp_text value DNP (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /IF2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A802012)
    (at 81 104.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0.25 -4.75 90) (layer F.SilkS))
    (fp_text value DNP (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /IF1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A802013)
    (at 82.5 104.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0.25 -4.75 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /IF0))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 73 35)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J3 (at 0 -4.2) (layer F.SilkS))
    (fp_text value HOLE (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 143 35)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J4 (at 0 -4.2) (layer F.SilkS))
    (fp_text value HOLE (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Symbols:KiCad-Logo_12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 89.25 61 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference J8 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KICAD_LOGO (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_24.3x20mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 126.75 61 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference J5 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW_LOGO (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module "Custom Parts:ICOTC" (layer B.Cu) (tedit 0)
    (at 89.25 79.75 180)
    (fp_text reference J6 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value ICOTC_LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module "Custom Parts:ICESTUDIO" (layer B.Cu) (tedit 0)
    (at 126.75 82.5 180)
    (fp_text reference J11 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value ICESTUDIO_LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text icoTC (at 89.25 90.75) (layer B.SilkS))
  (gr_text "POWERED BY" (at 108 45) (layer B.SilkS))
  (gr_text "FPGA 101 Workshop Badge" (at 108 35) (layer F.SilkS))
  (gr_line (start 145.5 34) (end 145.5 33.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 33.5) (end 70.5 33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.5 171) (end 145.5 171) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 71.5 171) (end 71.5 172) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 171) (end 70.5 171) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80 172) (end 71.5 172) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.5 172) (end 80 172) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 171) (end 145.5 171) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 157.5) (end 70.5 171) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 157.5) (end 145.5 171) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 157.5) (end 145.5 142.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 142.5) (end 70.5 157.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 102.5) (end 145.5 142.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 102.5) (end 70.5 142.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 71.5 33) (end 70.5 33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144 33.5) (end 144 32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.5 32) (end 81.8 32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 73.5) (end 70.5 33.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144 32) (end 81.8 32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 49.2) (end 145.5 34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 72.5) (end 145.5 49.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129 106.21) (end 129 106.21) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 72.5) (end 145.5 77.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 77.5) (end 70.5 72.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 77.5) (end 70.5 91.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 102.5) (end 145.5 77.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.5 102.5) (end 70.5 91.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147 173) (xy 69 173) (xy 69 31) (xy 147 31)
      )
    )
    (polygon
      (pts        (xy 86.5 103.5) (xy 86.5 104.5) (xy 114 104.5) (xy 114 103.5)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 30) (xy 68 30) (xy 68 174) (xy 148 174)
      )
    )
  )
)
