(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.051)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J3-Pad3)")
  (net 2 "GND")
  (net 3 "unconnected-(J3-Pad5)")
  (net 4 "+4V")
  (net 5 "unconnected-(J3-Pad7)")
  (net 6 "+3V3")
  (net 7 "unconnected-(J3-Pad8)")
  (net 8 "Net-(PMOD1-Pad1)")
  (net 9 "Net-(PMOD1-Pad2)")
  (net 10 "Net-(PMOD1-Pad3)")
  (net 11 "Net-(PMOD1-Pad5)")
  (net 12 "Net-(PMOD2-Pad1)")
  (net 13 "Net-(PMOD2-Pad2)")
  (net 14 "Net-(PMOD2-Pad3)")
  (net 15 "Net-(PMOD2-Pad5)")
  (net 16 "/GPIO21")
  (net 17 "Net-(PMOD3-Pad1)")
  (net 18 "Net-(PMOD3-Pad2)")
  (net 19 "Net-(PMOD3-Pad3)")
  (net 20 "Net-(PMOD3-Pad5)")
  (net 21 "/FPGA_P34")
  (net 22 "/VBAT")
  (net 23 "Net-(Q1-Pad1)")
  (net 24 "Net-(Q1-Pad3)")
  (net 25 "Net-(R2-Pad2)")
  (net 26 "Net-(R4-Pad2)")
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 161.671 91.9499 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0.0508 1.7272 90) (layer "F.SilkS"))
    (fp_text value "22 1/8W" (at 0 1.65 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 22 "/VBAT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 104.902 79.502)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.999992) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 167.3606 91.9988 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -2.8042 -0.0508 90) (layer "F.SilkS"))
    (fp_text value "47uF 10V 0805" (at 0 1.68 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/VBAT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 100.42 92.05)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -4) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 104.902 104.648)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.999992) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (footprint "programming-jig:821-22-002-10-004101" (layer "F.Cu")
    (tedit 615A3B0E)
    (at 170.5102 91.0336 180)
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -2.4384 1.3716 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 -2.9 180 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 22 "/VBAT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.54 180) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/lib/3d/mill-max-821-22-002-10-004101.step"
      (offset (xyz -1.27 0.96 3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.6672 101.1428)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/FPGA_P34") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "programming-jig:823-22-008-10-004101" (layer "F.Cu")
    (tedit 630667C8)
    (at 156.21 77.978 90)
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "PMOD3" (at -4.8514 3.937 unlocked) (layer "F.SilkS"))
    (fp_text value "CONN_02X06" (at 0 -2.9 90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 17 "Net-(PMOD3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 18 "Net-(PMOD3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 19 "Net-(PMOD3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -2.54 2.54 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 17 "Net-(PMOD3-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 20 "Net-(PMOD3-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.54 5.08 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 19 "Net-(PMOD3-Pad3)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 18 "Net-(PMOD3-Pad2)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -2.54 7.62 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 20 "Net-(PMOD3-Pad5)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/lib/3d/mill-max-821-22-002-10-004101.step"
      (offset (xyz -1.27 0.96 3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 163.9316 95.6037 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "22 1/8W" (at 0 1.65 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 25 "Net-(R2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 163.957 91.948 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "22 1/8W" (at 0 1.65 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 22 "/VBAT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 25 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 161.6456 100.2049 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.4 90) (layer "F.SilkS"))
    (fp_text value "MMBT3904" (at 0 2.4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(Q1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect locked (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(Q1-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "programming-jig:823-22-008-10-004101" (layer "F.Cu")
    (tedit 630667C8)
    (at 110.49 77.978 90)
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "PMOD1" (at -4.7498 3.9116 unlocked) (layer "F.SilkS"))
    (fp_text value "CONN_02X06" (at 0 -2.9 90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 8 "Net-(PMOD1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 9 "Net-(PMOD1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 10 "Net-(PMOD1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -2.54 2.54 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 8 "Net-(PMOD1-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 11 "Net-(PMOD1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.54 5.08 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 10 "Net-(PMOD1-Pad3)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 9 "Net-(PMOD1-Pad2)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -2.54 7.62 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 11 "Net-(PMOD1-Pad5)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/lib/3d/mill-max-821-22-002-10-004101.step"
      (offset (xyz -1.27 0.96 3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 174.498 79.502)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.999992) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 174.498 104.648)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.999992) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 161.671 95.5821 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 1.6764 90) (layer "F.SilkS"))
    (fp_text value "22 1/8W" (at 0 1.65 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(R4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "programming-jig:821-22-012-10-004101" (layer "F.Cu")
    (tedit 630666B5)
    (at 114.549 105.791 90)
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0.0254 -2.281 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Aux" (at 0 -2.9 90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 4 "+4V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.54 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 6 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 1 "unconnected-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 21 "/FPGA_P34") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J3-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 21 "/FPGA_P34") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 15.24 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 5 "unconnected-(J3-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" thru_hole circle (at 0 17.78 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J3-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect"))
    (pad "9" thru_hole circle (at 0 20.32 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 16 "/GPIO21") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 0 22.86 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 16 "/GPIO21") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 25.4 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 21 "/FPGA_P34") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 0 27.94 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KIPRJMOD}/lib/3d/mill-max-821-22-006-10-004101.step"
      (offset (xyz -1.27 0.96 3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "programming-jig:823-22-008-10-004101" (layer "F.Cu")
    (tedit 630667C8)
    (at 133.35 77.978 90)
    (property "Sheetfile" "ICE-V_Test.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "PMOD2" (at -4.826 3.8354 unlocked) (layer "F.SilkS"))
    (fp_text value "CONN_02X06" (at 0 -2.9 90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 12 "Net-(PMOD2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 13 "Net-(PMOD2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 14 "Net-(PMOD2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -2.54 2.54 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 12 "Net-(PMOD2-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 15 "Net-(PMOD2-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.54 5.08 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 14 "Net-(PMOD2-Pad3)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 13 "Net-(PMOD2-Pad2)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -2.54 7.62 90) (size 2.08 2.08) (drill 0.54) (layers *.Cu *.Mask)
      (net 15 "Net-(PMOD2-Pad5)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/lib/3d/mill-max-821-22-002-10-004101.step"
      (offset (xyz -1.27 0.96 3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (gr_line (start 96.1 79.5) (end 96.1 104.646) (layer "Edge.Cuts") (width 0.1016))
  (gr_arc (start 99.402 107.948) (mid 97.067133 106.980867) (end 96.1 104.646) (layer "Edge.Cuts") (width 0.1016))
  (gr_line (start 99.402 107.948) (end 174.498 107.95) (layer "Edge.Cuts") (width 0.1016))
  (gr_line (start 177.8 104.648) (end 177.8 79.502) (layer "Edge.Cuts") (width 0.1016))
  (gr_arc (start 177.8 104.648) (mid 176.832867 106.982867) (end 174.498 107.95) (layer "Edge.Cuts") (width 0.1016))
  (gr_arc (start 174.498 76.2) (mid 176.832867 77.167133) (end 177.8 79.502) (layer "Edge.Cuts") (width 0.1016))
  (gr_arc (start 96.1 79.5) (mid 97.067133 77.165133) (end 99.402 76.198) (layer "Edge.Cuts") (width 0.1016))
  (gr_line (start 174.498 76.2) (end 99.402 76.198) (layer "Edge.Cuts") (width 0.1016))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.8 107.95)
        (xy 96.1136 107.95)
        (xy 96.1136 76.2)
        (xy 177.8 76.2)
      )
    )
  )
)
