(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 60)
    (no_connects 0)
    (area 21.506667 24.295 52.783334 55.225)
    (thickness 1.6)
    (drawings 8)
    (tracks 233)
    (zones 0)
    (modules 10)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.22)
    (trace_clearance 0.18)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 VCC_A1)
  (net 2 GND_A1)
  (net 3 VCC_A2)
  (net 4 GND_A2)
  (net 5 VCC_B1)
  (net 6 GND_B1)
  (net 7 VCC_B2)
  (net 8 GND_B2)
  (net 9 A0)
  (net 10 A1)
  (net 11 A2)
  (net 12 A3)
  (net 13 A4)
  (net 14 A5)
  (net 15 A6)
  (net 16 A7)
  (net 17 A8)
  (net 18 A9)
  (net 19 A10)
  (net 20 A11)
  (net 21 A12)
  (net 22 A13)
  (net 23 A14)
  (net 24 A15)
  (net 25 B0)
  (net 26 B1)
  (net 27 B2)
  (net 28 B3)
  (net 29 B4)
  (net 30 B5)
  (net 31 B6)
  (net 32 B7)
  (net 33 B8)
  (net 34 B9)
  (net 35 B10)
  (net 36 B11)
  (net 37 B12)
  (net 38 B13)
  (net 39 B14)
  (net 40 B15)
  (net 41 T/#R1)
  (net 42 T/#R2)
  (net 43 "#OE1")
  (net 44 "#OE2")
  (net_class Default "This is the default net class."
    (clearance 0.18)
    (trace_width 0.22)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "#OE1")
    (add_net "#OE2")
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net B0)
    (add_net B1)
    (add_net B10)
    (add_net B11)
    (add_net B12)
    (add_net B13)
    (add_net B14)
    (add_net B15)
    (add_net B2)
    (add_net B3)
    (add_net B4)
    (add_net B5)
    (add_net B6)
    (add_net B7)
    (add_net B8)
    (add_net B9)
    (add_net GND_A1)
    (add_net GND_A2)
    (add_net GND_B1)
    (add_net GND_B2)
    (add_net T/#R1)
    (add_net T/#R2)
    (add_net VCC_A1)
    (add_net VCC_A2)
    (add_net VCC_B1)
    (add_net VCC_B2)
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 58CDAE95)
    (at 39.5 43 270)
    (fp_text reference JP1 (at 0 -1.75 270) (layer B.SilkS))
    (fp_text value Jumper (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC_A1))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC_A2))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 58CDAEA3)
    (at 35 43 270)
    (fp_text reference JP2 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value Jumper (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC_B1))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC_B2))
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 5862ED53)
    (at 46.5 34)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference P1 (at 1.27 -2.39) (layer F.SilkS))
    (fp_text value CONN_02X08 (at 1.27 20.17) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 A0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 A1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 A2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 A4))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 A5))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 A6))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 A7))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 A8))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 A9))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 A10))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 A11))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 A12))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 A13))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 A14))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 A15))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 5862ED53)
    (at 25.25 34)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference P2 (at 1.27 -2.39) (layer F.SilkS))
    (fp_text value CONN_02X08 (at 1.27 20.17) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 B0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 B1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 B2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 B3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 B4))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 B5))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 B6))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 B7))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 B8))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 B9))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 B10))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 B11))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 B12))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 B13))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 B14))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 B15))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 58CC6E5D)
    (at 30.75 30 90)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference P3 (at 1.27 -2.39 90) (layer F.SilkS))
    (fp_text value CONN_02X08 (at 4.75 2.25 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 T/#R1))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC_B1))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND_B1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VCC_B2))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND_B2))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 T/#R2))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "#OE2"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND_A2))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC_A2))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND_A1))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC_A1))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "#OE1"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SSOP:TSSOP-48_6.1x12.5mm_Pitch0.5mm (layer F.Cu) (tedit 58CDA305)
    (at 37.25 43)
    (descr "TSSOP48: plastic thin shrink small outline package; 48 leads; body width 6.1 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot362-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -7.3) (layer F.SilkS))
    (fp_text value LCX16245G (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.75 -5.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 41 T/#R1))
    (pad 2 smd rect (at -3.75 -5.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 25 B0))
    (pad 3 smd rect (at -3.75 -4.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 26 B1))
    (pad 4 smd rect (at -3.75 -4.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 6 GND_B1))
    (pad 5 smd rect (at -3.75 -3.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 27 B2))
    (pad 6 smd rect (at -3.75 -3.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 28 B3))
    (pad 7 smd rect (at -3.75 -2.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC_B1))
    (pad 8 smd rect (at -3.75 -2.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 29 B4))
    (pad 9 smd rect (at -3.75 -1.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 30 B5))
    (pad 10 smd rect (at -3.75 -1.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 6 GND_B1))
    (pad 11 smd rect (at -3.75 -0.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 31 B6))
    (pad 12 smd rect (at -3.75 -0.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 32 B7))
    (pad 13 smd rect (at -3.75 0.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 33 B8))
    (pad 14 smd rect (at -3.75 0.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 34 B9))
    (pad 15 smd rect (at -3.75 1.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 8 GND_B2))
    (pad 16 smd rect (at -3.75 1.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 35 B10))
    (pad 17 smd rect (at -3.75 2.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 36 B11))
    (pad 18 smd rect (at -3.75 2.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC_B2))
    (pad 19 smd rect (at -3.75 3.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 37 B12))
    (pad 20 smd rect (at -3.75 3.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 38 B13))
    (pad 21 smd rect (at -3.75 4.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 8 GND_B2))
    (pad 22 smd rect (at -3.75 4.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 39 B14))
    (pad 23 smd rect (at -3.75 5.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 40 B15))
    (pad 24 smd rect (at -3.75 5.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 42 T/#R2))
    (pad 25 smd rect (at 3.75 5.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 44 "#OE2"))
    (pad 26 smd rect (at 3.75 5.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 24 A15))
    (pad 27 smd rect (at 3.75 4.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 23 A14))
    (pad 28 smd rect (at 3.75 4.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 4 GND_A2))
    (pad 29 smd rect (at 3.75 3.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 22 A13))
    (pad 30 smd rect (at 3.75 3.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 21 A12))
    (pad 31 smd rect (at 3.75 2.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC_A2))
    (pad 32 smd rect (at 3.75 2.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 20 A11))
    (pad 33 smd rect (at 3.75 1.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 19 A10))
    (pad 34 smd rect (at 3.75 1.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 4 GND_A2))
    (pad 35 smd rect (at 3.75 0.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 18 A9))
    (pad 36 smd rect (at 3.75 0.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 17 A8))
    (pad 37 smd rect (at 3.75 -0.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 16 A7))
    (pad 38 smd rect (at 3.75 -0.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 15 A6))
    (pad 39 smd rect (at 3.75 -1.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 2 GND_A1))
    (pad 40 smd rect (at 3.75 -1.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 14 A5))
    (pad 41 smd rect (at 3.75 -2.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 13 A4))
    (pad 42 smd rect (at 3.75 -2.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC_A1))
    (pad 43 smd rect (at 3.75 -3.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 12 A3))
    (pad 44 smd rect (at 3.75 -3.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 11 A2))
    (pad 45 smd rect (at 3.75 -4.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 2 GND_A1))
    (pad 46 smd rect (at 3.75 -4.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 10 A1))
    (pad 47 smd rect (at 3.75 -5.25) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 9 A0))
    (pad 48 smd rect (at 3.75 -5.75) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 43 "#OE1"))
    (model Housings_SSOP.3dshapes/TSSOP-48_6.1x12.5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 31 39.5 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC_B1))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 GND_B1))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58CDAF73)
    (at 31 46.5 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC_B2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND_B2))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 43.5 46.5 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC_A2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND_A2))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58CDAE86)
    (at 43.5 39.5 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC_A1))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND_A1))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "LCX16245G\nBreakout v1.0" (at 37.25 51.5) (layer F.SilkS))
  (gr_text "Nick Palmer\n2017" (at 37.25 51.25) (layer B.Mask))
  (gr_text "Nick Palmer\n2017" (at 37.25 51.25) (layer B.Cu))
  (gr_line (start 22.5 53.75) (end 23 53.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 22.5 25) (end 22.5 53.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.5 25) (end 22.5 25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.5 53.75) (end 51.5 25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 23 53.75) (end 51.5 53.75) (angle 90) (layer Edge.Cuts) (width 0.15))
)
