(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (grid_origin 83.185 152.4)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer false)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../../../../Downloads/thruster_junction_board/")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad2)")
  (net 2 "Net-(U1-Pad4)")
  (net 3 "Net-(U1-Pad5)")
  (net 4 "Net-(U1-Pad6)")
  (net 5 "GND")
  (net 6 "Net-(U1-Pad3)")
  (net 7 "Net-(C7-Pad2)")
  (net 8 "/RS485_B")
  (net 9 "/RS485_A")
  (net 10 "/ISO_RS232_TO_A10")
  (net 11 "/ISO_RS232_FROM_A10")
  (net 12 "Net-(R1-Pad1)")
  (net 13 "/ISO_!RE")
  (net 14 "/ISO_RXD")
  (net 15 "/ISO_TXD")
  (net 16 "Net-(U1-Pad7)")
  (net 17 "Net-(J4-Pad3)")
  (net 18 "Net-(J4-Pad4)")
  (net 19 "+48V")
  (net 20 "Net-(J4-Pad5)")
  (net 21 "Net-(J5-Pad3)")
  (net 22 "Net-(J5-Pad4)")
  (net 23 "Net-(J5-Pad5)")
  (net 24 "Net-(J6-Pad3)")
  (net 25 "Net-(J6-Pad4)")
  (net 26 "Net-(J6-Pad5)")
  (net 27 "Net-(J7-Pad3)")
  (net 28 "Net-(J7-Pad4)")
  (net 29 "Net-(J7-Pad5)")
  (net 30 "Net-(J8-Pad3)")
  (net 31 "Net-(J8-Pad4)")
  (net 32 "Net-(J8-Pad5)")
  (net 33 "Net-(J9-Pad3)")
  (net 34 "Net-(J9-Pad4)")
  (net 35 "Net-(R4-Pad1)")
  (net 36 "/MODE")
  (net 37 "Net-(C12-Pad2)")
  (net 38 "Net-(C12-Pad1)")
  (net 39 "/VISO_5V")
  (net 40 "/ISO_EN")
  (net 41 "/ISO_DE")
  (net 42 "GNDS")
  (net 43 "VDD")
  (net 44 "/GSS_24V")
  (net 45 "Net-(J9-Pad5)")
  (net 46 "unconnected-(J4-Pad2)")
  (net 47 "unconnected-(J4-Pad1)")
  (net 48 "unconnected-(J5-Pad2)")
  (net 49 "unconnected-(J5-Pad1)")
  (net 50 "unconnected-(J6-Pad2)")
  (net 51 "unconnected-(J6-Pad1)")
  (net 52 "unconnected-(J7-Pad2)")
  (net 53 "unconnected-(J7-Pad1)")
  (net 54 "unconnected-(J8-Pad2)")
  (net 55 "unconnected-(J8-Pad1)")
  (net 56 "unconnected-(J9-Pad2)")
  (net 57 "unconnected-(J9-Pad1)")
  (net 58 "unconnected-(U1-Pad10)")
  (net 59 "unconnected-(U3-Pad14)")
  (net 60 "unconnected-(U3-Pad7)")
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 167.3005 43.756)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -3.1155 -0.106) (layer "F.SilkS"))
    (fp_text value "0.47uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Net-(U1-Pad6)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "Net-(U1-Pad5)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 151.003 44.4285 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 1.568 90) (layer "F.SilkS"))
    (fp_text value "0.22uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 7 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 157.5805 78.582 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 3.3955 -0.068) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 38 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 37 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 185.56 152.185)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 185.56 42.965)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 76.34 42.965)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 76.34 152.185)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.115 49.546 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.604 -0.32 90) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 12 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 43 "VDD") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 156.435 55.9)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 -1.648) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 "/ISO_EN") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 170.2495 61.302)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 3.4355 -0.152) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 43 "VDD") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 162.6475 61.15 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 1.75) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 43 "VDD") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 157.5375 80.868 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 3.3525 -0.032) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 38 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 37 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 157.0895 83.662 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 3.9045 0.012) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5625 0 180) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 38 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5625 0 180) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 37 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.575 87.456 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB1" (at -2.944 0.11 90) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 39 "/VISO_5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 38 "Net-(C12-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "raven_parts_library:Harwin_Mixtex_4+2_Horizontal" (layer "F.Cu")
    (tedit 6137A025)
    (at 165.149 127.176 90)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -3.445 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 0 -0.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 11.5 1 90) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5.5 1 90) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 49 "unconnected-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle locked (at -2 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 "unconnected-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle locked (at 0 2 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -2 2 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(J5-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3 2 90) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 7 2 90) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "raven_parts_library:Harwin_Mixtex_4+2_Horizontal" (layer "F.Cu")
    (tedit 6137A025)
    (at 142.757 133.716)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at -0.095 -2.445) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.5 1) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 11.5 1) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 51 "unconnected-(J6-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle locked (at -2 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 50 "unconnected-(J6-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle locked (at 0 2) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(J6-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -2 2) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(J6-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3 2) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 7 2) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "raven_parts_library:Harwin_Mixtex_4+2_Horizontal" (layer "F.Cu")
    (tedit 6137A025)
    (at 118.923 133.732)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 0.635 -2.54) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.5 1) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 11.5 1) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 53 "unconnected-(J7-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle locked (at -2 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 52 "unconnected-(J7-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle locked (at 0 2) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(J7-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -2 2) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(J7-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3 2) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 29 "Net-(J7-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 7 2) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "raven_parts_library:Harwin_Mixtex_4+2_Horizontal" (layer "F.Cu")
    (tedit 6137A025)
    (at 96.467 111.62 -90)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.54 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 0 -0.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.5 1 270) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 11.5 1 270) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 55 "unconnected-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle locked (at -2 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 54 "unconnected-(J8-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle locked (at 0 2 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(J8-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -2 2 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(J8-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3 2 270) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 32 "Net-(J8-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 7 2 270) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "raven_parts_library:Harwin_Mixtex_4+2_Horizontal" (layer "F.Cu")
    (tedit 6137A025)
    (at 96.467 85.746 -90)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -2.54 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 0 -0.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5.5 1 270) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 11.5 1 270) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 57 "unconnected-(J9-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle locked (at -2 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 56 "unconnected-(J9-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle locked (at 0 2 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(J9-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -2 2 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(J9-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3 2 270) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 45 "Net-(J9-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 7 2 270) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.685 61.15 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 3 0) (layer "F.SilkS"))
    (fp_text value "0k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 35 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 43 "VDD") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 163.159 70.446 -90)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -7.35 90) (layer "F.SilkS"))
    (fp_text value "ISOW14x2" (at 0 7.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.65 -5.715 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "VDD") (pinfunction "VIO") (pintype "input"))
    (pad "2" smd roundrect locked (at -4.65 -4.445 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/ISO_TXD") (pinfunction "D") (pintype "input"))
    (pad "3" smd roundrect locked (at -4.65 -3.175 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/ISO_DE") (pinfunction "DE") (pintype "input"))
    (pad "4" smd roundrect locked (at -4.65 -1.905 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/ISO_RXD") (pinfunction "R") (pintype "input"))
    (pad "5" smd roundrect locked (at -4.65 -0.635 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/ISO_!RE") (pinfunction "/RE") (pintype "input"))
    (pad "6" smd roundrect locked (at -4.65 0.635 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "GNDS") (pinfunction "GNDIO") (pintype "input"))
    (pad "7" smd roundrect locked (at -4.65 1.905 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "unconnected-(U3-Pad7)") (pinfunction "OUT") (pintype "input+no_connect"))
    (pad "8" smd roundrect locked (at -4.65 3.175 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(R4-Pad1)") (pinfunction "EN/FLT") (pintype "input"))
    (pad "9" smd roundrect locked (at -4.65 4.445 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "VDD") (pinfunction "VDD") (pintype "input"))
    (pad "10" smd roundrect locked (at -4.65 5.715 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "GNDS") (pinfunction "GND1") (pintype "input"))
    (pad "11" smd roundrect locked (at 4.65 5.715 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C12-Pad2)") (pinfunction "GND2") (pintype "input"))
    (pad "12" smd roundrect locked (at 4.65 4.445 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(C12-Pad1)") (pinfunction "VISOOUT") (pintype "input"))
    (pad "13" smd roundrect locked (at 4.65 3.175 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/MODE") (pinfunction "MODE") (pintype "input"))
    (pad "14" smd roundrect locked (at 4.65 1.905 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "unconnected-(U3-Pad14)") (pinfunction "IN") (pintype "input+no_connect"))
    (pad "15" smd roundrect locked (at 4.65 0.635 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pinfunction "GISOIN") (pintype "input"))
    (pad "16" smd roundrect locked (at 4.65 -0.635 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/VISO_5V") (pinfunction "VISOIN") (pintype "input"))
    (pad "17" smd roundrect locked (at 4.65 -1.905 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/RS485_A") (pinfunction "Y") (pintype "input"))
    (pad "18" smd roundrect locked (at 4.65 -3.175 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/RS485_B") (pinfunction "Z") (pintype "input"))
    (pad "19" smd roundrect locked (at 4.65 -4.445 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/RS485_B") (pinfunction "B") (pintype "input"))
    (pad "20" smd roundrect locked (at 4.65 -5.715 270) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/RS485_A") (pinfunction "A") (pintype "input"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "raven_parts_library:Harwin_Mixtex_4+2_Horizontal" (layer "F.Cu")
    (tedit 6137A025)
    (at 165.149 104.164 90)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0.215 -2.175 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 0 -0.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 11.5 1 90) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5.5 1 90) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 47 "unconnected-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle locked (at -2 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 "unconnected-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle locked (at 0 2 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -2 2 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3 2 90) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 20 "Net-(J4-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 7 2 90) (size 2.8 2.8) (drill 1.71) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "raven_parts_library:Harwin_JTek_2x2_through_hole_horizontal_jackscrews" (layer "F.Cu")
    (tedit 5FE428D5)
    (at 88.125 68.146 90)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -4.2 0) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Male" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -2 1 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 1 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -2 -1 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "/RS485_A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 -1 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "/RS485_B") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 170.2495 63.334)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 3.4355 -0.184) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 43 "VDD") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SSOP-16_5.3x6.2mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 170.073 49.852 -90)
    (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot338-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.2 90) (layer "F.SilkS"))
    (fp_text value "MAX3221" (at 0 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.45 -2.275 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "GNDS") (pinfunction "~{EN}") (pintype "input"))
    (pad "2" smd rect locked (at -3.45 -1.625 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(U1-Pad2)") (pinfunction "C1+") (pintype "passive"))
    (pad "3" smd rect locked (at -3.45 -0.975 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(U1-Pad3)") (pinfunction "V+") (pintype "power_out"))
    (pad "4" smd rect locked (at -3.45 -0.325 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(U1-Pad4)") (pinfunction "C1-") (pintype "passive"))
    (pad "5" smd rect locked (at -3.45 0.325 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(U1-Pad5)") (pinfunction "C2+") (pintype "passive"))
    (pad "6" smd rect locked (at -3.45 0.975 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U1-Pad6)") (pinfunction "C2-") (pintype "passive"))
    (pad "7" smd rect locked (at -3.45 1.625 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(U1-Pad7)") (pinfunction "V-") (pintype "power_out"))
    (pad "8" smd rect locked (at -3.45 2.275 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/ISO_RS232_FROM_A10") (pinfunction "RIN") (pintype "input"))
    (pad "9" smd rect locked (at 3.45 2.275 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/ISO_TXD") (pinfunction "ROUT") (pintype "output"))
    (pad "10" smd rect locked (at 3.45 1.625 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "unconnected-(U1-Pad10)") (pinfunction "~{INVALID}") (pintype "output+no_connect"))
    (pad "11" smd rect locked (at 3.45 0.975 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/ISO_RXD") (pinfunction "DIN") (pintype "input"))
    (pad "12" smd rect locked (at 3.45 0.325 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "GNDS") (pinfunction "FORCEON") (pintype "input"))
    (pad "13" smd rect locked (at 3.45 -0.325 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/ISO_RS232_TO_A10") (pinfunction "DOUT") (pintype "output"))
    (pad "14" smd rect locked (at 3.45 -0.975 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "GNDS") (pinfunction "GND") (pintype "power_in"))
    (pad "15" smd rect locked (at 3.45 -1.625 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "VDD") (pinfunction "VCC") (pintype "power_in"))
    (pad "16" smd rect locked (at 3.45 -2.275 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "VDD") (pinfunction "~{FORCEOFF}") (pintype "input"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SSOP-16_5.3x6.2mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 165.247 51.9375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 43 "VDD") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.003 48.244 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -0.094 1.568 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 7 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 43 "VDD") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 155.527 87.456 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB2" (at -3.194 -0.092 90) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 37 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.607 87.456 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 2.944 -0.078 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 36 "/MODE") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 39 "/VISO_5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 163.1375 78.828 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -3.5475 -0.072) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 39 "/VISO_5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 5 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 170.2325 58.508)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 3.4525 0.392) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 43 "VDD") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 42 "GNDS") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 171.1105 43.756)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 3.0745 0.144) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "Net-(U1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "Net-(U1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 165.247 47.3335 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "0.47uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 16 "Net-(U1-Pad7)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SSOP-8_2.95x2.8mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 156.513 45.649 180)
    (descr "SSOP-8 2.9 x2.8mm Pitch 0.65mm")
    (tags "SSOP-8 2.95x2.8mm Pitch 0.65mm")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "74LVC1G123" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.7 -0.975 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/ISO_TXD") (pinfunction "~{A}") (pintype "input"))
    (pad "2" smd rect locked (at -1.7 -0.325 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(R1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "3" smd rect locked (at -1.7 0.325 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(R1-Pad1)") (pinfunction "~{CLR}") (pintype "input"))
    (pad "4" smd rect locked (at -1.7 0.975 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "GNDS") (pinfunction "GNDS") (pintype "input"))
    (pad "5" smd rect locked (at 1.7 0.975 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/ISO_EN") (pinfunction "Q") (pintype "output"))
    (pad "6" smd rect locked (at 1.7 0.325 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "GNDS") (pinfunction "Cext") (pintype "input"))
    (pad "7" smd rect locked (at 1.7 -0.325 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C7-Pad2)") (pinfunction "Rext") (pintype "input"))
    (pad "8" smd rect locked (at 1.7 -0.975 90) (size 0.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "VDD") (pinfunction "VDD") (pintype "unspecified"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SSOP-8_2.95x2.8mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 154.559 49.5085 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 2.8915 -0.126 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 43 "VDD") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.999 69.15 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 3.032 0) (layer "F.SilkS"))
    (fp_text value "0k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 41 "/ISO_DE") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 40 "/ISO_EN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "raven_parts_library:Harwin_MixTek_0+4_horizontal" (layer "F.Cu")
    (tedit 6137A03C)
    (at 110.685 59.65 180)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 0.5) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Male" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -4.5 -1 180) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 16.5 -1 180) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 19 "+48V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 4 0 180) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 19 "+48V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 8 0 180) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 12 0 180) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "raven_parts_library:Harwin_MixTek_0+4_horizontal" (layer "F.Cu")
    (tedit 6137A03C)
    (at 137.685 59.65 180)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at 0 0.5) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Male" (at 0 -0.5 270) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 16.5 -1 180) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -4.5 -1 180) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 19 "+48V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 4 0 180) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 19 "+48V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 8 0 180) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 12 0 180) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "raven_parts_library:Harwin_JTek_5x2_through_hole_horizontal_jackscrews" (layer "F.Cu")
    (tedit 5FE428A5)
    (at 180.975 67.056 -90)
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -4.2 0) (layer "F.SilkS"))
    (fp_text value "Conn_01x10_Male" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -2 1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "/ISO_RS232_FROM_A10") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "/ISO_RS232_TO_A10") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2 1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "/RS485_A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 4 1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "/RS485_B") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 6 1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at -2 -1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 "GNDS") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 0 -1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 "/GSS_24V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 2 -1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "/RS485_A") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 4 -1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "/RS485_B") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle locked (at 6 -1 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_10") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 176.185 73.15 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 3 0 180) (layer "F.SilkS"))
    (fp_text value "n/p" (at 0 1.65 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.999 67.15 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 3.032 0) (layer "F.SilkS"))
    (fp_text value "0k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 13 "/ISO_!RE") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 40 "/ISO_EN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 163.2475 81.65 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at -3.9375 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5625 0 180) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 39 "/VISO_5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5625 0 180) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 176.185 69.15 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 3 0) (layer "F.SilkS"))
    (fp_text value "n/p" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 9 "/RS485_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 39 "/VISO_5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 172.1065 41.148)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -3.1715 0.002) (layer "F.SilkS"))
    (fp_text value "0.47uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 6 "Net-(U1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 151.765 39.878)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 2.673 0.127) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "/ISO_RXD") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 157.607 39.878)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at -0.508 1.92) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "/ISO_TXD") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 134.185 77.217621 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C19" (at 5.782379 -0.2 180) (layer "F.SilkS"))
    (fp_text value "33uF 63V" (at 1.25 4.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "+48V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 126.285 77.217621 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C18" (at 5.982379 0.1 180) (layer "F.SilkS"))
    (fp_text value "33uF 63V" (at 1.25 4.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "+48V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 102.785 77.3 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C22" (at 5.7 -0.2 180) (layer "F.SilkS"))
    (fp_text value "33uF 63V" (at 1.25 4.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "+48V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 110.485 77.217621 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C20" (at 5.682379 0.1 180) (layer "F.SilkS"))
    (fp_text value "33uF 63V" (at 1.25 4.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "+48V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 118.685 77.217621 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C21" (at 5.782379 -0.2 180) (layer "F.SilkS"))
    (fp_text value "33uF 63V" (at 1.25 4.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "+48V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 141.985 77.3 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C23" (at 5.682379 0.2 180) (layer "F.SilkS"))
    (fp_text value "33uF 63V" (at 1.25 4.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "+48V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 186.185 75.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 3 0) (layer "B.SilkS"))
    (fp_text value "120" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 9 "/RS485_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 175.81 104.15)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.524) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J4-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/RS485_A") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 175.81 106.15)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F2" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J4-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 158.4225 101.15 180)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F3" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "8A(T)" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 180) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 20 "Net-(J4-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4875 0 180) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 19 "+48V") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 175.56 127.15)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F4" (at 0 -1.524) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J5-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/RS485_A") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 158.6725 124.15 180)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F6" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "8A(T)" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 180) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 23 "Net-(J5-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4875 0 180) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 19 "+48V") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 145.885 126.5875 90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F9" (at 0.7375 2 270) (layer "B.SilkS"))
    (fp_text value "8A(T)" (at 0 -1.82 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 26 "Net-(J6-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 19 "+48V") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 118.935 144.025 -90)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F10" (at -0.069 -1.5 -90) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J7-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/RS485_A") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 116.935 144.025 -90)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F11" (at 0 1.43 -90) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J7-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 85.06 111.65 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F13" (at -0.125 -2) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J8-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/RS485_A") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 104.6975 114.65)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F15" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "8A(T)" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 32 "Net-(J8-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4875 0) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 19 "+48V") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 84.81 85.9 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F16" (at 3.125 -0.1) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J9-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/RS485_A") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 84.81 83.65 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F17" (at 3.125 -0.05) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at -0.575001 -3.064999) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J9-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 142.757 144.025 -90)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F7" (at -0.037 -1.678 90) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J6-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/RS485_A") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 104.6975 88.9)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F18" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "8A(T)" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 45 "Net-(J9-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4875 0) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 19 "+48V") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 121.935 126.8875 90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F12" (at 0.4875 2 90) (layer "B.SilkS"))
    (fp_text value "8A(T)" (at 0 -1.82 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 29 "Net-(J7-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.175439)
      (net 19 "+48V") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 140.685 144.025 -90)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F8" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J6-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 187.0925 62.484 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at -0.0925 -1.816) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 44 "/GSS_24V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 42 "GNDS") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "B.Cu")
    (tedit 5A70A390)
    (at 185.801 55.372 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 4.5 90) (layer "B.SilkS"))
    (fp_text value "LM78M05_TO252" (at 0 -4.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" smd rect locked (at 0.425 -1.525 90) (size 3.05 2.75) (layers "B.Paste"))
    (pad "" smd rect locked (at 3.775 -1.525 90) (size 3.05 2.75) (layers "B.Paste"))
    (pad "" smd rect locked (at 0.425 1.525 90) (size 3.05 2.75) (layers "B.Paste"))
    (pad "" smd rect locked (at 3.775 1.525 90) (size 3.05 2.75) (layers "B.Paste"))
    (pad "1" smd rect locked (at -4.2 2.28 90) (size 2.2 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "/GSS_24V") (pinfunction "VI") (pintype "power_in"))
    (pad "2" smd rect locked (at 2.1 0 90) (size 6.4 5.8) (layers "B.Cu" "B.Mask")
      (net 42 "GNDS") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect locked (at -4.2 -2.28 90) (size 2.2 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "VDD") (pinfunction "VO") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 83.807 69.162 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 3.512 -0.122 270) (layer "B.SilkS"))
    (fp_text value "120" (at 0 -1.65 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 9 "/RS485_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 175.56 129.15)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F5" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J5-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 85.06 109.65 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F14" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "250mA(F)" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(J8-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/RS485_B") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC_Handsoldering" (layer "B.Cu")
    (tedit 58642B03)
    (at 172.585 95.9 -90)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0.3 -4.1 90) (layer "B.SilkS"))
    (fp_text value "3.0SMCJ48CA" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.4 0 180) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 180) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "Net-(J4-Pad5)") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC_Handsoldering" (layer "B.Cu")
    (tedit 58642B03)
    (at 172.685 119.1 -90)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -4.4 90) (layer "B.SilkS"))
    (fp_text value "3.0SMCJ48CA" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.4 0 180) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 180) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "Net-(J5-Pad5)") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC_Handsoldering" (layer "B.Cu")
    (tedit 58642B03)
    (at 88.885 93.9 -90)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 4.1 90) (layer "B.SilkS"))
    (fp_text value "3.0SMCJ48CA" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.4 0 180) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "Net-(J9-Pad5)") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 180) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC_Handsoldering" (layer "B.Cu")
    (tedit 58642B03)
    (at 151.185 141 180)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at -1.2 -4.3) (layer "B.SilkS"))
    (fp_text value "3.0SMCJ48CA" (at 0 -4.2) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5) (layer "B.Fab"))
    (pad "1" smd rect (at -4.4 0 90) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 90) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "Net-(J6-Pad5)") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC_Handsoldering" (layer "B.Cu")
    (tedit 58642B03)
    (at 127.085 141 180)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at -2.2 -4.3) (layer "B.SilkS"))
    (fp_text value "3.0SMCJ48CA" (at 0 -4.2) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5) (layer "B.Fab"))
    (pad "1" smd rect (at -4.4 0 90) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0 90) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "Net-(J7-Pad5)") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC_Handsoldering" (layer "B.Cu")
    (tedit 58642B03)
    (at 89.285 119.6 90)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (property "Sheetfile" "File: /home/aaron/workspace/raven/vehicle_interface_board/thruster_junction_board_rev2/thruster_junction_board_rev2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at -0.1 -4.1 90) (layer "B.SilkS"))
    (fp_text value "3.0SMCJ48CA" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.4 0) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect (at 4.4 0) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "Net-(J8-Pad5)") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 69.85 43.18) (end 69.85 152.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 76.2 158.75) (end 185.42 158.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 191.77 152.4) (end 191.77 43.18) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 185.42 36.83) (end 76.2 36.83) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 76.2 158.75) (mid 71.709872 156.890128) (end 69.85 152.4) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 69.85 43.18) (mid 71.709872 38.689872) (end 76.2 36.83) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 185.42 36.83) (mid 189.910128 38.689872) (end 191.77 43.18) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 191.77 152.4) (mid 189.910128 156.890128) (end 185.42 158.75) (layer "Edge.Cuts") (width 0.1))
  (gr_text "To A10\n" (at 148.185 38.65) (layer "F.SilkS"))
  (gr_text "From A10\n" (at 162.435 38.65) (layer "F.SilkS"))
  (gr_text "J10" (at 131.5 63.281) (layer "F.SilkS"))
  (gr_text "RAVEN \nTHRUSTER JUNCTION BOARD\nREV C.  10/2022\nS/N                    " (at 122.809 70.104) (layer "F.SilkS"))
  (gr_text "J1" (at 105.838 63.535) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 191.643 45.212) (xy 69.723 45.212))
    (height 18.288)
    (gr_text "4.8000 in" (at 130.683 25.774) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 76.2 43.18) (xy 69.85 43.18))
    (height 10.922)
    (gr_text "0.2500 in" (at 73.025 31.108) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 74.041 42.926) (xy 78.613 42.926))
    (height -7.874)
    (gr_text "0.1800 in" (at 76.327 33.902) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 76.073 43.18) (xy 76.073 36.83))
    (height -12.192)
    (gr_text "0.2500 in" (at 62.731 40.005 90) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 75.565 158.75) (xy 75.819 36.83))
    (height -17.777843)
    (gr_text "4.8000 in" (at 56.764198 97.750567 89.88063397) (layer "Dwgs.User"))
    (format (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 5) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.935 58.65)
        (xy 144.935 67.65)
        (xy 149.935 72.15)
        (xy 183.185 72.15)
        (xy 183.185 81.15)
        (xy 173.185 91.15)
        (xy 173.185 130.15)
        (xy 161.185 142.15)
        (xy 110.185 142.15)
        (xy 88.435 120.15)
        (xy 88.435 60.4)
        (xy 97.185 54.9)
        (xy 141.185 54.9)
      )
    )
  )
  (zone (net 42) (net_name "GNDS") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.185 41.9)
        (xy 190.185 67.9)
        (xy 172.935 67.9)
        (xy 170.935 69.9)
        (xy 150.685 69.9)
        (xy 147.185 66.9)
        (xy 147.185 38.15)
        (xy 186.435 38.15)
      )
    )
  )
  (zone (net 42) (net_name "GNDS") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.119 66.802)
        (xy 183.515 66.802)
        (xy 179.959 63.246)
        (xy 179.959 48.514)
        (xy 190.119 48.514)
      )
    )
  )
  (zone (net 19) (net_name "+48V") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 1.1))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.185 63.4)
        (xy 145.885 69.1)
        (xy 145.985 96.1)
        (xy 148.785 98.9)
        (xy 157.585 98.9)
        (xy 158.185 99.5)
        (xy 158.185 125.4)
        (xy 157.185 126.4)
        (xy 114.685 126.4)
        (xy 105.185 118.4)
        (xy 105.185 84.1)
        (xy 100.385 81.2)
        (xy 100.385 65.9)
        (xy 104.185 61.65)
        (xy 104.185 58.9)
        (xy 106.185 56.9)
        (xy 138.935 56.9)
        (xy 140.185 58.15)
      )
    )
  )
)
