(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6002)
    (drawings 52)
    (tracks 1388)
    (zones 0)
    (modules 129)
    (nets 199)
  )
  (page A4)
  (layers
    (0 F.Cu jumper)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad1)")
  (net 2 AGND)
  (net 3 XBEE_VCC)
  (net 4 FT231_3V3OUT)
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad2)")
  (net 8 uC_accel_x)
  (net 9 uC_accel_y)
  (net 10 uC_accel_z)
  (net 11 FT231X_VCC)
  (net 12 433_VCC)
  (net 13 "/433 MHz Transmitter/LNA_P")
  (net 14 "Net-(C15-Pad2)")
  (net 15 "/433 MHz Transmitter/LNA_N")
  (net 16 "Net-(C17-Pad1)")
  (net 17 "Net-(C18-Pad1)")
  (net 18 "Net-(C19-Pad1)")
  (net 19 "Net-(C19-Pad2)")
  (net 20 "Net-(C22-Pad1)")
  (net 21 "Net-(C23-Pad2)")
  (net 22 "Net-(C23-Pad1)")
  (net 23 "Net-(C25-Pad1)")
  (net 24 "Net-(C27-Pad1)")
  (net 25 "Net-(C29-Pad1)")
  (net 26 "/433 MHz Transmitter/TRX_SW")
  (net 27 "Net-(C31-Pad1)")
  (net 28 "Net-(C36-Pad2)")
  (net 29 "Net-(C37-Pad1)")
  (net 30 ACCEL_VCC)
  (net 31 PRESSURE_VCC)
  (net 32 BNO_VCC)
  (net 33 MPU_VCC)
  (net 34 "Net-(C45-Pad2)")
  (net 35 "Net-(C46-Pad2)")
  (net 36 /Sensors/MPU_VIO)
  (net 37 "Net-(D1-Pad1)")
  (net 38 "Net-(D2-Pad1)")
  (net 39 "Net-(D3-Pad2)")
  (net 40 "Net-(D4-Pad2)")
  (net 41 "Net-(D5-Pad2)")
  (net 42 "Net-(D6-Pad2)")
  (net 43 "Net-(D7-Pad2)")
  (net 44 "Net-(D8-Pad2)")
  (net 45 uC_IMU_TX)
  (net 46 uC_IMU_RX)
  (net 47 uC_30_CAN0RX)
  (net 48 uC_29_CAN0TX)
  (net 49 uC_MOSI_433_trans)
  (net 50 uC_27_rx1-sck0)
  (net 51 uC_26_tx1)
  (net 52 uC_CS_433_trans)
  (net 53 uC_24_DIO)
  (net 54 uC_3V3_OUT)
  (net 55 uC_12_MISO0)
  (net 56 uC_11_MOSI0)
  (net 57 uC_gps_TX)
  (net 58 uC_gps_RX)
  (net 59 uC_TX3)
  (net 60 uC_RX3)
  (net 61 uC_6_pwm)
  (net 62 uC_5_pwm)
  (net 63 uC_4_pwm-SDA2)
  (net 64 uC_3_pwm-SCL2)
  (net 65 uC_2_pwm)
  (net 66 uC_xbee_TX)
  (net 67 uC_xbee_RX)
  (net 68 uC_33-A14-CAN1TX-SCL0-TX5)
  (net 69 uC_34-A15-CAN1RX-SDA0-RX5)
  (net 70 accel_self_test)
  (net 71 uC_433_reset)
  (net 72 uC_37-A18-SCL1)
  (net 73 uC_38-A19-SDA1)
  (net 74 uC_MISO_433_trans)
  (net 75 A21_DAC0)
  (net 76 A22_DAC1)
  (net 77 "uC_13-SCK0(LED)")
  (net 78 uC_SPI_SCK_433_trans)
  (net 79 uC_15-A1-CS0)
  (net 80 uC_16-A2-SCL0)
  (net 81 uC_17-A3-SDA0)
  (net 82 uC_SDA)
  (net 83 uC_SCL)
  (net 84 uC_21-A6-CS0-MOSI1-rx1)
  (net 85 uC_5Vin)
  (net 86 FT231X_VBUS)
  (net 87 "Net-(J3-Pad4)")
  (net 88 /xbee_breakout/XBEE_DOUT)
  (net 89 /xbee_breakout/XBEE_DIN)
  (net 90 /xbee_breakout/DO8)
  (net 91 /xbee_breakout/PWM1)
  (net 92 "Net-(J5-Pad8)")
  (net 93 /xbee_breakout/DTR_SLEEP)
  (net 94 /xbee_breakout/DIO0)
  (net 95 /xbee_breakout/DIO1)
  (net 96 /xbee_breakout/DIO2)
  (net 97 /xbee_breakout/DIO3)
  (net 98 /xbee_breakout/RTS_DIO6)
  (net 99 /xbee_breakout/ASSOC_DIO5)
  (net 100 /xbee_breakout/VREF)
  (net 101 /xbee_breakout/ON_SLEEP)
  (net 102 /xbee_breakout/CTS_DIO7)
  (net 103 /xbee_breakout/DIO4)
  (net 104 XBEE_3V3)
  (net 105 GPS_VCC)
  (net 106 "/433 MHz Transmitter/GPIO0")
  (net 107 "/433 MHz Transmitter/GPIO2")
  (net 108 "/433 MHz Transmitter/GPIO3")
  (net 109 433_VCC_IN)
  (net 110 FT_TX)
  (net 111 "Net-(J15-Pad2)")
  (net 112 "Net-(J16-Pad2)")
  (net 113 FT_RX)
  (net 114 "Net-(J17-Pad2)")
  (net 115 /Sensors/MPU_ADR_SEL)
  (net 116 /Sensors/MPU_XCL)
  (net 117 /Sensors/MPU_XDA)
  (net 118 FT231_D+)
  (net 119 FT231_D-)
  (net 120 "Net-(R3-Pad2)")
  (net 121 "Net-(R4-Pad2)")
  (net 122 "Net-(R5-Pad2)")
  (net 123 "Net-(R8-Pad1)")
  (net 124 "Net-(R10-Pad2)")
  (net 125 "Net-(R11-Pad1)")
  (net 126 "Net-(U2-Pad25)")
  (net 127 "Net-(U2-Pad26)")
  (net 128 "Net-(U2-Pad28)")
  (net 129 "Net-(U2-Pad51)")
  (net 130 "Net-(U2-Pad54)")
  (net 131 "Net-(U2-Pad55)")
  (net 132 "Net-(U2-Pad56)")
  (net 133 "Net-(U2-Pad57)")
  (net 134 "Net-(U2-Pad63)")
  (net 135 "Net-(U2-Pad64)")
  (net 136 "Net-(U2-Pad65)")
  (net 137 "Net-(U2-Pad66)")
  (net 138 "Net-(U2-Pad67)")
  (net 139 "Net-(U2-Pad68)")
  (net 140 "Net-(U2-Pad69)")
  (net 141 "Net-(U2-Pad70)")
  (net 142 "Net-(U2-Pad71)")
  (net 143 "Net-(U2-Pad72)")
  (net 144 "Net-(U2-Pad73)")
  (net 145 "Net-(U2-Pad75)")
  (net 146 "Net-(U2-Pad76)")
  (net 147 "Net-(U2-Pad77)")
  (net 148 "Net-(U2-Pad78)")
  (net 149 "Net-(U2-Pad79)")
  (net 150 "Net-(U2-Pad80)")
  (net 151 "Net-(U2-Pad81)")
  (net 152 "Net-(U2-Pad82)")
  (net 153 "Net-(U2-Pad83)")
  (net 154 "Net-(U2-Pad84)")
  (net 155 "Net-(U2-Pad85)")
  (net 156 "Net-(U2-Pad86)")
  (net 157 "Net-(U2-Pad58)")
  (net 158 "Net-(U2-Pad59)")
  (net 159 "Net-(U2-Pad60)")
  (net 160 "Net-(U5-Pad1)")
  (net 161 "Net-(U5-Pad2)")
  (net 162 "Net-(U5-Pad5)")
  (net 163 "Net-(U5-Pad7)")
  (net 164 "Net-(U5-Pad8)")
  (net 165 "Net-(U5-Pad9)")
  (net 166 "Net-(U5-Pad18)")
  (net 167 "Net-(U5-Pad19)")
  (net 168 "Net-(U7-Pad4)")
  (net 169 "Net-(U7-Pad5)")
  (net 170 "Net-(U7-Pad13)")
  (net 171 "Net-(U7-Pad14)")
  (net 172 "Net-(U7-Pad16)")
  (net 173 "Net-(U7-Pad17)")
  (net 174 "Net-(U7-Pad18)")
  (net 175 "Net-(U8-Pad8)")
  (net 176 "Net-(U13-Pad32)")
  (net 177 "Net-(U14-Pad12)")
  (net 178 "Net-(U14-Pad19)")
  (net 179 "Net-(U14-Pad21)")
  (net 180 "Net-(U14-Pad22)")
  (net 181 "Net-(U11-Pad6)")
  (net 182 "Net-(U11-Pad10)")
  (net 183 "Net-(U11-Pad4)")
  (net 184 "Net-(U11-Pad1)")
  (net 185 "Net-(U11-Pad2)")
  (net 186 "Net-(U11-Pad3)")
  (net 187 "Net-(MOD1-Pad8)")
  (net 188 "Net-(L8-Pad2)")
  (net 189 +8V)
  (net 190 "Net-(J21-Pad2)")
  (net 191 "Net-(J22-Pad1)")
  (net 192 "Net-(J23-Pad1)")
  (net 193 "Net-(J24-Pad1)")
  (net 194 "Net-(J25-Pad1)")
  (net 195 uC_PWR)
  (net 196 "Net-(U2-Pad29)")
  (net 197 uC_3V3_OUT_1)
  (net 198 Sensor_VCC)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +8V)
    (add_net "/433 MHz Transmitter/GPIO0")
    (add_net "/433 MHz Transmitter/GPIO2")
    (add_net "/433 MHz Transmitter/GPIO3")
    (add_net "/433 MHz Transmitter/LNA_N")
    (add_net "/433 MHz Transmitter/LNA_P")
    (add_net "/433 MHz Transmitter/TRX_SW")
    (add_net /Sensors/MPU_ADR_SEL)
    (add_net /Sensors/MPU_VIO)
    (add_net /Sensors/MPU_XCL)
    (add_net /Sensors/MPU_XDA)
    (add_net /xbee_breakout/ASSOC_DIO5)
    (add_net /xbee_breakout/CTS_DIO7)
    (add_net /xbee_breakout/DIO0)
    (add_net /xbee_breakout/DIO1)
    (add_net /xbee_breakout/DIO2)
    (add_net /xbee_breakout/DIO3)
    (add_net /xbee_breakout/DIO4)
    (add_net /xbee_breakout/DO8)
    (add_net /xbee_breakout/DTR_SLEEP)
    (add_net /xbee_breakout/ON_SLEEP)
    (add_net /xbee_breakout/PWM1)
    (add_net /xbee_breakout/RTS_DIO6)
    (add_net /xbee_breakout/VREF)
    (add_net /xbee_breakout/XBEE_DIN)
    (add_net /xbee_breakout/XBEE_DOUT)
    (add_net 433_VCC)
    (add_net 433_VCC_IN)
    (add_net A21_DAC0)
    (add_net A22_DAC1)
    (add_net ACCEL_VCC)
    (add_net AGND)
    (add_net BNO_VCC)
    (add_net FT231X_VBUS)
    (add_net FT231X_VCC)
    (add_net FT231_3V3OUT)
    (add_net FT231_D+)
    (add_net FT231_D-)
    (add_net FT_RX)
    (add_net FT_TX)
    (add_net GPS_VCC)
    (add_net MPU_VCC)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C36-Pad2)")
    (add_net "Net-(C37-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C45-Pad2)")
    (add_net "Net-(C46-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(J15-Pad2)")
    (add_net "Net-(J16-Pad2)")
    (add_net "Net-(J17-Pad2)")
    (add_net "Net-(J21-Pad2)")
    (add_net "Net-(J22-Pad1)")
    (add_net "Net-(J23-Pad1)")
    (add_net "Net-(J24-Pad1)")
    (add_net "Net-(J25-Pad1)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(L8-Pad2)")
    (add_net "Net-(MOD1-Pad8)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U11-Pad1)")
    (add_net "Net-(U11-Pad10)")
    (add_net "Net-(U11-Pad2)")
    (add_net "Net-(U11-Pad3)")
    (add_net "Net-(U11-Pad4)")
    (add_net "Net-(U11-Pad6)")
    (add_net "Net-(U13-Pad32)")
    (add_net "Net-(U14-Pad12)")
    (add_net "Net-(U14-Pad19)")
    (add_net "Net-(U14-Pad21)")
    (add_net "Net-(U14-Pad22)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad51)")
    (add_net "Net-(U2-Pad54)")
    (add_net "Net-(U2-Pad55)")
    (add_net "Net-(U2-Pad56)")
    (add_net "Net-(U2-Pad57)")
    (add_net "Net-(U2-Pad58)")
    (add_net "Net-(U2-Pad59)")
    (add_net "Net-(U2-Pad60)")
    (add_net "Net-(U2-Pad63)")
    (add_net "Net-(U2-Pad64)")
    (add_net "Net-(U2-Pad65)")
    (add_net "Net-(U2-Pad66)")
    (add_net "Net-(U2-Pad67)")
    (add_net "Net-(U2-Pad68)")
    (add_net "Net-(U2-Pad69)")
    (add_net "Net-(U2-Pad70)")
    (add_net "Net-(U2-Pad71)")
    (add_net "Net-(U2-Pad72)")
    (add_net "Net-(U2-Pad73)")
    (add_net "Net-(U2-Pad75)")
    (add_net "Net-(U2-Pad76)")
    (add_net "Net-(U2-Pad77)")
    (add_net "Net-(U2-Pad78)")
    (add_net "Net-(U2-Pad79)")
    (add_net "Net-(U2-Pad80)")
    (add_net "Net-(U2-Pad81)")
    (add_net "Net-(U2-Pad82)")
    (add_net "Net-(U2-Pad83)")
    (add_net "Net-(U2-Pad84)")
    (add_net "Net-(U2-Pad85)")
    (add_net "Net-(U2-Pad86)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad18)")
    (add_net "Net-(U5-Pad19)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U5-Pad9)")
    (add_net "Net-(U7-Pad13)")
    (add_net "Net-(U7-Pad14)")
    (add_net "Net-(U7-Pad16)")
    (add_net "Net-(U7-Pad17)")
    (add_net "Net-(U7-Pad18)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U8-Pad8)")
    (add_net PRESSURE_VCC)
    (add_net Sensor_VCC)
    (add_net XBEE_3V3)
    (add_net XBEE_VCC)
    (add_net accel_self_test)
    (add_net uC_11_MOSI0)
    (add_net uC_12_MISO0)
    (add_net "uC_13-SCK0(LED)")
    (add_net uC_15-A1-CS0)
    (add_net uC_16-A2-SCL0)
    (add_net uC_17-A3-SDA0)
    (add_net uC_21-A6-CS0-MOSI1-rx1)
    (add_net uC_24_DIO)
    (add_net uC_26_tx1)
    (add_net uC_27_rx1-sck0)
    (add_net uC_29_CAN0TX)
    (add_net uC_2_pwm)
    (add_net uC_30_CAN0RX)
    (add_net uC_33-A14-CAN1TX-SCL0-TX5)
    (add_net uC_34-A15-CAN1RX-SDA0-RX5)
    (add_net uC_37-A18-SCL1)
    (add_net uC_38-A19-SDA1)
    (add_net uC_3V3_OUT)
    (add_net uC_3V3_OUT_1)
    (add_net uC_3_pwm-SCL2)
    (add_net uC_433_reset)
    (add_net uC_4_pwm-SDA2)
    (add_net uC_5Vin)
    (add_net uC_5_pwm)
    (add_net uC_6_pwm)
    (add_net uC_CS_433_trans)
    (add_net uC_IMU_RX)
    (add_net uC_IMU_TX)
    (add_net uC_MISO_433_trans)
    (add_net uC_MOSI_433_trans)
    (add_net uC_PWR)
    (add_net uC_RX3)
    (add_net uC_SCL)
    (add_net uC_SDA)
    (add_net uC_SPI_SCK_433_trans)
    (add_net uC_TX3)
    (add_net uC_accel_x)
    (add_net uC_accel_y)
    (add_net uC_accel_z)
    (add_net uC_gps_RX)
    (add_net uC_gps_TX)
    (add_net uC_xbee_RX)
    (add_net uC_xbee_TX)
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.762)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module LOGO (layer B.Cu) (tedit 0)
    (at 116.84 120.904 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LOGO (layer B.Cu) (tedit 0)
    (at 141.732 150.368 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 140.716 86.36)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 94.996 98.044)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 89.662 130.81)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module LOGO (layer B.Cu) (tedit 0)
    (at 119.888 147.066 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LOGO (layer B.Cu) (tedit 0)
    (at 143.51 86.36 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module digikey-footprints:XBEE_PRO-20_THT (layer B.Cu) (tedit 59947AD9)
    (at 89.408 144.78 180)
    (fp_text reference MOD1 (at 0 18.49 180) (layer B.SilkS))
    (fp_text value XBP9B-DMWT-002 (at 0 13.97 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 20 thru_hole circle (at 11 9 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 94 /xbee_breakout/DIO0))
    (pad 19 thru_hole circle (at 11 7 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 95 /xbee_breakout/DIO1))
    (pad 18 thru_hole circle (at 11 5 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 96 /xbee_breakout/DIO2))
    (pad 17 thru_hole circle (at 11 3 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 97 /xbee_breakout/DIO3))
    (pad 16 thru_hole circle (at 11 1 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 98 /xbee_breakout/RTS_DIO6))
    (pad 15 thru_hole circle (at 11 -1 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 99 /xbee_breakout/ASSOC_DIO5))
    (pad 14 thru_hole circle (at 11 -3 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 100 /xbee_breakout/VREF))
    (pad 13 thru_hole circle (at 11 -5 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 101 /xbee_breakout/ON_SLEEP))
    (pad 12 thru_hole circle (at 11 -7 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 102 /xbee_breakout/CTS_DIO7))
    (pad 11 thru_hole circle (at 11 -9 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 103 /xbee_breakout/DIO4))
    (pad 10 thru_hole circle (at -11 -9 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 9 thru_hole circle (at -11 -7 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 93 /xbee_breakout/DTR_SLEEP))
    (pad 8 thru_hole circle (at -11 -5 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 187 "Net-(MOD1-Pad8)"))
    (pad 7 thru_hole circle (at -11 -3 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 91 /xbee_breakout/PWM1))
    (pad 6 thru_hole circle (at -11 -1 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 61 uC_6_pwm))
    (pad 5 thru_hole circle (at -11 1 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 uC_5_pwm))
    (pad 4 thru_hole circle (at -11 3 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 90 /xbee_breakout/DO8))
    (pad 3 thru_hole circle (at -11 5 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 89 /xbee_breakout/XBEE_DIN))
    (pad 2 thru_hole circle (at -11 7 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 88 /xbee_breakout/XBEE_DOUT))
    (pad 1 thru_hole circle (at -11 9 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 XBEE_VCC))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 128.016 67.564 270)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Teensy_RHS (at -2.667 53.848) (layer F.Fab))
    (fp_text user %R (at 0 29.21) (layer F.Fab))
    (pad 24 thru_hole oval (at 0 58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 195 uC_PWR))
    (pad 23 thru_hole oval (at 0 55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 22 thru_hole oval (at 0 53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 uC_3V3_OUT))
    (pad 21 thru_hole oval (at 0 50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 uC_accel_z))
    (pad 20 thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 uC_accel_y))
    (pad 19 thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 uC_21-A6-CS0-MOSI1-rx1))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 uC_accel_x))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 uC_SCL))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 uC_SDA))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 uC_17-A3-SDA0))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 uC_16-A2-SCL0))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 uC_15-A1-CS0))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 uC_SPI_SCK_433_trans))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "uC_13-SCK0(LED)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 A22_DAC1))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 A21_DAC0))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 uC_MISO_433_trans))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 uC_38-A19-SDA1))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 uC_37-A18-SCL1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 uC_433_reset))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 accel_self_test))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 uC_34-A15-CAN1RX-SDA0-RX5))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 uC_33-A14-CAN1TX-SCL0-TX5))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 136.652 157.988 180)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J11 (at 3.81 3.302 180) (layer F.SilkS))
    (fp_text value PRESSURE_SW (at 1.75 5.66 180) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 31 PRESSURE_VCC))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 198 Sensor_VCC))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 103.632 136.652 180)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J5 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value XBEE_LHS (at 1.905 -25.4 180) (layer B.Fab))
    (fp_text user %R (at 0 -11.43 90) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 /xbee_breakout/DTR_SLEEP))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(J5-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 /xbee_breakout/PWM1))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 uC_6_pwm))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 uC_5_pwm))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 /xbee_breakout/DO8))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /xbee_breakout/XBEE_DIN))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 /xbee_breakout/XBEE_DOUT))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 XBEE_VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294E91)
    (at 76.962 58.166)
    (descr "Terminal Block 4Ucon ItemNo. 20193, 3 pins, pitch 3.5mm, size 11.2x7mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.4uconnector.com/online/object/4udrawing/20193.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 20193 pitch 3.5mm size 11.2x7mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J15 (at 3.5 2.794) (layer F.SilkS))
    (fp_text value GPS_RX_JUMPER (at 3.5 4.66) (layer F.Fab))
    (fp_text user %R (at 3.5 2.9) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 110 FT_TX))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 111 "Net-(J15-Pad2)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 57 uC_gps_TX))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-3_TabPin2 (layer F.Cu) (tedit 5A70FB8C)
    (at 124.46 153.458 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U10 (at -5.376 -4.572 270) (layer F.SilkS))
    (fp_text value Sensor_3V3_Supply (at 0 6.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 198 Sensor_VCC))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 189 +8V))
    (pad 2 smd rect (at -5.775 0 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 198 Sensor_VCC))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 127.617792 101.80689 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C47 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 36 /Sensors/MPU_VIO))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Antenna:Patch_Antenna_18mmx18mm (layer F.Cu) (tedit 5BE538AF)
    (at 92.907574 114.901566)
    (fp_text reference A1 (at 0 8) (layer F.SilkS))
    (fp_text value ANTENNA (at 0 10) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 102.607 64.516 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.778 270) (layer B.SilkS))
    (fp_text value 4700pF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 195 uC_PWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 96.257 139.446 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 4700pF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 XBEE_VCC))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 148.59 63.763 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 2.295 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 FT231_3V3OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 152.409 65.278)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 2.785 0.042766) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 152.4 63.246)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -0.254 -1.524) (layer F.SilkS))
    (fp_text value 47pF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 76.209 104.14 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value 4700pF (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 136.398 114.309 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at -3.166 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 uC_accel_x))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 138.43 114.291 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at -3.166 -0.127 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 uC_accel_y))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 140.97 110.481 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 3.039 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 uC_accel_z))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 122.927 140.716 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 4700pF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 198 Sensor_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 104.521 127.762 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C17 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 104.276 132.207 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C18 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 114.808 125.476 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C19 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1.5nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 "Net-(C19-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 124.206 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C20 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.746 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C21 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5C13F464)
    (at 117.094 125.467 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C22 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.286 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C24 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 114.037 129.032 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C25 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 119.126 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C26 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 114.046 131.318 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C27 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 24 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 116.586 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C28 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.737 131.826)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C31 (at 3.311 -0.254) (layer F.SilkS))
    (fp_text value 220nF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 27 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 114.046 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C32 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 131.826 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C33 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 134.366 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C34 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 121.666 136.643 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C35 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 136.398 65.795 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C40 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4700pF (at 0.39 1.905 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 FT231X_VCC))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 142.875 110.481 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C41 (at -3.293 0.127 270) (layer F.SilkS))
    (fp_text value 4700pF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 30 ACCEL_VCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.677 151.384 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C42 (at 2.531 -0.127 270) (layer F.SilkS))
    (fp_text value 4700pF (at 0.88 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 PRESSURE_VCC))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 147.066 108.957 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C43 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 4700pF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 32 BNO_VCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 152.146 86.623 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C44 (at -0.263 1.778 270) (layer F.SilkS))
    (fp_text value 4700pF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 MPU_VCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 121.285 94.624 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C45 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 2.2nF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 "Net-(C45-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 127.617792 98.63189 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C46 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 35 "Net-(C46-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 124.596 56.134 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value Yellow (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 FT231_3V3OUT))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 124.705 60.706 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value Red (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 FT231_3V3OUT))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 38 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 112.903 116.958 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 433_Heartbeat (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C9)
    (at 87.582574 107.916566)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D4 (at 0 1.65) (layer B.SilkS))
    (fp_text value GPS_Heartbeat (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 40 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 131.563 104.902)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D5 (at 0 -1.65) (layer F.SilkS))
    (fp_text value IMU_heartbeat (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 41 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 137.151 130.556)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D6 (at 0 -1.65) (layer F.SilkS))
    (fp_text value MS0_heartbeat (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 42 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 132.724 109.601)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D7 (at 0 -1.65) (layer F.SilkS))
    (fp_text value ACCEL_heartbeat (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 43 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C9)
    (at 65.532 150.368 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D8 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value XBEE_HEARTBEAT (at 3.057 0 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 44 "Net-(D8-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 70.104 89.916 90)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Teensy_LHS (at -2.413 23.368 180) (layer F.Fab))
    (fp_text user %R (at 0 29.21 180) (layer F.Fab))
    (pad 24 thru_hole oval (at 0 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 uC_IMU_TX))
    (pad 23 thru_hole oval (at 0 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 uC_IMU_RX))
    (pad 22 thru_hole oval (at 0 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 uC_30_CAN0RX))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 uC_29_CAN0TX))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 uC_MOSI_433_trans))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 uC_27_rx1-sck0))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 uC_26_tx1))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 uC_CS_433_trans))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 uC_24_DIO))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 197 uC_3V3_OUT_1))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 uC_12_MISO0))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 uC_11_MOSI0))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 uC_gps_TX))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 uC_gps_RX))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 uC_TX3))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 uC_RX3))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 uC_6_pwm))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 uC_5_pwm))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 uC_4_pwm-SDA2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 uC_3_pwm-SCL2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 uC_2_pwm))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 uC_xbee_TX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 uC_xbee_RX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Wuerth_629105150521_CircularHoles (layer F.Cu) (tedit 5A142044)
    (at 145.796 57.404 180)
    (descr "USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf")
    (tags "usb micro receptacle")
    (attr smd)
    (fp_text reference J3 (at 0.254 0.254 180) (layer F.SilkS))
    (fp_text value FT231X_USB (at 0.254 3.048 180) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.75 180) (layer Dwgs.User))
    (fp_text user %R (at 0 1.05 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.5 -0.8 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.5 -0.8 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 3.875 1.95 180) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 6 thru_hole circle (at -3.875 1.95 180) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 6 thru_hole circle (at 3.725 -1.85 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 6 thru_hole circle (at -3.725 -1.85 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 5 smd rect (at 1.3 -1.9 180) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (pad 4 smd rect (at 0.65 -1.9 180) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(J3-Pad4)"))
    (pad 3 smd rect (at 0 -1.9 180) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -0.65 -1.9 180) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -1.3 -1.9 180) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 86 FT231X_VBUS))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Wuerth_629105150521_CircularHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 74.676 159.512)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J6 (at 0.254 -25.654) (layer B.SilkS))
    (fp_text value XBEE_RHS (at 3.175 3.175 90) (layer B.Fab))
    (fp_text user %R (at 0 -11.43 -90) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 /xbee_breakout/DIO0))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 /xbee_breakout/DIO1))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 /xbee_breakout/DIO2))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 /xbee_breakout/DIO3))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /xbee_breakout/RTS_DIO6))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 /xbee_breakout/ASSOC_DIO5))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /xbee_breakout/VREF))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 /xbee_breakout/ON_SLEEP))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 /xbee_breakout/CTS_DIO7))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 /xbee_breakout/DIO4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 126.746 105.918 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J13 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value DEBUG_BREAKOUT_433 (at 2.794 8.89) (layer F.Fab))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "/433 MHz Transmitter/GPIO3"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "/433 MHz Transmitter/GPIO2"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "/433 MHz Transmitter/GPIO0"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 uC_CS_433_trans))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 uC_MISO_433_trans))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 uC_MOSI_433_trans))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 uC_SPI_SCK_433_trans))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 uC_433_reset))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 160.02 82.296 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J20 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value MPU_BREAKOUT (at 2.286 7.62 270) (layer F.Fab))
    (fp_text user %R (at 0 6.35 270) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 /Sensors/MPU_ADR_SEL))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 uC_SDA))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 uC_SCL))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 /Sensors/MPU_XDA))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 /Sensors/MPU_XCL))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /Sensors/MPU_VIO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5C13F45D)
    (at 123.952 127.508)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L5 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 56nH (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(C36-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C23-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 151.765 68.589 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0.263 1.651 90) (layer F.SilkS))
    (fp_text value 27 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 118 FT231_D+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 149.86 68.589 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -0.263 1.524 270) (layer F.SilkS))
    (fp_text value 27 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 119 FT231_D-))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 128.66 60.706)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 120 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 38 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 128.651 56.134)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 121 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 78.74 110.989 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 3k3 (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 122 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 145.406 139.827)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 83 uC_SCL))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 PRESSURE_VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 141.596 139.827)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 PRESSURE_VCC))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 82 uC_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 82.55 106.925 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0.009 -1.524 270) (layer B.SilkS))
    (fp_text value 20 (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 124 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 112 "Net-(J16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 80.264 106.891566 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.524 90) (layer B.SilkS))
    (fp_text value 20 (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 111 "Net-(J15-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 125 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 112.903 112.658 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 72 uC_37-A18-SCL1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 91.882574 107.916566 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 40 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 73 uC_38-A19-SDA1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 135.627 104.902 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 41 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 75 A21_DAC0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 141.233 130.556 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 42 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 76 A22_DAC1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.024 109.601 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 43 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 79 uC_15-A1-CS0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 70.113 149.86)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at 0 1.65) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 99 /xbee_breakout/ASSOC_DIO5))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 44 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 118.745 94.479 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 2.531 -0.127 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 MPU_VCC))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 83 uC_SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 116.332 94.479 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 MPU_VCC))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 82 uC_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module teensy:Teensy35_36 (layer F.Cu) (tedit 58E3CF68)
    (at 99.06 78.74)
    (fp_text reference U2 (at 0 -10.16) (layer F.SilkS))
    (fp_text value Teensy3.6 (at 1.016 0.127) (layer F.Fab))
    (pad 62 thru_hole circle (at -12.7 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 61 thru_hole circle (at -15.24 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 60 thru_hole circle (at -17.78 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 159 "Net-(U2-Pad60)"))
    (pad 59 thru_hole circle (at -20.32 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 158 "Net-(U2-Pad59)"))
    (pad 58 thru_hole circle (at -22.86 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 157 "Net-(U2-Pad58)"))
    (pad 86 thru_hole circle (at -13.97 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 156 "Net-(U2-Pad86)"))
    (pad 85 thru_hole circle (at -11.43 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 155 "Net-(U2-Pad85)"))
    (pad 84 thru_hole circle (at -8.89 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 154 "Net-(U2-Pad84)"))
    (pad 83 thru_hole circle (at -6.35 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 153 "Net-(U2-Pad83)"))
    (pad 82 thru_hole circle (at 8.89 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 152 "Net-(U2-Pad82)"))
    (pad 81 thru_hole circle (at 11.43 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 151 "Net-(U2-Pad81)"))
    (pad 80 thru_hole circle (at 13.97 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 150 "Net-(U2-Pad80)"))
    (pad 79 thru_hole circle (at 19.05 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 149 "Net-(U2-Pad79)"))
    (pad 78 thru_hole circle (at 21.59 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 148 "Net-(U2-Pad78)"))
    (pad 77 thru_hole circle (at 24.13 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 147 "Net-(U2-Pad77)"))
    (pad 76 thru_hole circle (at 26.67 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 146 "Net-(U2-Pad76)"))
    (pad 75 thru_hole circle (at 29.21 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 145 "Net-(U2-Pad75)"))
    (pad 74 thru_hole circle (at 29.21 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 73 thru_hole circle (at 26.67 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 144 "Net-(U2-Pad73)"))
    (pad 72 thru_hole circle (at 24.13 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 143 "Net-(U2-Pad72)"))
    (pad 71 thru_hole circle (at 21.59 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 142 "Net-(U2-Pad71)"))
    (pad 70 thru_hole circle (at 19.05 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 141 "Net-(U2-Pad70)"))
    (pad 69 thru_hole circle (at 13.97 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 140 "Net-(U2-Pad69)"))
    (pad 68 thru_hole circle (at 11.43 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 139 "Net-(U2-Pad68)"))
    (pad 67 thru_hole circle (at 8.89 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 138 "Net-(U2-Pad67)"))
    (pad 66 thru_hole circle (at -6.35 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 137 "Net-(U2-Pad66)"))
    (pad 65 thru_hole circle (at -8.89 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 136 "Net-(U2-Pad65)"))
    (pad 64 thru_hole circle (at -11.43 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 135 "Net-(U2-Pad64)"))
    (pad 63 thru_hole circle (at -13.97 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 134 "Net-(U2-Pad63)"))
    (pad 57 thru_hole circle (at -16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 133 "Net-(U2-Pad57)"))
    (pad 56 thru_hole circle (at -19.05 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 132 "Net-(U2-Pad56)"))
    (pad 55 thru_hole circle (at -21.59 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 131 "Net-(U2-Pad55)"))
    (pad 54 thru_hole circle (at -26.67 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 130 "Net-(U2-Pad54)"))
    (pad 53 thru_hole circle (at -29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 195 uC_PWR))
    (pad 52 thru_hole circle (at -26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 51 thru_hole circle (at -24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 129 "Net-(U2-Pad51)"))
    (pad 50 thru_hole circle (at -21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 uC_accel_z))
    (pad 49 thru_hole circle (at -19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 uC_accel_y))
    (pad 48 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 84 uC_21-A6-CS0-MOSI1-rx1))
    (pad 47 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 uC_accel_x))
    (pad 46 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 83 uC_SCL))
    (pad 45 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 82 uC_SDA))
    (pad 44 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 81 uC_17-A3-SDA0))
    (pad 43 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 80 uC_16-A2-SCL0))
    (pad 42 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 79 uC_15-A1-CS0))
    (pad 41 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 uC_SPI_SCK_433_trans))
    (pad 40 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "uC_13-SCK0(LED)"))
    (pad 39 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 38 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 A22_DAC1))
    (pad 1 thru_hole rect (at -29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 2 thru_hole circle (at -26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 uC_xbee_RX))
    (pad 3 thru_hole circle (at -24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 uC_xbee_TX))
    (pad 4 thru_hole circle (at -21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 uC_2_pwm))
    (pad 5 thru_hole circle (at -19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 uC_3_pwm-SCL2))
    (pad 6 thru_hole circle (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 uC_4_pwm-SDA2))
    (pad 7 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 uC_5_pwm))
    (pad 8 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 uC_6_pwm))
    (pad 9 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 uC_RX3))
    (pad 10 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 uC_TX3))
    (pad 11 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 uC_gps_RX))
    (pad 12 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 uC_gps_TX))
    (pad 13 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 uC_11_MOSI0))
    (pad 37 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 A21_DAC0))
    (pad 36 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 uC_MISO_433_trans))
    (pad 35 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 uC_38-A19-SDA1))
    (pad 34 thru_hole circle (at 19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 uC_37-A18-SCL1))
    (pad 33 thru_hole circle (at 21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 uC_433_reset))
    (pad 32 thru_hole circle (at 24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 accel_self_test))
    (pad 31 thru_hole circle (at 26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 uC_34-A15-CAN1RX-SDA0-RX5))
    (pad 30 thru_hole circle (at 29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 uC_33-A14-CAN1TX-SCL0-TX5))
    (pad 29 thru_hole circle (at 16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 196 "Net-(U2-Pad29)"))
    (pad 28 thru_hole circle (at 16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 128 "Net-(U2-Pad28)"))
    (pad 27 thru_hole circle (at 16.51 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 26 thru_hole circle (at 16.51 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 127 "Net-(U2-Pad26)"))
    (pad 25 thru_hole circle (at 16.51 5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 126 "Net-(U2-Pad25)"))
    (pad 24 thru_hole circle (at 29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 uC_IMU_TX))
    (pad 23 thru_hole circle (at 26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 uC_IMU_RX))
    (pad 22 thru_hole circle (at 24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 uC_30_CAN0RX))
    (pad 21 thru_hole circle (at 21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 uC_29_CAN0TX))
    (pad 14 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 uC_12_MISO0))
    (pad 15 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 197 uC_3V3_OUT_1))
    (pad 16 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 uC_24_DIO))
    (pad 20 thru_hole circle (at 19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 uC_MOSI_433_trans))
    (pad 19 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 uC_27_rx1-sck0))
    (pad 18 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 uC_26_tx1))
    (pad 17 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 uC_CS_433_trans))
  )
  (module Package_SO:SSOP-20_3.9x8.7mm_P0.635mm (layer F.Cu) (tedit 5A4A2523)
    (at 144.018 66.548)
    (descr "SSOP20: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT231X.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U5 (at 0 -0.254) (layer F.SilkS))
    (fp_text value FT231XS (at 0 5.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 2.6 -2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 110 FT_TX))
    (pad 19 smd rect (at 2.6 -2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U5-Pad19)"))
    (pad 18 smd rect (at 2.6 -1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U5-Pad18)"))
    (pad 17 smd rect (at 2.6 -0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R3-Pad2)"))
    (pad 16 smd rect (at 2.6 -0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (pad 15 smd rect (at 2.6 0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 FT231X_VCC))
    (pad 14 smd rect (at 2.6 0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 FT231_3V3OUT))
    (pad 13 smd rect (at 2.6 1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 FT231_3V3OUT))
    (pad 12 smd rect (at 2.6 2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 119 FT231_D-))
    (pad 11 smd rect (at 2.6 2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 118 FT231_D+))
    (pad 10 smd rect (at -2.6 2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R4-Pad2)"))
    (pad 9 smd rect (at -2.6 2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U5-Pad9)"))
    (pad 8 smd rect (at -2.6 1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(U5-Pad8)"))
    (pad 7 smd rect (at -2.6 0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U5-Pad7)"))
    (pad 6 smd rect (at -2.6 0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (pad 5 smd rect (at -2.6 -0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U5-Pad5)"))
    (pad 4 smd rect (at -2.6 -0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 113 FT_RX))
    (pad 3 smd rect (at -2.6 -1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 FT231_3V3OUT))
    (pad 2 smd rect (at -2.6 -2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(U5-Pad2)"))
    (pad 1 smd rect (at -2.6 -2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(U5-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-20_3.9x8.7mm_P0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module _sensors:MAX-M8 (layer B.Cu) (tedit 55AD70C4)
    (at 85.922574 122.521566)
    (fp_text reference U7 (at 0.05 -5.35) (layer B.SilkS))
    (fp_text value MAX-M8 (at -0.05 -0.35) (layer B.Fab))
    (pad 18 smd rect (at 4.8 0) (size 1.8 0.7) (layers B.Cu B.Paste B.Mask)
      (net 174 "Net-(U7-Pad18)"))
    (pad 17 smd rect (at 4.8 -1.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 173 "Net-(U7-Pad17)"))
    (pad 16 smd rect (at 4.8 -2.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 172 "Net-(U7-Pad16)"))
    (pad 15 smd rect (at 4.8 -3.3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 AGND))
    (pad 14 smd rect (at 4.8 -4.4) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 171 "Net-(U7-Pad14)"))
    (pad 13 smd rect (at 4.8 -5.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 170 "Net-(U7-Pad13)"))
    (pad 12 smd rect (at 4.8 -6.6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 AGND))
    (pad 11 smd rect (at 4.8 -7.7) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 10 smd rect (at 4.8 -8.8) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 AGND))
    (pad 9 smd rect (at -4.8 -8.8) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(R5-Pad2)"))
    (pad 8 smd rect (at -4.8 -7.7) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 7 smd rect (at -4.8 -6.6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 6 smd rect (at -4.8 -5.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 5 smd rect (at -4.8 -4.4) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 169 "Net-(U7-Pad5)"))
    (pad 4 smd rect (at -4.8 -3.3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 168 "Net-(U7-Pad4)"))
    (pad 3 smd rect (at -4.8 -2.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 125 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at -4.8 -1.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 124 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -4.8 0) (size 1.8 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 AGND))
    (model Sensors/ublox-gps-max-m8.wrl
      (offset (xyz 0.1269999980926514 -4.457699933052063 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS580314BA01-00:XDCR_MS580314BA01-00 (layer F.Cu) (tedit 0)
    (at 140.716 145.796)
    (attr smd)
    (fp_text reference U8 (at -1.37578 -4.41083) (layer F.SilkS))
    (fp_text value MS580314BA01-00 (at 0.127 3.429) (layer F.SilkS))
    (pad 1 smd rect (at 2.67528 1.89883) (size 2.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 uC_SCL))
    (pad 2 smd rect (at 2.67528 0.648831) (size 2.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (pad 3 smd rect (at 2.40028 -0.651169) (size 2.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(J17-Pad2)"))
    (pad 4 smd rect (at 2.67528 -1.90117) (size 2.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -2.67473 1.89883) (size 2.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U8-Pad8)"))
    (pad 7 smd rect (at -2.67473 0.648831) (size 2.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 uC_SDA))
    (pad 6 smd rect (at -2.67473 -0.651169) (size 2.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 PRESSURE_VCC))
    (pad 5 smd rect (at -2.67473 -1.90117) (size 2.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 PRESSURE_VCC))
  )
  (module Sensor_Motion:ADXL377 (layer F.Cu) (tedit 5BE9B78B)
    (at 142.24 114.681)
    (fp_text reference U9 (at 0 2.5) (layer F.SilkS))
    (fp_text value ADXL377 (at 0 3.937) (layer F.Fab))
    (pad 17 smd rect (at 0 0) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd roundrect (at -0.8 -1.35) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 uC_accel_z))
    (pad 15 smd roundrect (at -0.25 -1.35) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 ACCEL_VCC))
    (pad 14 smd roundrect (at 0.25 -1.35) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 ACCEL_VCC))
    (pad 13 smd roundrect (at 0.8 -1.35 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 1.35 -0.8 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 1.35 -0.25 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 1.35 0.25 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 1.35 0.8 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at 0.8 1.35) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 0.25 1.35) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 AGND))
    (pad 6 smd roundrect (at -0.25 1.35) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 AGND))
    (pad 5 smd roundrect (at -0.8 1.35) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 uC_accel_x))
    (pad 4 smd roundrect (at -1.35 0.8 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 uC_accel_y))
    (pad 3 smd roundrect (at -1.35 0.3 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -1.35 -0.3 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 accel_self_test))
    (pad 1 smd roundrect (at -1.35 -0.8 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module CC1200RHBT:QFN50P500X500X100-33N (layer F.Cu) (tedit 0)
    (at 119.634 130.302 90)
    (attr smd)
    (fp_text reference U13 (at -0.254 3.556 90) (layer F.SilkS))
    (fp_text value CC1200RHBT (at -3.048 6.858 180) (layer F.SilkS))
    (pad EXP smd rect (at 0 0 90) (size 3.53 3.53) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (pad 32 smd rect (at -1.75 -2.3) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U13-Pad32)"))
    (pad 31 smd rect (at -1.25 -2.3) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C18-Pad1)"))
    (pad 30 smd rect (at -0.75 -2.3) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C17-Pad1)"))
    (pad 29 smd rect (at -0.25 -2.3) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C27-Pad1)"))
    (pad 28 smd rect (at 0.25 -2.3) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
    (pad 27 smd rect (at 0.75 -2.3) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
    (pad 26 smd rect (at 1.25 -2.3) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C25-Pad1)"))
    (pad 25 smd rect (at 1.75 -2.3) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
    (pad 24 smd rect (at 2.3 -1.75 270) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C19-Pad2)"))
    (pad 23 smd rect (at 2.3 -1.25 270) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C19-Pad1)"))
    (pad 22 smd rect (at 2.3 -0.75 270) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
    (pad 21 smd rect (at 2.3 -0.25 270) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C22-Pad1)"))
    (pad 20 smd rect (at 2.3 0.25 270) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "/433 MHz Transmitter/LNA_N"))
    (pad 19 smd rect (at 2.3 0.75 270) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "/433 MHz Transmitter/LNA_P"))
    (pad 18 smd rect (at 2.3 1.25 270) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "/433 MHz Transmitter/TRX_SW"))
    (pad 17 smd rect (at 2.3 1.75 270) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C23-Pad2)"))
    (pad 16 smd rect (at 1.75 2.3 180) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.25 2.3 180) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
    (pad 14 smd rect (at 0.75 2.3 180) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R8-Pad1)"))
    (pad 13 smd rect (at 0.25 2.3 180) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
    (pad 12 smd rect (at -0.25 2.3 180) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
    (pad 11 smd rect (at -0.75 2.3 180) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 uC_CS_433_trans))
    (pad 10 smd rect (at -1.25 2.3 180) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 106 "/433 MHz Transmitter/GPIO0"))
    (pad 9 smd rect (at -1.75 2.3 180) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 uC_MISO_433_trans))
    (pad 8 smd rect (at -2.3 1.75 90) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 uC_SPI_SCK_433_trans))
    (pad 7 smd rect (at -2.3 1.25 90) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 uC_MOSI_433_trans))
    (pad 6 smd rect (at -2.3 0.75 90) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C31-Pad1)"))
    (pad 5 smd rect (at -2.3 0.25 90) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
    (pad 4 smd rect (at -2.3 -0.25 90) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 "/433 MHz Transmitter/GPIO2"))
    (pad 3 smd rect (at -2.3 -0.75 90) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 108 "/433 MHz Transmitter/GPIO3"))
    (pad 2 smd rect (at -2.3 -1.25 90) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 uC_433_reset))
    (pad 1 smd rect (at -2.3 -1.75 90) (size 0.7 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 433_VCC))
  )
  (module MPU-6050:QFN50P400X400X95-24N (layer F.Cu) (tedit 0)
    (at 119.38 99.949)
    (attr smd)
    (fp_text reference U14 (at 3.302 -0.127 270) (layer F.SilkS))
    (fp_text value MPU-6050 (at 0 3.175) (layer F.SilkS))
    (pad 24 smd rect (at -1.25 -1.97 270) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 82 uC_SDA))
    (pad 23 smd rect (at -0.75 -1.97 270) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 83 uC_SCL))
    (pad 22 smd rect (at -0.25 -1.97 270) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(U14-Pad22)"))
    (pad 21 smd rect (at 0.25 -1.97 270) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U14-Pad21)"))
    (pad 20 smd rect (at 0.75 -1.97 270) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C45-Pad2)"))
    (pad 19 smd rect (at 1.25 -1.97 270) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U14-Pad19)"))
    (pad 18 smd rect (at 1.97 -1.25 180) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (pad 17 smd rect (at 1.97 -0.75 180) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 1.97 -0.25 180) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.97 0.25 180) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 1.97 0.75 180) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 1.97 1.25 180) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 33 MPU_VCC))
    (pad 12 smd rect (at 1.25 1.97 90) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U14-Pad12)"))
    (pad 11 smd rect (at 0.75 1.97 90) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (pad 10 smd rect (at 0.25 1.97 90) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C46-Pad2)"))
    (pad 9 smd rect (at -0.25 1.97 90) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 115 /Sensors/MPU_ADR_SEL))
    (pad 8 smd rect (at -0.75 1.97 90) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 36 /Sensors/MPU_VIO))
    (pad 7 smd rect (at -1.25 1.97 90) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 116 /Sensors/MPU_XCL))
    (pad 6 smd rect (at -1.97 1.25) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 117 /Sensors/MPU_XDA))
    (pad 5 smd rect (at -1.97 0.75) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.97 0.25) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.97 -0.25) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.97 -0.75) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.97 -1.25) (size 0.79 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
  )
  (module Crystal:Crystal_SMD_7050-2Pin_7.0x5.0mm_HandSoldering (layer F.Cu) (tedit 5A0FD1B2)
    (at 108.966 131.732 90)
    (descr "SMD Crystal SERIES SMD7050/4 https://www.foxonline.com/pdfs/FQ7050.pdf, hand-soldering, 7.0x5.0mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y2 (at 7.526 -0.254 180) (layer F.SilkS))
    (fp_text value 40MHz (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 3.65 0 90) (size 4.9 3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C17-Pad1)"))
    (pad 1 smd rect (at -3.65 0 90) (size 4.9 3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_7050-2Pin_7.0x5.0mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BNO:Adafruit_BNO055_breakout (layer B.Cu) (tedit 5BF5F70E)
    (at 138.684 119.634 270)
    (fp_text reference U11 (at 0 -1.225 270) (layer B.SilkS))
    (fp_text value Adafruit_BNO055_breakout (at -0.025 2.975 270) (layer B.Fab))
    (fp_text user PS0 (at -3.81 6.35 180) (layer B.SilkS))
    (fp_text user PS1 (at -1.27 6.35 180) (layer B.SilkS))
    (fp_text user INT (at 1.27 6.35 180) (layer B.SilkS))
    (fp_text user ADR (at 3.81 6.35 180) (layer B.SilkS))
    (fp_text user Vin (at -6.35 -6.35 180) (layer B.SilkS))
    (fp_text user 3vo (at -3.81 -6.35 180) (layer B.SilkS))
    (fp_text user GND (at -1.27 -6.35 180) (layer B.SilkS))
    (fp_text user SDA (at 1.27 -6.35 180) (layer B.SilkS))
    (fp_text user SCL (at 3.81 -6.35 180) (layer B.SilkS))
    (fp_text user RST (at 6.35 -6.35 180) (layer B.SilkS))
    (pad 3 thru_hole circle (at 1.27 8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 186 "Net-(U11-Pad3)"))
    (pad 2 thru_hole circle (at -1.27 8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 185 "Net-(U11-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 184 "Net-(U11-Pad1)"))
    (pad 4 thru_hole circle (at 3.81 8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 183 "Net-(U11-Pad4)"))
    (pad 7 thru_hole circle (at -1.27 -8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 8 thru_hole circle (at 1.27 -8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 uC_SDA))
    (pad 9 thru_hole circle (at 3.81 -8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 uC_SCL))
    (pad 10 thru_hole circle (at 6.35 -8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 182 "Net-(U11-Pad10)"))
    (pad 6 thru_hole circle (at -3.81 -8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 181 "Net-(U11-Pad6)"))
    (pad 5 thru_hole circle (at -6.35 -8.89 270) (size 2.016 2.016) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 BNO_VCC))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.492 127.508 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0.762 0.508 180) (layer F.SilkS))
    (fp_text value 18 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(C36-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.158 123.421 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 5.1pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C15-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "/433 MHz Transmitter/LNA_P"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.872 123.421 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 5.1pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 AGND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "/433 MHz Transmitter/LNA_N"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.952 126.238 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 39pF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C23-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.984 124.206 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value 2.2pF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C23-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.698 121.158 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 5.1pF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "/433 MHz Transmitter/TRX_SW"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.492 126.238 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 0.508 -0.254) (layer F.SilkS))
    (fp_text value 56pF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(C36-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.46 117.094)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C37 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 6.2pF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 AGND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(C37-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.286 126.238)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 AGND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.286 127.508)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at 2.54 0) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 AGND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 433_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.428 123.421 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 1.547 0 270) (layer F.SilkS))
    (fp_text value 27nH (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "/433 MHz Transmitter/LNA_P"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.158 121.158 180)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 15nH (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C15-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "/433 MHz Transmitter/TRX_SW"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.881 125.222 180)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 56nH (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "/433 MHz Transmitter/LNA_N"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "/433 MHz Transmitter/LNA_P"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.142 123.444 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L4 (at 0 -1.17 270) (layer F.SilkS))
    (fp_text value 27nH (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "/433 MHz Transmitter/LNA_N"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.46 124.206 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L6 (at -0.508 -0.762 90) (layer F.SilkS))
    (fp_text value 15nH (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C29-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.952 119.126 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L7 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 43nH (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(C37-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.389 117.094 180)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L8 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 22nH (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 188 "Net-(L8-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(C37-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.737 129.54)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 2.803 0) (layer F.SilkS))
    (fp_text value 56k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 AGND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 123 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-3_TabPin2 (layer F.Cu) (tedit 5A70FB8C)
    (at 93.472 149.539 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U3 (at 0 -6.65 270) (layer F.SilkS))
    (fp_text value XBEE_3.3v_supply (at 0 6.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 104 XBEE_3V3))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 189 +8V))
    (pad 2 smd rect (at -5.775 0 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 104 XBEE_3V3))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-3_TabPin2 (layer B.Cu) (tedit 5A70FB8C)
    (at 101.162574 116.171566 90)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U6 (at 0 6.65 90) (layer B.SilkS))
    (fp_text value GPS_3V3_Supply (at 0 -6.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad "" smd rect (at 0.95 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad 2 smd rect (at 3.375 0 90) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 105 GPS_VCC))
    (pad 3 smd rect (at -5.775 -2.54 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 189 +8V))
    (pad 2 smd rect (at -5.775 0 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 105 GPS_VCC))
    (pad 1 smd rect (at -5.775 2.54 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-3_TabPin2 (layer F.Cu) (tedit 5A70FB8C)
    (at 111.741 153.482 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U12 (at -5.654 -4.337 270) (layer F.SilkS))
    (fp_text value 433_MHz_3V3 (at 0 6.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 109 433_VCC_IN))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 189 +8V))
    (pad 2 smd rect (at -5.775 0 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 109 433_VCC_IN))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-3_TabPin2 (layer B.Cu) (tedit 5A70FB8C)
    (at 114.554 98.298)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U1 (at 0 6.65) (layer B.SilkS))
    (fp_text value Teensy_5V (at 0 -6.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers B.Paste))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 85 uC_5Vin))
    (pad 3 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 189 +8V))
    (pad 2 smd rect (at -5.775 0) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 85 uC_5Vin))
    (pad 1 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:test_point_antenna (layer F.Cu) (tedit 5BFAD35B)
    (at 117.602 115.824)
    (fp_text reference TP1 (at 0 2.54) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(L8-Pad2)"))
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E80)
    (at 158.496 141.732 270)
    (descr "Terminal Block 4Ucon ItemNo. 10694, vertical (cable from top), 3 pins, pitch 3.5mm, size 11.5x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10694.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10694 vertical pitch 3.5mm size 11.5x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J21 (at 2.794 2.794 270) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 3.5 5.66 270) (layer F.Fab))
    (fp_text user %R (at 3.5 3.45 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 190 "Net-(J21-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 189 +8V))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 110.744 57.912)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J4 (at 1.778 3.048) (layer F.SilkS))
    (fp_text value TEENSY_SW (at 1.75 5.66) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 195 uC_PWR))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 85 uC_5Vin))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294E91)
    (at 90.17 58.166)
    (descr "Terminal Block 4Ucon ItemNo. 20193, 3 pins, pitch 3.5mm, size 11.2x7mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.4uconnector.com/online/object/4udrawing/20193.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 20193 pitch 3.5mm size 11.2x7mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J16 (at 3.048 2.794) (layer F.SilkS))
    (fp_text value GPS_TX_JUMPER (at 3.5 4.66) (layer F.Fab))
    (fp_text user %R (at 3.5 2.9) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 113 FT_RX))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 112 "Net-(J16-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 58 uC_gps_RX))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 68.58 58.42)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference J22 (at 0 -5.3) (layer F.SilkS))
    (fp_text value standoff_1 (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 191 "Net-(J22-Pad1)"))
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 68.58 156.972)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference J23 (at 0 -5.3) (layer F.SilkS))
    (fp_text value standoff_2 (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 192 "Net-(J23-Pad1)"))
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 157.48 58.928)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference J24 (at 0 -5.3) (layer F.SilkS))
    (fp_text value standoff_3 (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 193 "Net-(J24-Pad1)"))
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 157.48 156.972)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference J25 (at 0 -5.3) (layer F.SilkS))
    (fp_text value standoff_4 (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 194 "Net-(J25-Pad1)"))
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E80)
    (at 68.072 125.476 90)
    (descr "Terminal Block 4Ucon ItemNo. 10694, vertical (cable from top), 3 pins, pitch 3.5mm, size 11.5x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10694.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10694 vertical pitch 3.5mm size 11.5x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference JP1 (at 3.5 3.302 90) (layer F.SilkS))
    (fp_text value XBEE_RX_JUMPER (at 3.5 5.66 90) (layer F.Fab))
    (fp_text user %R (at 3.5 3.45 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 110 FT_TX))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 89 /xbee_breakout/XBEE_DIN))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 66 uC_xbee_TX))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E80)
    (at 68.072 112.268 90)
    (descr "Terminal Block 4Ucon ItemNo. 10694, vertical (cable from top), 3 pins, pitch 3.5mm, size 11.5x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10694.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10694 vertical pitch 3.5mm size 11.5x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference JP2 (at 4.064 3.048 90) (layer F.SilkS))
    (fp_text value XBEE_TX_JUMPER (at 3.5 5.66 90) (layer F.Fab))
    (fp_text user %R (at 3.5 3.45 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 113 FT_RX))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 88 /xbee_breakout/XBEE_DOUT))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 67 uC_xbee_RX))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 68.072 135.128 90)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J7 (at 1.75 3.302 90) (layer F.SilkS))
    (fp_text value XBEE_SW (at 1.75 5.66 90) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 104 XBEE_3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 XBEE_VCC))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 133.604 57.912)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J8 (at 1.778 3.556) (layer F.SilkS))
    (fp_text value FT231_SW (at 1.75 5.66) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 FT231X_VCC))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 86 FT231X_VBUS))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 68.072 99.06 90)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J9 (at 1.75 3.048 90) (layer F.SilkS))
    (fp_text value GPS_SW (at 1.75 5.66 90) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 105 GPS_VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 158.496 132.588 270)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J10 (at 1.75 5.334 270) (layer F.SilkS))
    (fp_text value ACCEL_SW (at 1.75 5.66 270) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 198 Sensor_VCC))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 ACCEL_VCC))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 158.496 96.52 270)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J12 (at 1.524 3.048 270) (layer F.SilkS))
    (fp_text value IMU_SW (at 1.75 5.66 270) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 32 BNO_VCC))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 198 Sensor_VCC))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 158.496 123.444 270)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J14 (at 1.778 3.556 90) (layer F.SilkS))
    (fp_text value CC1200_SW (at 1.75 5.66 270) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 433_VCC))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 109 433_VCC_IN))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E80)
    (at 158.496 105.156 270)
    (descr "Terminal Block 4Ucon ItemNo. 10694, vertical (cable from top), 3 pins, pitch 3.5mm, size 11.5x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10694.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10694 vertical pitch 3.5mm size 11.5x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J18 (at 3.81 2.794 270) (layer F.SilkS))
    (fp_text value ADDR_SEL_MPU (at 3.5 5.66 270) (layer F.Fab))
    (fp_text user %R (at 3.5 3.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 115 /Sensors/MPU_ADR_SEL))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 MPU_VCC))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E7F)
    (at 158.496 87.884 270)
    (descr "Terminal Block 4Ucon ItemNo. 10693, vertical (cable from top), 2 pins, pitch 3.5mm, size 8x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10693.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10693 vertical pitch 3.5mm size 8x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J19 (at 1.524 3.048 270) (layer F.SilkS))
    (fp_text value MPU_SW (at 1.75 5.66 270) (layer F.Fab))
    (fp_text user %R (at 1.75 3.45 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 198 Sensor_VCC))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 MPU_VCC))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Vertical (layer F.Cu) (tedit 5B294E80)
    (at 148.336 157.988 180)
    (descr "Terminal Block 4Ucon ItemNo. 10694, vertical (cable from top), 3 pins, pitch 3.5mm, size 11.5x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10694.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10694 vertical pitch 3.5mm size 11.5x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J17 (at 2.794 3.048 180) (layer F.SilkS))
    (fp_text value ADDR_SEL_PRESSURE (at 3.5 5.66 180) (layer F.Fab))
    (fp_text user %R (at 3.5 3.45 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 114 "Net-(J17-Pad2)"))
    (pad 3 thru_hole circle (at 7 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 31 PRESSURE_VCC))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GPS_LDO (at 101.346 106.426) (layer B.SilkS))
  (gr_text MPU_DEBUG (at 157.48 75.438 90) (layer F.SilkS))
  (gr_text MPU_SW (at 150.622 90.17) (layer F.SilkS))
  (gr_text BNO_SW (at 152.146 97.79 90) (layer F.SilkS))
  (gr_text GND (at 152.654 104.902 90) (layer F.SilkS))
  (gr_text VCC (at 152.654 112.014 90) (layer F.SilkS))
  (gr_text MPU_ADR_SEL (at 150.114 108.204 90) (layer F.SilkS))
  (gr_text 433_SW (at 157.48 119.38) (layer F.SilkS))
  (gr_text GND (at 151.384 149.352) (layer F.SilkS))
  (gr_text +8V (at 150.368 141.478) (layer F.SilkS))
  (gr_text DEBUG_433 (at 118.872 108.712) (layer F.SilkS))
  (gr_text uC_LDO (at 104.648 98.552 90) (layer B.SilkS))
  (gr_text 433_Antenna (at 120.142 112.776) (layer F.SilkS))
  (gr_text XBEE_SW (at 74.168 131.572 90) (layer F.SilkS))
  (gr_text uC (at 74.422 125.73 90) (layer F.SilkS))
  (gr_text FT (at 74.168 118.364 90) (layer F.SilkS))
  (gr_text XBEE_RX_SEL (at 76.962 121.92 90) (layer F.SilkS))
  (gr_text FT (at 74.168 112.776 90) (layer F.SilkS))
  (gr_text uC (at 73.914 104.648 90) (layer F.SilkS))
  (gr_text XBEE_TX_SEL (at 76.962 108.458 90) (layer F.SilkS))
  (gr_text GPS_SW (at 74.168 97.536 90) (layer F.SilkS))
  (gr_text FT (at 76.708 63.246) (layer F.SilkS))
  (gr_text uC (at 84.328 62.992) (layer F.SilkS))
  (gr_text GPS_RX_SEL (at 80.01 65.024) (layer F.SilkS))
  (gr_text FT (at 97.536 62.992) (layer F.SilkS))
  (gr_text uC (at 90.17 62.738) (layer F.SilkS))
  (gr_text GPS_TX_SEL (at 93.726 64.77) (layer F.SilkS))
  (gr_text uC_SW (at 117.856 58.166 90) (layer F.SilkS))
  (gr_text FT231_SW (at 135.382 63.246) (layer F.SilkS))
  (gr_text XBEE_UP (at 89.154 129.032) (layer B.SilkS))
  (gr_text XBEE_LDO (at 92.71 160.02) (layer F.SilkS))
  (gr_text Pressure (at 133.604 147.32 90) (layer F.SilkS))
  (gr_text 433_LDO (at 111.76 143.256) (layer F.SilkS))
  (gr_text Sensor_LDO (at 124.46 143.51) (layer F.SilkS))
  (gr_text GND (at 151.384 158.75 90) (layer F.SilkS))
  (gr_text Press_ADDR_SEL (at 144.78 151.638) (layer F.SilkS))
  (gr_text Batt_VCC (at 147.32 145.034 90) (layer F.SilkS))
  (gr_text Accel_SW (at 151.13 134.62 90) (layer F.SilkS))
  (gr_line (start 162.56 162.052) (end 162.56 53.848) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.754 162.052) (end 162.56 162.052) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.754 53.848) (end 63.754 162.052) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 53.848) (end 63.754 53.848) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name AGND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.56 53.848) (xy 63.754 53.848) (xy 63.754 162.052) (xy 162.56 162.052)
      )
    )
  )
  (zone (net 2) (net_name AGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.56 53.848) (xy 63.754 53.848) (xy 63.754 162.052) (xy 162.56 162.052)
      )
    )
  )
  (zone (net 189) (net_name +8V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.56 53.848) (xy 63.754 53.848) (xy 63.754 162.052) (xy 162.56 162.052)
      )
    )
  )
  (zone (net 2) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.56 53.848) (xy 63.754 53.848) (xy 63.754 162.052) (xy 162.56 162.052)
      )
    )
  )
)
