(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 25)
    (no_connects 0)
    (area 116.939287 79.886799 144.736534 120.810001)
    (thickness 1.6)
    (drawings 36)
    (tracks 35)
    (zones 0)
    (modules 11)
    (nets 22)
  )
  (page A4)
  (title_block
    (title "ZX Nuvo Kempston Fixer")
    (date 2017-06-14)
    (rev 0.2)
    (company fatla.eu)
    (comment 4 "Add-on board for Kepmston decoging fix")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6096)
    (via_drill 0.4064)
    (via_min_size 0.4064)
    (via_min_drill 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /A5RD)
  (net 2 /A6)
  (net 3 /A7)
  (net 4 "Net-(D3-Pad1)")
  (net 5 /D5)
  (net 6 /D6)
  (net 7 /D7)
  (net 8 /S0)
  (net 9 /D0)
  (net 10 /S1)
  (net 11 /D1)
  (net 12 /S2)
  (net 13 /D2)
  (net 14 GND)
  (net 15 VCC)
  (net 16 /~IORQ~)
  (net 17 /S4)
  (net 18 /D4)
  (net 19 /S3)
  (net 20 /D3)
  (net 21 /V)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.6096)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A5RD)
    (add_net /A6)
    (add_net /A7)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /S0)
    (add_net /S1)
    (add_net /S2)
    (add_net /S3)
    (add_net /S4)
    (add_net /V)
    (add_net /~IORQ~)
    (add_net "Net-(D3-Pad1)")
  )
  (net_class PWR ""
    (clearance 0.2032)
    (trace_width 0.4064)
    (via_dia 0.6096)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5940DDF8)
    (at 134.62 87.63)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U26 (at 2.54 0.635) (layer F.SilkS))
    (fp_text value 74HC366 (at 3.81 20.17) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /A5RD))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /D3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /S0))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /S3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /D4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /S1))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /S4))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /D1))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /S2))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /V))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /D2))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /~IORQ~))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5940E842)
    (at 132.08 87.63 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 -20.11 180) (layer B.Fab))
    (fp_text user %R (at 0 2.33 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A5RD))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /S0))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /S1))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D1))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /S2))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D2))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5940E849)
    (at 139.7 87.63 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 -20.11 180) (layer B.Fab))
    (fp_text user %R (at 0 2.33 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 VCC))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /~IORQ~))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /V))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /D5))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /S4))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D4))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /S3))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /D3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5940DE0D)
    (at 142.24 81.915)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value A_IN (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5940DE16)
    (at 128.905 111.125)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value D_OUT (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5940DCC4)
    (at 134.62 81.915)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference D1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 /A5RD))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 /A6))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5940DCC1)
    (at 134.62 84.455)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference D2 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 /A5RD))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 /A7))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5940DCB8)
    (at 137.16 108.585 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference D3 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 2.54 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 /D5))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5940DCB4)
    (at 137.16 111.125 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference D4 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 2.54 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 /D6))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5940DCB1)
    (at 137.16 113.665 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference D5 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 2.54 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /D7))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module "ZX Speccy:logo-speccypl" (layer B.Cu) (tedit 0)
    (at 137.16 96.52 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text v.0.2 (at 137.16 80.645) (layer B.Cu))
  (dimension 35.56 (width 0.3) (layer Dwgs.User)
    (gr_text "1.4000 in" (at 122.475 97.79 90) (layer Dwgs.User))
    (feature1 (pts (xy 127 80.01) (xy 121.125 80.01)))
    (feature2 (pts (xy 127 115.57) (xy 121.125 115.57)))
    (crossbar (pts (xy 123.825 115.57) (xy 123.825 80.01)))
    (arrow1a (pts (xy 123.825 80.01) (xy 124.411421 81.136504)))
    (arrow1b (pts (xy 123.825 80.01) (xy 123.238579 81.136504)))
    (arrow2a (pts (xy 123.825 115.57) (xy 124.411421 114.443496)))
    (arrow2b (pts (xy 123.825 115.57) (xy 123.238579 114.443496)))
  )
  (dimension 17.145 (width 0.3) (layer Dwgs.User)
    (gr_text "0.6750 in" (at 135.5725 119.46) (layer Dwgs.User))
    (feature1 (pts (xy 127 115.57) (xy 127 120.81)))
    (feature2 (pts (xy 144.145 115.57) (xy 144.145 120.81)))
    (crossbar (pts (xy 144.145 118.11) (xy 127 118.11)))
    (arrow1a (pts (xy 127 118.11) (xy 128.126504 117.523579)))
    (arrow1b (pts (xy 127 118.11) (xy 128.126504 118.696421)))
    (arrow2a (pts (xy 144.145 118.11) (xy 143.018496 117.523579)))
    (arrow2b (pts (xy 144.145 118.11) (xy 143.018496 118.696421)))
  )
  (gr_line (start 127 114.935) (end 127 109.855) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.795 115.57) (end 127.635 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 108.585) (end 130.175 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 109.22) (end 130.175 108.585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.635 109.22) (end 129.54 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 109.855) (end 127.635 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.065 107.315) (end 140.335 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 107.95) (end 139.065 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text fatla.eu (at 134.62 111.125 90) (layer B.SilkS))
  (gr_text "ZX Nuvo Kempston Fixer" (at 137.16 97.155 270) (layer F.SilkS))
  (gr_text A7 (at 140.335 83.185) (layer F.SilkS))
  (gr_text A6 (at 140.335 80.645) (layer F.SilkS))
  (gr_text D7 (at 130.81 113.665 270) (layer F.SilkS))
  (gr_line (start 140.335 107.315) (end 143.51 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 114.935) (end 127.635 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text D6 (at 130.81 111.125 270) (layer F.SilkS))
  (gr_line (start 144.145 80.645) (end 143.51 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.145 106.68) (end 144.145 80.645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 86.36) (end 130.175 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 85.725) (end 130.175 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.715 85.725) (end 130.81 85.725) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 85.09) (end 132.715 85.725) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 80.645) (end 133.35 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.985 80.01) (end 133.35 80.645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 80.01) (end 133.985 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 107.315) (end 144.145 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 114.935) (end 138.43 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.795 115.57) (end 138.43 114.935) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 14) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.145 80.645) (xy 144.145 106.68) (xy 143.51 107.315) (xy 139.065 107.315) (xy 138.43 107.95)
        (xy 138.43 114.935) (xy 137.795 115.57) (xy 127.635 115.57) (xy 127 114.935) (xy 127 109.855)
        (xy 127.635 109.22) (xy 129.54 109.22) (xy 130.175 108.585) (xy 130.175 86.36) (xy 130.81 85.725)
        (xy 132.715 85.725) (xy 133.35 85.09) (xy 133.35 80.645) (xy 133.985 80.01) (xy 143.51 80.01)
      )
    )
  )
)
