(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 98)
    (no_connects 0)
    (area 59.614999 62.154999 108.025001 110.565001)
    (thickness 1.6)
    (drawings 11)
    (tracks 250)
    (zones 0)
    (modules 49)
    (nets 60)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1.524)
    (pad_drill 0.85)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(R1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 GND)
  (net 6 "Net-(J3-Pad1)")
  (net 7 "Net-(R3-Pad1)")
  (net 8 "Net-(SW2-Pad2)")
  (net 9 "Net-(SW3-Pad1)")
  (net 10 "Net-(SWDIO1-Pad1)")
  (net 11 "Net-(SWDIO1-Pad2)")
  (net 12 "Net-(SWDIO1-Pad3)")
  (net 13 "Net-(SWDIO1-Pad4)")
  (net 14 "Net-(SWDIO1-Pad5)")
  (net 15 "Net-(D6-Pad1)")
  (net 16 "Net-(U2-Pad2)")
  (net 17 "Net-(U3-Pad2)")
  (net 18 "Net-(U4-Pad2)")
  (net 19 "Net-(U5-Pad2)")
  (net 20 "Net-(J3-Pad2)")
  (net 21 "Net-(D1-Pad1)")
  (net 22 ID)
  (net 23 "Net-(U1-Pad13)")
  (net 24 "Net-(U1-Pad12)")
  (net 25 "Net-(D4-Pad1)")
  (net 26 "Net-(D3-Pad1)")
  (net 27 "Net-(D2-Pad1)")
  (net 28 "Net-(D5-Pad1)")
  (net 29 "Net-(J3-Pad3)")
  (net 30 "Net-(D8-Pad2)")
  (net 31 "Net-(D9-Pad2)")
  (net 32 "Net-(D10-Pad2)")
  (net 33 "Net-(D11-Pad2)")
  (net 34 "Net-(D12-Pad2)")
  (net 35 "Net-(D13-Pad2)")
  (net 36 "Net-(D14-Pad2)")
  (net 37 "Net-(D15-Pad2)")
  (net 38 "Net-(J2-Pad1)")
  (net 39 "Net-(J2-Pad2)")
  (net 40 "Net-(J2-Pad3)")
  (net 41 "Net-(J2-Pad4)")
  (net 42 "Net-(J3-Pad4)")
  (net 43 "Net-(J3-Pad5)")
  (net 44 "Net-(J3-Pad6)")
  (net 45 "Net-(J1-Pad5)")
  (net 46 "Net-(J1-Pad6)")
  (net 47 "Net-(J1-Pad4)")
  (net 48 "Net-(J2-Pad5)")
  (net 49 "Net-(SW1-Pad1)")
  (net 50 "Net-(J2-Pad6)")
  (net 51 "Net-(SW4-Pad1)")
  (net 52 "Net-(SW4-Pad3)")
  (net 53 "Net-(J4-Pad1)")
  (net 54 "Net-(J4-Pad3)")
  (net 55 "Net-(J4-Pad5)")
  (net 56 "Net-(J5-Pad1)")
  (net 57 "Net-(J5-Pad3)")
  (net 58 "Net-(J5-Pad5)")
  (net 59 "Net-(U2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ID)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(SW3-Pad1)")
    (add_net "Net-(SW4-Pad1)")
    (add_net "Net-(SW4-Pad3)")
    (add_net "Net-(SWDIO1-Pad1)")
    (add_net "Net-(SWDIO1-Pad2)")
    (add_net "Net-(SWDIO1-Pad3)")
    (add_net "Net-(SWDIO1-Pad4)")
    (add_net "Net-(SWDIO1-Pad5)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U5-Pad2)")
  )
  (net_class powa ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
  )
  (module lightsaber_parts:slide_switch (layer F.Cu) (tedit 5A702D33)
    (at 80.01 64.77 180)
    (fp_text reference SW4 (at 0 0.5 180) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -0.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(SW4-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(SW4-Pad3)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 71.12 95.25 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J2-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_parts:screw_hole locked (layer F.Cu) (tedit 582573F1)
    (at 104.14 106.68)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:screw_hole locked (layer F.Cu) (tedit 582573F1)
    (at 104.14 66.04)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:screw_hole locked (layer F.Cu) (tedit 582573F1)
    (at 63.5 106.68)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:screw_hole locked (layer F.Cu) (tedit 582573F1)
    (at 63.5 66.04)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 87.376 64.516 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference power1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(SW4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 58724A80)
    (at 72.39 106.045 180)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.05 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.15 180) (layer F.Fab))
    (fp_text user %R (at 0 -4.05 180) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -3.98 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(SW1-Pad1)"))
    (pad 1 smd rect (at 3.98 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(SW1-Pad1)"))
    (pad 2 smd rect (at 3.98 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 58724A80)
    (at 83.185 106.045 180)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 -4.05 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.15 180) (layer F.Fab))
    (fp_text user %R (at 0 -4.05 180) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(SW2-Pad2)"))
    (pad 1 smd rect (at -3.98 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at 3.98 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 3.98 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(SW2-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 58724A80)
    (at 93.98 106.045)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW3 (at 0 -4.05) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.15) (layer F.Fab))
    (fp_text user %R (at 0 -4.05) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -3.98 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(SW3-Pad1)"))
    (pad 1 smd rect (at 3.98 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(SW3-Pad1)"))
    (pad 2 smd rect (at 3.98 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 69.596 69.088 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference SWDIO1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(SWDIO1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(SWDIO1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(SWDIO1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(SWDIO1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(SWDIO1-Pad5)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 96.52 91.948)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 96.52 87.376)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 96.52 82.804)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 96.52 78.232)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 96.52 73.66)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 96.52 69.088)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 88.9 92.71)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference speaker1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad13)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 79.375 95.25 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 79.375 100.33 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D8 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 81.915 100.33 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D9 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 84.455 100.33 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D10 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 64.77 100.33 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D11 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 67.31 100.33 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D12 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 73.66 100.33 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D13 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 76.2 100.33 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D14 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 71.12 100.33 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D15 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D15-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 64.77 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 67.31 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 73.66 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 76.2 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J2-Pad5)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 79.375 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 81.915 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 84.455 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J3-Pad5)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 71.12 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 62.23 95.25 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 ID))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 62.865 97.79 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.35 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 ID))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 61.595 97.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 ID))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 97.79 100.965 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 300 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 72.39 64.77 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference test_short1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(SW4-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_parts:ProffieBoardV1.2 (layer F.Cu) (tedit 5AAE1882)
    (at 77.47 81.28)
    (fp_text reference U1 (at 0 2.54) (layer F.SilkS))
    (fp_text value ProffieBoardV1 (at 0 -2.54) (layer F.Fab))
    (pad 25 thru_hole oval (at -0.508 -8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(SW1-Pad1)"))
    (pad 24 thru_hole oval (at 1.27 -8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(SW3-Pad1)"))
    (pad 23 thru_hole oval (at 3.048 -8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(R1-Pad1)"))
    (pad 14 thru_hole circle (at 10.16 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(J4-Pad5)"))
    (pad 11 thru_hole oval (at 3.048 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(J3-Pad6)"))
    (pad 10 thru_hole oval (at 1.27 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J3-Pad4)"))
    (pad 9 thru_hole oval (at -0.508 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(SW2-Pad2)"))
    (pad 8 thru_hole oval (at -2.286 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J3-Pad2)"))
    (pad 7 thru_hole oval (at -4.064 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(J2-Pad6)"))
    (pad 6 thru_hole oval (at -5.842 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at -7.62 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J2-Pad2)"))
    (pad 4 thru_hole oval (at -9.398 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(J1-Pad6)"))
    (pad 3 thru_hole oval (at -11.176 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(J1-Pad4)"))
    (pad 2 thru_hole oval (at -12.954 8.128) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 21 thru_hole circle (at 10.16 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(J5-Pad1)"))
    (pad 13 thru_hole circle (at 7.62 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-Pad13)"))
    (pad 12 thru_hole circle (at 5.08 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-Pad12)"))
    (pad 19 thru_hole circle (at 15.24 -5.08) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 18 thru_hole circle (at 15.24 -2.54) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(J5-Pad5)"))
    (pad 17 thru_hole circle (at 15.24 2.54) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(J4-Pad1)"))
    (pad 1 thru_hole oval (at -15.24 7.62) (size 1.4 1.9) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 16 thru_hole circle (at 15.24 5.08) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 15 thru_hole circle (at 15.24 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(J4-Pad3)"))
    (pad 20 thru_hole circle (at 15.24 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(J5-Pad3)"))
    (pad 22 thru_hole circle (at 5.08 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 26 thru_hole circle (at -5.08 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SWDIO1-Pad5)"))
    (pad 27 thru_hole circle (at -7.62 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SWDIO1-Pad4)"))
    (pad 28 thru_hole circle (at -10.16 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SWDIO1-Pad3)"))
    (pad 29 thru_hole circle (at -12.7 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SWDIO1-Pad2)"))
    (pad 30 thru_hole circle (at -15.24 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SWDIO1-Pad1)"))
  )
  (module lightsaber_parts:PL9823-F5 (layer F.Cu) (tedit 5AAE190C)
    (at 103.505 73.66 180)
    (fp_text reference U6 (at 0 1 180) (layer F.SilkS))
    (fp_text value WS2811 (at 0 -1 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad1)"))
    (pad 3 thru_hole oval (at -0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at -1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 19 "Net-(U5-Pad2)"))
  )
  (module lightsaber_parts:PL9823-F5 (layer F.Cu) (tedit 5AAE190C)
    (at 103.505 80.01 180)
    (fp_text reference U5 (at 0 1 180) (layer F.SilkS))
    (fp_text value WS2811 (at 0 -1 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 19 "Net-(U5-Pad2)"))
    (pad 1 thru_hole oval (at 0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad1)"))
    (pad 3 thru_hole oval (at -0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at -1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 18 "Net-(U4-Pad2)"))
  )
  (module lightsaber_parts:PL9823-F5 (layer F.Cu) (tedit 5AAE190C)
    (at 103.505 86.36 180)
    (fp_text reference U4 (at 0 1 180) (layer F.SilkS))
    (fp_text value WS2811 (at 0 -1 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 18 "Net-(U4-Pad2)"))
    (pad 1 thru_hole oval (at 0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad1)"))
    (pad 3 thru_hole oval (at -0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at -1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 17 "Net-(U3-Pad2)"))
  )
  (module lightsaber_parts:PL9823-F5 (layer F.Cu) (tedit 5AAE190C)
    (at 103.505 92.71 180)
    (fp_text reference U3 (at 0 1 180) (layer F.SilkS))
    (fp_text value WS2811 (at 0 -1 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 17 "Net-(U3-Pad2)"))
    (pad 1 thru_hole oval (at 0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad1)"))
    (pad 3 thru_hole oval (at -0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at -1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad2)"))
  )
  (module lightsaber_parts:PL9823-F5 (layer F.Cu) (tedit 5AAE193D)
    (at 103.505 99.06 180)
    (fp_text reference U2 (at 0 1 180) (layer F.SilkS))
    (fp_text value WS2811 (at 0 -1 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad2)"))
    (pad 1 thru_hole oval (at 0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad1)"))
    (pad 3 thru_hole oval (at -0.66 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at -1.98 0 180) (size 1 1.524) (drill 0.85) (layers *.Cu *.Mask)
      (net 7 "Net-(R3-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 98.044 96.52 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J4 (at 1.27 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41 270) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(D3-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(D2-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 87.376 70.612 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J5 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(D6-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(D5-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 94.996 64.516 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference nppower1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "- +\n" (at 71.12 66.802) (layer F.SilkS))
  (gr_line (start 59.69 106.68) (end 59.69 66.04) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 66.04) (end 107.95 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.5 62.23) (end 104.14 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 104.14 66.04) (end 104.14 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 63.5 66.04) (end 59.69 66.04) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "ProffieBoard V1.4\nTest Rig\n" (at 76.2 79.248) (layer F.SilkS))
  (gr_text "+\n-\n" (at 99.06 64.77) (layer F.SilkS))
  (gr_arc (start 104.14 106.68) (end 107.95 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 63.5 106.68) (end 63.5 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.5 110.49) (end 104.14 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 110.49) (xy 59.69 110.49) (xy 59.69 59.69) (xy 107.95 59.69)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.166 58.42) (xy 108.966 58.42) (xy 108.966 112.014) (xy 58.293 111.887)
      )
    )
  )
)
