(kicad_pcb (version 20170123) (host pcbnew "(2017-03-19 revision 2637835)-master")
  (general
    (links 80)
    (no_connects 0)
    (area 99.949999 79.121999 260.050001 115.029373)
    (thickness 1.6)
    (drawings 5)
    (tracks 260)
    (zones 0)
    (modules 47)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.125)
    (pad_size 2.5 2.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100.01 79.18)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /Users/Drc3p0/Desktop/CMOSworkshopGIT/CMOSworkshop/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 VCC)
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 GND)
  (net 6 MIXOUTA)
  (net 7 MIXOUTB)
  (net 8 "Net-(P1-Pad1)")
  (net 9 "Net-(P1-Pad2)")
  (net 10 "Net-(P1-Pad3)")
  (net 11 "Net-(P3-Pad1)")
  (net 12 "Net-(P3-Pad2)")
  (net 13 "Net-(P3-Pad3)")
  (net 14 "Net-(P5-Pad1)")
  (net 15 "Net-(P5-Pad2)")
  (net 16 "Net-(P5-Pad3)")
  (net 17 MIX4)
  (net 18 MIX3)
  (net 19 MIX2)
  (net 20 MIX1)
  (net 21 "Net-(S7-Pad1)")
  (net 22 "Net-(C1-Pad+)")
  (net 23 "Net-(C7-Pad1)")
  (net 24 "Net-(C7-Pad2)")
  (net 25 "Net-(C13-Pad+)")
  (net 26 "Net-(C13-Pad-)")
  (net 27 "Net-(R11-Pad1)")
  (net 28 "Net-(R11-Pad2)")
  (net 29 "Net-(C2-Pad1)")
  (net 30 "Net-(C3-Pad1)")
  (net 31 "Net-(C4-Pad1)")
  (net 32 "Net-(C5-Pad1)")
  (net 33 "Net-(P2-Pad1)")
  (net 34 "Net-(P2-Pad2)")
  (net 35 "Net-(P2-Pad3)")
  (net 36 "Net-(P4-Pad1)")
  (net 37 "Net-(P4-Pad2)")
  (net 38 "Net-(P4-Pad3)")
  (net 39 "Net-(P6-Pad1)")
  (net 40 "Net-(P6-Pad2)")
  (net 41 "Net-(P6-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net MIX1)
    (add_net MIX2)
    (add_net MIX3)
    (add_net MIX4)
    (add_net MIXOUTA)
    (add_net MIXOUTB)
    (add_net "Net-(C1-Pad+)")
    (add_net "Net-(C13-Pad+)")
    (add_net "Net-(C13-Pad-)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(S7-Pad1)")
    (add_net VCC)
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CE2CC7)
    (at 168.6687 108.23194 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P18 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "MIX IN" (at -2.62128 4.13258 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 MIX4))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 MIX3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 MIX2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 MIX1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:LadyBrainSilk (layer F.Cu) (tedit 0)
    (at 158.33852 85.0519)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Prototyping_PCB:LED_D3.0mm (layer F.Cu) (tedit 58CEF152)
    (at 181.61508 81.8388)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LED (at 1.53924 2.8448) (layer F.SilkS))
    (fp_text value LED (at 2.54 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prototyping_PCB:SPDT-SUB (layer F.Cu) (tedit 55CE7527)
    (at 195.56984 93.24848 90)
    (fp_text reference S7 (at -3.59664 -3.34518) (layer F.SilkS))
    (fp_text value SPDT (at -3.59664 -0.33274) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -2.54 90) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 21 "Net-(S7-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model "/Users/design/Google Drive/4ms/kicad/packages3d/spdt-toggle-submini.wrl"
      (at (xyz 0 0 0.11))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 270 0 90))
    )
  )
  (module Prototyping_PCB:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 58BCB551)
    (at 202.90282 98.60026 90)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D2 (at 5.715 -0.63754 90) (layer F.SilkS))
    (fp_text value B140HW-7 (at 5.715 0.63246 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 270) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
  )
  (module Prototyping_PCB:9V_BatteryHolder_MOUSERMOD (layer F.Cu) (tedit 58CE2C9E)
    (at 205.16 89.1626)
    (descr "9 Volt Battery Holder, PC Terminals, plastic housing")
    (tags "Keystone battery holder 9V")
    (fp_text reference U8 (at 6.715 6 90) (layer F.SilkS) hide)
    (fp_text value BAT9V (at 19.05 6.35) (layer F.Fab))
    (pad + thru_hole circle (at 2.3 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad2)"))
    (pad - thru_hole circle (at 2.3 12.7) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Battery_Holders.3dshapes/BatteryHolder_9Volt_Keystone_1294.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prototyping_PCB:J355W (layer F.Cu) (tedit 58CEF5B1)
    (at 194.6428 83.6175 90)
    (descr "Connect-teck J355W, 3.5mm Stereo Jack")
    (fp_text reference J1 (at 3.10966 4.88436 180) (layer F.SilkS))
    (fp_text value STEREO_OUT (at -5.95814 -3.88372 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.45 0.6 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 0.75 -4.6 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 6 MIXOUTA))
    (pad 3 thru_hole circle (at 0.75 3.2 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 7 MIXOUTB))
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CEF1B4)
    (at 183.65216 108.34624 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P22 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value " +9VDC GND" (at -2.58318 0.43688 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:DIP-8__300 (layer F.Cu) (tedit 58CEF1D3)
    (at 182.62092 91.49842 90)
    (descr "8 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U1 (at -5.92328 0.2159 180) (layer F.SilkS))
    (fp_text value TL082 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C7-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C1-Pad+)"))
    (pad 4 thru_hole circle (at 3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C1-Pad+)"))
    (pad 6 thru_hole circle (at 1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R11-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C13-Pad+)"))
    (pad 8 thru_hole circle (at -3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prototyping_PCB:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 58CE297C)
    (at 186.23026 103.0986)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at -0.2921 -3.64744) (layer F.SilkS))
    (fp_text value 100uF (at 2.30378 -3.64744) (layer F.SilkS))
    (pad + thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C1-Pad+)"))
    (pad - thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 58CE297C)
    (at 182.79428 102.96398 180)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C13 (at 3.2747 3.59918 180) (layer F.SilkS))
    (fp_text value 100uF (at 0.31814 3.59918 180) (layer F.SilkS))
    (pad + thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C13-Pad+)"))
    (pad - thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(C13-Pad-)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 58CEF12D)
    (at 189.64148 94.72676 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C7 (at -3.0353 -0.23876) (layer F.SilkS))
    (fp_text value 47pF (at -1.75768 -0.04064) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C7-Pad2)"))
    (model Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prototyping_PCB:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 58CEF12D)
    (at 176.28362 102.58552 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 1.53416 10.02284 270) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.31 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 MIX1))
    (model Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prototyping_PCB:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 58CEF12D)
    (at 173.7614 102.58552 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 1.5113 8.53948 270) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.31 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 MIX2))
    (model Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prototyping_PCB:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 58CEF12D)
    (at 171.23918 102.58552 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 1.5113 7.04596 270) (layer F.SilkS))
    (fp_text value .1uF (at 0.722 5.25272 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 MIX3))
    (model Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prototyping_PCB:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 58CEF12D)
    (at 168.66616 102.58552 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 1.53416 5.47878 270) (layer F.SilkS))
    (fp_text value .1uF (at -0.11938 4.01828) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 MIX4))
    (model Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 171.2087 83.06562 270)
    (fp_text reference R1 (at 1.17856 5.81152 270) (layer F.SilkS))
    (fp_text value 100k (at 1.31318 -0.38354 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 22 "Net-(C1-Pad+)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 171.21632 90.23096 90)
    (fp_text reference R2 (at -1.27 -6.35 90) (layer F.SilkS))
    (fp_text value 100k (at -1.36906 0.48006 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 22 "Net-(C1-Pad+)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 176.26838 97.40138 270)
    (fp_text reference R6 (at 1.45034 8.96112 270) (layer F.SilkS))
    (fp_text value 100k (at 1.41478 -0.49022 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 24 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad1)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 173.75378 97.40138 270)
    (fp_text reference R7 (at 1.4732 7.62254 270) (layer F.SilkS))
    (fp_text value 100k (at 1.41478 -0.33782 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 24 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 30 "Net-(C3-Pad1)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 171.21632 97.4217 270)
    (fp_text reference R8 (at 1.45034 6.31952 270) (layer F.SilkS))
    (fp_text value 100k (at 1.41478 -0.3937 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 24 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 31 "Net-(C4-Pad1)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 168.66108 97.4217 270)
    (fp_text reference R9 (at 1.45034 4.98094 90) (layer F.SilkS))
    (fp_text value 100k (at 1.41478 -0.41656 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 24 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 32 "Net-(C5-Pad1)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 168.71696 90.23096 270)
    (fp_text reference R10 (at 1.27 5.08 270) (layer F.SilkS))
    (fp_text value 100k (at 1.36906 -0.44958 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 23 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 24 "Net-(C7-Pad2)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 176.2887 83.06562 90)
    (fp_text reference R11 (at -1.18364 -8.79602 90) (layer F.SilkS))
    (fp_text value 100k (at -1.41224 0.39116 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 27 "Net-(R11-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 28 "Net-(R11-Pad2)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 168.7703 83.0707 270)
    (fp_text reference R13 (at 1.17348 4.3561 270) (layer F.SilkS))
    (fp_text value 1K (at 0.635 -0.635 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 173.7487 83.06562 270)
    (fp_text reference R14 (at 1.2065 7.28472 270) (layer F.SilkS))
    (fp_text value 100k (at 1.36144 -0.38862 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 25 "Net-(C13-Pad+)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 27 "Net-(R11-Pad1)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 173.77156 90.17762 90)
    (fp_text reference R15 (at -1.27 -7.62 90) (layer F.SilkS))
    (fp_text value 1k (at -0.66802 0.3937 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 6 MIXOUTA))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 26 "Net-(C13-Pad-)"))
  )
  (module Prototyping_PCB:R-TH (layer F.Cu) (tedit 58A7CE1D)
    (at 176.27346 90.17762 90)
    (fp_text reference R16 (at -1.27 -8.89 90) (layer F.SilkS))
    (fp_text value 1k (at -0.63754 0.39624 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 7 MIXOUTB))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.27 1.27) (drill 0.7112) (layers *.Cu *.Mask)
      (net 26 "Net-(C13-Pad-)"))
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 134.6327 109.9058 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P4-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 114.32032 106.40568 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P6-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 134.6327 106.36504 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P4-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 124.51334 106.39552 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P2-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 124.51334 109.92104 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P2-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 114.31016 109.92104 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P6-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 154.96286 106.39552 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 104.13746 106.3625 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P3-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 104.13746 109.92104 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P3-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 144.82318 109.92104 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P5-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 144.82318 106.39552 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P5-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CE2C2D)
    (at 154.96286 109.92104 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.2286 1.2446 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Prototyping_PCB:POT-9MM-ALPHA (layer F.Cu) (tedit 56640EB3)
    (at 157.48 96.52 180)
    (fp_text reference RV1 (at 1.27 3.81 180) (layer F.SilkS))
    (fp_text value 100K (at 1.27 5.715 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at -2.540163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at -0.000163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at 2.539837 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad1)"))
    (pad 4 thru_hole circle (at 4.394037 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -4.394363 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
  )
  (module Prototyping_PCB:POT-9MM-ALPHA (layer F.Cu) (tedit 56640EB3)
    (at 126.999837 86.36 180)
    (fp_text reference RV2 (at 1.269837 3.81 180) (layer F.SilkS))
    (fp_text value 100K (at 1.269837 5.715 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at -2.540163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 35 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at -0.000163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 34 "Net-(P2-Pad2)"))
    (pad 1 thru_hole circle (at 2.539837 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 33 "Net-(P2-Pad1)"))
    (pad 4 thru_hole circle (at 4.394037 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -4.394363 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
  )
  (module Prototyping_PCB:POT-9MM-ALPHA (layer F.Cu) (tedit 56640EB3)
    (at 106.679837 86.36 180)
    (fp_text reference RV3 (at 1.269837 3.81 180) (layer F.SilkS))
    (fp_text value 100K (at 1.269837 5.715 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at -2.540163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 13 "Net-(P3-Pad3)"))
    (pad 2 thru_hole circle (at -0.000163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad2)"))
    (pad 1 thru_hole circle (at 2.539837 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(P3-Pad1)"))
    (pad 4 thru_hole circle (at 4.394037 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -4.394363 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
  )
  (module Prototyping_PCB:POT-9MM-ALPHA (layer F.Cu) (tedit 56640EB3)
    (at 137.16 96.52 180)
    (fp_text reference RV4 (at 1.27 3.81 180) (layer F.SilkS))
    (fp_text value 100K (at 1.27 5.715 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at -2.540163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 38 "Net-(P4-Pad3)"))
    (pad 2 thru_hole circle (at -0.000163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 37 "Net-(P4-Pad2)"))
    (pad 1 thru_hole circle (at 2.539837 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 36 "Net-(P4-Pad1)"))
    (pad 4 thru_hole circle (at 4.394037 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -4.394363 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
  )
  (module Prototyping_PCB:POT-9MM-ALPHA (layer F.Cu) (tedit 56640EB3)
    (at 147.32 86.36 180)
    (fp_text reference RV5 (at 1.27 3.81 180) (layer F.SilkS))
    (fp_text value 100K (at 1.27 5.715 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at -2.540163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 16 "Net-(P5-Pad3)"))
    (pad 2 thru_hole circle (at -0.000163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 15 "Net-(P5-Pad2)"))
    (pad 1 thru_hole circle (at 2.539837 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 14 "Net-(P5-Pad1)"))
    (pad 4 thru_hole circle (at 4.394037 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -4.394363 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
  )
  (module Prototyping_PCB:POT-9MM-ALPHA (layer F.Cu) (tedit 56640EB3)
    (at 116.84 96.52 180)
    (fp_text reference RV6 (at 1.27 3.81 180) (layer F.SilkS))
    (fp_text value 100K (at 1.27 5.715 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at -2.540163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 41 "Net-(P6-Pad3)"))
    (pad 2 thru_hole circle (at -0.000163 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 40 "Net-(P6-Pad2)"))
    (pad 1 thru_hole circle (at 2.539837 -7.012243 90) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 39 "Net-(P6-Pad1)"))
    (pad 4 thru_hole circle (at 4.394037 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -4.394363 -0.001843 180) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
  )
  (module Prototyping_PCB:POT-9MM-ALPHA (layer F.Cu) (tedit 56640EB3)
    (at 196.431063 105.772523)
    (fp_text reference RV8 (at -0.891703 4.547297 180) (layer F.SilkS))
    (fp_text value 10K (at -5.067463 4.590477 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at -2.540163 -7.012243 270) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at -0.000163 -7.012243 270) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 28 "Net-(R11-Pad2)"))
    (pad 1 thru_hole circle (at 2.539837 -7.012243 270) (size 1.8034 1.8034) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "Net-(C1-Pad+)"))
    (pad 4 thru_hole circle (at 4.394037 -0.001843) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -4.394363 -0.001843) (size 2.667 2.667) (drill 2.0574) (layers *.Cu *.Mask))
  )
  (gr_text "Prototyping board v1.2\nLadyBrain Studios" (at 231.73436 95.504) (layer B.Cu))
  (gr_line (start 260 79.172) (end 260 111.76) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 79.172) (end 260 79.172) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 111.76) (end 260 111.76) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 79.172) (end 100 111.76) (angle 90) (layer Edge.Cuts) (width 0.1))
)
