(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(U1-PIN14)")
	(net 2 "Net-(C2-Pad1)")
	(net 3 "Net-(U2-PIN2)")
	(net 4 "Net-(U1-PIN15)")
	(net 5 "Net-(C4-Pad1)")
	(net 6 "Net-(U2-PIN3)")
	(net 7 "Net-(U1-PIN16)")
	(net 8 "Net-(C6-Pad1)")
	(net 9 "Net-(U2-PIN4)")
	(net 10 "Net-(U1-PIN17)")
	(net 11 "Net-(C8-Pad1)")
	(net 12 "Net-(C10-Pad1)")
	(net 13 "Net-(U1-PIN18)")
	(net 14 "Net-(U1-PIN19)")
	(net 15 "Net-(C12-Pad1)")
	(net 16 "Net-(U2-PIN5)")
	(net 17 "Net-(U2-PIN6)")
	(net 18 "Net-(U2-PIN7)")
	(net 19 "Net-(C14-Pad1)")
	(net 20 "Net-(U1-PIN20)")
	(net 21 "Net-(U1-PIN21)")
	(net 22 "Net-(C16-Pad1)")
	(net 23 "Net-(C18-Pad1)")
	(net 24 "Net-(U1-PIN22)")
	(net 25 "Net-(U2-PIN8)")
	(net 26 "Net-(U2-PIN9)")
	(net 27 "Net-(C48-Pad1)")
	(net 28 "Net-(C20-Pad1)")
	(net 29 "Net-(U1-PIN23)")
	(net 30 "Net-(U1-PIN24)")
	(net 31 "Net-(C22-Pad1)")
	(net 32 "Net-(C24-Pad1)")
	(net 33 "Net-(U1-PIN25)")
	(net 34 "Net-(U2-PIN11)")
	(net 35 "Net-(U2-PIN12)")
	(net 36 "Net-(U1-PIN2)")
	(net 37 "Net-(U1-PIN3)")
	(net 38 "Net-(U1-PIN4)")
	(net 39 "Net-(C47-Pad1)")
	(net 40 "Net-(U1-PIN7)")
	(net 41 "Net-(U1-PIN8)")
	(net 42 "Net-(U1-PIN9)")
	(net 43 "Net-(U1-PIN10)")
	(net 44 "Net-(C46-Pad1)")
	(net 45 "Net-(U1-PIN12)")
	(net 46 "Net-(U2-PIN1)")
	(net 47 "Net-(U1-PIN1)")
	(net 48 "unconnected-(U2-PIN13-Pad13)")
	(net 49 "Net-(U1-PIN6)")
	(net 50 "unconnected-(U1-PIN13-Pad13)")
	(net 51 "Net-(C11-Pad1)")
	(net 52 "Net-(C23-Pad1)")
	(net 53 "Net-(C21-Pad1)")
	(net 54 "Net-(C19-Pad1)")
	(net 55 "Net-(C17-Pad1)")
	(net 56 "Net-(C15-Pad1)")
	(net 57 "Net-(C13-Pad1)")
	(net 58 "Net-(C9-Pad1)")
	(net 59 "Net-(C5-Pad1)")
	(net 60 "Net-(C3-Pad1)")
	(net 61 "Net-(C1-Pad1)")
	(net 62 "Net-(C7-Pad1)")
	(net 63 "Net-(C45-Pad1)")
	(net 64 "Net-(U2-PIN25)")
	(net 65 "Net-(C44-Pad1)")
	(net 66 "Net-(U2-PIN24)")
	(net 67 "Net-(C43-Pad1)")
	(net 68 "Net-(C42-Pad1)")
	(net 69 "Net-(U2-PIN23)")
	(net 70 "Net-(C41-Pad1)")
	(net 71 "Net-(C40-Pad1)")
	(net 72 "Net-(U2-PIN22)")
	(net 73 "Net-(C39-Pad1)")
	(net 74 "Net-(C38-Pad1)")
	(net 75 "Net-(C37-Pad1)")
	(net 76 "Net-(C36-Pad1)")
	(net 77 "Net-(U2-PIN14)")
	(net 78 "Net-(C35-Pad1)")
	(net 79 "Net-(C34-Pad1)")
	(net 80 "Net-(U2-PIN15)")
	(net 81 "Net-(C33-Pad1)")
	(net 82 "Net-(C32-Pad1)")
	(net 83 "Net-(U2-PIN16)")
	(net 84 "Net-(C31-Pad1)")
	(net 85 "Net-(C30-Pad1)")
	(net 86 "Net-(U2-PIN17)")
	(net 87 "Net-(C29-Pad1)")
	(net 88 "Net-(C28-Pad1)")
	(net 89 "Net-(U2-PIN18)")
	(net 90 "Net-(C27-Pad1)")
	(net 91 "Net-(C26-Pad1)")
	(net 92 "Net-(U2-PIN19)")
	(net 93 "Net-(C25-Pad1)")
	(net 94 "Net-(U2-PIN10)")
	(net 95 "Net-(U2-PIN20)")
	(net 96 "Net-(U1-PIN11)")
	(net 97 "Net-(U1-PIN5)")
	(net 98 "Net-(U2-PIN21)")
	(net 99 "GND")
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 143.7894 94.2995 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 19 "Net-(C14-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 57 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 97.282 110.3409 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at -0.0508 -0.9398 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 23 "Net-(C18-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 106.0704 99.7023 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -0.0762 -0.8636 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 5 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 136.4742 110.1778 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at -0.0615 -0.889 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 88 "Net-(C28-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 96.2914 120.9728 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -0.8128 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 79 "Net-(C34-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 105.1052 110.3302 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0.0254 -0.8636 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 28 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 125.9078 94.2774 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.0254 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 37 "Net-(U1-PIN3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 58 "Net-(C9-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 109.2026 105.043 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0.0254 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 49 "Net-(U1-PIN6)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 53 "Net-(C21-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 94.3386 99.7491 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at -0.0508 -0.8158 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 55 "Net-(C17-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 118.3894 115.6134 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R59"
			(at 0 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 73 "Net-(C39-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 71 "Net-(C40-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 132.7658 104.8946 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 0.0401 -0.1778 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 20 "Net-(U1-PIN20)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 90 "Net-(C27-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 150.6728 104.8946 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at -0.0254 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 82 "Net-(C32-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 84 "Net-(C31-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMPORTED:BEL_DCCM25PCBR"
		(layer "F.Cu")
		(at 78.7654 104.978 90)
		(property "Reference" "U1"
			(at -13.7957 1.0717 90)
			(layer "F.SilkS")
		)
		(property "Value" "RIGHT-ANGLE-MICRO-D"
			(at -0.3591 -6.4213 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 -6.35 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 -6.35 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr through_hole)
		(fp_text user "PCB Edge"
			(at 2.8413 1.0209 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at -14.5831 11.8413 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -12.268 6.35 90)
			(size 2.44 2.44)
			(drill 2.44)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 12.268 6.35 90)
			(size 2.44 2.44)
			(drill 2.44)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at 10.16 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(U1-PIN1)")
			(pinfunction "PIN1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 8.89 3.302 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(U1-PIN2)")
			(pinfunction "PIN2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 6.35 3.302 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(U1-PIN3)")
			(pinfunction "PIN3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 3.302 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(U1-PIN4)")
			(pinfunction "PIN4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 2.54 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "Net-(U1-PIN5)")
			(pinfunction "PIN5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 1.27 3.302 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(U1-PIN6)")
			(pinfunction "PIN6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 0 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(U1-PIN7)")
			(pinfunction "PIN7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -1.27 3.302 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(U1-PIN8)")
			(pinfunction "PIN8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at -2.54 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(U1-PIN9)")
			(pinfunction "PIN9")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at -3.81 3.302 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(U1-PIN10)")
			(pinfunction "PIN10")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at -6.35 3.302 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "Net-(U1-PIN11)")
			(pinfunction "PIN11")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at -8.89 3.302 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(U1-PIN12)")
			(pinfunction "PIN12")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at -10.16 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(U1-PIN13-Pad13)")
			(pinfunction "PIN13")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 8.89 8.382 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(U1-PIN14)")
			(pinfunction "PIN14")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 7.62 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1-PIN15)")
			(pinfunction "PIN15")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 6.35 8.382 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(U1-PIN16)")
			(pinfunction "PIN16")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at 5.08 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(U1-PIN17)")
			(pinfunction "PIN17")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at 3.81 8.382 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(U1-PIN18)")
			(pinfunction "PIN18")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at 1.27 8.382 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(U1-PIN19)")
			(pinfunction "PIN19")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at -1.27 8.382 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U1-PIN20)")
			(pinfunction "PIN20")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" thru_hole circle
			(at -3.81 8.382 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(U1-PIN21)")
			(pinfunction "PIN21")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" thru_hole circle
			(at -5.08 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(U1-PIN22)")
			(pinfunction "PIN22")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "23" thru_hole circle
			(at -6.35 8.382 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(U1-PIN23)")
			(pinfunction "PIN23")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "24" thru_hole circle
			(at -7.62 5.842 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(U1-PIN24)")
			(pinfunction "PIN24")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "25" thru_hole circle
			(at -8.89 8.382 90)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(U1-PIN25)")
			(pinfunction "PIN25")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 142.8496 104.92 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at -0.0508 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 85 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 87 "Net-(C29-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 125.6792 99.6368 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at -0.0254 -0.7874 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 93 "Net-(C25-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 109.993 99.727 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at -0.0328 -0.7904 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 53 "Net-(C21-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 124.714 110.2794 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0 -0.8382 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 70 "Net-(C41-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 94.8944 115.6896 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at -0.0508 -0.1524 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 81 "Net-(C33-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 79 "Net-(C34-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 114.7318 94.3937 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0.0254 0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 3 "Net-(U2-PIN2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 8 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 126.238 115.588 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R62"
			(at -0.0762 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 68 "Net-(C42-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 70 "Net-(C41-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 134.0612 115.5118 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R65"
			(at -0.0508 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 65 "Net-(C44-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 67 "Net-(C43-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMPORTED:BEL_M83513_13-D01NP"
		(layer "F.Cu")
		(at 167.6654 104.978 -90)
		(property "Reference" "U2"
			(at 13.3893 1.2905 90)
			(layer "F.SilkS")
		)
		(property "Value" "RIGHT-ANGLE-MICRO-D"
			(at 2.259 -5.885 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 -6.35 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 -6.35 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 14.6847 12.0347 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "PCB EDGE"
			(at -11.53 6.254 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -12.2555 6.35 270)
			(size 2.4384 2.4384)
			(drill 2.4384)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 12.2555 6.35 270)
			(size 2.4384 2.4384)
			(drill 2.4384)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -10.16 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(U2-PIN1)")
			(pinfunction "PIN1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -8.89 3.302 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(U2-PIN2)")
			(pinfunction "PIN2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -6.35 3.302 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(U2-PIN3)")
			(pinfunction "PIN3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -3.81 3.302 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(U2-PIN4)")
			(pinfunction "PIN4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at -2.54 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U2-PIN5)")
			(pinfunction "PIN5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at -1.27 3.302 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(U2-PIN6)")
			(pinfunction "PIN6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 0 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(U2-PIN7)")
			(pinfunction "PIN7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at 1.27 3.302 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(U2-PIN8)")
			(pinfunction "PIN8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at 2.54 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(U2-PIN9)")
			(pinfunction "PIN9")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at 3.81 3.302 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "Net-(U2-PIN10)")
			(pinfunction "PIN10")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at 6.35 3.302 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U2-PIN11)")
			(pinfunction "PIN11")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at 8.89 3.302 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(U2-PIN12)")
			(pinfunction "PIN12")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at 10.16 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(U2-PIN13-Pad13)")
			(pinfunction "PIN13")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at -8.89 8.382 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "Net-(U2-PIN14)")
			(pinfunction "PIN14")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at -7.62 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "Net-(U2-PIN15)")
			(pinfunction "PIN15")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at -6.35 8.382 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "Net-(U2-PIN16)")
			(pinfunction "PIN16")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at -5.08 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "Net-(U2-PIN17)")
			(pinfunction "PIN17")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at -3.81 8.382 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "Net-(U2-PIN18)")
			(pinfunction "PIN18")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at -1.27 8.382 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "Net-(U2-PIN19)")
			(pinfunction "PIN19")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at 1.27 8.382 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "Net-(U2-PIN20)")
			(pinfunction "PIN20")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" thru_hole circle
			(at 3.81 8.382 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "Net-(U2-PIN21)")
			(pinfunction "PIN21")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" thru_hole circle
			(at 5.08 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(U2-PIN22)")
			(pinfunction "PIN22")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "23" thru_hole circle
			(at 6.35 8.382 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(U2-PIN23)")
			(pinfunction "PIN23")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "24" thru_hole circle
			(at 7.62 5.842 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(U2-PIN24)")
			(pinfunction "PIN24")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "25" thru_hole circle
			(at 8.89 8.382 270)
			(size 1.53 1.53)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(U2-PIN25)")
			(pinfunction "PIN25")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 123.952 115.588 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R61"
			(at 0.0254 -0.1778 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 96 "Net-(U1-PIN11)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 70 "Net-(C41-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 112.8014 115.6642 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R57"
			(at -0.0254 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 94 "Net-(U2-PIN10)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 74 "Net-(C38-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 98.0948 105.0577 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 16 "Net-(U2-PIN5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 23 "Net-(C18-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 102.1618 99.731 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at -0.0074 -0.8158 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 54 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 151.59455 94.2955 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 0.1524 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 56 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 22 "Net-(C16-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 149.1488 99.586 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0.0254 -0.889 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 84 "Net-(C31-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 151.9428 115.5118 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R72"
			(at 0 -1.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 64 "Net-(U2-PIN25)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 27 "Net-(C48-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 128.6256 110.2286 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -0.7874 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 91 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 128.1938 94.2774 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -0.0762 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 58 "Net-(C9-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 12 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 133.728 94.3102 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 7 "Net-(U1-PIN16)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 51 "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 104.14 120.9474 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 -0.8636 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 76 "Net-(C36-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 112.4458 94.3937 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at -0.0254 0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 8 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 59 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 93.5736 105.047 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0 -0.1524 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 97 "Net-(U1-PIN5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 55 "Net-(C17-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 134.5438 89.009 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at -0.018 -0.892 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 51 "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 148.1836 110.2032 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at 0 -0.8128 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 39 "Net-(C47-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 101.1936 110.3556 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at -0.0508 -0.7874 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 78 "Net-(C35-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 106.8832 94.4191 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0.0508 0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 5 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 77 "Net-(U2-PIN14)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 104.9528 115.6642 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R54"
			(at 0 -0.1778 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 72 "Net-(U2-PIN22)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 76 "Net-(C36-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 122.6058 94.3429 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -0.0254 0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 80 "Net-(U2-PIN15)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 11 "Net-(C8-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 132.5372 110.2032 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at -0.0254 -0.8382 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 67 "Net-(C43-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 110.1598 94.3937 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0.0762 0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 36 "Net-(U1-PIN2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 59 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 104.5972 94.4191 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0.0254 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 60 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 5 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 95.8342 105.0577 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at -0.0762 0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 23 "Net-(C18-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 55 "Net-(C17-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 141.5034 94.2995 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 38 "Net-(U1-PIN4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 57 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 137.287 104.8946 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at -0.0361 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 88 "Net-(C28-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 95 "Net-(U2-PIN20)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 136.2964 115.5118 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R66"
			(at -0.0254 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 66 "Net-(U2-PIN24)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 65 "Net-(C44-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 150.09895 88.9976 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -0.0254 -0.8158 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 56 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 116.8654 110.3048 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at -0.0254 -0.7874 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 73 "Net-(C39-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 96.774 94.4298 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0.0508 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 61 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 146.0754 94.2995 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 9 "Net-(U2-PIN4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 19 "Net-(C14-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 147.4216 115.5118 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R70"
			(at 0 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 33 "Net-(U1-PIN25)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 39 "Net-(C47-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 97.1296 115.6896 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R51"
			(at 0.0254 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 79 "Net-(C34-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 26 "Net-(U2-PIN9)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 149.30855 94.2955 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 10 "Net-(U1-PIN17)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 56 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 141.9098 115.5372 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R68"
			(at -0.0508 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 63 "Net-(C45-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 44 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 119.38 104.9708 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at -0.0254 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 32 "Net-(C24-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 52 "Net-(C23-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 118.8466 89.0925 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -0.0434 -0.8382 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 62 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 95.3008 89.1466 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0.0254 -0.9144 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 61 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 138.3 94.3102 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 83 "Net-(U2-PIN16)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 15 "Net-(C12-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 140.3858 110.2286 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at -0.0254 -0.8382 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 63 "Net-(C45-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 120.6246 115.6134 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R60"
			(at -0.0254 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 71 "Net-(C40-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 69 "Net-(U2-PIN23)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 121.7676 99.6261 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -0.0762 -0.8636 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 11 "Net-(C8-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 98.2472 99.713 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.0508 -0.9144 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 2 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 136.014 94.2995 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at -0.0361 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 15 "Net-(C12-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 51 "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 130.4798 94.2774 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 12 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 6 "Net-(U2-PIN3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 111.9886 120.9474 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at -0.0254 -0.889 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 74 "Net-(C38-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 124.9172 104.9454 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 40 "Net-(U1-PIN7)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 93 "Net-(C25-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 148.3868 104.8946 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at -0.0254 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 21 "Net-(U1-PIN21)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 84 "Net-(C31-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 110.9472 89.1359 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -0.9398 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 59 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 103.6574 105.0216 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at -0.0508 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 28 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 54 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 100.4316 115.6642 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R52"
			(at 0 -0.1778 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 24 "Net-(U1-PIN22)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 78 "Net-(C35-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 142.3192 89.0089 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at -0.0328 -0.8666 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 57 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 141.3256 99.6114 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at -0.0508 -0.8382 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 87 "Net-(C29-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 108.2802 115.6642 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R55"
			(at 0.0508 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 43 "Net-(U1-PIN10)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 75 "Net-(C37-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 127.6604 120.8712 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0 -0.7112 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 68 "Net-(C42-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 119.8118 120.8966 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at -0.0254 -0.8128 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 71 "Net-(C40-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 120.2944 94.3175 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -0.0508 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 11 "Net-(C8-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 62 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 144.145 115.5372 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R69"
			(at -0.0254 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 44 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 35 "Net-(U2-PIN12)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 120.8024 110.254 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0.1016 0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 32 "Net-(C24-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 149.7076 115.5118 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R71"
			(at 0.0508 2.032 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 27 "Net-(C48-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 39 "Net-(C47-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 135.4836 120.795 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0 -0.9144 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 65 "Net-(C44-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 129.6416 99.586 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -0.0508 -0.9652 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 12 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 140.5636 104.92 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at -0.0508 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 41 "Net-(U1-PIN8)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 87 "Net-(C29-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 152.908 104.8946 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at -0.0254 -0.1524 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 98 "Net-(U2-PIN21)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 82 "Net-(C32-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 152.0952 110.1778 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -0.7874 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 82 "Net-(C32-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 113.7492 105.043 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at -0.0254 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 31 "Net-(C22-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 17 "Net-(U2-PIN6)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 137.4618 99.5934 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at -0.0254 -0.9906 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 15 "Net-(C12-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 153.04235 99.5894 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0.0508 -0.8382 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 22 "Net-(C16-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 118.0592 94.3683 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0.0762 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 4 "Net-(U1-PIN15)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 62 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 113.8936 99.6769 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0.0254 -0.9398 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 8 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 121.6152 104.9708 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at -0.0508 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 92 "Net-(U2-PIN19)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 32 "Net-(C24-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 145.0848 104.92 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at -0.0254 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 25 "Net-(U2-PIN8)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 85 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 129.4384 104.9454 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 18 "Net-(U2-PIN7)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 91 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 109.0422 110.3556 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at -0.0254 -0.8382 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 75 "Net-(C37-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 131.7752 115.5118 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R64"
			(at 0.0508 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 30 "Net-(U1-PIN24)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 67 "Net-(C43-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 116.1034 115.6134 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R58"
			(at 0 -0.1524 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 29 "Net-(U1-PIN23)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 73 "Net-(C39-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 93.3704 110.381 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 0 -0.8636 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 81 "Net-(C33-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 112.9364 110.3262 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -0.9652 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 31 "Net-(C22-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 110.5662 115.6642 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R56"
			(at -0.0254 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 74 "Net-(C38-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 75 "Net-(C37-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 92.6084 115.6896 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at 0 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 42 "Net-(U1-PIN9)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 81 "Net-(C33-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 153.82975 94.2808 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 22 "Net-(C16-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 86 "Net-(U2-PIN17)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 101.3714 105.0216 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at -0.0254 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 13 "Net-(U1-PIN18)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 54 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 102.7176 115.6642 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R53"
			(at -0.0254 -0.1778 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 76 "Net-(C36-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 78 "Net-(C35-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 135.0518 104.8946 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at -0.0869 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 90 "Net-(C27-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 88 "Net-(C28-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 127.2032 104.9454 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 91 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 93 "Net-(C25-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 99.06 94.4298 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -0.0508 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 46 "Net-(U2-PIN1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 144.272 110.2032 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at -0.0508 -0.8128 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 85 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 111.4806 105.0323 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0.0147 0.0842 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 53 "Net-(C21-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 31 "Net-(C22-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 117.094 104.9708 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at 0.0254 -0.1524 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 14 "Net-(U1-PIN19)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 52 "Net-(C23-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 151.13 120.795 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0 -0.9144 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 27 "Net-(C48-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 143.3322 120.8204 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at -0.0254 -0.762 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 44 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 102.3112 94.4191 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0.0762 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 1 "Net-(U1-PIN14)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 60 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 126.7206 88.9688 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -0.889 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 58 "Net-(C9-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 139.6238 115.5372 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R67"
			(at 0 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 45 "Net-(U1-PIN12)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 63 "Net-(C45-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 105.918 104.9962 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at -0.0254 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 89 "Net-(U2-PIN18)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 28 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 103.124 89.1359 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -0.889 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 60 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 133.5278 99.586 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at -0.0869 -0.8382 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 90 "Net-(C27-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 117.856 99.6622 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0.0254 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 52 "Net-(C23-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 145.2372 99.6081 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -0.0508 -1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 19 "Net-(C14-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 99 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 128.4732 115.588 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R63"
			(at 0 -0.1524 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 34 "Net-(U2-PIN11)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 68 "Net-(C42-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 94.488 94.4298 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0.0762 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4K_uD_filterboard_V3.24.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 47 "Net-(U1-PIN1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 61 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 78.74 127.838)
		(end 80.01 129.108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.64 82.118)
		(end 166.37 80.848)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.37 129.108)
		(end 167.64 127.838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.01 129.108)
		(end 166.37 129.108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.74 82.118)
		(end 78.74 127.838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.64 127.838)
		(end 167.64 82.118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.01 80.848)
		(end 78.74 82.118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.37 80.848)
		(end 80.01 80.848)
		(layer "Edge.Cuts")
	)
	(gr_text "V3.24"
		(at 156.0576 88.4682 0)
		(layer "F.SilkS")
	)
	(gr_text "DC Ground Plane\nFilter Board V3.24\n2025-09-18"
		(at 79.4004 88.6714 0)
		(layer "F.SilkS")
	)
	(gr_text "DC FILTER"
		(at 93.6244 84.074 0)
		(layer "F.SilkS")
	)
	(gr_text "BOARD"
		(at 125.8316 84.2264 0)
		(layer "F.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 78.7195 81.1565) (xy 167.6449 81.153)
		)
		(height -6.9088)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.501"
			(at 123.1822 72.4477 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 78.74 128.143) (xy 80.01 129.413)
		)
		(height 6.9631)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.05)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.05"
			(at 79.375 133.9561 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 78.7195 81.1565) (xy 78.7449 129.416502)
		)
		(height -13.2588)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "1.9"
			(at 63.6607 105.286501 90)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.64 127.838) (xy 166.37 129.108) (xy 80.01 129.108) (xy 78.74 127.838) (xy 78.74 125.0694)
				(xy 167.64 125.0694)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.7407 82.1175) (xy 80.0107 80.8475) (xy 166.3707 80.8475) (xy 167.6407 82.1175) (xy 167.64 84.8868)
				(xy 78.74 84.8868)
			)
		)
	)
	(zone
		(net 99)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.3707 80.8475) (xy 167.6407 82.1175) (xy 167.64 127.838) (xy 166.37 129.108) (xy 80.01 129.108)
				(xy 78.74 127.838) (xy 78.7407 82.1175) (xy 80.0107 80.8475)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Mask")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 78.714919 129.111702) (xy 78.7146 125.073102) (xy 167.64 125.073102) (xy 167.64 129.111702)
				(xy 78.7146 129.111702)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Mask")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 78.7449 84.8868) (xy 78.7195 80.8482) (xy 167.6449 80.8482) (xy 167.6449 84.8868) (xy 78.7195 84.8868)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.64 127.838) (xy 166.37 129.108) (xy 80.01 129.108) (xy 78.74 127.838) (xy 78.74 125.0696)
				(xy 167.64 125.0696)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.74 82.118) (xy 80.01 80.848) (xy 166.37 80.848) (xy 167.64 82.118) (xy 167.64 84.8866) (xy 78.74 84.8866)
			)
		)
	)
	(zone
		(net 99)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.37 80.848) (xy 167.64 82.118) (xy 167.64 127.838) (xy 166.37 129.108) (xy 80.01 129.108)
				(xy 78.74 127.838) (xy 78.74 82.118) (xy 80.01 80.848)
			)
		)
	)
	(zone
		(net 99)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 80.01 80.8482) (xy 78.74 82.1182) (xy 78.74 127.8382) (xy 80.01 129.1082) (xy 166.37 129.1082)
				(xy 167.64 127.8382) (xy 167.64 82.1182) (xy 166.37 80.8482)
			)
		)
	)
	(zone
		(net 99)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 78.74 82.1182) (xy 80.01 80.8482) (xy 166.37 80.8482) (xy 167.64 82.1182) (xy 167.64 127.8382)
				(xy 166.37 129.1082) (xy 80.01 129.1082) (xy 78.74 127.8382)
			)
		)
	)
	(embedded_fonts no)
)
