(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 57)
    (no_connects 0)
    (area 103.424999 80.424999 178.075001 104.075001)
    (thickness 1.6)
    (drawings 28)
    (tracks 219)
    (zones 0)
    (modules 28)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 5)
    (trace_clearance 0.4)
    (zone_clearance 0.5)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.5 0.6)
    (user_via 2 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010b0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C_HG1-Pad2)")
  (net 4 "Net-(C_OUT1-Pad1)")
  (net 5 "Net-(C_TMR1-Pad1)")
  (net 6 "Net-(D3-Pad1)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(D5-Pad2)")
  (net 9 "Net-(J_TEST1-Pad1)")
  (net 10 "Net-(J_TEST1-Pad2)")
  (net 11 "Net-(M1-Pad1)")
  (net 12 "Net-(M1-Pad3)")
  (net 13 "Net-(M2-Pad1)")
  (net 14 "Net-(M2-Pad2)")
  (net 15 "Net-(R1-Pad2)")
  (net 16 "Net-(R2-Pad2)")
  (net 17 "Net-(R7-Pad2)")
  (net 18 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C_HG1-Pad2)")
    (add_net "Net-(C_OUT1-Pad1)")
    (add_net "Net-(C_TMR1-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(J_TEST1-Pad1)")
    (add_net "Net-(J_TEST1-Pad2)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M2-Pad1)")
    (add_net "Net-(M2-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R7-Pad2)")
  )
  (module SMD_Packages:SO-16-N (layer F.Cu) (tedit 59D167BB)
    (at 155.448 98.298 180)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 3.81 4.699 180) (layer F.SilkS))
    (fp_text value LTC4364 (at 0 1.27 180) (layer F.Fab))
    (pad 16 smd rect (at -4.445 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R7-Pad2)"))
    (pad 14 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J_TEST1-Pad1)"))
    (pad 13 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J_TEST1-Pad2)"))
    (pad 12 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 10 smd rect (at 3.175 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (pad 9 smd rect (at 4.445 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 8 smd rect (at 4.445 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 3.175 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (pad 5 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(M1-Pad3)"))
    (pad 4 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(M2-Pad1)"))
    (pad 3 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.175 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M2-Pad2)"))
    (pad 1 smd rect (at -4.445 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_OUT1-Pad1)"))
    (pad 15 smd rect (at -3.175 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C_TMR1-Pad1)"))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.3 (layer F.Cu) (tedit 59D16A18)
    (at 159.766 85.598 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C_OUT1 (at 0.635 -3.937 90) (layer F.SilkS))
    (fp_text value 22uF (at 0 -4.56 90) (layer F.Fab))
    (fp_text user + (at -1.75 -0.08 90) (layer F.Fab))
    (fp_text user + (at -3.937 -3.175 90) (layer F.SilkS))
    (fp_text user %R (at 0 4.56 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_OUT1-Pad1)"))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59D16754)
    (at 148.59 95.758 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.413 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59D16733)
    (at 139.7 96.012)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C_HG1 (at -2.794 -1.27 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C_HG1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59D167B4)
    (at 157.607 102.997 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C_TMR1 (at 4.572 -0.127 180) (layer F.SilkS))
    (fp_text value 6.8nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C_TMR1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 59D1674E)
    (at 146.304 96.266 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value "MMSZ5266 68V" (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P12.70mm_Horizontal (layer F.Cu) (tedit 59D1670E)
    (at 121.666 96.266)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 12.7mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D3 (at 0 -2.413) (layer F.SilkS))
    (fp_text value 1.5KE200A (at 6.35 3.66) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 115.824 95.25 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D4 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value SMAJ24A (at 0 2.6 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer F.Cu) (tedit 59D16742)
    (at 142.494 95.25 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at 2.032 -0.127 180) (layer F.SilkS))
    (fp_text value 1N4148W (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C_HG1-Pad2)"))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pcm:pad_bullet (layer F.Cu) (tedit 59D169EF)
    (at 114.808 87.122)
    (fp_text reference J_IN1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
  )
  (module pcm:xt60 (layer F.Cu) (tedit 59D169F2)
    (at 166.878 87.122 180)
    (fp_text reference J_OUT1 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 -0.5 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -3 180) (size 5 5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_OUT1-Pad1)"))
    (pad 2 smd rect (at 0 3 180) (size 5 5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59D167A7)
    (at 167.64 101.092 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J_TEST1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J_TEST1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J_TEST1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-263-2 (layer F.Cu) (tedit 59D167CA)
    (at 128.778 87.122 180)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference M1 (at -5.461 4.445 180) (layer F.SilkS))
    (fp_text value FDB33N25 (at 0 6.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -2.54 180) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(M1-Pad1)"))
    (pad 3 smd rect (at -5.775 2.54 180) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(M1-Pad3)"))
    (pad 2 smd rect (at 3.375 0 180) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 5.8 2.775 180) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.95 -2.775 180) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 5.8 -2.775 180) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.95 2.775 180) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 7 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-263-2 (layer F.Cu) (tedit 59D167C4)
    (at 147.066 87.122)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference M2 (at -5.461 -4.445) (layer F.SilkS))
    (fp_text value FDB3682 (at 0 6.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(M2-Pad1)"))
    (pad 3 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(M1-Pad3)"))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 14 "Net-(M2-Pad2)"))
    (pad 2 smd rect (at 5.8 2.775) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 14 "Net-(M2-Pad2)"))
    (pad 2 smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 14 "Net-(M2-Pad2)"))
    (pad 2 smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 14 "Net-(M2-Pad2)"))
    (pad 2 smd rect (at 0.95 2.775) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 14 "Net-(M2-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D16719)
    (at 138.684 100.076)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.921 0) (layer F.SilkS))
    (fp_text value 115k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D1671C)
    (at 138.684 101.854 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.921 0 180) (layer F.SilkS))
    (fp_text value 2k (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 148.59 100.584 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59D1673B)
    (at 139.954 98.044)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -4.064 0.381) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D16729)
    (at 139.7 94.488)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.27 -1.397) (layer F.SilkS))
    (fp_text value 10R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(M1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D16747)
    (at 144.272 95.25 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C_HG1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D167E5)
    (at 163.322 100.838 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 1.143 1.143 180) (layer F.SilkS))
    (fp_text value 54.9k (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_OUT1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D167ED)
    (at 163.322 102.616)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.667 0.381) (layer F.SilkS))
    (fp_text value 4.99k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D167A1)
    (at 164.592 96.012 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 2.54 -0.254 360) (layer F.SilkS))
    (fp_text value 0R (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J_TEST1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D1679C)
    (at 162.814 96.012 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 2.54 0.381 360) (layer F.SilkS))
    (fp_text value 0R (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J_TEST1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pcm:trimmer (layer F.Cu) (tedit 59D16722)
    (at 144.526 101.092 90)
    (fp_text reference RV1 (at -1.905 -2.032 180) (layer F.SilkS))
    (fp_text value 2k (at 0 -0.5 90) (layer F.Fab))
    (pad 3 smd rect (at 1.4 1.8 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.4 1.8 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0 -1.45 90) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad2)"))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 159.766 91.694 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_SNS1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 3mR (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_OUT1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 59D207A5)
    (at 108 97.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MP1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value "Mounting point" (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 59D207A8)
    (at 173.5 97.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MP2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value "Mounting point" (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (gr_line (start 169.5 92.5) (end 169.5 82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.5 93) (end 170 93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170 102) (end 173.5 102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170 102.5) (end 169.5 102.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170 92.5) (end 170 93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112 92.5) (end 112 82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.5 102) (end 108 102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.5 93) (end 108 93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 111.5 102.5) (end 111.5 102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 111.5 92.5) (end 112 92.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.5 97.5) (end 173.5 93) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 108 97.5) (end 108 102) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.5 102.5) (end 113.5 104) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168 102.5) (end 169.5 102.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168 82) (end 168 80.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.5 82) (end 112 82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text OUT (at 167.259 94.234) (layer F.SilkS))
  (gr_text - (at 163.322 81.153) (layer F.SilkS))
  (gr_text IN+ (at 119.126 87.122 90) (layer F.SilkS))
  (gr_text "Overvoltage protection : 16V\nLoad dump surge protection : 200V\nUVLO : 12.4V typ. trimmable\nShort circuit protection\nCurrent limiting : 15A\nReverse input protection" (at 168.656 88.519) (layer B.SilkS))
  (gr_text "protection circuit" (at 122.428 102.362) (layer F.SilkS))
  (gr_text "Car battery" (at 118.999 100.33) (layer F.SilkS))
  (gr_text ~FLT (at 167.64 96.393) (layer F.SilkS))
  (gr_text ENOUT (at 167.132 103.124) (layer F.SilkS))
  (gr_text + (at 163.195 89.408) (layer F.SilkS))
  (gr_line (start 168 104) (end 113.5 104) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.5 80.5) (end 168 80.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 3))
    (polygon
      (pts
        (xy 103.5 80.5) (xy 178 80.5) (xy 178 104) (xy 103.5 104)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 3))
    (polygon
      (pts
        (xy 103.5 80.5) (xy 178 80.5) (xy 178 104) (xy 103.5 104)
      )
    )
  )
)
