(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 1269)
    (no_connects 0)
    (area 14.847599 13.924999 242.575001 169.575001)
    (thickness 1.6002)
    (drawings 12)
    (tracks 6750)
    (zones 0)
    (modules 382)
    (nets 513)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.26)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 3)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.8 0.4)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0.65)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C_BOOST1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C_BOOST2-Pad1)")
  (net 4 "Net-(C_BOOST3-Pad1)")
  (net 5 "Net-(C_BOOST4-Pad1)")
  (net 6 "Net-(C_BOOST5-Pad1)")
  (net 7 "Net-(C_BOOST6-Pad1)")
  (net 8 "Net-(C_BOOST7-Pad1)")
  (net 9 "Net-(C_BOOST8-Pad1)")
  (net 10 "Net-(C_BOOST9-Pad1)")
  (net 11 "Net-(C_BOOST10-Pad1)")
  (net 12 "Net-(C_BOOST11-Pad1)")
  (net 13 "Net-(C_BOOST12-Pad1)")
  (net 14 "Net-(C_BOOST13-Pad1)")
  (net 15 "Net-(C_BOOST14-Pad1)")
  (net 16 "Net-(C_BOOST15-Pad1)")
  (net 17 "Net-(C_BOOST16-Pad1)")
  (net 18 "Net-(C_BOOST17-Pad1)")
  (net 19 "Net-(C_BOOST18-Pad1)")
  (net 20 "Net-(C_BOOST19-Pad1)")
  (net 21 "Net-(C_BOOST20-Pad1)")
  (net 22 "Net-(C_BOOST21-Pad1)")
  (net 23 "Net-(C_BOOST22-Pad1)")
  (net 24 "Net-(C_BOOST23-Pad1)")
  (net 25 "Net-(C_BOOST24-Pad1)")
  (net 26 "Net-(C_BOOST25-Pad1)")
  (net 27 "Net-(C_BOOST26-Pad1)")
  (net 28 "Net-(C_BOOST27-Pad1)")
  (net 29 "Net-(C_BOOST28-Pad1)")
  (net 30 "Net-(C_BOOST29-Pad1)")
  (net 31 "Net-(C_BOOST30-Pad1)")
  (net 32 "Net-(C_BOOST31-Pad1)")
  (net 33 "Net-(C_BOOST32-Pad1)")
  (net 34 "Net-(C_BOOST33-Pad1)")
  (net 35 "Net-(C_BOOST34-Pad1)")
  (net 36 "Net-(C_BOOST35-Pad1)")
  (net 37 "Net-(C_BOOST36-Pad1)")
  (net 38 VDD)
  (net 39 "Net-(C_PUMP1-Pad2)")
  (net 40 "Net-(C_PUMP2-Pad2)")
  (net 41 "Net-(C_PUMP3-Pad2)")
  (net 42 "Net-(C_PUMP4-Pad2)")
  (net 43 "Net-(C_PUMP5-Pad2)")
  (net 44 "Net-(C_PUMP6-Pad2)")
  (net 45 "Net-(C_PUMP7-Pad2)")
  (net 46 "Net-(C_PUMP8-Pad2)")
  (net 47 "Net-(C_PUMP9-Pad2)")
  (net 48 "Net-(C_PUMP10-Pad2)")
  (net 49 "Net-(C_PUMP11-Pad2)")
  (net 50 "Net-(C_PUMP12-Pad2)")
  (net 51 "Net-(C_PUMP13-Pad2)")
  (net 52 "Net-(C_PUMP14-Pad2)")
  (net 53 "Net-(C_PUMP15-Pad2)")
  (net 54 "Net-(C_PUMP16-Pad2)")
  (net 55 "Net-(C_PUMP17-Pad2)")
  (net 56 "Net-(C_PUMP18-Pad2)")
  (net 57 "Net-(C_PUMP19-Pad2)")
  (net 58 "Net-(C_PUMP20-Pad2)")
  (net 59 "Net-(C_PUMP21-Pad2)")
  (net 60 "Net-(C_PUMP22-Pad2)")
  (net 61 "Net-(C_PUMP23-Pad2)")
  (net 62 "Net-(C_PUMP24-Pad2)")
  (net 63 "Net-(C_PUMP25-Pad2)")
  (net 64 "Net-(C_PUMP26-Pad2)")
  (net 65 "Net-(C_PUMP27-Pad2)")
  (net 66 "Net-(C_PUMP28-Pad2)")
  (net 67 "Net-(C_PUMP29-Pad2)")
  (net 68 "Net-(C_PUMP30-Pad2)")
  (net 69 "Net-(C_PUMP31-Pad2)")
  (net 70 "Net-(C_PUMP32-Pad2)")
  (net 71 "Net-(C_PUMP33-Pad2)")
  (net 72 "Net-(C_PUMP34-Pad2)")
  (net 73 "Net-(C_PUMP35-Pad2)")
  (net 74 "Net-(C_PUMP36-Pad2)")
  (net 75 "Net-(C_REG1-Pad1)")
  (net 76 "Net-(C_REG2-Pad1)")
  (net 77 "Net-(C_REG3-Pad1)")
  (net 78 "Net-(C_REG4-Pad1)")
  (net 79 "Net-(C_REG5-Pad1)")
  (net 80 "Net-(C_REG6-Pad1)")
  (net 81 "Net-(C_REG7-Pad1)")
  (net 82 "Net-(C_REG8-Pad1)")
  (net 83 "Net-(C_REG9-Pad1)")
  (net 84 "Net-(C_REG10-Pad1)")
  (net 85 "Net-(C_REG11-Pad1)")
  (net 86 "Net-(C_REG12-Pad1)")
  (net 87 "Net-(C_REG13-Pad1)")
  (net 88 "Net-(C_REG14-Pad1)")
  (net 89 "Net-(C_REG15-Pad1)")
  (net 90 "Net-(C_REG16-Pad1)")
  (net 91 "Net-(C_REG17-Pad1)")
  (net 92 "Net-(C_REG18-Pad1)")
  (net 93 "Net-(C_REG19-Pad1)")
  (net 94 "Net-(C_REG20-Pad1)")
  (net 95 "Net-(C_REG21-Pad1)")
  (net 96 "Net-(C_REG22-Pad1)")
  (net 97 "Net-(C_REG23-Pad1)")
  (net 98 "Net-(C_REG24-Pad1)")
  (net 99 "Net-(C_REG25-Pad1)")
  (net 100 "Net-(C_REG26-Pad1)")
  (net 101 "Net-(C_REG27-Pad1)")
  (net 102 "Net-(C_REG28-Pad1)")
  (net 103 "Net-(C_REG29-Pad1)")
  (net 104 "Net-(C_REG30-Pad1)")
  (net 105 "Net-(C_REG31-Pad1)")
  (net 106 "Net-(C_REG32-Pad1)")
  (net 107 "Net-(C_REG33-Pad1)")
  (net 108 "Net-(C_REG34-Pad1)")
  (net 109 "Net-(C_REG35-Pad1)")
  (net 110 "Net-(C_REG36-Pad1)")
  (net 111 OUT36+)
  (net 112 OUT35+)
  (net 113 OUT34+)
  (net 114 OUT33+)
  (net 115 OUT32+)
  (net 116 OUT31+)
  (net 117 OUT30+)
  (net 118 OUT29+)
  (net 119 OUT28+)
  (net 120 OUT27+)
  (net 121 OUT26+)
  (net 122 OUT25+)
  (net 123 OUT24+)
  (net 124 OUT23+)
  (net 125 OUT22+)
  (net 126 OUT21+)
  (net 127 OUT20+)
  (net 128 OUT19+)
  (net 129 OUT18+)
  (net 130 OUT17+)
  (net 131 OUT16+)
  (net 132 OUT15+)
  (net 133 OUT14+)
  (net 134 OUT13+)
  (net 135 OUT12+)
  (net 136 OUT11+)
  (net 137 OUT10+)
  (net 138 OUT9+)
  (net 139 OUT8+)
  (net 140 OUT7+)
  (net 141 OUT6+)
  (net 142 OUT5+)
  (net 143 OUT4+)
  (net 144 OUT3+)
  (net 145 OUT2+)
  (net 146 OUT1+)
  (net 147 "Net-(J3-Pad1)")
  (net 148 "Net-(J3-Pad2)")
  (net 149 OUT36-)
  (net 150 OUT35-)
  (net 151 OUT34-)
  (net 152 OUT33-)
  (net 153 OUT32-)
  (net 154 OUT31-)
  (net 155 OUT30-)
  (net 156 OUT29-)
  (net 157 OUT28-)
  (net 158 OUT27-)
  (net 159 OUT26-)
  (net 160 OUT25-)
  (net 161 OUT24-)
  (net 162 OUT23-)
  (net 163 OUT22-)
  (net 164 OUT21-)
  (net 165 OUT20-)
  (net 166 OUT19-)
  (net 167 OUT18-)
  (net 168 OUT17-)
  (net 169 OUT16-)
  (net 170 OUT15-)
  (net 171 OUT14-)
  (net 172 OUT13-)
  (net 173 OUT12-)
  (net 174 OUT11-)
  (net 175 OUT10-)
  (net 176 OUT9-)
  (net 177 OUT8-)
  (net 178 OUT7-)
  (net 179 OUT6-)
  (net 180 OUT5-)
  (net 181 OUT4-)
  (net 182 OUT3-)
  (net 183 OUT2-)
  (net 184 OUT1-)
  (net 185 "Net-(L_SMALL1-Pad1)")
  (net 186 "Net-(L_SMALL2-Pad1)")
  (net 187 "Net-(L_SMALL3-Pad1)")
  (net 188 "Net-(L_SMALL4-Pad1)")
  (net 189 "Net-(L_SMALL5-Pad1)")
  (net 190 "Net-(L_SMALL6-Pad1)")
  (net 191 "Net-(L_SMALL7-Pad1)")
  (net 192 "Net-(L_SMALL8-Pad1)")
  (net 193 "Net-(L_SMALL9-Pad1)")
  (net 194 "Net-(L_SMALL10-Pad1)")
  (net 195 "Net-(L_SMALL11-Pad1)")
  (net 196 "Net-(L_SMALL12-Pad1)")
  (net 197 "Net-(L_SMALL13-Pad1)")
  (net 198 "Net-(L_SMALL14-Pad1)")
  (net 199 "Net-(L_SMALL15-Pad1)")
  (net 200 "Net-(L_SMALL16-Pad1)")
  (net 201 "Net-(L_SMALL17-Pad1)")
  (net 202 "Net-(L_SMALL18-Pad1)")
  (net 203 "Net-(L_SMALL19-Pad1)")
  (net 204 "Net-(L_SMALL20-Pad1)")
  (net 205 "Net-(L_SMALL21-Pad1)")
  (net 206 "Net-(L_SMALL22-Pad1)")
  (net 207 "Net-(L_SMALL23-Pad1)")
  (net 208 "Net-(L_SMALL24-Pad1)")
  (net 209 "Net-(L_SMALL25-Pad1)")
  (net 210 "Net-(L_SMALL26-Pad1)")
  (net 211 "Net-(L_SMALL27-Pad1)")
  (net 212 "Net-(L_SMALL28-Pad1)")
  (net 213 "Net-(L_SMALL29-Pad1)")
  (net 214 "Net-(L_SMALL30-Pad1)")
  (net 215 "Net-(L_SMALL31-Pad1)")
  (net 216 "Net-(L_SMALL32-Pad1)")
  (net 217 "Net-(L_SMALL33-Pad1)")
  (net 218 "Net-(L_SMALL34-Pad1)")
  (net 219 "Net-(L_SMALL35-Pad1)")
  (net 220 "Net-(L_SMALL36-Pad1)")
  (net 221 "Net-(R_1-Pad1)")
  (net 222 "Net-(R_2-Pad1)")
  (net 223 "Net-(R_3-Pad1)")
  (net 224 "Net-(R_10-Pad2)")
  (net 225 "Net-(R_11-Pad2)")
  (net 226 "Net-(R_12-Pad2)")
  (net 227 "Net-(R_13-Pad1)")
  (net 228 "Net-(R_14-Pad1)")
  (net 229 "Net-(R_15-Pad1)")
  (net 230 "Net-(R_16-Pad1)")
  (net 231 "Net-(R_17-Pad1)")
  (net 232 "Net-(R_18-Pad1)")
  (net 233 "Net-(R_25-Pad1)")
  (net 234 "Net-(R_26-Pad1)")
  (net 235 "Net-(R_27-Pad1)")
  (net 236 "Net-(R_28-Pad1)")
  (net 237 "Net-(R_29-Pad1)")
  (net 238 "Net-(R_30-Pad1)")
  (net 239 "Net-(R_37-Pad1)")
  (net 240 "Net-(R_38-Pad1)")
  (net 241 "Net-(R_39-Pad1)")
  (net 242 "Net-(R_40-Pad1)")
  (net 243 "Net-(R_41-Pad1)")
  (net 244 "Net-(R_42-Pad1)")
  (net 245 "Net-(R_49-Pad1)")
  (net 246 "Net-(R_50-Pad1)")
  (net 247 "Net-(R_51-Pad1)")
  (net 248 "Net-(R_52-Pad1)")
  (net 249 "Net-(R_53-Pad1)")
  (net 250 "Net-(R_54-Pad1)")
  (net 251 "Net-(R_61-Pad1)")
  (net 252 "Net-(R_62-Pad1)")
  (net 253 "Net-(R_63-Pad1)")
  (net 254 "Net-(R_64-Pad1)")
  (net 255 "Net-(R_65-Pad1)")
  (net 256 "Net-(R_66-Pad1)")
  (net 257 "Net-(R_REXT1-Pad1)")
  (net 258 "Net-(R_REXT2-Pad1)")
  (net 259 "Net-(R_REXT3-Pad1)")
  (net 260 "Net-(R_REXT4-Pad1)")
  (net 261 "Net-(R_REXT5-Pad1)")
  (net 262 "Net-(R_REXT6-Pad1)")
  (net 263 "Net-(R_REXT7-Pad1)")
  (net 264 "Net-(R_REXT8-Pad1)")
  (net 265 "Net-(R_REXT9-Pad1)")
  (net 266 "Net-(R_REXT10-Pad1)")
  (net 267 "Net-(R_REXT11-Pad1)")
  (net 268 "Net-(R_REXT12-Pad1)")
  (net 269 "Net-(R_REXT13-Pad1)")
  (net 270 "Net-(R_REXT14-Pad1)")
  (net 271 "Net-(R_REXT15-Pad1)")
  (net 272 "Net-(R_REXT16-Pad1)")
  (net 273 "Net-(R_REXT17-Pad1)")
  (net 274 "Net-(R_REXT18-Pad1)")
  (net 275 "Net-(R_REXT19-Pad1)")
  (net 276 "Net-(R_REXT20-Pad1)")
  (net 277 "Net-(R_REXT21-Pad1)")
  (net 278 "Net-(R_REXT22-Pad1)")
  (net 279 "Net-(R_REXT23-Pad1)")
  (net 280 "Net-(R_REXT24-Pad1)")
  (net 281 "Net-(R_REXT25-Pad1)")
  (net 282 "Net-(R_REXT26-Pad1)")
  (net 283 "Net-(R_REXT27-Pad1)")
  (net 284 "Net-(R_REXT28-Pad1)")
  (net 285 "Net-(R_REXT29-Pad1)")
  (net 286 "Net-(R_REXT30-Pad1)")
  (net 287 "Net-(R_REXT31-Pad1)")
  (net 288 "Net-(R_REXT32-Pad1)")
  (net 289 "Net-(R_REXT33-Pad1)")
  (net 290 "Net-(R_REXT34-Pad1)")
  (net 291 "Net-(R_REXT35-Pad1)")
  (net 292 "Net-(R_REXT36-Pad1)")
  (net 293 SDA1)
  (net 294 SCL1)
  (net 295 SDA2)
  (net 296 SCL2)
  (net 297 SDA3)
  (net 298 SCL3)
  (net 299 SDA4)
  (net 300 SCL4)
  (net 301 SDA5)
  (net 302 SCL5)
  (net 303 SDA6)
  (net 304 SCL6)
  (net 305 "Net-(U1-Pad14)")
  (net 306 "Net-(U1-Pad15)")
  (net 307 "Net-(U1-Pad16)")
  (net 308 "Net-(U1-Pad17)")
  (net 309 SDA7)
  (net 310 SCL7)
  (net 311 SDA8)
  (net 312 SCL8)
  (net 313 SDA9)
  (net 314 SCL9)
  (net 315 SDA10)
  (net 316 SCL10)
  (net 317 SDA11)
  (net 318 SCL11)
  (net 319 SDA12)
  (net 320 SCL12)
  (net 321 "Net-(U2-Pad14)")
  (net 322 "Net-(U2-Pad15)")
  (net 323 "Net-(U2-Pad16)")
  (net 324 "Net-(U2-Pad17)")
  (net 325 SDA13)
  (net 326 SCL13)
  (net 327 SDA14)
  (net 328 SCL14)
  (net 329 SDA15)
  (net 330 SCL15)
  (net 331 SDA16)
  (net 332 SCL16)
  (net 333 SDA17)
  (net 334 SCL17)
  (net 335 SDA18)
  (net 336 SCL18)
  (net 337 "Net-(U3-Pad14)")
  (net 338 "Net-(U3-Pad15)")
  (net 339 "Net-(U3-Pad16)")
  (net 340 "Net-(U3-Pad17)")
  (net 341 SDA19)
  (net 342 SCL19)
  (net 343 SDA20)
  (net 344 SCL20)
  (net 345 SDA21)
  (net 346 SCL21)
  (net 347 SDA22)
  (net 348 SCL22)
  (net 349 SDA23)
  (net 350 SCL23)
  (net 351 SDA24)
  (net 352 SCL24)
  (net 353 "Net-(U4-Pad14)")
  (net 354 "Net-(U4-Pad15)")
  (net 355 "Net-(U4-Pad16)")
  (net 356 "Net-(U4-Pad17)")
  (net 357 SDA25)
  (net 358 SCL25)
  (net 359 SDA26)
  (net 360 SCL26)
  (net 361 SDA27)
  (net 362 SCL27)
  (net 363 SDA28)
  (net 364 SCL28)
  (net 365 SDA29)
  (net 366 SCL29)
  (net 367 SDA30)
  (net 368 SCL30)
  (net 369 "Net-(U5-Pad14)")
  (net 370 "Net-(U5-Pad15)")
  (net 371 "Net-(U5-Pad16)")
  (net 372 "Net-(U5-Pad17)")
  (net 373 SDA31)
  (net 374 SCL31)
  (net 375 SDA32)
  (net 376 SCL32)
  (net 377 SDA33)
  (net 378 SCL33)
  (net 379 SDA34)
  (net 380 SCL34)
  (net 381 SDA35)
  (net 382 SCL35)
  (net 383 SDA36)
  (net 384 SCL36)
  (net 385 "Net-(U6-Pad14)")
  (net 386 "Net-(U6-Pad15)")
  (net 387 "Net-(U6-Pad16)")
  (net 388 "Net-(U6-Pad17)")
  (net 389 "Net-(U7-Pad15)")
  (net 390 "Net-(U8-Pad13)")
  (net 391 "Net-(U8-Pad14)")
  (net 392 "Net-(U8-Pad15)")
  (net 393 "Net-(U9-Pad13)")
  (net 394 "Net-(U9-Pad14)")
  (net 395 "Net-(U9-Pad15)")
  (net 396 "Net-(U10-Pad13)")
  (net 397 "Net-(U10-Pad14)")
  (net 398 "Net-(U10-Pad15)")
  (net 399 "Net-(U11-Pad13)")
  (net 400 "Net-(U11-Pad14)")
  (net 401 "Net-(U11-Pad15)")
  (net 402 "Net-(U12-Pad13)")
  (net 403 "Net-(U12-Pad14)")
  (net 404 "Net-(U12-Pad15)")
  (net 405 "Net-(U13-Pad9)")
  (net 406 "Net-(U13-Pad16)")
  (net 407 "Net-(U13-Pad17)")
  (net 408 "Net-(U14-Pad9)")
  (net 409 "Net-(U14-Pad16)")
  (net 410 "Net-(U14-Pad17)")
  (net 411 "Net-(U15-Pad9)")
  (net 412 "Net-(U15-Pad16)")
  (net 413 "Net-(U15-Pad17)")
  (net 414 "Net-(U16-Pad9)")
  (net 415 "Net-(U16-Pad16)")
  (net 416 "Net-(U16-Pad17)")
  (net 417 "Net-(U17-Pad9)")
  (net 418 "Net-(U17-Pad16)")
  (net 419 "Net-(U17-Pad17)")
  (net 420 "Net-(U18-Pad9)")
  (net 421 "Net-(U18-Pad16)")
  (net 422 "Net-(U18-Pad17)")
  (net 423 "Net-(U19-Pad9)")
  (net 424 "Net-(U19-Pad16)")
  (net 425 "Net-(U19-Pad17)")
  (net 426 "Net-(U20-Pad9)")
  (net 427 "Net-(U20-Pad16)")
  (net 428 "Net-(U20-Pad17)")
  (net 429 "Net-(U21-Pad9)")
  (net 430 "Net-(U21-Pad16)")
  (net 431 "Net-(U21-Pad17)")
  (net 432 "Net-(U22-Pad9)")
  (net 433 "Net-(U22-Pad16)")
  (net 434 "Net-(U22-Pad17)")
  (net 435 "Net-(U23-Pad9)")
  (net 436 "Net-(U23-Pad16)")
  (net 437 "Net-(U23-Pad17)")
  (net 438 "Net-(U24-Pad9)")
  (net 439 "Net-(U24-Pad16)")
  (net 440 "Net-(U24-Pad17)")
  (net 441 "Net-(U25-Pad9)")
  (net 442 "Net-(U25-Pad16)")
  (net 443 "Net-(U25-Pad17)")
  (net 444 "Net-(U26-Pad9)")
  (net 445 "Net-(U26-Pad16)")
  (net 446 "Net-(U26-Pad17)")
  (net 447 "Net-(U27-Pad9)")
  (net 448 "Net-(U27-Pad16)")
  (net 449 "Net-(U27-Pad17)")
  (net 450 "Net-(U28-Pad9)")
  (net 451 "Net-(U28-Pad16)")
  (net 452 "Net-(U28-Pad17)")
  (net 453 "Net-(U29-Pad9)")
  (net 454 "Net-(U29-Pad16)")
  (net 455 "Net-(U29-Pad17)")
  (net 456 "Net-(U30-Pad9)")
  (net 457 "Net-(U30-Pad16)")
  (net 458 "Net-(U30-Pad17)")
  (net 459 "Net-(U31-Pad9)")
  (net 460 "Net-(U31-Pad16)")
  (net 461 "Net-(U31-Pad17)")
  (net 462 "Net-(U32-Pad9)")
  (net 463 "Net-(U32-Pad16)")
  (net 464 "Net-(U32-Pad17)")
  (net 465 "Net-(U33-Pad9)")
  (net 466 "Net-(U33-Pad16)")
  (net 467 "Net-(U33-Pad17)")
  (net 468 "Net-(U34-Pad9)")
  (net 469 "Net-(U34-Pad16)")
  (net 470 "Net-(U34-Pad17)")
  (net 471 "Net-(U35-Pad9)")
  (net 472 "Net-(U35-Pad16)")
  (net 473 "Net-(U35-Pad17)")
  (net 474 "Net-(U36-Pad9)")
  (net 475 "Net-(U36-Pad16)")
  (net 476 "Net-(U36-Pad17)")
  (net 477 "Net-(U37-Pad9)")
  (net 478 "Net-(U37-Pad16)")
  (net 479 "Net-(U37-Pad17)")
  (net 480 "Net-(U38-Pad9)")
  (net 481 "Net-(U38-Pad16)")
  (net 482 "Net-(U38-Pad17)")
  (net 483 "Net-(U39-Pad9)")
  (net 484 "Net-(U39-Pad16)")
  (net 485 "Net-(U39-Pad17)")
  (net 486 "Net-(U40-Pad9)")
  (net 487 "Net-(U40-Pad16)")
  (net 488 "Net-(U40-Pad17)")
  (net 489 "Net-(U41-Pad9)")
  (net 490 "Net-(U41-Pad16)")
  (net 491 "Net-(U41-Pad17)")
  (net 492 "Net-(U42-Pad9)")
  (net 493 "Net-(U42-Pad16)")
  (net 494 "Net-(U42-Pad17)")
  (net 495 "Net-(U43-Pad9)")
  (net 496 "Net-(U43-Pad16)")
  (net 497 "Net-(U43-Pad17)")
  (net 498 "Net-(U44-Pad9)")
  (net 499 "Net-(U44-Pad16)")
  (net 500 "Net-(U44-Pad17)")
  (net 501 "Net-(U45-Pad9)")
  (net 502 "Net-(U45-Pad16)")
  (net 503 "Net-(U45-Pad17)")
  (net 504 "Net-(U46-Pad9)")
  (net 505 "Net-(U46-Pad16)")
  (net 506 "Net-(U46-Pad17)")
  (net 507 "Net-(U47-Pad9)")
  (net 508 "Net-(U47-Pad16)")
  (net 509 "Net-(U47-Pad17)")
  (net 510 "Net-(U48-Pad9)")
  (net 511 "Net-(U48-Pad16)")
  (net 512 "Net-(U48-Pad17)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.26)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(C_BOOST1-Pad1)")
    (add_net "Net-(C_BOOST10-Pad1)")
    (add_net "Net-(C_BOOST11-Pad1)")
    (add_net "Net-(C_BOOST12-Pad1)")
    (add_net "Net-(C_BOOST13-Pad1)")
    (add_net "Net-(C_BOOST14-Pad1)")
    (add_net "Net-(C_BOOST15-Pad1)")
    (add_net "Net-(C_BOOST16-Pad1)")
    (add_net "Net-(C_BOOST17-Pad1)")
    (add_net "Net-(C_BOOST18-Pad1)")
    (add_net "Net-(C_BOOST19-Pad1)")
    (add_net "Net-(C_BOOST2-Pad1)")
    (add_net "Net-(C_BOOST20-Pad1)")
    (add_net "Net-(C_BOOST21-Pad1)")
    (add_net "Net-(C_BOOST22-Pad1)")
    (add_net "Net-(C_BOOST23-Pad1)")
    (add_net "Net-(C_BOOST24-Pad1)")
    (add_net "Net-(C_BOOST25-Pad1)")
    (add_net "Net-(C_BOOST26-Pad1)")
    (add_net "Net-(C_BOOST27-Pad1)")
    (add_net "Net-(C_BOOST28-Pad1)")
    (add_net "Net-(C_BOOST29-Pad1)")
    (add_net "Net-(C_BOOST3-Pad1)")
    (add_net "Net-(C_BOOST30-Pad1)")
    (add_net "Net-(C_BOOST31-Pad1)")
    (add_net "Net-(C_BOOST32-Pad1)")
    (add_net "Net-(C_BOOST33-Pad1)")
    (add_net "Net-(C_BOOST34-Pad1)")
    (add_net "Net-(C_BOOST35-Pad1)")
    (add_net "Net-(C_BOOST36-Pad1)")
    (add_net "Net-(C_BOOST4-Pad1)")
    (add_net "Net-(C_BOOST5-Pad1)")
    (add_net "Net-(C_BOOST6-Pad1)")
    (add_net "Net-(C_BOOST7-Pad1)")
    (add_net "Net-(C_BOOST8-Pad1)")
    (add_net "Net-(C_BOOST9-Pad1)")
    (add_net "Net-(C_PUMP1-Pad2)")
    (add_net "Net-(C_PUMP10-Pad2)")
    (add_net "Net-(C_PUMP11-Pad2)")
    (add_net "Net-(C_PUMP12-Pad2)")
    (add_net "Net-(C_PUMP13-Pad2)")
    (add_net "Net-(C_PUMP14-Pad2)")
    (add_net "Net-(C_PUMP15-Pad2)")
    (add_net "Net-(C_PUMP16-Pad2)")
    (add_net "Net-(C_PUMP17-Pad2)")
    (add_net "Net-(C_PUMP18-Pad2)")
    (add_net "Net-(C_PUMP19-Pad2)")
    (add_net "Net-(C_PUMP2-Pad2)")
    (add_net "Net-(C_PUMP20-Pad2)")
    (add_net "Net-(C_PUMP21-Pad2)")
    (add_net "Net-(C_PUMP22-Pad2)")
    (add_net "Net-(C_PUMP23-Pad2)")
    (add_net "Net-(C_PUMP24-Pad2)")
    (add_net "Net-(C_PUMP25-Pad2)")
    (add_net "Net-(C_PUMP26-Pad2)")
    (add_net "Net-(C_PUMP27-Pad2)")
    (add_net "Net-(C_PUMP28-Pad2)")
    (add_net "Net-(C_PUMP29-Pad2)")
    (add_net "Net-(C_PUMP3-Pad2)")
    (add_net "Net-(C_PUMP30-Pad2)")
    (add_net "Net-(C_PUMP31-Pad2)")
    (add_net "Net-(C_PUMP32-Pad2)")
    (add_net "Net-(C_PUMP33-Pad2)")
    (add_net "Net-(C_PUMP34-Pad2)")
    (add_net "Net-(C_PUMP35-Pad2)")
    (add_net "Net-(C_PUMP36-Pad2)")
    (add_net "Net-(C_PUMP4-Pad2)")
    (add_net "Net-(C_PUMP5-Pad2)")
    (add_net "Net-(C_PUMP6-Pad2)")
    (add_net "Net-(C_PUMP7-Pad2)")
    (add_net "Net-(C_PUMP8-Pad2)")
    (add_net "Net-(C_PUMP9-Pad2)")
    (add_net "Net-(C_REG1-Pad1)")
    (add_net "Net-(C_REG10-Pad1)")
    (add_net "Net-(C_REG11-Pad1)")
    (add_net "Net-(C_REG12-Pad1)")
    (add_net "Net-(C_REG13-Pad1)")
    (add_net "Net-(C_REG14-Pad1)")
    (add_net "Net-(C_REG15-Pad1)")
    (add_net "Net-(C_REG16-Pad1)")
    (add_net "Net-(C_REG17-Pad1)")
    (add_net "Net-(C_REG18-Pad1)")
    (add_net "Net-(C_REG19-Pad1)")
    (add_net "Net-(C_REG2-Pad1)")
    (add_net "Net-(C_REG20-Pad1)")
    (add_net "Net-(C_REG21-Pad1)")
    (add_net "Net-(C_REG22-Pad1)")
    (add_net "Net-(C_REG23-Pad1)")
    (add_net "Net-(C_REG24-Pad1)")
    (add_net "Net-(C_REG25-Pad1)")
    (add_net "Net-(C_REG26-Pad1)")
    (add_net "Net-(C_REG27-Pad1)")
    (add_net "Net-(C_REG28-Pad1)")
    (add_net "Net-(C_REG29-Pad1)")
    (add_net "Net-(C_REG3-Pad1)")
    (add_net "Net-(C_REG30-Pad1)")
    (add_net "Net-(C_REG31-Pad1)")
    (add_net "Net-(C_REG32-Pad1)")
    (add_net "Net-(C_REG33-Pad1)")
    (add_net "Net-(C_REG34-Pad1)")
    (add_net "Net-(C_REG35-Pad1)")
    (add_net "Net-(C_REG36-Pad1)")
    (add_net "Net-(C_REG4-Pad1)")
    (add_net "Net-(C_REG5-Pad1)")
    (add_net "Net-(C_REG6-Pad1)")
    (add_net "Net-(C_REG7-Pad1)")
    (add_net "Net-(C_REG8-Pad1)")
    (add_net "Net-(C_REG9-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(L_SMALL1-Pad1)")
    (add_net "Net-(L_SMALL10-Pad1)")
    (add_net "Net-(L_SMALL11-Pad1)")
    (add_net "Net-(L_SMALL12-Pad1)")
    (add_net "Net-(L_SMALL13-Pad1)")
    (add_net "Net-(L_SMALL14-Pad1)")
    (add_net "Net-(L_SMALL15-Pad1)")
    (add_net "Net-(L_SMALL16-Pad1)")
    (add_net "Net-(L_SMALL17-Pad1)")
    (add_net "Net-(L_SMALL18-Pad1)")
    (add_net "Net-(L_SMALL19-Pad1)")
    (add_net "Net-(L_SMALL2-Pad1)")
    (add_net "Net-(L_SMALL20-Pad1)")
    (add_net "Net-(L_SMALL21-Pad1)")
    (add_net "Net-(L_SMALL22-Pad1)")
    (add_net "Net-(L_SMALL23-Pad1)")
    (add_net "Net-(L_SMALL24-Pad1)")
    (add_net "Net-(L_SMALL25-Pad1)")
    (add_net "Net-(L_SMALL26-Pad1)")
    (add_net "Net-(L_SMALL27-Pad1)")
    (add_net "Net-(L_SMALL28-Pad1)")
    (add_net "Net-(L_SMALL29-Pad1)")
    (add_net "Net-(L_SMALL3-Pad1)")
    (add_net "Net-(L_SMALL30-Pad1)")
    (add_net "Net-(L_SMALL31-Pad1)")
    (add_net "Net-(L_SMALL32-Pad1)")
    (add_net "Net-(L_SMALL33-Pad1)")
    (add_net "Net-(L_SMALL34-Pad1)")
    (add_net "Net-(L_SMALL35-Pad1)")
    (add_net "Net-(L_SMALL36-Pad1)")
    (add_net "Net-(L_SMALL4-Pad1)")
    (add_net "Net-(L_SMALL5-Pad1)")
    (add_net "Net-(L_SMALL6-Pad1)")
    (add_net "Net-(L_SMALL7-Pad1)")
    (add_net "Net-(L_SMALL8-Pad1)")
    (add_net "Net-(L_SMALL9-Pad1)")
    (add_net "Net-(R_1-Pad1)")
    (add_net "Net-(R_10-Pad2)")
    (add_net "Net-(R_11-Pad2)")
    (add_net "Net-(R_12-Pad2)")
    (add_net "Net-(R_13-Pad1)")
    (add_net "Net-(R_14-Pad1)")
    (add_net "Net-(R_15-Pad1)")
    (add_net "Net-(R_16-Pad1)")
    (add_net "Net-(R_17-Pad1)")
    (add_net "Net-(R_18-Pad1)")
    (add_net "Net-(R_2-Pad1)")
    (add_net "Net-(R_25-Pad1)")
    (add_net "Net-(R_26-Pad1)")
    (add_net "Net-(R_27-Pad1)")
    (add_net "Net-(R_28-Pad1)")
    (add_net "Net-(R_29-Pad1)")
    (add_net "Net-(R_3-Pad1)")
    (add_net "Net-(R_30-Pad1)")
    (add_net "Net-(R_37-Pad1)")
    (add_net "Net-(R_38-Pad1)")
    (add_net "Net-(R_39-Pad1)")
    (add_net "Net-(R_40-Pad1)")
    (add_net "Net-(R_41-Pad1)")
    (add_net "Net-(R_42-Pad1)")
    (add_net "Net-(R_49-Pad1)")
    (add_net "Net-(R_50-Pad1)")
    (add_net "Net-(R_51-Pad1)")
    (add_net "Net-(R_52-Pad1)")
    (add_net "Net-(R_53-Pad1)")
    (add_net "Net-(R_54-Pad1)")
    (add_net "Net-(R_61-Pad1)")
    (add_net "Net-(R_62-Pad1)")
    (add_net "Net-(R_63-Pad1)")
    (add_net "Net-(R_64-Pad1)")
    (add_net "Net-(R_65-Pad1)")
    (add_net "Net-(R_66-Pad1)")
    (add_net "Net-(R_REXT1-Pad1)")
    (add_net "Net-(R_REXT10-Pad1)")
    (add_net "Net-(R_REXT11-Pad1)")
    (add_net "Net-(R_REXT12-Pad1)")
    (add_net "Net-(R_REXT13-Pad1)")
    (add_net "Net-(R_REXT14-Pad1)")
    (add_net "Net-(R_REXT15-Pad1)")
    (add_net "Net-(R_REXT16-Pad1)")
    (add_net "Net-(R_REXT17-Pad1)")
    (add_net "Net-(R_REXT18-Pad1)")
    (add_net "Net-(R_REXT19-Pad1)")
    (add_net "Net-(R_REXT2-Pad1)")
    (add_net "Net-(R_REXT20-Pad1)")
    (add_net "Net-(R_REXT21-Pad1)")
    (add_net "Net-(R_REXT22-Pad1)")
    (add_net "Net-(R_REXT23-Pad1)")
    (add_net "Net-(R_REXT24-Pad1)")
    (add_net "Net-(R_REXT25-Pad1)")
    (add_net "Net-(R_REXT26-Pad1)")
    (add_net "Net-(R_REXT27-Pad1)")
    (add_net "Net-(R_REXT28-Pad1)")
    (add_net "Net-(R_REXT29-Pad1)")
    (add_net "Net-(R_REXT3-Pad1)")
    (add_net "Net-(R_REXT30-Pad1)")
    (add_net "Net-(R_REXT31-Pad1)")
    (add_net "Net-(R_REXT32-Pad1)")
    (add_net "Net-(R_REXT33-Pad1)")
    (add_net "Net-(R_REXT34-Pad1)")
    (add_net "Net-(R_REXT35-Pad1)")
    (add_net "Net-(R_REXT36-Pad1)")
    (add_net "Net-(R_REXT4-Pad1)")
    (add_net "Net-(R_REXT5-Pad1)")
    (add_net "Net-(R_REXT6-Pad1)")
    (add_net "Net-(R_REXT7-Pad1)")
    (add_net "Net-(R_REXT8-Pad1)")
    (add_net "Net-(R_REXT9-Pad1)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U10-Pad13)")
    (add_net "Net-(U10-Pad14)")
    (add_net "Net-(U10-Pad15)")
    (add_net "Net-(U11-Pad13)")
    (add_net "Net-(U11-Pad14)")
    (add_net "Net-(U11-Pad15)")
    (add_net "Net-(U12-Pad13)")
    (add_net "Net-(U12-Pad14)")
    (add_net "Net-(U12-Pad15)")
    (add_net "Net-(U13-Pad16)")
    (add_net "Net-(U13-Pad17)")
    (add_net "Net-(U13-Pad9)")
    (add_net "Net-(U14-Pad16)")
    (add_net "Net-(U14-Pad17)")
    (add_net "Net-(U14-Pad9)")
    (add_net "Net-(U15-Pad16)")
    (add_net "Net-(U15-Pad17)")
    (add_net "Net-(U15-Pad9)")
    (add_net "Net-(U16-Pad16)")
    (add_net "Net-(U16-Pad17)")
    (add_net "Net-(U16-Pad9)")
    (add_net "Net-(U17-Pad16)")
    (add_net "Net-(U17-Pad17)")
    (add_net "Net-(U17-Pad9)")
    (add_net "Net-(U18-Pad16)")
    (add_net "Net-(U18-Pad17)")
    (add_net "Net-(U18-Pad9)")
    (add_net "Net-(U19-Pad16)")
    (add_net "Net-(U19-Pad17)")
    (add_net "Net-(U19-Pad9)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U20-Pad16)")
    (add_net "Net-(U20-Pad17)")
    (add_net "Net-(U20-Pad9)")
    (add_net "Net-(U21-Pad16)")
    (add_net "Net-(U21-Pad17)")
    (add_net "Net-(U21-Pad9)")
    (add_net "Net-(U22-Pad16)")
    (add_net "Net-(U22-Pad17)")
    (add_net "Net-(U22-Pad9)")
    (add_net "Net-(U23-Pad16)")
    (add_net "Net-(U23-Pad17)")
    (add_net "Net-(U23-Pad9)")
    (add_net "Net-(U24-Pad16)")
    (add_net "Net-(U24-Pad17)")
    (add_net "Net-(U24-Pad9)")
    (add_net "Net-(U25-Pad16)")
    (add_net "Net-(U25-Pad17)")
    (add_net "Net-(U25-Pad9)")
    (add_net "Net-(U26-Pad16)")
    (add_net "Net-(U26-Pad17)")
    (add_net "Net-(U26-Pad9)")
    (add_net "Net-(U27-Pad16)")
    (add_net "Net-(U27-Pad17)")
    (add_net "Net-(U27-Pad9)")
    (add_net "Net-(U28-Pad16)")
    (add_net "Net-(U28-Pad17)")
    (add_net "Net-(U28-Pad9)")
    (add_net "Net-(U29-Pad16)")
    (add_net "Net-(U29-Pad17)")
    (add_net "Net-(U29-Pad9)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U30-Pad16)")
    (add_net "Net-(U30-Pad17)")
    (add_net "Net-(U30-Pad9)")
    (add_net "Net-(U31-Pad16)")
    (add_net "Net-(U31-Pad17)")
    (add_net "Net-(U31-Pad9)")
    (add_net "Net-(U32-Pad16)")
    (add_net "Net-(U32-Pad17)")
    (add_net "Net-(U32-Pad9)")
    (add_net "Net-(U33-Pad16)")
    (add_net "Net-(U33-Pad17)")
    (add_net "Net-(U33-Pad9)")
    (add_net "Net-(U34-Pad16)")
    (add_net "Net-(U34-Pad17)")
    (add_net "Net-(U34-Pad9)")
    (add_net "Net-(U35-Pad16)")
    (add_net "Net-(U35-Pad17)")
    (add_net "Net-(U35-Pad9)")
    (add_net "Net-(U36-Pad16)")
    (add_net "Net-(U36-Pad17)")
    (add_net "Net-(U36-Pad9)")
    (add_net "Net-(U37-Pad16)")
    (add_net "Net-(U37-Pad17)")
    (add_net "Net-(U37-Pad9)")
    (add_net "Net-(U38-Pad16)")
    (add_net "Net-(U38-Pad17)")
    (add_net "Net-(U38-Pad9)")
    (add_net "Net-(U39-Pad16)")
    (add_net "Net-(U39-Pad17)")
    (add_net "Net-(U39-Pad9)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad17)")
    (add_net "Net-(U40-Pad16)")
    (add_net "Net-(U40-Pad17)")
    (add_net "Net-(U40-Pad9)")
    (add_net "Net-(U41-Pad16)")
    (add_net "Net-(U41-Pad17)")
    (add_net "Net-(U41-Pad9)")
    (add_net "Net-(U42-Pad16)")
    (add_net "Net-(U42-Pad17)")
    (add_net "Net-(U42-Pad9)")
    (add_net "Net-(U43-Pad16)")
    (add_net "Net-(U43-Pad17)")
    (add_net "Net-(U43-Pad9)")
    (add_net "Net-(U44-Pad16)")
    (add_net "Net-(U44-Pad17)")
    (add_net "Net-(U44-Pad9)")
    (add_net "Net-(U45-Pad16)")
    (add_net "Net-(U45-Pad17)")
    (add_net "Net-(U45-Pad9)")
    (add_net "Net-(U46-Pad16)")
    (add_net "Net-(U46-Pad17)")
    (add_net "Net-(U46-Pad9)")
    (add_net "Net-(U47-Pad16)")
    (add_net "Net-(U47-Pad17)")
    (add_net "Net-(U47-Pad9)")
    (add_net "Net-(U48-Pad16)")
    (add_net "Net-(U48-Pad17)")
    (add_net "Net-(U48-Pad9)")
    (add_net "Net-(U5-Pad14)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad16)")
    (add_net "Net-(U5-Pad17)")
    (add_net "Net-(U6-Pad14)")
    (add_net "Net-(U6-Pad15)")
    (add_net "Net-(U6-Pad16)")
    (add_net "Net-(U6-Pad17)")
    (add_net "Net-(U7-Pad15)")
    (add_net "Net-(U8-Pad13)")
    (add_net "Net-(U8-Pad14)")
    (add_net "Net-(U8-Pad15)")
    (add_net "Net-(U9-Pad13)")
    (add_net "Net-(U9-Pad14)")
    (add_net "Net-(U9-Pad15)")
    (add_net OUT1+)
    (add_net OUT1-)
    (add_net OUT10+)
    (add_net OUT10-)
    (add_net OUT11+)
    (add_net OUT11-)
    (add_net OUT12+)
    (add_net OUT12-)
    (add_net OUT13+)
    (add_net OUT13-)
    (add_net OUT14+)
    (add_net OUT14-)
    (add_net OUT15+)
    (add_net OUT15-)
    (add_net OUT16+)
    (add_net OUT16-)
    (add_net OUT17+)
    (add_net OUT17-)
    (add_net OUT18+)
    (add_net OUT18-)
    (add_net OUT19+)
    (add_net OUT19-)
    (add_net OUT2+)
    (add_net OUT2-)
    (add_net OUT20+)
    (add_net OUT20-)
    (add_net OUT21+)
    (add_net OUT21-)
    (add_net OUT22+)
    (add_net OUT22-)
    (add_net OUT23+)
    (add_net OUT23-)
    (add_net OUT24+)
    (add_net OUT24-)
    (add_net OUT25+)
    (add_net OUT25-)
    (add_net OUT26+)
    (add_net OUT26-)
    (add_net OUT27+)
    (add_net OUT27-)
    (add_net OUT28+)
    (add_net OUT28-)
    (add_net OUT29+)
    (add_net OUT29-)
    (add_net OUT3+)
    (add_net OUT3-)
    (add_net OUT30+)
    (add_net OUT30-)
    (add_net OUT31+)
    (add_net OUT31-)
    (add_net OUT32+)
    (add_net OUT32-)
    (add_net OUT33+)
    (add_net OUT33-)
    (add_net OUT34+)
    (add_net OUT34-)
    (add_net OUT35+)
    (add_net OUT35-)
    (add_net OUT36+)
    (add_net OUT36-)
    (add_net OUT4+)
    (add_net OUT4-)
    (add_net OUT5+)
    (add_net OUT5-)
    (add_net OUT6+)
    (add_net OUT6-)
    (add_net OUT7+)
    (add_net OUT7-)
    (add_net OUT8+)
    (add_net OUT8-)
    (add_net OUT9+)
    (add_net OUT9-)
    (add_net SCL1)
    (add_net SCL10)
    (add_net SCL11)
    (add_net SCL12)
    (add_net SCL13)
    (add_net SCL14)
    (add_net SCL15)
    (add_net SCL16)
    (add_net SCL17)
    (add_net SCL18)
    (add_net SCL19)
    (add_net SCL2)
    (add_net SCL20)
    (add_net SCL21)
    (add_net SCL22)
    (add_net SCL23)
    (add_net SCL24)
    (add_net SCL25)
    (add_net SCL26)
    (add_net SCL27)
    (add_net SCL28)
    (add_net SCL29)
    (add_net SCL3)
    (add_net SCL30)
    (add_net SCL31)
    (add_net SCL32)
    (add_net SCL33)
    (add_net SCL34)
    (add_net SCL35)
    (add_net SCL36)
    (add_net SCL4)
    (add_net SCL5)
    (add_net SCL6)
    (add_net SCL7)
    (add_net SCL8)
    (add_net SCL9)
    (add_net SDA1)
    (add_net SDA10)
    (add_net SDA11)
    (add_net SDA12)
    (add_net SDA13)
    (add_net SDA14)
    (add_net SDA15)
    (add_net SDA16)
    (add_net SDA17)
    (add_net SDA18)
    (add_net SDA19)
    (add_net SDA2)
    (add_net SDA20)
    (add_net SDA21)
    (add_net SDA22)
    (add_net SDA23)
    (add_net SDA24)
    (add_net SDA25)
    (add_net SDA26)
    (add_net SDA27)
    (add_net SDA28)
    (add_net SDA29)
    (add_net SDA3)
    (add_net SDA30)
    (add_net SDA31)
    (add_net SDA32)
    (add_net SDA33)
    (add_net SDA34)
    (add_net SDA35)
    (add_net SDA36)
    (add_net SDA4)
    (add_net SDA5)
    (add_net SDA6)
    (add_net SDA7)
    (add_net SDA8)
    (add_net SDA9)
  )
  (net_class GNDCLASS ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
  )
  (net_class VDDCLASS ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net VDD)
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 86 86.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST1 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C_BOOST1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 85.75 43 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST2 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C_BOOST2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 85.5 63.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST3 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_BOOST3-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 85.5 107.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST4 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C_BOOST4-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 85.75 129.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST5 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_BOOST5-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 84.75 151.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST6 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C_BOOST6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 109.75 86 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST7 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_BOOST7-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 109.75 42.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST8 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C_BOOST8-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 110 63.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST9 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C_BOOST9-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 110.5 108.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST10 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C_BOOST10-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 110.5 130.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST11 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C_BOOST11-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 110.75 151.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST12 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C_BOOST12-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 132.75 86.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST13 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C_BOOST13-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 133 43.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST14 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C_BOOST14-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 132.5 64.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST15 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_BOOST15-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 132.5 108.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST16 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_BOOST16-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 132.25 130.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST17 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C_BOOST17-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 133.25 152 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST18 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C_BOOST18-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 156 87.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST19 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C_BOOST19-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 154.75 43 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST20 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C_BOOST20-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 155.75 64.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST21 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C_BOOST21-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 156 108.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST22 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C_BOOST22-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 156 130.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST23 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C_BOOST23-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 155.25 152.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST24 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C_BOOST24-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 178.25 86.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST25 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C_BOOST25-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 178 42.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST26 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C_BOOST26-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 178.5 65.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST27 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C_BOOST27-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 178.5 109 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST28 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C_BOOST28-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 178 130.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST29 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C_BOOST29-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 178.75 152.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST30 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C_BOOST30-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 201 88.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST31 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C_BOOST31-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 201.5 42 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST32 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C_BOOST32-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 201.75 65.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST33 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C_BOOST33-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 201 109.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST34 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C_BOOST34-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 200.5 131 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST35 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C_BOOST35-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 201.25 152.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_BOOST36 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C_BOOST36-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 69 83.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK1 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 69 37.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK2 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 69.25 60.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK3 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 68.75 106.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK4 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 68.75 128.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK5 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 68.75 150.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK6 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 93.75 83.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK7 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 93.5 38.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK8 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 93.5 60.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK9 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 94.25 105.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK10 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 94.75 128.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK11 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 94.5 150.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK12 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 117.25 83.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK13 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 117.5 39.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK14 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 117.25 60.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK15 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 118.25 105.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK16 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 117.5 128.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK17 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 118.25 151)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK18 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 140.25 84.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK19 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 140 40)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK20 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 140.25 61.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK21 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 140.75 106.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK22 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 140 128.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK23 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 140.25 150.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK24 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 163.25 84.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK25 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 162.5 40.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK26 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 163.25 61.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK27 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 163.5 106.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK28 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 163.5 128.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK29 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 162.75 150)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK30 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 186 85.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK31 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 186 40.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK32 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 186.75 62.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK33 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 186.25 106.75)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK34 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 186.75 128.5)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK35 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x5.4 (layer F.Cu) (tedit 58AA8B87)
    (at 186.75 150.25)
    (descr "SMT capacitor, aluminium electrolytic, 8x5.4")
    (attr smd)
    (fp_text reference C_BULK36 (at 0 5.45) (layer F.SilkS))
    (fp_text value 10uF (at 0 -5.45) (layer F.Fab))
    (fp_text user + (at -1.93 -0.06) (layer F.Fab))
    (fp_text user + (at -4.72 3.85) (layer F.SilkS))
    (fp_text user %R (at 0 5.45) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 78 78.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP1 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C_PUMP1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 78 35.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP2 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C_PUMP2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 78 56 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP3 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C_PUMP3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 77 99.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP4 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C_PUMP4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 77 123 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP5 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C_PUMP5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 77 144 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP6 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C_PUMP6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 102 78.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP7 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C_PUMP7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 101.5 35.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP8 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C_PUMP8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 102 56 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP9 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C_PUMP9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 103 101 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP10 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C_PUMP10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 102.5 122.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP11 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C_PUMP11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 103 144.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP12 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C_PUMP12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 125 78.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP13 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C_PUMP13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 125 35 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP14 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C_PUMP14-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 125 56.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP15 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C_PUMP15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 125 101.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP16 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C_PUMP16-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 124.5 122.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP17 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C_PUMP17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 125.5 144.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP18 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C_PUMP18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 148 79.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP19 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C_PUMP19-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 147.5 35 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP20 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C_PUMP20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 147.5 56.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP21 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C_PUMP21-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 148 101 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP22 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C_PUMP22-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 148 123 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP23 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C_PUMP23-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 147.5 144.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP24 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C_PUMP24-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 170.5 80 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP25 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C_PUMP25-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 170.5 35.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP26 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C_PUMP26-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 170.5 57 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP27 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C_PUMP27-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 170.5 101.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP28 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C_PUMP28-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 170.5 123 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP29 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C_PUMP29-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 170.5 145 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP30 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C_PUMP30-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 193.5 81 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP31 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C_PUMP31-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 193.5 35.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP32 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C_PUMP32-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 194 58 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP33 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C_PUMP33-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 193.5 101.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP34 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C_PUMP34-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 193.5 123 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP35 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C_PUMP35-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 194 145 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_PUMP36 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C_PUMP36-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 80 78.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG1 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C_REG1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 80 35.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C_REG2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 80.5 56 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG3 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C_REG3-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 79.5 99.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG4 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C_REG4-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 79.5 123 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG5 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C_REG5-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 79 144 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG6 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C_REG6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 104.5 78.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG7 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(C_REG7-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 104 35.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG8 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C_REG8-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 104.5 56 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG9 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(C_REG9-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 105 101 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG10 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C_REG10-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 105 122.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG11 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C_REG11-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 105.5 144.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG12 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(C_REG12-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 127.5 78.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG13 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(C_REG13-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 127 35 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG14 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C_REG14-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 127 56.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG15 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(C_REG15-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 127 101.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG16 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C_REG16-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 126.5 122.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG17 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C_REG17-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 128 144.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG18 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(C_REG18-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 150 79.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG19 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(C_REG19-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 149.5 35 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG20 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(C_REG20-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 150 56.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG21 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(C_REG21-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 150.5 101 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG22 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(C_REG22-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 150.5 123 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG23 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C_REG23-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 149.5 144.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG24 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(C_REG24-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 172.5 80 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG25 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C_REG25-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 173 35.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG26 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C_REG26-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 172.5 57 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG27 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C_REG27-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 172.5 101.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG28 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C_REG28-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 172.5 123 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG29 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(C_REG29-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 173 145 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG30 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(C_REG30-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 195.5 81 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG31 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(C_REG31-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 196 35.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG32 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(C_REG32-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 196 58 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG33 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C_REG33-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 195 101.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG34 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(C_REG34-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 195 123 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG35 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C_REG35-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 58AA8408)
    (at 195.5 145 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C_REG36 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C_REG36-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 73 76 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD1 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 73.5 30 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD2 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 73 53 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD3 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 72.5 98.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD4 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 72.5 120.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD5 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 72 142 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD6 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 97.5 75 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD7 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 97.5 30.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD8 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 97 52 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD9 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 98.5 97.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD10 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 98.5 120.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD11 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 98 142.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD12 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 121 76 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD13 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 121 31 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD14 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 121 52.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD15 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 121.5 97.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD16 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 120.5 120 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD17 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 121.5 143 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD18 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 144 77 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD19 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 143.5 32 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD20 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 143.5 53 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD21 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 144.5 98 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD22 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 143.5 120.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD23 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 144 143 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD24 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 166.5 76.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD25 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 166 33 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD26 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 167 53.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD27 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 167 98.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD28 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 167 121 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD29 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 166 142.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD30 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 190 77.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD31 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 189.5 32.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD32 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 190 54.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD33 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 189.5 98.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD34 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 189.5 120.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD35 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 189.5 142.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_VDD36 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x36_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 224.75 144.25 180)
    (descr "Through hole straight pin header, 1x36, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x36 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x36_Female (at 0 91.23 180) (layer F.Fab))
    (fp_text user %R (at 0 44.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 OUT36+))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 OUT35+))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 OUT34+))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 OUT33+))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 OUT32+))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 OUT31+))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 OUT30+))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 OUT29+))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 OUT28+))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 OUT27+))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 121 OUT26+))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 OUT25+))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 123 OUT24+))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 124 OUT23+))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 OUT22+))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 OUT21+))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 OUT20+))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 OUT19+))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 OUT18+))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 OUT17+))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 OUT16+))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 132 OUT15+))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 133 OUT14+))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 134 OUT13+))
    (pad 25 thru_hole oval (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 OUT12+))
    (pad 26 thru_hole oval (at 0 63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 136 OUT11+))
    (pad 27 thru_hole oval (at 0 66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 OUT10+))
    (pad 28 thru_hole oval (at 0 68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 OUT9+))
    (pad 29 thru_hole oval (at 0 71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 139 OUT8+))
    (pad 30 thru_hole oval (at 0 73.66 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 140 OUT7+))
    (pad 31 thru_hole oval (at 0 76.2 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 141 OUT6+))
    (pad 32 thru_hole oval (at 0 78.74 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 142 OUT5+))
    (pad 33 thru_hole oval (at 0 81.28 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 OUT4+))
    (pad 34 thru_hole oval (at 0 83.82 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 144 OUT3+))
    (pad 35 thru_hole oval (at 0 86.36 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 145 OUT2+))
    (pad 36 thru_hole oval (at 0 88.9 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 146 OUT1+))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x36_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x36_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 228.75 144.25 180)
    (descr "Through hole straight pin header, 1x36, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x36 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x36_Female (at 0 91.23 180) (layer F.Fab))
    (fp_text user %R (at 0 44.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 25 thru_hole oval (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 0 63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 27 thru_hole oval (at 0 66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 28 thru_hole oval (at 0 68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 29 thru_hole oval (at 0 71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 30 thru_hole oval (at 0 73.66 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 76.2 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 32 thru_hole oval (at 0 78.74 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 33 thru_hole oval (at 0 81.28 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 34 thru_hole oval (at 0 83.82 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 86.36 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 36 thru_hole oval (at 0 88.9 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x36_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 36.75 32.5)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x36_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 232.75 144.25 180)
    (descr "Through hole straight pin header, 1x36, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x36 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x36_Female (at 0 91.23 180) (layer F.Fab))
    (fp_text user %R (at 0 44.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 149 OUT36-))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 150 OUT35-))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 151 OUT34-))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 152 OUT33-))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 153 OUT32-))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 OUT31-))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 155 OUT30-))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 156 OUT29-))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 157 OUT28-))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 158 OUT27-))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 159 OUT26-))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 160 OUT25-))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 161 OUT24-))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 162 OUT23-))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 163 OUT22-))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 164 OUT21-))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 OUT20-))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 166 OUT19-))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 167 OUT18-))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 168 OUT17-))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 169 OUT16-))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 170 OUT15-))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 OUT14-))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 172 OUT13-))
    (pad 25 thru_hole oval (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 173 OUT12-))
    (pad 26 thru_hole oval (at 0 63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 174 OUT11-))
    (pad 27 thru_hole oval (at 0 66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 175 OUT10-))
    (pad 28 thru_hole oval (at 0 68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 176 OUT9-))
    (pad 29 thru_hole oval (at 0 71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 177 OUT8-))
    (pad 30 thru_hole oval (at 0 73.66 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 178 OUT7-))
    (pad 31 thru_hole oval (at 0 76.2 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 179 OUT6-))
    (pad 32 thru_hole oval (at 0 78.74 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 180 OUT5-))
    (pad 33 thru_hole oval (at 0 81.28 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 181 OUT4-))
    (pad 34 thru_hole oval (at 0 83.82 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 182 OUT3-))
    (pad 35 thru_hole oval (at 0 86.36 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 183 OUT2-))
    (pad 36 thru_hole oval (at 0 88.9 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 184 OUT1-))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x36_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:PJ-082BH (layer F.Cu) (tedit 5A927599)
    (at 224.25 24.5 90)
    (fp_text reference J5 (at -3.26629 -6.49753 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial_Power (at -3.38489 6.63438 90) (layer F.SilkS))
    (pad Hole np_thru_hole circle (at -1 4.75 90) (size 0.8 0.8) (drill 0.8) (layers))
    (pad Hole np_thru_hole circle (at -0.5 0 90) (size 0.8 0.8) (drill 0.8) (layers))
    (pad Hole np_thru_hole circle (at -1 -4.75 90) (size 0.8 0.8) (drill 0.8) (layers))
    (pad Hole np_thru_hole circle (at 3.7 4.75 90) (size 0.8 0.8) (drill 0.8) (layers))
    (pad Hole np_thru_hole circle (at 3.7 -4.75 90) (size 0.8 0.8) (drill 0.8) (layers))
    (pad 1 thru_hole circle (at 5.5 0 90) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 38 VDD))
    (pad Hole np_thru_hole circle (at -3.75 0 90) (size 1.7 1.7) (drill 1.7) (layers))
    (pad 2 smd rect (at -1.75 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 81 89 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL1 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(L_SMALL1-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 80.75 46.25 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL2 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(L_SMALL2-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 81.25 66.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL3 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(L_SMALL3-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 80.5 110.25 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL4 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(L_SMALL4-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 80.75 133.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL5 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(L_SMALL5-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 80.25 154.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL6 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(L_SMALL6-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 105.5 89.75 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL7 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(L_SMALL7-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 104.25 45.75 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL8 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(L_SMALL8-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 105.75 66.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL9 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(L_SMALL9-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 105.75 111 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL10 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(L_SMALL10-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 105.5 133.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL11 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(L_SMALL11-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 106.5 155.25 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL12 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(L_SMALL12-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 128.25 89.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL13 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(L_SMALL13-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 128 46.75 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL14 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(L_SMALL14-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 127.75 67.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL15 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(L_SMALL15-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 127.25 111.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL16 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(L_SMALL16-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 126.5 133.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL17 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(L_SMALL17-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 128.5 154.75 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL18 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(L_SMALL18-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 150 89.75 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL19 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(L_SMALL19-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 150.5 46 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL20 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(L_SMALL20-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 151 67.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL21 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(L_SMALL21-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 151.5 111.75 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL22 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(L_SMALL22-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 150.25 133.25 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL23 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(L_SMALL23-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 150.75 155.25 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL24 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(L_SMALL24-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 172.25 90 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL25 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(L_SMALL25-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 174 45.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL26 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(L_SMALL26-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 173.75 68.25 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL27 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(L_SMALL27-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 172.5 111.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL28 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(L_SMALL28-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 172.5 133.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL29 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(L_SMALL29-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 173.75 155.25 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL30 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(L_SMALL30-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 195.5 91 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL31 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(L_SMALL31-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 196.5 45.75 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL32 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(L_SMALL32-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 197 68.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL33 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(L_SMALL33-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 195 112.5 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL34 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(L_SMALL34-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 195.25 134.25 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL35 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(L_SMALL35-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 195.5 155.75 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L_SMALL36 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(L_SMALL36-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 67 91 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R_1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 66.5 45 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_2 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(R_2-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 67 68 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_3 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(R_3-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 66.5 114 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_4 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R_10-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 66.5 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_5 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(R_11-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 66.5 158.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_6 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(R_12-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 72 91 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_7 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C_BOOST1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R_1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 71.5 45 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_8 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C_BOOST2-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(R_2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 72 68 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_9 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_BOOST3-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(R_3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 71.5 114 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C_BOOST4-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R_10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 71.5 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_11 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_BOOST5-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(R_11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 71.5 158.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_12 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C_BOOST6-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(R_12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 91.5 90.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_13 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R_13-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 90.5 46 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_14 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(R_14-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 91.5 68 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_15 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(R_15-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 92.5 113 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_16 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(R_16-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 92.5 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_17 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(R_17-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 92 158.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_18 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(R_18-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 96.5 90.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_19 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_BOOST7-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R_13-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 96 46 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_20 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C_BOOST8-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(R_14-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 96.5 68 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_21 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C_BOOST9-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(R_15-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 97.5 113 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_22 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C_BOOST10-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(R_16-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 97.5 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_23 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C_BOOST11-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(R_17-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 97 158.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_24 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C_BOOST12-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(R_18-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 115 91 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_25 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(R_25-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 114.5 46.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_26 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(R_26-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 115.5 68 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_27 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(R_27-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 116 113 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_28 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(R_28-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 115 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_29 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(R_29-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 115.5 158.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_30 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(R_30-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 120 91 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_31 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C_BOOST13-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(R_25-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 119.5 46.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_32 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C_BOOST14-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(R_26-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 120.5 68 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_33 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_BOOST15-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(R_27-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 121 113 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_34 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_BOOST16-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(R_28-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 120 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_35 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C_BOOST17-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(R_29-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 120.5 158.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_36 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C_BOOST18-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(R_30-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 138 91.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_37 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(R_37-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 137.5 47 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_38 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(R_38-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 138 68.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_39 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(R_39-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 138.5 114 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_40 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(R_40-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 137.5 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_41 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(R_41-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 138 158.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_42 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(R_42-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 143 91.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_43 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C_BOOST19-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(R_37-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 142.5 47 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_44 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C_BOOST20-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(R_38-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 143 68.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_45 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C_BOOST21-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(R_39-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 143.5 114 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_46 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C_BOOST22-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(R_40-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 142.5 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_47 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C_BOOST23-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(R_41-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 143.5 158.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_48 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C_BOOST24-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(R_42-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 161 92 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_49 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(R_49-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 160.5 48 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_50 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(R_50-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 160.5 69 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_51 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(R_51-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 161.5 114.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_52 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R_52-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 161 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_53 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(R_53-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 160.5 158 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_54 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(R_54-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 166.5 92 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_55 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C_BOOST25-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(R_49-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 165.5 48 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_56 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C_BOOST26-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(R_50-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 165.5 69 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_57 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C_BOOST27-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(R_51-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 166.5 114.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_58 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C_BOOST28-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R_52-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 166.5 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_59 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C_BOOST29-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(R_53-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 165.5 158 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_60 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C_BOOST30-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(R_54-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 184 92.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_61 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(R_61-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 183.5 48 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_62 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(R_62-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 184 70 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_63 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(R_63-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 183.5 114.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_64 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(R_64-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 184 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_65 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(R_65-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 184 158 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_66 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 9.76k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(R_66-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 189 92.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_67 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C_BOOST31-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(R_61-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 188.5 48 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_68 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C_BOOST32-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(R_62-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 189.5 70 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_69 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C_BOOST33-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(R_63-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 188.5 114.5 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_70 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C_BOOST34-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(R_64-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 189 136 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_71 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C_BOOST35-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(R_65-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 189.5 158 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_72 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 768k (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C_BOOST36-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(R_66-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 85 77 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(R_REXT1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 85 34 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 258 "Net-(R_REXT2-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 85.5 54.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT3 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(R_REXT3-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 84.5 98.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT4 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(R_REXT4-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 85.5 121.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT5 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(R_REXT5-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 85 143.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 262 "Net-(R_REXT6-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 109 77 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT7 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 263 "Net-(R_REXT7-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 109.5 34 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT8 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(R_REXT8-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 109.5 54.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT9 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(R_REXT9-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 110.5 99.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT10 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(R_REXT10-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 110 121.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT11 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 267 "Net-(R_REXT11-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 110.5 143.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT12 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 268 "Net-(R_REXT12-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 132.5 77.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT13 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 269 "Net-(R_REXT13-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 132 33.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT14 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 270 "Net-(R_REXT14-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 132 55 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT15 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 271 "Net-(R_REXT15-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 132 100 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT16 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 272 "Net-(R_REXT16-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 132 121 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT17 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 273 "Net-(R_REXT17-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 133 143.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT18 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 274 "Net-(R_REXT18-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 155 77.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT19 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 275 "Net-(R_REXT19-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 154.5 33 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT20 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 276 "Net-(R_REXT20-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 155 55.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT21 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 277 "Net-(R_REXT21-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 155.5 99 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT22 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 278 "Net-(R_REXT22-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 155.5 121.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT23 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 279 "Net-(R_REXT23-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 154.5 143 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT24 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 280 "Net-(R_REXT24-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 178 78.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT25 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 281 "Net-(R_REXT25-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 178 33.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT26 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 282 "Net-(R_REXT26-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 177.5 56 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT27 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 283 "Net-(R_REXT27-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 178 99.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT28 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 284 "Net-(R_REXT28-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 177.5 121 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT29 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 285 "Net-(R_REXT29-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 178 143.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT30 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 286 "Net-(R_REXT30-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 201 77.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT31 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 287 "Net-(R_REXT31-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 202 34 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT32 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 288 "Net-(R_REXT32-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 201.5 56.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT33 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(R_REXT33-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 200.5 100.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT34 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 290 "Net-(R_REXT34-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 200.5 121.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT35 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 291 "Net-(R_REXT35-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 201 144.5 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_REXT36 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(R_REXT36-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5A90D07F)
    (at 36 49)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -3.375) (layer F.SilkS))
    (fp_text value TCA9548A_QFN (at 0 3.375) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 293 SDA1))
    (pad 2 smd rect (at -1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 294 SCL1))
    (pad 3 smd rect (at -1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 295 SDA2))
    (pad 4 smd rect (at -1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 296 SCL2))
    (pad 5 smd rect (at -1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 297 SDA3))
    (pad 6 smd rect (at -1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 298 SCL3))
    (pad 7 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 299 SDA4))
    (pad 8 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 300 SCL4))
    (pad 9 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 301 SDA5))
    (pad 11 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 302 SCL5))
    (pad 12 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 303 SDA6))
    (pad 13 smd rect (at 1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 304 SCL6))
    (pad 14 smd rect (at 1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 305 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 306 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at 1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 307 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 308 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(J3-Pad1)"))
    (pad 20 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(J3-Pad2)"))
    (pad 21 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 22 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5A90D090)
    (at 35.75 71.75)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 -3.375) (layer F.SilkS))
    (fp_text value TCA9548A_QFN (at 0 3.375) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 309 SDA7))
    (pad 2 smd rect (at -1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 310 SCL7))
    (pad 3 smd rect (at -1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 311 SDA8))
    (pad 4 smd rect (at -1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 312 SCL8))
    (pad 5 smd rect (at -1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 313 SDA9))
    (pad 6 smd rect (at -1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 314 SCL9))
    (pad 7 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 315 SDA10))
    (pad 8 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 316 SCL10))
    (pad 9 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 317 SDA11))
    (pad 11 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 318 SCL11))
    (pad 12 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 319 SDA12))
    (pad 13 smd rect (at 1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 320 SCL12))
    (pad 14 smd rect (at 1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 321 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 322 "Net-(U2-Pad15)"))
    (pad 16 smd rect (at 1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 323 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 324 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(J3-Pad1)"))
    (pad 20 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(J3-Pad2)"))
    (pad 21 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 22 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 23 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5A90D0A2)
    (at 35.75 94.75)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U3 (at 0 -3.375) (layer F.SilkS))
    (fp_text value TCA9548A_QFN (at 0 3.375) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 325 SDA13))
    (pad 2 smd rect (at -1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 326 SCL13))
    (pad 3 smd rect (at -1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 327 SDA14))
    (pad 4 smd rect (at -1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 328 SCL14))
    (pad 5 smd rect (at -1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 329 SDA15))
    (pad 6 smd rect (at -1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 330 SCL15))
    (pad 7 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 331 SDA16))
    (pad 8 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 332 SCL16))
    (pad 9 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 333 SDA17))
    (pad 11 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 334 SCL17))
    (pad 12 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 335 SDA18))
    (pad 13 smd rect (at 1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 336 SCL18))
    (pad 14 smd rect (at 1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(U3-Pad14)"))
    (pad 15 smd rect (at 1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(U3-Pad15)"))
    (pad 16 smd rect (at 1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 339 "Net-(U3-Pad16)"))
    (pad 17 smd rect (at 1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 340 "Net-(U3-Pad17)"))
    (pad 18 smd rect (at 1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(J3-Pad1)"))
    (pad 20 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(J3-Pad2)"))
    (pad 21 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 22 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 24 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5A90D0B6)
    (at 36.25 116.5)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U4 (at 0 -3.375) (layer F.SilkS))
    (fp_text value TCA9548A_QFN (at 0 3.375) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 341 SDA19))
    (pad 2 smd rect (at -1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 342 SCL19))
    (pad 3 smd rect (at -1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 343 SDA20))
    (pad 4 smd rect (at -1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 344 SCL20))
    (pad 5 smd rect (at -1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 345 SDA21))
    (pad 6 smd rect (at -1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 346 SCL21))
    (pad 7 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 347 SDA22))
    (pad 8 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 348 SCL22))
    (pad 9 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 349 SDA23))
    (pad 11 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 350 SCL23))
    (pad 12 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 351 SDA24))
    (pad 13 smd rect (at 1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 352 SCL24))
    (pad 14 smd rect (at 1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 353 "Net-(U4-Pad14)"))
    (pad 15 smd rect (at 1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 354 "Net-(U4-Pad15)"))
    (pad 16 smd rect (at 1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 355 "Net-(U4-Pad16)"))
    (pad 17 smd rect (at 1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 356 "Net-(U4-Pad17)"))
    (pad 18 smd rect (at 1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(J3-Pad1)"))
    (pad 20 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(J3-Pad2)"))
    (pad 21 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 22 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 23 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 24 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5A90D0BE)
    (at 36.5 139.5)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U5 (at 0 -3.375) (layer F.SilkS))
    (fp_text value TCA9548A_QFN (at 0 3.375) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 357 SDA25))
    (pad 2 smd rect (at -1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 358 SCL25))
    (pad 3 smd rect (at -1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 359 SDA26))
    (pad 4 smd rect (at -1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 360 SCL26))
    (pad 5 smd rect (at -1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 361 SDA27))
    (pad 6 smd rect (at -1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 362 SCL27))
    (pad 7 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 363 SDA28))
    (pad 8 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 364 SCL28))
    (pad 9 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 365 SDA29))
    (pad 11 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 366 SCL29))
    (pad 12 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 367 SDA30))
    (pad 13 smd rect (at 1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 368 SCL30))
    (pad 14 smd rect (at 1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(U5-Pad14)"))
    (pad 15 smd rect (at 1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 370 "Net-(U5-Pad15)"))
    (pad 16 smd rect (at 1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(U5-Pad16)"))
    (pad 17 smd rect (at 1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 372 "Net-(U5-Pad17)"))
    (pad 18 smd rect (at 1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 19 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(J3-Pad1)"))
    (pad 20 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(J3-Pad2)"))
    (pad 21 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 22 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5A90D0D4)
    (at 36.5 161)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U6 (at 0 -3.375) (layer F.SilkS))
    (fp_text value TCA9548A_QFN (at 0 3.375) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 373 SDA31))
    (pad 2 smd rect (at -1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 374 SCL31))
    (pad 3 smd rect (at -1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 375 SDA32))
    (pad 4 smd rect (at -1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 376 SCL32))
    (pad 5 smd rect (at -1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 377 SDA33))
    (pad 6 smd rect (at -1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 378 SCL33))
    (pad 7 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 379 SDA34))
    (pad 8 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 380 SCL34))
    (pad 9 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 381 SDA35))
    (pad 11 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 382 SCL35))
    (pad 12 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 383 SDA36))
    (pad 13 smd rect (at 1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 384 SCL36))
    (pad 14 smd rect (at 1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 385 "Net-(U6-Pad14)"))
    (pad 15 smd rect (at 1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 386 "Net-(U6-Pad15)"))
    (pad 16 smd rect (at 1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 387 "Net-(U6-Pad16)"))
    (pad 17 smd rect (at 1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 388 "Net-(U6-Pad17)"))
    (pad 18 smd rect (at 1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 19 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(J3-Pad1)"))
    (pad 20 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(J3-Pad2)"))
    (pad 21 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 22 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 23 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module resistor:SOIC16ok-16N (layer F.Cu) (tedit 0)
    (at 53.75 36.25)
    (attr smd)
    (fp_text reference U7 (at -2.06252 -6.99566) (layer F.SilkS))
    (fp_text value Resistor_array_15_16soic (at -1.36981 6.9696) (layer F.SilkS))
    (pad 1 smd rect (at -3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at -3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 294 SCL1))
    (pad 4 smd rect (at -3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 293 SDA1))
    (pad 5 smd rect (at -3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 296 SCL2))
    (pad 6 smd rect (at -3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 295 SDA2))
    (pad 7 smd rect (at -3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 298 SCL3))
    (pad 8 smd rect (at -3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 297 SDA3))
    (pad 9 smd rect (at 3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 300 SCL4))
    (pad 10 smd rect (at 3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 299 SDA4))
    (pad 11 smd rect (at 3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 302 SCL5))
    (pad 12 smd rect (at 3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 301 SDA5))
    (pad 13 smd rect (at 3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 304 SCL6))
    (pad 14 smd rect (at 3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 303 SDA6))
    (pad 15 smd rect (at 3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 389 "Net-(U7-Pad15)"))
    (pad 16 smd rect (at 3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
  )
  (module resistor:SOIC16ok-16N (layer F.Cu) (tedit 0)
    (at 54 59.75)
    (attr smd)
    (fp_text reference U8 (at -2.06252 -6.99566) (layer F.SilkS))
    (fp_text value Resistor_array_15_16soic (at -1.36981 6.9696) (layer F.SilkS))
    (pad 1 smd rect (at -3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 310 SCL7))
    (pad 2 smd rect (at -3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 309 SDA7))
    (pad 3 smd rect (at -3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 312 SCL8))
    (pad 4 smd rect (at -3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 311 SDA8))
    (pad 5 smd rect (at -3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 314 SCL9))
    (pad 6 smd rect (at -3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 313 SDA9))
    (pad 7 smd rect (at -3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 316 SCL10))
    (pad 8 smd rect (at -3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 315 SDA10))
    (pad 9 smd rect (at 3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 318 SCL11))
    (pad 10 smd rect (at 3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 317 SDA11))
    (pad 11 smd rect (at 3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 320 SCL12))
    (pad 12 smd rect (at 3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 319 SDA12))
    (pad 13 smd rect (at 3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 390 "Net-(U8-Pad13)"))
    (pad 14 smd rect (at 3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 391 "Net-(U8-Pad14)"))
    (pad 15 smd rect (at 3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 392 "Net-(U8-Pad15)"))
    (pad 16 smd rect (at 3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
  )
  (module resistor:SOIC16ok-16N (layer F.Cu) (tedit 0)
    (at 54.25 82.5)
    (attr smd)
    (fp_text reference U9 (at -2.06252 -6.99566) (layer F.SilkS))
    (fp_text value Resistor_array_15_16soic (at -1.36981 6.9696) (layer F.SilkS))
    (pad 1 smd rect (at -3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 326 SCL13))
    (pad 2 smd rect (at -3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 325 SDA13))
    (pad 3 smd rect (at -3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 328 SCL14))
    (pad 4 smd rect (at -3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 327 SDA14))
    (pad 5 smd rect (at -3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 330 SCL15))
    (pad 6 smd rect (at -3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 329 SDA15))
    (pad 7 smd rect (at -3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 332 SCL16))
    (pad 8 smd rect (at -3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 331 SDA16))
    (pad 9 smd rect (at 3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 334 SCL17))
    (pad 10 smd rect (at 3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 333 SDA17))
    (pad 11 smd rect (at 3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 336 SCL18))
    (pad 12 smd rect (at 3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 335 SDA18))
    (pad 13 smd rect (at 3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 393 "Net-(U9-Pad13)"))
    (pad 14 smd rect (at 3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 394 "Net-(U9-Pad14)"))
    (pad 15 smd rect (at 3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 395 "Net-(U9-Pad15)"))
    (pad 16 smd rect (at 3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
  )
  (module resistor:SOIC16ok-16N (layer F.Cu) (tedit 0)
    (at 54.25 104.75)
    (attr smd)
    (fp_text reference U10 (at -2.06252 -6.99566) (layer F.SilkS))
    (fp_text value Resistor_array_15_16soic (at -1.36981 6.9696) (layer F.SilkS))
    (pad 1 smd rect (at -3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 342 SCL19))
    (pad 2 smd rect (at -3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 341 SDA19))
    (pad 3 smd rect (at -3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 344 SCL20))
    (pad 4 smd rect (at -3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 343 SDA20))
    (pad 5 smd rect (at -3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 346 SCL21))
    (pad 6 smd rect (at -3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 345 SDA21))
    (pad 7 smd rect (at -3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 348 SCL22))
    (pad 8 smd rect (at -3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 347 SDA22))
    (pad 9 smd rect (at 3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 350 SCL23))
    (pad 10 smd rect (at 3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 349 SDA23))
    (pad 11 smd rect (at 3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 352 SCL24))
    (pad 12 smd rect (at 3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 351 SDA24))
    (pad 13 smd rect (at 3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 396 "Net-(U10-Pad13)"))
    (pad 14 smd rect (at 3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 397 "Net-(U10-Pad14)"))
    (pad 15 smd rect (at 3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 398 "Net-(U10-Pad15)"))
    (pad 16 smd rect (at 3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
  )
  (module resistor:SOIC16ok-16N (layer F.Cu) (tedit 0)
    (at 54.5 127)
    (attr smd)
    (fp_text reference U11 (at -2.06252 -6.99566) (layer F.SilkS))
    (fp_text value Resistor_array_15_16soic (at -1.36981 6.9696) (layer F.SilkS))
    (pad 1 smd rect (at -3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 358 SCL25))
    (pad 2 smd rect (at -3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 357 SDA25))
    (pad 3 smd rect (at -3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 360 SCL26))
    (pad 4 smd rect (at -3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 359 SDA26))
    (pad 5 smd rect (at -3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 362 SCL27))
    (pad 6 smd rect (at -3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 361 SDA27))
    (pad 7 smd rect (at -3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 364 SCL28))
    (pad 8 smd rect (at -3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 363 SDA28))
    (pad 9 smd rect (at 3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 366 SCL29))
    (pad 10 smd rect (at 3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 365 SDA29))
    (pad 11 smd rect (at 3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 368 SCL30))
    (pad 12 smd rect (at 3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 367 SDA30))
    (pad 13 smd rect (at 3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 399 "Net-(U11-Pad13)"))
    (pad 14 smd rect (at 3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 400 "Net-(U11-Pad14)"))
    (pad 15 smd rect (at 3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 401 "Net-(U11-Pad15)"))
    (pad 16 smd rect (at 3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
  )
  (module resistor:SOIC16ok-16N (layer F.Cu) (tedit 0)
    (at 54.25 149.25)
    (attr smd)
    (fp_text reference U12 (at -2.06252 -6.99566) (layer F.SilkS))
    (fp_text value Resistor_array_15_16soic (at -1.36981 6.9696) (layer F.SilkS))
    (pad 1 smd rect (at -3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 374 SCL31))
    (pad 2 smd rect (at -3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 373 SDA31))
    (pad 3 smd rect (at -3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 376 SCL32))
    (pad 4 smd rect (at -3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 375 SDA32))
    (pad 5 smd rect (at -3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 378 SCL33))
    (pad 6 smd rect (at -3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 377 SDA33))
    (pad 7 smd rect (at -3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 380 SCL34))
    (pad 8 smd rect (at -3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 379 SDA34))
    (pad 9 smd rect (at 3.495 4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 382 SCL35))
    (pad 10 smd rect (at 3.495 3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 381 SDA35))
    (pad 11 smd rect (at 3.495 1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 384 SCL36))
    (pad 12 smd rect (at 3.495 0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 383 SDA36))
    (pad 13 smd rect (at 3.495 -0.635) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 402 "Net-(U12-Pad13)"))
    (pad 14 smd rect (at 3.495 -1.905) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 403 "Net-(U12-Pad14)"))
    (pad 15 smd rect (at 3.495 -3.175) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 404 "Net-(U12-Pad15)"))
    (pad 16 smd rect (at 3.495 -4.445) (size 1.59 0.61) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D14D)
    (at 81.25 83.75)
    (attr smd)
    (fp_text reference U13 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(L_SMALL1-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(L_SMALL1-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 405 "Net-(U13-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C_BOOST1-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 406 "Net-(U13-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 407 "Net-(U13-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 326 SCL13))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 325 SDA13))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C_REG1-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C_PUMP1-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R_1-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C_BOOST1-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C_BOOST1-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 134 OUT13+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 172 OUT13-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(R_REXT1-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D0E8)
    (at 81.25 40.5)
    (attr smd)
    (fp_text reference U14 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(L_SMALL2-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(L_SMALL2-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 408 "Net-(U14-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C_BOOST2-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 409 "Net-(U14-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 410 "Net-(U14-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 294 SCL1))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 293 SDA1))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C_REG2-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C_PUMP2-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(R_2-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C_BOOST2-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C_BOOST2-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 146 OUT1+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 184 OUT1-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 258 "Net-(R_REXT2-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D152)
    (at 81.75 60.75)
    (attr smd)
    (fp_text reference U15 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(L_SMALL3-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(L_SMALL3-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 411 "Net-(U15-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_BOOST3-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 412 "Net-(U15-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 413 "Net-(U15-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 310 SCL7))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 309 SDA7))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C_REG3-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C_PUMP3-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(R_3-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_BOOST3-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_BOOST3-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 140 OUT7+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 178 OUT7-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(R_REXT3-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D162)
    (at 80.75 104.75)
    (attr smd)
    (fp_text reference U16 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(L_SMALL4-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(L_SMALL4-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 414 "Net-(U16-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C_BOOST4-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 415 "Net-(U16-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 416 "Net-(U16-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 342 SCL19))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 341 SDA19))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C_REG4-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C_PUMP4-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R_10-Pad2)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C_BOOST4-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C_BOOST4-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 128 OUT19+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 166 OUT19-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(R_REXT4-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D166)
    (at 81 127.75)
    (attr smd)
    (fp_text reference U17 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(L_SMALL5-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(L_SMALL5-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 417 "Net-(U17-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_BOOST5-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 418 "Net-(U17-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 419 "Net-(U17-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 358 SCL25))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 357 SDA25))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C_REG5-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C_PUMP5-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(R_11-Pad2)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_BOOST5-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_BOOST5-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 122 OUT25+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 160 OUT25-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(R_REXT5-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D1C7)
    (at 80.5 149)
    (attr smd)
    (fp_text reference U18 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(L_SMALL6-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(L_SMALL6-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 420 "Net-(U18-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C_BOOST6-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 421 "Net-(U18-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(U18-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 374 SCL31))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 373 SDA31))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C_REG6-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C_PUMP6-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(R_12-Pad2)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C_BOOST6-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C_BOOST6-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 116 OUT31+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 154 OUT31-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 262 "Net-(R_REXT6-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D143)
    (at 105.75 84)
    (attr smd)
    (fp_text reference U19 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(L_SMALL7-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(L_SMALL7-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 423 "Net-(U19-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_BOOST7-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 424 "Net-(U19-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 425 "Net-(U19-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 328 SCL14))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 327 SDA14))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(C_REG7-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C_PUMP7-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R_13-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_BOOST7-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_BOOST7-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 133 OUT14+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 171 OUT14-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 263 "Net-(R_REXT7-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D0ED)
    (at 105.25 40.5)
    (attr smd)
    (fp_text reference U20 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(L_SMALL8-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(L_SMALL8-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 426 "Net-(U20-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C_BOOST8-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 427 "Net-(U20-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 428 "Net-(U20-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 296 SCL2))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 295 SDA2))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C_REG8-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C_PUMP8-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(R_14-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C_BOOST8-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C_BOOST8-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 145 OUT2+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 183 OUT2-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(R_REXT8-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D148)
    (at 106 61)
    (attr smd)
    (fp_text reference U21 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(L_SMALL9-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(L_SMALL9-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 429 "Net-(U21-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C_BOOST9-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 430 "Net-(U21-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 431 "Net-(U21-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 312 SCL8))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 311 SDA8))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(C_REG9-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C_PUMP9-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(R_15-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C_BOOST9-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C_BOOST9-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 139 OUT8+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 177 OUT8-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(R_REXT9-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D16B)
    (at 106.5 106)
    (attr smd)
    (fp_text reference U22 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(L_SMALL10-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(L_SMALL10-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 432 "Net-(U22-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C_BOOST10-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 433 "Net-(U22-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 434 "Net-(U22-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 344 SCL20))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 343 SDA20))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C_REG10-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C_PUMP10-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(R_16-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C_BOOST10-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C_BOOST10-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 127 OUT20+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 165 OUT20-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(R_REXT10-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D16F)
    (at 106.25 128)
    (attr smd)
    (fp_text reference U23 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(L_SMALL11-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(L_SMALL11-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 435 "Net-(U23-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C_BOOST11-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 436 "Net-(U23-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 437 "Net-(U23-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 360 SCL26))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 359 SDA26))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C_REG11-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C_PUMP11-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(R_17-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C_BOOST11-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C_BOOST11-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 121 OUT26+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 159 OUT26-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 267 "Net-(R_REXT11-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D1BF)
    (at 106.75 149.5)
    (attr smd)
    (fp_text reference U24 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(L_SMALL12-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(L_SMALL12-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 438 "Net-(U24-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C_BOOST12-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 439 "Net-(U24-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 440 "Net-(U24-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 376 SCL32))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 375 SDA32))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(C_REG12-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C_PUMP12-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(R_18-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C_BOOST12-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C_BOOST12-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 115 OUT32+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 153 OUT32-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 268 "Net-(R_REXT12-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D136)
    (at 128.75 84)
    (attr smd)
    (fp_text reference U25 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(L_SMALL13-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(L_SMALL13-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 441 "Net-(U25-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C_BOOST13-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 442 "Net-(U25-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 443 "Net-(U25-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 330 SCL15))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 329 SDA15))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(C_REG13-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C_PUMP13-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(R_25-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C_BOOST13-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C_BOOST13-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 132 OUT15+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 170 OUT15-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 269 "Net-(R_REXT13-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D0F7)
    (at 128.5 41.25)
    (attr smd)
    (fp_text reference U26 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(L_SMALL14-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(L_SMALL14-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 444 "Net-(U26-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C_BOOST14-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 445 "Net-(U26-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 446 "Net-(U26-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 298 SCL3))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 297 SDA3))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C_REG14-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C_PUMP14-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(R_26-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C_BOOST14-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C_BOOST14-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 144 OUT3+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 182 OUT3-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 270 "Net-(R_REXT14-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D13B)
    (at 128.25 62.25)
    (attr smd)
    (fp_text reference U27 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(L_SMALL15-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(L_SMALL15-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 447 "Net-(U27-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_BOOST15-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 448 "Net-(U27-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 449 "Net-(U27-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 314 SCL9))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 313 SDA9))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(C_REG15-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C_PUMP15-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(R_27-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_BOOST15-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_BOOST15-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 138 OUT9+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 176 OUT9-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 271 "Net-(R_REXT15-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D179)
    (at 128.5 106.25)
    (attr smd)
    (fp_text reference U28 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(L_SMALL16-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(L_SMALL16-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 450 "Net-(U28-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_BOOST16-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 451 "Net-(U28-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 452 "Net-(U28-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 346 SCL21))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 345 SDA21))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C_REG16-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C_PUMP16-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(R_28-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_BOOST16-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_BOOST16-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 126 OUT21+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 164 OUT21-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 272 "Net-(R_REXT16-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D17E)
    (at 128 128)
    (attr smd)
    (fp_text reference U29 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(L_SMALL17-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(L_SMALL17-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 453 "Net-(U29-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C_BOOST17-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 454 "Net-(U29-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 455 "Net-(U29-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 362 SCL27))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 361 SDA27))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C_REG17-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C_PUMP17-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(R_29-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C_BOOST17-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C_BOOST17-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 120 OUT27+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 158 OUT27-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 273 "Net-(R_REXT17-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D1BA)
    (at 129.25 149.75)
    (attr smd)
    (fp_text reference U30 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(L_SMALL18-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(L_SMALL18-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 456 "Net-(U30-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C_BOOST18-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 457 "Net-(U30-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 458 "Net-(U30-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 378 SCL33))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 377 SDA33))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(C_REG18-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C_PUMP18-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(R_30-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C_BOOST18-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C_BOOST18-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 114 OUT33+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 152 OUT33-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 274 "Net-(R_REXT18-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D132)
    (at 151.5 84.5)
    (attr smd)
    (fp_text reference U31 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(L_SMALL19-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(L_SMALL19-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 459 "Net-(U31-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C_BOOST19-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 460 "Net-(U31-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 461 "Net-(U31-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 332 SCL16))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 331 SDA16))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(C_REG19-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C_PUMP19-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(R_37-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C_BOOST19-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C_BOOST19-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 131 OUT16+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 169 OUT16-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 275 "Net-(R_REXT19-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D0FC)
    (at 151 40.25)
    (attr smd)
    (fp_text reference U32 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(L_SMALL20-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(L_SMALL20-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 462 "Net-(U32-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C_BOOST20-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 463 "Net-(U32-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 464 "Net-(U32-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 300 SCL4))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 299 SDA4))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(C_REG20-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C_PUMP20-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(R_38-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C_BOOST20-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C_BOOST20-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 143 OUT4+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 181 OUT4-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 276 "Net-(R_REXT20-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D12D)
    (at 151.25 61.75)
    (attr smd)
    (fp_text reference U33 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(L_SMALL21-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(L_SMALL21-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 465 "Net-(U33-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C_BOOST21-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 466 "Net-(U33-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 467 "Net-(U33-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 316 SCL10))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 315 SDA10))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(C_REG21-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C_PUMP21-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(R_39-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C_BOOST21-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C_BOOST21-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 137 OUT10+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 175 OUT10-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 277 "Net-(R_REXT21-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D182)
    (at 151.75 106.25)
    (attr smd)
    (fp_text reference U34 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(L_SMALL22-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(L_SMALL22-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 468 "Net-(U34-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C_BOOST22-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 469 "Net-(U34-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 470 "Net-(U34-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 348 SCL22))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 347 SDA22))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(C_REG22-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C_PUMP22-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(R_40-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C_BOOST22-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C_BOOST22-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 125 OUT22+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 163 OUT22-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 278 "Net-(R_REXT22-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D186)
    (at 151.75 128)
    (attr smd)
    (fp_text reference U35 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(L_SMALL23-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(L_SMALL23-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 471 "Net-(U35-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C_BOOST23-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 472 "Net-(U35-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 473 "Net-(U35-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 364 SCL28))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 363 SDA28))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C_REG23-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C_PUMP23-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(R_41-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C_BOOST23-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C_BOOST23-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 119 OUT28+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 157 OUT28-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 279 "Net-(R_REXT23-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D1B2)
    (at 151 149.75)
    (attr smd)
    (fp_text reference U36 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(L_SMALL24-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(L_SMALL24-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 474 "Net-(U36-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C_BOOST24-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 475 "Net-(U36-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 476 "Net-(U36-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 380 SCL34))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 379 SDA34))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(C_REG24-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C_PUMP24-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(R_42-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C_BOOST24-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C_BOOST24-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 113 OUT34+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 151 OUT34-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 280 "Net-(R_REXT24-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D11E)
    (at 174 85)
    (attr smd)
    (fp_text reference U37 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(L_SMALL25-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(L_SMALL25-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 477 "Net-(U37-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C_BOOST25-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 478 "Net-(U37-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 479 "Net-(U37-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 334 SCL17))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 333 SDA17))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C_REG25-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C_PUMP25-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(R_49-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C_BOOST25-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C_BOOST25-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 130 OUT17+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 168 OUT17-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 281 "Net-(R_REXT25-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D104)
    (at 174.25 40)
    (attr smd)
    (fp_text reference U38 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(L_SMALL26-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(L_SMALL26-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 480 "Net-(U38-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C_BOOST26-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 481 "Net-(U38-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 482 "Net-(U38-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 302 SCL5))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 301 SDA5))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C_REG26-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C_PUMP26-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(R_50-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C_BOOST26-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C_BOOST26-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 142 OUT5+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 180 OUT5-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 282 "Net-(R_REXT26-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D123)
    (at 174 62.75)
    (attr smd)
    (fp_text reference U39 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(L_SMALL27-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(L_SMALL27-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 483 "Net-(U39-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C_BOOST27-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 484 "Net-(U39-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 485 "Net-(U39-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 318 SCL11))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 317 SDA11))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C_REG27-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C_PUMP27-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(R_51-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C_BOOST27-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C_BOOST27-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 136 OUT11+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 174 OUT11-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 283 "Net-(R_REXT27-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D18B)
    (at 173.75 106.25)
    (attr smd)
    (fp_text reference U40 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(L_SMALL28-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(L_SMALL28-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 486 "Net-(U40-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C_BOOST28-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 487 "Net-(U40-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 488 "Net-(U40-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 350 SCL23))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 349 SDA23))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C_REG28-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C_PUMP28-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R_52-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C_BOOST28-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C_BOOST28-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 124 OUT23+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 162 OUT23-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 284 "Net-(R_REXT28-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D190)
    (at 174 128)
    (attr smd)
    (fp_text reference U41 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(L_SMALL29-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(L_SMALL29-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 489 "Net-(U41-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C_BOOST29-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 490 "Net-(U41-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 491 "Net-(U41-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 366 SCL29))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 365 SDA29))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(C_REG29-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C_PUMP29-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(R_53-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C_BOOST29-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C_BOOST29-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 118 OUT29+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 156 OUT29-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 285 "Net-(R_REXT29-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D1AD)
    (at 174.25 150)
    (attr smd)
    (fp_text reference U42 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(L_SMALL30-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(L_SMALL30-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 492 "Net-(U42-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C_BOOST30-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 493 "Net-(U42-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 494 "Net-(U42-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 382 SCL35))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 381 SDA35))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(C_REG30-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C_PUMP30-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(R_54-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C_BOOST30-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C_BOOST30-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 112 OUT35+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 150 OUT35-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 286 "Net-(R_REXT30-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D11A)
    (at 196.75 86)
    (attr smd)
    (fp_text reference U43 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(L_SMALL31-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(L_SMALL31-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 495 "Net-(U43-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C_BOOST31-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 496 "Net-(U43-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 497 "Net-(U43-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 336 SCL18))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 335 SDA18))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(C_REG31-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C_PUMP31-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(R_61-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C_BOOST31-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C_BOOST31-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 129 OUT18+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 167 OUT18-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 287 "Net-(R_REXT31-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D109)
    (at 197.25 40)
    (attr smd)
    (fp_text reference U44 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(L_SMALL32-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(L_SMALL32-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 498 "Net-(U44-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C_BOOST32-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 499 "Net-(U44-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 500 "Net-(U44-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 304 SCL6))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 303 SDA6))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(C_REG32-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C_PUMP32-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(R_62-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C_BOOST32-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C_BOOST32-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 141 OUT6+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 179 OUT6-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 288 "Net-(R_REXT32-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D115)
    (at 197.25 63)
    (attr smd)
    (fp_text reference U45 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(L_SMALL33-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(L_SMALL33-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 501 "Net-(U45-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C_BOOST33-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 502 "Net-(U45-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 503 "Net-(U45-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 320 SCL12))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 319 SDA12))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C_REG33-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C_PUMP33-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(R_63-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C_BOOST33-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C_BOOST33-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 135 OUT12+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 173 OUT12-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(R_REXT33-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D199)
    (at 196.25 107.25)
    (attr smd)
    (fp_text reference U46 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(L_SMALL34-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(L_SMALL34-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 504 "Net-(U46-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C_BOOST34-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 505 "Net-(U46-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 506 "Net-(U46-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 352 SCL24))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 351 SDA24))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(C_REG34-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C_PUMP34-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(R_64-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C_BOOST34-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C_BOOST34-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 123 OUT24+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 161 OUT24-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 290 "Net-(R_REXT34-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D19D)
    (at 196.5 128.5)
    (attr smd)
    (fp_text reference U47 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(L_SMALL35-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(L_SMALL35-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 507 "Net-(U47-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C_BOOST35-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 508 "Net-(U47-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 509 "Net-(U47-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 368 SCL30))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 367 SDA30))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C_REG35-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C_PUMP35-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(R_65-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C_BOOST35-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C_BOOST35-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 117 OUT30+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 155 OUT30-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 291 "Net-(R_REXT35-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module .pretty:QFN20-4x4-21N (layer F.Cu) (tedit 5A90D1A8)
    (at 197 150.5)
    (attr smd)
    (fp_text reference U48 (at -0.36135 -5.10658) (layer F.SilkS))
    (fp_text value DRV2667 (at 0.407576 5.15913) (layer F.SilkS))
    (pad 6 smd rect (at -1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(L_SMALL36-Pad1)"))
    (pad 8 smd rect (at 0 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(L_SMALL36-Pad1)"))
    (pad 9 smd rect (at 0.5 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 510 "Net-(U48-Pad9)"))
    (pad 10 smd rect (at 1 1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C_BOOST36-Pad1)"))
    (pad 16 smd rect (at 1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 511 "Net-(U48-Pad16)"))
    (pad 17 smd rect (at 0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 512 "Net-(U48-Pad17)"))
    (pad 18 smd rect (at 0 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 384 SCL36))
    (pad 19 smd rect (at -0.5 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 383 SDA36))
    (pad 20 smd rect (at -1 -1.935 90) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C_REG36-Pad1)"))
    (pad 1 smd rect (at -1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C_PUMP36-Pad2)"))
    (pad 2 smd rect (at -1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 38 VDD))
    (pad 3 smd rect (at -1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(R_66-Pad1)"))
    (pad 4 smd rect (at -1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.935 1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C_BOOST36-Pad1)"))
    (pad 12 smd rect (at 1.935 0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C_BOOST36-Pad1)"))
    (pad 13 smd rect (at 1.935 0) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 111 OUT36+))
    (pad 14 smd rect (at 1.935 -0.5) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 149 OUT36-))
    (pad 15 smd rect (at 1.935 -1) (size 0.84 0.26) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(R_REXT36-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.63 2.63) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 30 20)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 30 150)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 235 160)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 235 35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.27mm (layer F.Cu) (tedit 5A939886)
    (at 30 35)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference GND (at 0 -1.695) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch1.27mm (at 0 1.695) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Team: Suny Ly, Orlando Salas, Jacolby Griffin\nAdvisor: Dr. Dhanya Nair\nMentor: Dr. Suketu Naik" (at 30 95 90) (layer B.SilkS))
  (gr_text "Tactile Display Board\nWeber State University" (at 82.5 20) (layer B.SilkS))
  (gr_line (start 242.5 16) (end 242.5 27) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 25.5 14) (end 240.5 14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 23.5 28) (end 23.5 16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 25.5 16) (end 23.5 16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 240.5 16) (end 240.5 14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 23.5 167.5) (end 23.5 28) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 25.5 167.5) (end 25.5 169.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 240.5 169.5) (end 25.5 169.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 242.5 27) (end 242.5 167.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 240.5 167.5) (end 242.5 167.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 38) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 241.75 14.75) (xy 241.75 169) (xy 23.75 169) (xy 23.75 14.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 241.75 14.75) (xy 241.75 169) (xy 23.75 169) (xy 23.75 14.5)
      )
    )
  )
)
