(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "1")
  (net 2 "3")
  (net 3 "4")
  (net 4 "6")
  (net 5 "7")
  (net 6 "8")
  (net 7 "10")
  (net 8 "11")
  (net 9 "12")
  (net 10 "13")
  (net 11 "14")
  (net 12 "15")
  (net 13 "16")
  (net 14 "17")
  (net 15 "18")
  (net 16 "19")
  (net 17 "20")
  (net 18 "21")
  (net 19 "22")
  (net 20 "23")
  (net 21 "24")
  (net 22 "25")
  (net 23 "26")
  (net 24 "27")
  (net 25 "28")
  (net 26 "2")
  (net 27 "5")
  (net 28 "9")
  (footprint "Package_SO:TSOP-I-28_11.8x8mm_P0.55mm" (layer "F.Cu")
    (tedit 5AC6A6FB)
    (at 111.76 66.675 -90)
    (descr "TSOP I, 28 pins, 18.8x8mm body, 0.55mm pitch, IPC-calculated pads (http://ww1.microchip.com/downloads/en/devicedoc/doc0807.pdf)")
    (tags "TSOP I 28 pins")
    (property "Sheetfile" "tsop-i-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -0.127 -12.954 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "AT28C16-T" (at 0 5.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.5 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -6.27 -3.575 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1") (pinfunction "~{OE}") (pintype "input"))
    (pad "2" smd rect (at -6.27 -3.025 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "2") (pinfunction "n/c") (pintype "passive"))
    (pad "3" smd rect (at -6.27 -2.475 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3") (pinfunction "A9") (pintype "input"))
    (pad "4" smd rect (at -6.27 -1.925 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "4") (pinfunction "A8") (pintype "input"))
    (pad "5" smd rect (at -6.27 -1.375 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "5") (pinfunction "n/c") (pintype "passive"))
    (pad "6" smd rect (at -6.27 -0.825 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "6") (pinfunction "~{WE}") (pintype "input"))
    (pad "7" smd rect (at -6.27 -0.275 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "7") (pinfunction "VCC") (pintype "power_in"))
    (pad "8" smd rect (at -6.27 0.275 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "8") (pinfunction "RDY/~{BUSY}") (pintype "output"))
    (pad "9" smd rect (at -6.27 0.825 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "9") (pinfunction "n/c") (pintype "passive"))
    (pad "10" smd rect (at -6.27 1.375 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "10") (pinfunction "A7") (pintype "input"))
    (pad "11" smd rect (at -6.27 1.925 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "11") (pinfunction "A6") (pintype "input"))
    (pad "12" smd rect (at -6.27 2.475 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "12") (pinfunction "A5") (pintype "input"))
    (pad "13" smd rect (at -6.27 3.025 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "13") (pinfunction "A4") (pintype "input"))
    (pad "14" smd rect (at -6.27 3.575 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "14") (pinfunction "A3") (pintype "input"))
    (pad "15" smd rect (at 6.27 3.575 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "15") (pinfunction "A2") (pintype "input"))
    (pad "16" smd rect (at 6.27 3.025 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "16") (pinfunction "A1") (pintype "input"))
    (pad "17" smd rect (at 6.27 2.475 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "17") (pinfunction "A0") (pintype "input"))
    (pad "18" smd rect (at 6.27 1.925 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "18") (pinfunction "D0") (pintype "bidirectional"))
    (pad "19" smd rect (at 6.27 1.375 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "19") (pinfunction "D1") (pintype "bidirectional"))
    (pad "20" smd rect (at 6.27 0.825 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "20") (pinfunction "D2") (pintype "bidirectional"))
    (pad "21" smd rect (at 6.27 0.275 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "21") (pinfunction "GND") (pintype "output"))
    (pad "22" smd rect (at 6.27 -0.275 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "22") (pinfunction "D3") (pintype "bidirectional"))
    (pad "23" smd rect (at 6.27 -0.825 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "23") (pinfunction "D4") (pintype "bidirectional"))
    (pad "24" smd rect (at 6.27 -1.375 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "24") (pinfunction "D5") (pintype "bidirectional"))
    (pad "25" smd rect (at 6.27 -1.925 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "25") (pinfunction "D6") (pintype "bidirectional"))
    (pad "26" smd rect (at 6.27 -2.475 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "26") (pinfunction "D7") (pintype "bidirectional"))
    (pad "27" smd rect (at 6.27 -3.025 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "27") (pinfunction "~{CE}") (pintype "input"))
    (pad "28" smd rect (at 6.27 -3.575 270) (size 1.87 0.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "28") (pinfunction "A10") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-I-28_11.8x8mm_P0.55mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 101.6 50.165 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (property "Sheetfile" "tsop-i-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.921) (layer "B.SilkS"))
    (fp_text value "Conn_01x14_Male" (at 0 -35.35) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -16.51 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "5") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "6") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "7") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "8") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "9") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "11") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "12") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "13") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "14") (pinfunction "Pin_14") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 121.92 50.165 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (property "Sheetfile" "tsop-i-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 3.556) (layer "B.SilkS"))
    (fp_text value "Conn_01x14_Male" (at 0 -35.35) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -16.51 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "28") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "27") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "26") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "25") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "24") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "23") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "22") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "21") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "20") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "19") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "18") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "17") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "16") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "15") (pinfunction "Pin_14") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 123.444 84.345688) (mid 123.300391 84.692391) (end 122.953688 84.836) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 100.566312 84.836) (end 122.953688 84.836) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 123.444 84.345688) (end 123.444 49.004312) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 100.566312 84.836) (mid 100.219609 84.692391) (end 100.076 84.345688) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 100.076 49.004312) (end 100.076 84.345688) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 100.076 49.004312) (mid 100.219609 48.657609) (end 100.566312 48.514) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 122.953688 48.514) (mid 123.300391 48.657609) (end 123.444 49.004312) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 122.953688 48.514) (end 100.566312 48.514) (layer "Edge.Cuts") (width 0.1))
  (gr_text "CC BY-NC-SA 4.0" (at 111.76 72.136 90) (layer "B.Cu"))
  (gr_text "TSOP-28\nTYPE I\nBREAKOUT" (at 111.76 53.34) (layer "B.SilkS"))
  (gr_text "by @xunker" (at 111.506 58.674) (layer "B.SilkS"))
  (gr_text "1" (at 103.632 50.038) (layer "B.SilkS"))
  (gr_text "28" (at 119.38 50.038) (layer "B.SilkS"))
  (gr_text "1" (at 103.632 50.038) (layer "F.SilkS"))
  (gr_text "1" (at 116.586 58.928 -90) (layer "F.SilkS"))
  (gr_text "TSOP-28 TYPE I\nBREAKOUT" (at 111.506 82.804) (layer "F.SilkS"))
  (gr_text "28" (at 119.38 50.038) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 86.36)
        (xy 96.52 86.36)
        (xy 96.52 45.72)
        (xy 127 45.72)
      )
    )
  )
)
