(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 111)
    (zones 0)
    (modules 13)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.524)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.524)
    (user_trace_width 2.032)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "outputs/"))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad32)")
  (net 2 "Net-(A1-Pad31)")
  (net 3 "Net-(A1-Pad1)")
  (net 4 "Net-(A1-Pad17)")
  (net 5 "Net-(A1-Pad2)")
  (net 6 "Net-(A1-Pad18)")
  (net 7 "Net-(A1-Pad3)")
  (net 8 "Net-(A1-Pad19)")
  (net 9 "Net-(A1-Pad4)")
  (net 10 "Net-(A1-Pad20)")
  (net 11 +5V)
  (net 12 "Net-(A1-Pad21)")
  (net 13 GND)
  (net 14 "Net-(A1-Pad22)")
  (net 15 "Net-(A1-Pad23)")
  (net 16 VCC)
  (net 17 "Net-(A1-Pad24)")
  (net 18 "Net-(A1-Pad9)")
  (net 19 "Net-(A1-Pad25)")
  (net 20 "Net-(A1-Pad10)")
  (net 21 "Net-(A1-Pad26)")
  (net 22 "Net-(A1-Pad11)")
  (net 23 "Net-(A1-Pad27)")
  (net 24 "Net-(A1-Pad12)")
  (net 25 "Net-(A1-Pad28)")
  (net 26 "Net-(A1-Pad13)")
  (net 27 "Net-(A1-Pad14)")
  (net 28 "Net-(A1-Pad30)")
  (net 29 "Net-(A1-Pad15)")
  (net 30 "Net-(A1-Pad16)")
  (net 31 "Net-(C1-Pad2)")
  (net 32 "Net-(C1-Pad1)")
  (net 33 "Net-(C2-Pad1)")
  (net 34 "Net-(C2-Pad2)")
  (net 35 "Net-(J1-Pad1)")
  (net 36 "Net-(J1-Pad2)")
  (net 37 "Net-(U1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad31)")
    (add_net "Net-(A1-Pad32)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(U1-Pad5)")
    (add_net VCC)
  )
  (module Button_Switch_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5D160D14)
    (at 164.9 96.44 180)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW3 (at 6.08 -4.66) (layer F.SilkS))
    (fp_text value SW_SL (at 6.62 9.93) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad27)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 2 thru_hole oval (at 12.5 5 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad27)"))
    (pad 1 thru_hole oval (at 12.5 0 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5D160D14)
    (at 164.9 70.104 180)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW2 (at 6.08 -4.66) (layer F.SilkS))
    (fp_text value SW_UP (at 6.62 9.93) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad26)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 2 thru_hole oval (at 12.5 5 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad26)"))
    (pad 1 thru_hole oval (at 12.5 0 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5D160D14)
    (at 164.9 83.312 180)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW1 (at 6.08 -4.66) (layer F.SilkS))
    (fp_text value SW_DN (at 6.62 9.93) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad25)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 2 thru_hole oval (at 12.5 5 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad25)"))
    (pad 1 thru_hole oval (at 12.5 0 180) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.844 88.9 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad27)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal locked (layer F.Cu) (tedit 5AE5139B)
    (at 148.844 62.484 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad26)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.844 75.692 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad25)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 139.7 92.964 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad20)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal (layer F.Cu) (tedit 5B103613)
    (at 132.08 91.44 270)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags RJ45)
    (fp_text reference J1 (at 4.445 -5 90) (layer F.SilkS))
    (fp_text value RJ45 (at 4.445 4 90) (layer F.Fab))
    (fp_text user %R (at 4.445 2 90) (layer F.Fab))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 31 "Net-(C1-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 32 "Net-(C1-Pad1)"))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 34 "Net-(C2-Pad2)"))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 33 "Net-(C2-Pad1)"))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad20)"))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad1)"))
    (pad "" np_thru_hole circle (at -1.27 6.35 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.16 6.35 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 143.256 98.552 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C3 (at 1.25 -4.4) (layer F.SilkS))
    (fp_text value CP1 (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 139.7 74.676 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.5 -2.5) (layer F.SilkS))
    (fp_text value C (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 132.08 74.676 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.5 -2.5) (layer F.SilkS))
    (fp_text value C (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:Pololu_Breakout-16_15.2x20.3mm (layer F.Cu) (tedit 58AB602C)
    (at 142.24 65.024 270)
    (descr "Pololu Breakout 16-pin 15.2x20.3mm 0.6x0.8\\")
    (tags "Pololu Breakout")
    (fp_text reference U1 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Pololu_motor_driver (at 6.35 20.17 90) (layer F.Fab))
    (fp_text user %R (at 6.35 0 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VCC))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad18)"))
    (pad 15 thru_hole oval (at 12.7 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad17)"))
    (pad 14 thru_hole oval (at 12.7 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C2-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad5)"))
    (pad 13 thru_hole oval (at 12.7 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C2-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad5)"))
    (pad 12 thru_hole oval (at 12.7 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad23)"))
    (pad 11 thru_hole oval (at 12.7 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad22)"))
    (pad 10 thru_hole oval (at 12.7 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad21)"))
    (pad 9 thru_hole oval (at 12.7 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad28)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Pololu_Breakout-16_15.2x20.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:Arduino_UNO_R3 locked (layer B.Cu) (tedit 58AB60FC)
    (at 133.625001 105.41)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (fp_text reference A1 (at 1.27 3.81 -180) (layer B.SilkS))
    (fp_text value Arduino_UNO_R3 (at 0 -22.86) (layer B.Fab))
    (fp_text user %R (at 0 -20.32 -180) (layer B.Fab))
    (pad 32 thru_hole oval (at -9.14 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad32)"))
    (pad 31 thru_hole oval (at -6.6 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad31)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad1)"))
    (pad 17 thru_hole oval (at 30.48 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad17)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad2)"))
    (pad 18 thru_hole oval (at 27.94 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad18)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad3)"))
    (pad 19 thru_hole oval (at 25.4 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad19)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad4)"))
    (pad 20 thru_hole oval (at 22.86 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad20)"))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 21 thru_hole oval (at 20.32 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad21)"))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 22 thru_hole oval (at 17.78 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad22)"))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 23 thru_hole oval (at 13.72 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad23)"))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VCC))
    (pad 24 thru_hole oval (at 11.18 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad24)"))
    (pad 9 thru_hole oval (at 22.86 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad9)"))
    (pad 25 thru_hole oval (at 8.64 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad25)"))
    (pad 10 thru_hole oval (at 25.4 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad10)"))
    (pad 26 thru_hole oval (at 6.1 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad26)"))
    (pad 11 thru_hole oval (at 27.94 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad11)"))
    (pad 27 thru_hole oval (at 3.56 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad27)"))
    (pad 12 thru_hole oval (at 30.48 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad12)"))
    (pad 28 thru_hole oval (at 1.02 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad28)"))
    (pad 13 thru_hole oval (at 33.02 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad13)"))
    (pad 29 thru_hole oval (at -1.52 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 14 thru_hole oval (at 35.56 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad14)"))
    (pad 30 thru_hole oval (at -4.06 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad30)"))
    (pad 15 thru_hole oval (at 35.56 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-Pad15)"))
    (pad 16 thru_hole oval (at 33.02 -48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(A1-Pad16)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_UNO_R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 172.212 108.204) (end 172.212 54.356) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.412 108.204) (end 172.212 108.204) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.412 54.356) (end 121.412 108.204) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.212 54.356) (end 121.412 54.356) (layer Edge.Cuts) (width 0.05))
  (gr_text "Antenna Driver\n20.01.07" (at 169.672 86.868 90) (layer B.SilkS))
  (gr_text - (at 169.799 77.978) (layer F.Cu))
  (gr_text + (at 169.799 70.104) (layer F.Cu))
  (gr_text S (at 169.672 93.472 180) (layer F.Cu))
  (zone (net 13) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.704 107.696) (xy 121.92 107.696) (xy 121.92 54.864) (xy 171.704 54.864)
      )
    )
  )
)
