(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 87)
    (no_connects 0)
    (area 117.08 69.365 200.235001 131.993096)
    (thickness 1.6)
    (drawings 21)
    (tracks 210)
    (zones 0)
    (modules 27)
    (nets 22)
  )
  (page USLetter)
  (title_block
    (title "NeoPixel and potentiometer adapter for micro:bit")
    (date 2018-09-23)
    (rev 2.0)
    (company "Patrick Pelletier")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEE77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C4-Pad1)")
  (net 4 +3V3)
  (net 5 /P0)
  (net 6 /P1)
  (net 7 /P2)
  (net 8 "Net-(R2-Pad1)")
  (net 9 +VDC)
  (net 10 /SDA)
  (net 11 /SCL)
  (net 12 /SCK)
  (net 13 /MOSI)
  (net 14 /P16)
  (net 15 "Net-(J6-Pad2)")
  (net 16 /SCK5)
  (net 17 /MOSI5)
  (net 18 "Net-(C8-Pad1)")
  (net 19 "Net-(C8-Pad2)")
  (net 20 "Net-(C10-Pad1)")
  (net 21 "Net-(C9-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net +VDC)
    (add_net /MOSI)
    (add_net /MOSI5)
    (add_net /P0)
    (add_net /P1)
    (add_net /P16)
    (add_net /P2)
    (add_net /SCK)
    (add_net /SCK5)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(R2-Pad1)")
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5BA7C655)
    (at 173.99 111.76 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 6.858 -4.318 180) (layer F.SilkS))
    (fp_text value 1000µF (at 2.5 6.31 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 +VDC))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5BA6643D)
    (at 146.05 116.84)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C2 (at -2.54 -0.635) (layer F.SilkS))
    (fp_text value 0.1µF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5BA7C5CC)
    (at 163.83 111.125 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 6.985 0 360) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +VDC))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5BA7C5BC)
    (at 154.305 111.125 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 6.985 -0.127 360) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:BarrelJack_CUI_PJ-063AH_Horizontal_CircularHoles (layer F.Cu) (tedit 5BA663AF)
    (at 183.515 122.555 90)
    (descr "Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf")
    (tags "barrel jack cui dc power")
    (fp_text reference J2 (at 3.81 -1.905 90) (layer F.SilkS))
    (fp_text value Barrel_Jack_MountingPin (at 0 13 90) (layer F.Fab))
    (fp_text user %R (at 0 5.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 9 +VDC))
    (pad 2 thru_hole circle (at 0 6 90) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at -4.5 7 90) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 4.5 7 90) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 9 90) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal_CircularHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5BA663EB)
    (at 150.495 106.045 270)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value 74AHCT125 (at 3.81 17.57 270) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /MOSI5))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /P16))
    (pad 9 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /MOSI))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /SCK))
    (pad 12 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /SCK5))
    (pad 13 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5BA7C5DF)
    (at 160.274 115.57 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U2 (at -1.27 -2.54 180) (layer F.SilkS))
    (fp_text value MCP1702-3302E_TO92 (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 +VDC))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module footprints:Bourns_PTA4543 (layer F.Cu) (tedit 5BA66418)
    (at 120.65 97.79)
    (descr "Bourns single-gang slide potentiometer, 45mm travel")
    (tags "Bourns single-gang slide potentiometer 45mm")
    (fp_text reference RV1 (at 47.625 7.62) (layer F.SilkS))
    (fp_text value 10K (at 29.25 7.5) (layer F.Fab))
    (fp_text user %R (at 29.25 1.75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 3.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 3 thru_hole circle (at 58.5 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad MP thru_hole circle (at 5.35 -2.45) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 53.15 -2.45) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 4.15 5.95) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 54.35 5.95) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometers_THT.3dshapes/Bourns_PTA4543.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Bourns_PTA4543 (layer F.Cu) (tedit 5BA6640B)
    (at 120.65 121.92)
    (descr "Bourns single-gang slide potentiometer, 45mm travel")
    (tags "Bourns single-gang slide potentiometer 45mm")
    (fp_text reference RV2 (at 46.99 -3.81) (layer F.SilkS))
    (fp_text value 10K (at 29.25 7.5) (layer F.Fab))
    (fp_text user %R (at 29.25 1.75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 3.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 3 thru_hole circle (at 58.5 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad MP thru_hole circle (at 5.35 -2.45) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 53.15 -2.45) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 4.15 5.95) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 54.35 5.95) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometers_THT.3dshapes/Bourns_PTA4543.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Fingerprint (layer B.Cu) (tedit 0)
    (at 161.29 123.825 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 140.97 123.825 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5BA66DBE)
    (at 135.255 116.84)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 7.62 0.635) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +VDC))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5BA66DD6)
    (at 125.73 115.57 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.54 -2.54 180) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 2.56 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled (layer F.Cu) (tedit 5BA6647F)
    (at 122.555 109.855 270)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J3 (at 3.175 -3.175 270) (layer F.SilkS))
    (fp_text value Qwiic (at 0 4.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at 0.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /SDA))
    (pad 4 smd rect (at 1.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCL))
    (pad "" smd rect (at -2.8 1.9375 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.8 1.9375 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module footprints:TerminalBlock_4Ucon_1x04_P3.50mm_Vertical (layer F.Cu) (tedit 5BA7C776)
    (at 191.77 88.9 180)
    (descr "Terminal Block 4Ucon ItemNo. 10695, vertical (cable from top), 4 pins, pitch 3.5mm, size 15.0x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10695.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10695 vertical pitch 3.5mm size 15.0x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J4 (at 11.176 -4.572 180) (layer F.SilkS))
    (fp_text value DotStars (at 5.25 5.66 180) (layer F.Fab))
    (fp_text user %R (at 5.25 3.45 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 +VDC))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 /SCK5))
    (pad 3 thru_hole circle (at 7 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 /MOSI5))
    (pad 4 thru_hole circle (at 10.5 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x04_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:TerminalBlock_4Ucon_1x03_P3.50mm_Vertical (layer F.Cu) (tedit 5BA7CB37)
    (at 191.008 103.632 90)
    (descr "Terminal Block 4Ucon ItemNo. 10694, vertical (cable from top), 3 pins, pitch 3.5mm, size 11.5x8.3mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.4uconnector.com/online/object/4udrawing/10694.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 10694 vertical pitch 3.5mm size 11.5x8.3mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J6 (at 9.144 -4.572 180) (layer F.SilkS))
    (fp_text value NeoPixels (at 3.5 5.66 90) (layer F.Fab))
    (fp_text user %R (at 3.5 3.45 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 +VDC))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(J6-Pad2)"))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5BA66467)
    (at 128.905 116.205)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U3 (at 3.81 -2.54) (layer F.SilkS))
    (fp_text value MCP1702-5002E_TO92 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 +VDC))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5BA663EF)
    (at 164.465 107.315 180)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 10.16 0.635 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 3.81 2.41 180) (layer F.Fab))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SJ1-3533NG (layer F.Cu) (tedit 5BA663AA)
    (at 194.31 111.125 270)
    (descr https://www.cui.com/product/resource/sj1-353xng.pdf)
    (tags "audio jack stereo")
    (fp_text reference J1 (at 5.715 11.43 270) (layer F.SilkS))
    (fp_text value AudioJack3_Ground (at 0.1 14.05 270) (layer F.Fab))
    (fp_text user %R (at 0.1 3.8 270) (layer F.Fab))
    (pad S thru_hole circle (at 0 0 270) (size 2.8 2.8) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad T thru_hole circle (at 2 2.4 270) (size 2.8 2.8) (drill 2) (layers *.Cu *.Mask)
      (net 19 "Net-(C8-Pad2)"))
    (pad R thru_hole circle (at 2 7.9 270) (size 2.8 2.8) (drill 2) (layers *.Cu *.Mask)
      (net 21 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/SJ1-3533NG.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5BA66460)
    (at 128.27 109.22)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C7 (at 3.81 -3.175) (layer F.SilkS))
    (fp_text value 47µF (at 1.25 4.46) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:4UCON_10156_2x40_P1.27mm_Socket_Horizontal (layer F.Cu) (tedit 5BA6E10F)
    (at 172.72 91.44 180)
    (descr "Card edge socket with 80 contacts (40 each side), through-hole, http://www.4uconnector.com/online/object/4udrawing/10156.pdf")
    (tags "bbc microbit edge connector right-angle")
    (fp_text reference J5 (at 24.765 -2.54 180) (layer F.SilkS))
    (fp_text value microbit_edge_connector (at 24.765 21.1 180) (layer F.Fab))
    (fp_text user %R (at 24.765 9.165 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 1.27 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.54 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 3.81 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 3.81 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 5.08 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 6.35 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at 6.35 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 7.62 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SDA))
    (pad 14 thru_hole circle (at 7.62 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 8.89 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCL))
    (pad 16 thru_hole circle (at 8.89 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 10.16 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 18 thru_hole circle (at 10.16 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 11.43 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 20 thru_hole circle (at 11.43 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 12.7 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 22 thru_hole circle (at 12.7 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 13.97 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 24 thru_hole circle (at 13.97 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 15.24 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 26 thru_hole circle (at 15.24 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at 16.51 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 28 thru_hole circle (at 16.51 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at 17.78 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 14 /P16))
    (pad 30 thru_hole circle (at 17.78 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 19.05 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 /MOSI))
    (pad 32 thru_hole circle (at 19.05 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 20.32 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 20.32 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 21.59 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SCK))
    (pad 36 thru_hole circle (at 21.59 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 22.86 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 38 thru_hole circle (at 22.86 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 24.13 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 40 thru_hole circle (at 24.13 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 41 thru_hole circle (at 25.4 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 42 thru_hole circle (at 25.4 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at 26.67 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 44 thru_hole circle (at 26.67 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 45 thru_hole circle (at 27.94 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 46 thru_hole circle (at 27.94 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 47 thru_hole circle (at 29.21 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 48 thru_hole circle (at 29.21 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at 30.48 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 50 thru_hole circle (at 30.48 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 51 thru_hole circle (at 31.75 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 52 thru_hole circle (at 31.75 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 53 thru_hole circle (at 33.02 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 54 thru_hole circle (at 33.02 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 55 thru_hole circle (at 34.29 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 56 thru_hole circle (at 34.29 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 57 thru_hole circle (at 35.56 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 58 thru_hole circle (at 35.56 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 59 thru_hole circle (at 36.83 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 60 thru_hole circle (at 36.83 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 61 thru_hole circle (at 38.1 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 62 thru_hole circle (at 38.1 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 63 thru_hole circle (at 39.37 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 64 thru_hole circle (at 39.37 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 65 thru_hole circle (at 40.64 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 66 thru_hole circle (at 40.64 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 67 thru_hole circle (at 41.91 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 68 thru_hole circle (at 41.91 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 69 thru_hole circle (at 43.18 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 70 thru_hole circle (at 43.18 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 71 thru_hole circle (at 44.45 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 72 thru_hole circle (at 44.45 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 73 thru_hole circle (at 45.72 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 74 thru_hole circle (at 45.72 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 75 thru_hole circle (at 46.99 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 76 thru_hole circle (at 46.99 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 77 thru_hole circle (at 48.26 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 78 thru_hole circle (at 48.26 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 79 thru_hole circle (at 49.53 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad 80 thru_hole circle (at 49.53 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PCBEdge.3dshapes/4UCON_10156_2x40_P1.27mm_Socket_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5BA7CB1C)
    (at 182.626 97.028)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C8 (at -1.27 2.54) (layer F.SilkS))
    (fp_text value 220uF (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5BA7CB14)
    (at 182.626 102.87)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C9 (at -1.27 2.54) (layer F.SilkS))
    (fp_text value 220uF (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5BA7C67A)
    (at 179.07 113.03 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C10 (at -1.524 0.508 180) (layer F.SilkS))
    (fp_text value 10nF (at 1.25 2.61 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5BA7C5F3)
    (at 177.165 107.315)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.905 -1.651) (layer F.SilkS))
    (fp_text value 100 (at 1.27 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C8-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /P0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5BA7C5E6)
    (at 158.115 111.76)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 1.905 -1.778) (layer F.SilkS))
    (fp_text value 470 (at 1.27 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5BA7C601)
    (at 177.165 116.205)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 2.159 1.905) (layer F.SilkS))
    (fp_text value 22 (at 1.27 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /P0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text QWIIC (at 120.65 109.855 270) (layer B.SilkS))
  (gr_text DotStars (at 186.69 91.44) (layer B.SilkS))
  (gr_text GND (at 181.356 87.376 90) (layer B.SilkS))
  (gr_text DAT (at 184.912 87.376 90) (layer B.SilkS))
  (gr_text CLK (at 188.468 87.376 90) (layer B.SilkS))
  (gr_text +V (at 191.77 87.376 90) (layer B.SilkS))
  (gr_text headphones (at 190.754 108.458) (layer B.SilkS))
  (gr_line (start 121.285 129.54) (end 193.675 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.285 83.82) (end 193.675 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text NeoPixels (at 187.96 99.695 90) (layer B.SilkS))
  (gr_text "5-12VDC IN" (at 194.945 122.555 90) (layer B.SilkS))
  (gr_text DATA (at 192.405 100.33) (layer B.SilkS))
  (gr_text GND (at 192.405 96.52) (layer B.SilkS))
  (gr_text +V (at 192.405 103.505) (layer B.SilkS))
  (gr_text "2018-09-23\nhttps://github.com/ppelleti/NeoBit\ndesigned by Patrick Pelletier" (at 154.94 99.06) (layer B.SilkS))
  (gr_line (start 196.215 127) (end 196.215 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.745 86.36) (end 118.745 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 193.675 127) (end 196.215 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 193.675 86.36) (end 193.675 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.285 127) (end 121.285 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.285 86.36) (end 118.745 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 9) (net_name +VDC) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.31 85.725) (xy 194.31 108.585) (xy 187.96 108.585) (xy 187.96 123.825) (xy 171.45 123.825)
        (xy 171.45 106.68) (xy 190.5 85.725)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.215 129.54) (xy 118.745 129.54) (xy 118.745 83.82) (xy 196.215 83.82)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.215 129.54) (xy 118.745 129.54) (xy 118.745 83.82) (xy 196.215 83.82)
      )
    )
  )
)
