<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="-0.127" y1="5.207" x2="27.93945" y2="5.207" width="0" layer="20"/>
<wire x1="27.93945" y1="5.207" x2="31.040034375" y2="8.304659375" width="0" layer="20"/>
<wire x1="31.040034375" y1="8.304659375" x2="31.0488625" y2="34.742378125" width="0" layer="20"/>
<wire x1="31.0488625" y1="34.742378125" x2="28.199325" y2="37.582" width="0" layer="20"/>
<wire x1="28.199325" y1="37.582" x2="3.03275" y2="37.582" width="0" layer="20"/>
<wire x1="3.03275" y1="37.582" x2="-0.116025" y2="34.422065625" width="0" layer="20"/>
<wire x1="-0.116025" y1="34.422065625" x2="-0.127" y2="5.207" width="0" layer="20"/>
<text>suchahardvibe
v1.4  2018
Berlin, 
Germany
</text>
<text>made 
with 
 &lt;3</text>
<text>IN</text>
<text>+9V</text>
<text>GND</text>
<text>OUT</text>
<text>suchahardman.com</text>
</plain>
<libraries>
<library name="caps-film">
<packages>
<package name="0.2&quot;.SML">
<description>0.2" (5.08mm) spacing
&lt;p&gt;
&lt;b&gt; 
10pf - 180n&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diodes">
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
<package name="DO35-3">
<description>&lt;B&gt;DO-35 0.3" spacing&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="9MM_METAL_SHAFT">
<description>&lt;b&gt;9mm / Right-Angle /  PC Mount / Metal Shaft&lt;/b&gt;
&lt;p&gt;
&lt;a href="http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-9mm-right-angle-pc-mount/"&gt;http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-9mm-right-angle-pc-mount/&lt;/a&gt;</description>
</package>
<package name="TRIM1">
<description>&lt;b&gt;Bourns 3362p&lt;/b&gt;
&lt;p&gt;
&lt;a href="http://www.taydaelectronics.com/potentiometer-variable-resistors/cermet-potentiometers/3362p.html"&gt;http://www.taydaelectronics.com/potentiometer-variable-resistors/cermet-potentiometers/3362p.html&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="transistors-BJT">
<packages>
<package name="TO92">
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT54E">
<description>&lt;b&gt;SOT-54&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="0.2&quot;">
<description>0.2"  (5mm) lead spacing, 1/8W (flat), 1/4W (standing)</description>
</package>
</packages>
</library>
<library name="supply pins">
<packages>
<package name="PAD2">
<description>&lt;b&gt;Round Pad (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
<package name="PAD4">
<description>&lt;b&gt;Square (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="caps-film" package="0.2&quot;.SML" value="100nF"/>
<element name="C2" library="caps-film" package="0.2&quot;.SML" value="100nF"/>
<element name="C3" library="caps-film" package="0.2&quot;.SML" value="100nF"/>
<element name="C4" library="caps-film" package="0.2&quot;.SML" value="100nF"/>
<element name="C5" library="gm-caps-electro-pol" package="050_020_1" value="10uF"/>
<element name="C6" library="caps-film" package="0.2&quot;.SML" value="100nF"/>
<element name="D1" library="diodes" package="DO41-3" value="6v8">
<attribute name="NAME"/>
</element>
<element name="D2" library="diodes" package="DO35-3" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D3" library="diodes" package="DO35-3" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="DEPTH" library="potentiometers" package="9MM_METAL_SHAFT" value="100k B">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="Q1" library="transistors-BJT" package="TO92" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="Q2" library="transistors-BJT" package="TO92" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="Q3" library="transistor-small-signal" package="SOT54E" value="BS170">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistors" package="0.2&quot;" value="27k"/>
<element name="R10" library="resistors" package="0.2&quot;" value="1M"/>
<element name="R11" library="resistors" package="0.2&quot;" value="100k"/>
<element name="R12" library="resistors" package="0.2&quot;" value="5k1"/>
<element name="R2" library="resistors" package="0.2&quot;" value="27k"/>
<element name="R3" library="resistors" package="0.2&quot;" value="120k"/>
<element name="R4" library="resistors" package="0.2&quot;" value="1M"/>
<element name="R5" library="resistors" package="0.2&quot;" value="39k"/>
<element name="R6" library="resistors" package="0.2&quot;" value="3k3"/>
<element name="R7" library="resistors" package="0.2&quot;" value="560k"/>
<element name="R8" library="resistors" package="0.2&quot;" value="560k"/>
<element name="R9" library="resistors" package="0.2&quot;" value="1M"/>
<element name="RATE" library="potentiometers" package="9MM_METAL_SHAFT" value="100k B">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="TREM" library="potentiometers" package="TRIM1" value="1M"/>
<element name="BOOST" library="potentiometers" package="TRIM1" value="5k"/>
<element name="U$2" library="supply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="U$1" library="supply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="U$3" library="supply pins" package="PAD4" value="PADS.SQR_NL"/>
<element name="U$4" library="supply pins" package="PAD4" value="PADS.SQR_NL"/>
<element name="U$5" library="supply pins" package="PAD4" value="PADS.SQR_NL"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="TREM" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="Q2" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="BOOST" pad="1"/>
<contactref element="BOOST" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="Q1" pad="3"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="RATE" pad="P$1"/>
<contactref element="RATE" pad="P$2"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="1"/>
<contactref element="TREM" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="TREM" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="+9V">
<contactref element="DEPTH" pad="P$1"/>
<contactref element="R5" pad="1"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C1" pad="1"/>
<contactref element="DEPTH" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="C2" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="DEPTH" pad="P$3"/>
</signal>
<signal name="N$9">
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="2"/>
<contactref element="RATE" pad="P$3"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="Q2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="Q3" pad="G"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R12" pad="1"/>
<contactref element="Q3" pad="D"/>
<contactref element="R9" pad="2"/>
<contactref element="C5" pad="+"/>
</signal>
<signal name="N$14">
<contactref element="D2" pad="C"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R2" pad="1"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="BOOST" pad="3"/>
<contactref element="Q3" pad="S"/>
</signal>
<signal name="OUT">
<contactref element="R11" pad="2"/>
<contactref element="C5" pad="-"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="IN">
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
