(kicad_pcb (version 20171130) (host pcbnew 5.1.6)
  (general
    (thickness 1.6)
    (drawings 105)
    (tracks 885)
    (zones 0)
    (modules 91)
    (nets 72)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.7 0.7)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 146.445 95.488)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /D0)
  (net 3 /D1)
  (net 4 /D2)
  (net 5 GND)
  (net 6 /D3)
  (net 7 /D4)
  (net 8 /D5)
  (net 9 /D6)
  (net 10 /D7)
  (net 11 +3V3)
  (net 12 /CLK)
  (net 13 /WR)
  (net 14 /RD)
  (net 15 /CS)
  (net 16 /A0)
  (net 17 /A1)
  (net 18 /A2)
  (net 19 /A3)
  (net 20 /A4)
  (net 21 /A5)
  (net 22 /A6)
  (net 23 /A7)
  (net 24 /A8)
  (net 25 /A9)
  (net 26 /A10)
  (net 27 /A11)
  (net 28 /A12)
  (net 29 /A13)
  (net 30 /A14)
  (net 31 /A15)
  (net 32 /RESET)
  (net 33 /DATA_OE)
  (net 34 /DIR)
  (net 35 /3V_D0)
  (net 36 /3V_D1)
  (net 37 /3V_D2)
  (net 38 /3V_D3)
  (net 39 /3V_D4)
  (net 40 /3V_D5)
  (net 41 /3V_D6)
  (net 42 /3V_D7)
  (net 43 /GB_RESET)
  (net 44 /3V_A12)
  (net 45 /3V_A13)
  (net 46 /3V_A14)
  (net 47 /3V_A15)
  (net 48 /3V_A11)
  (net 49 /3V_A10)
  (net 50 /3V_A9)
  (net 51 /3V_A8)
  (net 52 /3V_A7)
  (net 53 /3V_A6)
  (net 54 /3V_A5)
  (net 55 /3V_A4)
  (net 56 /3V_CLK)
  (net 57 /3V_WR)
  (net 58 /3V_RD)
  (net 59 /3V_CS)
  (net 60 /3V_A0)
  (net 61 /3V_A1)
  (net 62 /3V_A2)
  (net 63 /3V_A3)
  (net 64 "Net-(D3-Pad1)")
  (net 65 /AUD)
  (net 66 "Net-(J1-Pad1)")
  (net 67 "Net-(J2-Pad1)")
  (net 68 "Net-(U3-Pad3)")
  (net 69 "Net-(U3-Pad5)")
  (net 70 "Net-(U3-Pad7)")
  (net 71 "Net-(U3-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /3V_A0)
    (add_net /3V_A1)
    (add_net /3V_A10)
    (add_net /3V_A11)
    (add_net /3V_A12)
    (add_net /3V_A13)
    (add_net /3V_A14)
    (add_net /3V_A15)
    (add_net /3V_A2)
    (add_net /3V_A3)
    (add_net /3V_A4)
    (add_net /3V_A5)
    (add_net /3V_A6)
    (add_net /3V_A7)
    (add_net /3V_A8)
    (add_net /3V_A9)
    (add_net /3V_CLK)
    (add_net /3V_CS)
    (add_net /3V_D0)
    (add_net /3V_D1)
    (add_net /3V_D2)
    (add_net /3V_D3)
    (add_net /3V_D4)
    (add_net /3V_D5)
    (add_net /3V_D6)
    (add_net /3V_D7)
    (add_net /3V_RD)
    (add_net /3V_WR)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AUD)
    (add_net /CLK)
    (add_net /CS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DATA_OE)
    (add_net /DIR)
    (add_net /GB_RESET)
    (add_net /RD)
    (add_net /RESET)
    (add_net /WR)
    (add_net GND)
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad9)")
  )
  (module chickadee:chickadee_3mm_fcu (layer F.Cu) (tedit 0)
    (at 122.95 60.309 180)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Chickadee 3mm" (at 0.75 0) (layer F.SilkS) hide)
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 132.348 57.642 90)
    (fp_text reference TP39 (at 0 2.25 90) (layer F.SilkS) hide)
    (fp_text value batt (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module adafruit:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 5F3C9C70)
    (at 136.285 44.053 90)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J6 (at 0 -4.235 90) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 37 /3V_D2))
    (pad 4 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 36 /3V_D1))
    (pad 5 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 38 /3V_D3))
    (pad 6 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 35 /3V_D0))
    (pad 7 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 39 /3V_D4))
    (pad 8 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 42 /3V_D7))
    (pad 9 smd rect (at -1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 40 /3V_D5))
    (pad 10 smd rect (at 1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 41 /3V_D6))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 5F3C9C70)
    (at 124.855 51.038 90)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J5 (at 0 -4.235 90) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 49 /3V_A10))
    (pad 4 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 50 /3V_A9))
    (pad 5 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 48 /3V_A11))
    (pad 6 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 51 /3V_A8))
    (pad 7 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 44 /3V_A12))
    (pad 8 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 47 /3V_A15))
    (pad 9 smd rect (at -1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 45 /3V_A13))
    (pad 10 smd rect (at 1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 46 /3V_A14))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 5F3C9C70)
    (at 115.33 43.418 90)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J4 (at 0 -4.235 90) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 62 /3V_A2))
    (pad 4 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 61 /3V_A1))
    (pad 5 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 63 /3V_A3))
    (pad 6 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 60 /3V_A0))
    (pad 7 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 55 /3V_A4))
    (pad 8 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 52 /3V_A7))
    (pad 9 smd rect (at -1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 54 /3V_A5))
    (pad 10 smd rect (at 1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 53 /3V_A6))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 5F3C9C70)
    (at 107.075 51.673 90)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J3 (at 0 -4.235 90) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 58 /3V_RD))
    (pad 4 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 57 /3V_WR))
    (pad 5 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 59 /3V_CS))
    (pad 6 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 56 /3V_CLK))
    (pad 7 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 65 /AUD))
    (pad 8 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 33 /DATA_OE))
    (pad 9 smd rect (at -1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 43 /GB_RESET))
    (pad 10 smd rect (at 1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 34 /DIR))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 103.9 40.878)
    (fp_text reference TP38 (at 0 2.25) (layer F.SilkS) hide)
    (fp_text value 3.3v (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 103.9 44.434)
    (fp_text reference TP37 (at 0 2.25) (layer F.SilkS) hide)
    (fp_text value gnd (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 147.715 45.323 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducial:Fiducial_1mm_Mask2mm (layer F.Cu) (tedit 5C85CF20)
    (at 138.945 82.488)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID0 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial:Fiducial_1mm_Mask2mm (layer F.Cu) (tedit 5C85C699)
    (at 102.1474 54.0352)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID1 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C2C9)
    (at 146.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP78 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 65 /AUD))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1D2)
    (at 101.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP48 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 1 +5V))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C230)
    (at 132.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP69 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 2 /D0))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1D7)
    (at 102.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP49 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 12 /CLK))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1DC)
    (at 104.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP50 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 /WR))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1E2)
    (at 105.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP51 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 /RD))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1E7)
    (at 107.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP52 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 15 /CS))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1EB)
    (at 108.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP53 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 16 /A0))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C233)
    (at 131.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP68 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 31 /A15))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C25E)
    (at 147.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP79 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 5 GND))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C25A)
    (at 144.945 92.5)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP77 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 32 /RESET))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C253)
    (at 143.445 95.377)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP76 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 10 /D7))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C250)
    (at 141.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP75 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 9 /D6))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C24B)
    (at 140.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP74 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 8 /D5))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C247)
    (at 138.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP73 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 7 /D4))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C242)
    (at 137.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP72 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 6 /D3))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C22B)
    (at 129.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP67 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 30 /A14))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C227)
    (at 128.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP66 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 29 /A13))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1F6)
    (at 110.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP54 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 17 /A1))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1F2)
    (at 111.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP55 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 18 /A2))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1FA)
    (at 113.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP56 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 /A3))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C1FE)
    (at 114.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP57 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 /A4))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C224)
    (at 125.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP64 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 27 /A11))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C207)
    (at 116.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP58 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 /A5))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C203)
    (at 117.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP59 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 /A6))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C20B)
    (at 119.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP60 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 /A7))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C23E)
    (at 134.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP70 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 3 /D1))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C20F)
    (at 120.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP61 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 /A8))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C218)
    (at 122.445 95.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP62 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 25 /A9))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C214)
    (at 123.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP63 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 26 /A10))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C21F)
    (at 126.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP65 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 28 /A12))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5C85C239)
    (at 135.945 92.488)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP71 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 4 /D2))
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5C84B884)
    (at 145.175 45.323 270)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D3 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(D3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 133.945 80.738 90)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 4.519 180) (layer F.SilkS))
    (fp_text value 74LVC244 (at 0 4.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at -2.95 -2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 /A12))
    (pad 3 smd rect (at -2.95 -1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 /A13))
    (pad 5 smd rect (at -2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 /A14))
    (pad 7 smd rect (at -2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -2.95 1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 /A15))
    (pad 9 smd rect (at -2.95 2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at -2.95 2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 11 smd rect (at 2.95 2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 12 smd rect (at 2.95 2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 47 /3V_A15))
    (pad 13 smd rect (at 2.95 1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 14 smd rect (at 2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 /3V_A14))
    (pad 15 smd rect (at 2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 16 smd rect (at 2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 /3V_A13))
    (pad 17 smd rect (at 2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 18 smd rect (at 2.95 -1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 /3V_A12))
    (pad 19 smd rect (at 2.95 -2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 20 smd rect (at 2.95 -2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 115.824 82.296)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at -0.0295 4.2545) (layer F.SilkS))
    (fp_text value 74LVC244 (at 0 4.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 /3V_A7))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 /A11))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 /3V_A6))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 /A10))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 54 /3V_A5))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 /A9))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 /3V_A4))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 /A8))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 /3V_A8))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /A4))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 /3V_A9))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /A5))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 49 /3V_A10))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 /A6))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 /3V_A11))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 /A7))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 105.664 82.296)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U6 (at 0.161 4.2545) (layer F.SilkS))
    (fp_text value 74LVC244 (at 0 4.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 /CLK))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 /3V_A0))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 /WR))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 61 /3V_A1))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 /RD))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 62 /3V_A2))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /CS))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 /3V_A3))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 /A3))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 59 /3V_CS))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 /A2))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 58 /3V_RD))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 /A1))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 57 /3V_WR))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 /A0))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 /3V_CLK))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 140.73 52.943 90)
    (descr "TSSOP24: plastic thin shrink small outline package; 24 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot355-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U5 (at -0.014 0.016 270) (layer F.SilkS))
    (fp_text value 74x4245 (at 0 4.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 /DIR))
    (pad 3 smd rect (at -2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /D0))
    (pad 4 smd rect (at -2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /D1))
    (pad 5 smd rect (at -2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /D2))
    (pad 6 smd rect (at -2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /D3))
    (pad 7 smd rect (at -2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /D4))
    (pad 8 smd rect (at -2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /D5))
    (pad 9 smd rect (at -2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /D6))
    (pad 10 smd rect (at -2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /D7))
    (pad 11 smd rect (at -2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 12 smd rect (at -2.85 3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 13 smd rect (at 2.85 3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 14 smd rect (at 2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 /3V_D7))
    (pad 15 smd rect (at 2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 /3V_D6))
    (pad 16 smd rect (at 2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 /3V_D5))
    (pad 17 smd rect (at 2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 /3V_D4))
    (pad 18 smd rect (at 2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 /3V_D3))
    (pad 19 smd rect (at 2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 /3V_D2))
    (pad 20 smd rect (at 2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 /3V_D1))
    (pad 21 smd rect (at 2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /3V_D0))
    (pad 22 smd rect (at 2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /DATA_OE))
    (pad 23 smd rect (at 2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 24 smd rect (at 2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-24_4.4x7.8mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 137.287 65.532 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.54 -0.034 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /GB_RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 127.903 42.021 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.6965 -0.0635 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /DATA_OE))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 135.015 54.707 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 135.015 51.038 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at -0.127 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 129.445 80.137 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at -2.54 -0.0655 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 111.887 77.724)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 3.0185 0.0635) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 121.5022 79.0288 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at 3.125129 0 45) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.874999 0 45) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.874999 0 45) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gameboy:Cartridge (layer F.Cu) (tedit 5B6F11B9)
    (at 123.445 96.988)
    (fp_text reference U1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value CARTRIDGE (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at -22 -2.54) (size 1.4 6) (drill (offset -0.2 0)) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -20.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 12 /CLK))
    (pad 3 smd rect (at -19 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 13 /WR))
    (pad 4 smd rect (at -17.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 14 /RD))
    (pad 5 smd rect (at -16 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 15 /CS))
    (pad 6 smd rect (at -14.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 16 /A0))
    (pad 7 smd rect (at -13 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 17 /A1))
    (pad 8 smd rect (at -11.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 18 /A2))
    (pad 9 smd rect (at -10 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 19 /A3))
    (pad 10 smd rect (at -8.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 20 /A4))
    (pad 11 smd rect (at -7 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 21 /A5))
    (pad 12 smd rect (at -5.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 22 /A6))
    (pad 13 smd rect (at -4 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 23 /A7))
    (pad 14 smd rect (at -2.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 24 /A8))
    (pad 15 smd rect (at -1 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 25 /A9))
    (pad 16 smd rect (at 0.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 26 /A10))
    (pad 17 smd rect (at 2 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 27 /A11))
    (pad 18 smd rect (at 3.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 28 /A12))
    (pad 19 smd rect (at 5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 29 /A13))
    (pad 20 smd rect (at 6.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 30 /A14))
    (pad 21 smd rect (at 8 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 31 /A15))
    (pad 22 smd rect (at 9.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 2 /D0))
    (pad 23 smd rect (at 11 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 3 /D1))
    (pad 24 smd rect (at 12.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 4 /D2))
    (pad 25 smd rect (at 14 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 6 /D3))
    (pad 26 smd rect (at 15.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 7 /D4))
    (pad 27 smd rect (at 17 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 8 /D5))
    (pad 28 smd rect (at 18.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 9 /D6))
    (pad 29 smd rect (at 20 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 10 /D7))
    (pad 30 smd rect (at 21.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 32 /RESET))
    (pad 31 smd rect (at 23 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 65 /AUD))
    (pad 32 smd rect (at 24.5 -2.5) (size 1.4 6) (drill (offset 0.2 0)) (layers F.Cu F.Mask)
      (net 5 GND))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 110.445 87.738)
    (fp_text reference TP7 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 17 /A1))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 120.945 87.738)
    (fp_text reference TP14 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 24 /A8))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 111.945 87.738)
    (fp_text reference TP8 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 18 /A2))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 108.945 87.738)
    (fp_text reference TP6 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 16 /A0))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 107.445 87.738)
    (fp_text reference TP5 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 15 /CS))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 105.945 87.738)
    (fp_text reference TP4 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 14 /RD))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 104.445 87.738)
    (fp_text reference TP3 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 13 /WR))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 102.945 87.738)
    (fp_text reference TP2 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 12 /CLK))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 101.219 87.738)
    (fp_text reference TP1 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 1 +5V))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 122.445 87.738)
    (fp_text reference TP15 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 25 /A9))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 123.945 87.738)
    (fp_text reference TP16 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 26 /A10))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 125.445 87.738)
    (fp_text reference TP17 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 27 /A11))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 126.945 87.738)
    (fp_text reference TP18 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 28 /A12))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 128.445 87.738)
    (fp_text reference TP19 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 29 /A13))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 114.945 87.738)
    (fp_text reference TP10 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 20 /A4))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 129.945 87.738)
    (fp_text reference TP20 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 30 /A14))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 116.445 87.738)
    (fp_text reference TP11 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 21 /A5))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 117.945 87.738)
    (fp_text reference TP12 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 22 /A6))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 131.445 87.738)
    (fp_text reference TP21 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 31 /A15))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 132.945 87.738)
    (fp_text reference TP22 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 2 /D0))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 134.445 87.738)
    (fp_text reference TP23 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 3 /D1))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 135.945 87.738)
    (fp_text reference TP24 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 4 /D2))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 137.445 87.738)
    (fp_text reference TP25 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 6 /D3))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 138.945 87.738)
    (fp_text reference TP26 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 7 /D4))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 140.445 87.738)
    (fp_text reference TP27 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 8 /D5))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 141.945 87.738)
    (fp_text reference TP28 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 9 /D6))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 143.445 87.738)
    (fp_text reference TP29 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 10 /D7))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 144.945 87.738)
    (fp_text reference TP30 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 32 /RESET))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 145.795 85.738)
    (fp_text reference TP31 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 65 /AUD))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 148.045 87.688)
    (fp_text reference TP32 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 5 GND))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 119.445 87.738)
    (fp_text reference TP13 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 23 /A7))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 113.445 87.738)
    (fp_text reference TP9 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 19 /A3))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 136.271 69.723 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.515 -0.674) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /RESET))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 /GB_RESET))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "gameboy:Large Hole" (layer F.Cu) (tedit 5C843B67)
    (at 124.65 82.35)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 7.3) (layers *.Cu *.Mask)
      (net 67 "Net-(J2-Pad1)"))
  )
  (module "gameboy:Small Hole" (layer F.Cu) (tedit 5AE80885)
    (at 124.65 57.3)
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.3 2.3) (drill 2.2) (layers *.Cu *.Mask)
      (net 66 "Net-(J1-Pad1)"))
  )
  (gr_text 3.3V (at 107.456 40.878 180) (layer F.SilkS))
  (gr_text GND (at 107.456 44.434 180) (layer F.SilkS))
  (gr_text +5V (at 135.015 57.896 180) (layer F.SilkS))
  (gr_text CONTROL (at 106.821 47.355 180) (layer F.SilkS))
  (gr_text A0-A7 (at 115.203 39.354 180) (layer F.SilkS))
  (gr_text A8-A15 (at 124.728 46.593 180) (layer F.SilkS))
  (gr_text D0-D7 (at 136.285 39.862 180) (layer F.SilkS))
  (gr_text GND (at 147.88 91.41 270) (layer B.SilkS))
  (gr_text AUD (at 146.445 91.44 270) (layer B.SilkS))
  (gr_text RST (at 144.945 91.44 270) (layer B.SilkS))
  (gr_text D7 (at 143.445 91.44 270) (layer B.SilkS))
  (gr_text D6 (at 141.945 91.44 270) (layer B.SilkS))
  (gr_text D5 (at 140.445 91.44 270) (layer B.SilkS))
  (gr_text D4 (at 138.945 91.44 270) (layer B.SilkS))
  (gr_text D3 (at 137.445 91.44 270) (layer B.SilkS))
  (gr_text D2 (at 135.945 91.44 270) (layer B.SilkS))
  (gr_text D1 (at 134.36 91.45 270) (layer B.SilkS))
  (gr_text D0 (at 132.945 91.44 270) (layer B.SilkS))
  (gr_text A15 (at 131.445 91.44 270) (layer B.SilkS))
  (gr_text A14 (at 129.945 91.44 270) (layer B.SilkS))
  (gr_text A13 (at 128.445 91.44 270) (layer B.SilkS))
  (gr_text A12 (at 126.945 91.44 270) (layer B.SilkS))
  (gr_text A11 (at 125.445 91.44 270) (layer B.SilkS))
  (gr_text A10 (at 123.945 91.44 270) (layer B.SilkS))
  (gr_text A9 (at 122.445 91.44 270) (layer B.SilkS))
  (gr_text A8 (at 120.945 91.44 270) (layer B.SilkS))
  (gr_text A7 (at 119.445 91.44 270) (layer B.SilkS))
  (gr_text A6 (at 117.945 91.44 270) (layer B.SilkS))
  (gr_text A5 (at 116.445 91.44 270) (layer B.SilkS))
  (gr_text A4 (at 114.945 91.44 270) (layer B.SilkS))
  (gr_text A3 (at 113.445 91.44 270) (layer B.SilkS))
  (gr_text A2 (at 111.945 91.44 270) (layer B.SilkS))
  (gr_text A1 (at 110.445 91.44 270) (layer B.SilkS))
  (gr_text A0 (at 108.945 91.44 270) (layer B.SilkS))
  (gr_text CS (at 107.442 91.44 270) (layer B.SilkS))
  (gr_text RD (at 105.945 91.44 270) (layer B.SilkS))
  (gr_text WR (at 104.445 91.44 270) (layer B.SilkS))
  (gr_text CLK (at 102.945 91.44 270) (layer B.SilkS))
  (gr_text +5V (at 101.219 91.44 270) (layer B.SilkS))
  (gr_line (start 100 80.25) (end 100 98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 53.75) (end 100 77.71) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100 52.48) (end 100 53.75) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100 78.98) (end 100 80.25) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 85.37) (end 149.3 98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 51.77) (end 149.3 82.83) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.3 50.5) (end 149.3 49.23) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.3 84.1) (end 149.3 82.83) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_text PWR (at 143.524 45.069 90) (layer F.SilkS))
  (gr_text Data (at 142.782 82.296 45) (layer F.SilkS))
  (gr_text ckd.tech/gb-bo/v1 (at 144.845 68.488 90) (layer F.SilkS))
  (gr_text GND (at 147.945 91.44 90) (layer F.SilkS))
  (gr_text AUD (at 146.445 91.44 90) (layer F.SilkS))
  (gr_text RST (at 144.945 91.44 90) (layer F.SilkS))
  (gr_text D7 (at 143.445 91.44 90) (layer F.SilkS))
  (gr_text D6 (at 141.945 91.44 90) (layer F.SilkS))
  (gr_text D5 (at 140.445 91.44 90) (layer F.SilkS))
  (gr_text D4 (at 138.945 91.44 90) (layer F.SilkS))
  (gr_text D3 (at 137.445 91.44 90) (layer F.SilkS))
  (gr_text D2 (at 135.945 91.44 90) (layer F.SilkS))
  (gr_text D1 (at 134.445 91.44 90) (layer F.SilkS))
  (gr_text D0 (at 132.945 91.44 90) (layer F.SilkS))
  (gr_text A15 (at 131.445 91.44 90) (layer F.SilkS))
  (gr_text A14 (at 129.945 91.44 90) (layer F.SilkS))
  (gr_text A13 (at 128.445 91.44 90) (layer F.SilkS))
  (gr_text A12 (at 126.945 91.44 90) (layer F.SilkS))
  (gr_text A11 (at 125.445 91.44 90) (layer F.SilkS))
  (gr_text A10 (at 123.945 91.44 90) (layer F.SilkS))
  (gr_text A9 (at 122.445 91.44 90) (layer F.SilkS))
  (gr_text A8 (at 120.945 91.44 90) (layer F.SilkS))
  (gr_text A7 (at 119.445 91.44 90) (layer F.SilkS))
  (gr_text A6 (at 117.945 91.44 90) (layer F.SilkS))
  (gr_text A5 (at 116.445 91.44 90) (layer F.SilkS))
  (gr_text A4 (at 114.945 91.44 90) (layer F.SilkS))
  (gr_text A3 (at 113.445 91.44 90) (layer F.SilkS))
  (gr_text A2 (at 111.945 91.44 90) (layer F.SilkS))
  (gr_text A1 (at 110.445 91.44 90) (layer F.SilkS))
  (gr_text A0 (at 108.945 91.44 90) (layer F.SilkS))
  (gr_text CS (at 107.442 91.44 90) (layer F.SilkS))
  (gr_text RD (at 105.945 91.44 90) (layer F.SilkS))
  (gr_text WR (at 104.445 91.44 90) (layer F.SilkS))
  (gr_text CLK (at 102.945 91.44 90) (layer F.SilkS))
  (gr_text +5V (at 101.219 91.44 90) (layer F.SilkS))
  (gr_line (start 143.3 42.3) (end 143.3 38.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 42.3) (end 143.3 42.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 98) (end 100 98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 42.3) (end 149.3 49.23) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 38.3) (end 143.3 38.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 38.3) (end 100 51.21) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.366 98.028) (xy 99.963 98.028) (xy 99.963 38.338) (xy 149.493 38.338)
      )
    )
  )
)
