(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 46)
    (tracks 334)
    (zones 0)
    (modules 71)
    (nets 31)
  )
  (page USLetter)
  (title_block
    (title "MPW008 Test board")
    (date 2019-01-10)
    (company Wispry)
    (comment 1 "Designed by DMG")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.4572)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 48.768 20.32)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00034_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VDD_FILT)
  (net 3 /VDD_2_FILT)
  (net 4 "Net-(B_VDD1-Pad1)")
  (net 5 "Net-(EN_CP3-Pad1)")
  (net 6 "Net-(MODE_DRV0-Pad1)")
  (net 7 "Net-(EN_CP2-Pad1)")
  (net 8 "Net-(B_VDD2-Pad1)")
  (net 9 "Net-(EN_OSC0-Pad1)")
  (net 10 "Net-(EN_DRV0-Pad1)")
  (net 11 "Net-(R7-Pad1)")
  (net 12 "Net-(R8-Pad1)")
  (net 13 "Net-(R9-Pad1)")
  (net 14 "Net-(EN_CP1-Pad1)")
  (net 15 "Net-(R6-Pad1)")
  (net 16 "Net-(NC1-Pad1)")
  (net 17 "Net-(NC15-Pad1)")
  (net 18 "Net-(NC25-Pad1)")
  (net 19 "Net-(B_HW0-Pad1)")
  (net 20 "Net-(BNC_CLK_EXT0-Pad1)")
  (net 21 "Net-(B_DN0-Pad1)")
  (net 22 "Net-(B_DP0-Pad1)")
  (net 23 "Net-(B_GN0-Pad1)")
  (net 24 "Net-(B_GP0-Pad1)")
  (net 25 "Net-(B_SN0-Pad1)")
  (net 26 "Net-(B_SP0-Pad1)")
  (net 27 "Net-(U1-Pad22)")
  (net 28 "Net-(U1-Pad24)")
  (net 29 "Net-(U1-Pad23)")
  (net 30 "Net-(CLK_MUX0-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
  )
  (net_class VC ""
    (clearance 0.508)
    (trace_width 0.508)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
    (add_net /VDD_2_FILT)
    (add_net /VDD_FILT)
    (add_net GND)
    (add_net "Net-(BNC_CLK_EXT0-Pad1)")
    (add_net "Net-(B_DN0-Pad1)")
    (add_net "Net-(B_DP0-Pad1)")
    (add_net "Net-(B_GN0-Pad1)")
    (add_net "Net-(B_GP0-Pad1)")
    (add_net "Net-(B_HW0-Pad1)")
    (add_net "Net-(B_SN0-Pad1)")
    (add_net "Net-(B_SP0-Pad1)")
    (add_net "Net-(B_VDD1-Pad1)")
    (add_net "Net-(B_VDD2-Pad1)")
    (add_net "Net-(CLK_MUX0-Pad1)")
    (add_net "Net-(EN_CP1-Pad1)")
    (add_net "Net-(EN_CP2-Pad1)")
    (add_net "Net-(EN_CP3-Pad1)")
    (add_net "Net-(EN_DRV0-Pad1)")
    (add_net "Net-(EN_OSC0-Pad1)")
    (add_net "Net-(MODE_DRV0-Pad1)")
    (add_net "Net-(NC1-Pad1)")
    (add_net "Net-(NC15-Pad1)")
    (add_net "Net-(NC25-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
  )
  (module 0000_VC_Library:Socket_28lead_dip_soic (layer F.Cu) (tedit 5C50F503)
    (at 88.646 82.296)
    (fp_text reference U1 (at 0.1778 -12.9286) (layer F.SilkS))
    (fp_text value Socket_MPW008_BA_BB_BD_BE (at 0.2032 -11.049) (layer F.Fab))
    (pad 1 thru_hole circle (at -10.2108 -8.255) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 16 "Net-(NC1-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5748 1.5748) (drill 1.5748) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.1308 -6.985) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 /VDD_2_FILT))
    (pad 3 thru_hole circle (at -10.2108 -5.715) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -5.1308 -4.445) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (pad 5 thru_hole circle (at -10.2108 -3.175) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(EN_OSC0-Pad1)"))
    (pad 6 thru_hole circle (at -5.1308 -1.905) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 13 "Net-(R9-Pad1)"))
    (pad 7 thru_hole circle (at -10.2108 -0.635) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 "Net-(R8-Pad1)"))
    (pad 8 thru_hole circle (at -5.1308 0.635) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)"))
    (pad 9 thru_hole circle (at -10.2108 1.905) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(EN_DRV0-Pad1)"))
    (pad 10 thru_hole circle (at -5.1308 3.175) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 "Net-(MODE_DRV0-Pad1)"))
    (pad 11 thru_hole circle (at -10.2108 4.445) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 15 "Net-(R6-Pad1)"))
    (pad 12 thru_hole circle (at -5.1308 5.715) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 14 "Net-(EN_CP1-Pad1)"))
    (pad 13 thru_hole circle (at -10.2108 6.985) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(EN_CP2-Pad1)"))
    (pad 14 thru_hole circle (at -5.1308 8.255) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(EN_CP3-Pad1)"))
    (pad 15 thru_hole circle (at 10.2108 8.255) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 17 "Net-(NC15-Pad1)"))
    (pad 16 thru_hole circle (at 5.1308 6.985) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "Net-(B_DP0-Pad1)"))
    (pad 17 thru_hole circle (at 10.2108 5.715) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 26 "Net-(B_SP0-Pad1)"))
    (pad 18 thru_hole circle (at 5.1308 4.445) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 24 "Net-(B_GP0-Pad1)"))
    (pad 19 thru_hole circle (at 10.2108 3.175) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 21 "Net-(B_DN0-Pad1)"))
    (pad 20 thru_hole circle (at 5.1308 1.905) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 25 "Net-(B_SN0-Pad1)"))
    (pad 21 thru_hole circle (at 10.2108 0.635) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 "Net-(B_GN0-Pad1)"))
    (pad 22 thru_hole circle (at 5.1308 -0.635) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at 10.2108 -1.905) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at 5.1308 -3.175) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at 10.2108 -4.445) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 18 "Net-(NC25-Pad1)"))
    (pad 26 thru_hole circle (at 5.1308 -5.715) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 20 "Net-(BNC_CLK_EXT0-Pad1)"))
    (pad 27 thru_hole circle (at 10.2108 -6.985) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 19 "Net-(B_HW0-Pad1)"))
    (pad 28 thru_hole circle (at 5.1308 -8.255) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 30 "Net-(CLK_MUX0-Pad1)"))
    (model ${VC_3D_DIR}/Socket_28lead_dip_soic.wrl
      (offset (xyz -3 0 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_black (layer F.Cu) (tedit 5C50F523)
    (at 89.154 114.3)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference GND3 (at 0 -2.794) (layer F.SilkS))
    (fp_text value Testpoint_black (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_black.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 37.084)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference CLK_EXT0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 20 "Net-(BNC_CLK_EXT0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_green (layer F.Cu) (tedit 5C50F53E)
    (at 95.504 114.3 180)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference GP0 (at 0.7 2.5 180) (layer F.SilkS))
    (fp_text value Testpoint_green (at 0 -2.8 180) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 24 "Net-(B_GP0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_green.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:BNC_Molex_73100_0105 (layer F.Cu) (tedit 5C50F4F2)
    (at 35.052 37.338 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference BNC_CLK_EXT0 (at 0.40132 15.69212 90) (layer F.SilkS))
    (fp_text value BNC_female (at 0 18.03908 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.8 4.6 90) (size 3.81 3.81) (drill 1.8034) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.8 4.6 90) (size 3.81 3.81) (drill 1.8034) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 12.4 90) (size 1.6002 1.6002) (drill 0.9144) (layers *.Cu *.Mask)
      (net 20 "Net-(BNC_CLK_EXT0-Pad1)"))
    (model ${VC_3D_DIR}/BNC_Molex_73100_0131_2.step
      (offset (xyz 0 3 5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_green (layer F.Cu) (tedit 5C52610A)
    (at 82.804 134.734 90)
    (fp_text reference B_DN0 (at 14.084 0 180) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_green (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(B_DN0-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(B_DN0-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_green_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_green (layer F.Cu) (tedit 5C526102)
    (at 120.904 134.734 90)
    (fp_text reference B_DP0 (at 14.592 0 180) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_green (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(B_DP0-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(B_DP0-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_green_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_green (layer F.Cu) (tedit 5C5260E0)
    (at 57.404 134.734 90)
    (fp_text reference B_GN0 (at 14.084 0 180) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_green (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(B_GN0-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(B_GN0-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_green_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_green (layer F.Cu) (tedit 5C526107)
    (at 95.504 134.734 90)
    (fp_text reference B_GP0 (at 14.084 0 180) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_green (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(B_GP0-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(B_GP0-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_green_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_green (layer F.Cu) (tedit 5C52610D)
    (at 70.104 134.734 90)
    (fp_text reference B_SN0 (at 14.084 -0.254 180) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_green (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(B_SN0-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(B_SN0-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_green_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_green (layer F.Cu) (tedit 5C526104)
    (at 108.204 134.734 90)
    (fp_text reference B_SP0 (at 14.338 -0.254 180) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_green (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(B_SP0-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 90) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(B_SP0-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_green_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_green (layer F.Cu) (tedit 5C50F53E)
    (at 108.204 114.554 180)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference SP0 (at 0.7 2.5 180) (layer F.SilkS))
    (fp_text value Testpoint_green (at 0 -2.8 180) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 26 "Net-(B_SP0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_green.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_green (layer F.Cu) (tedit 5C50F53E)
    (at 70.104 114.554 180)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference SN0 (at 0.7 2.5 180) (layer F.SilkS))
    (fp_text value Testpoint_green (at 0 -2.8 180) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 25 "Net-(B_SN0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_green.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_green (layer F.Cu) (tedit 5C50F53E)
    (at 57.404 114.554 180)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference GN0 (at 0.7 2.5 180) (layer F.SilkS))
    (fp_text value Testpoint_green (at 0 -2.8 180) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 23 "Net-(B_GN0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_green.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_green (layer F.Cu) (tedit 5C50F53E)
    (at 120.904 114.554 180)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference DP0 (at 0.7 2.5 180) (layer F.SilkS))
    (fp_text value Testpoint_green (at 0 -2.8 180) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 22 "Net-(B_DP0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_green.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_green (layer F.Cu) (tedit 5C50F53E)
    (at 82.804 114.554 180)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference DN0 (at 0.7 2.5 180) (layer F.SilkS))
    (fp_text value Testpoint_green (at 0 -2.8 180) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 21 "Net-(B_DN0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_green.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_white (layer F.Cu) (tedit 5C50F570)
    (at 121.158 105.664)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference NC25 (at 0.254 2.5) (layer F.SilkS))
    (fp_text value Testpoint_white (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 18 "Net-(NC25-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_white.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_white (layer F.Cu) (tedit 5C50F570)
    (at 121.158 100.33)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference NC15 (at 0 2.5) (layer F.SilkS))
    (fp_text value Testpoint_white (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 17 "Net-(NC15-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_white.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_white (layer F.Cu) (tedit 5C50F570)
    (at 121.158 94.742)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference NC1 (at 0 2.794) (layer F.SilkS))
    (fp_text value Testpoint_white (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 16 "Net-(NC1-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_white.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 83.519815)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference SEL_FRQ0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 "Net-(R9-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_black (layer F.Cu) (tedit 5C50F523)
    (at 56.896 66.34018)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference GND5 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_black (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_black.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_black (layer F.Cu) (tedit 5C50F523)
    (at 56.896 89.24636)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference GND4 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_black (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_black.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 50.8 106.68)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(EN_CP3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 50.8 102.616)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(EN_CP2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 43.434)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference EN_OSC0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 9 "Net-(EN_OSC0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm (layer F.Cu) (tedit 5A4E1404)
    (at 38.862 101.6)
    (descr "3x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x9.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (fp_text reference SW_EN_PUMP0 (at 3.81 -3.42) (layer F.SilkS))
    (fp_text value SW_DIP_x03 (at 3.81 8.5) (layer F.Fab))
    (fp_text user on (at 5.365 -1.4975) (layer F.Fab))
    (fp_text user %R (at 7.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(EN_CP1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(EN_CP2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(EN_CP3-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Button_Switch_THT:SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm (layer F.Cu) (tedit 5A4E1404)
    (at 38.862 78.74)
    (descr "3x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x9.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (fp_text reference SW_SEL_FRQ0 (at 3.81 -3.42) (layer F.SilkS))
    (fp_text value SW_DIP_x03 (at 3.81 8.5) (layer F.Fab))
    (fp_text user on (at 5.365 -1.4975) (layer F.Fab))
    (fp_text user %R (at 7.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R9-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Button_Switch_THT:SW_DIP_SPSTx04_Slide_9.78x12.34mm_W7.62mm_P2.54mm (layer F.Cu) (tedit 5A4E1404)
    (at 38.862 52.832)
    (descr "4x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x12.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (fp_text reference SW_ETC0 (at 3.81 -3.42) (layer F.SilkS))
    (fp_text value SW_DIP_x04 (at 3.81 11.04) (layer F.Fab))
    (fp_text user on (at 5.365 -1.4975) (layer F.Fab))
    (fp_text user %R (at 7.27 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(EN_OSC0-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(EN_DRV0-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(MODE_DRV0-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R6-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx04_Slide_9.78x12.34mm_W7.62mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_red (layer F.Cu) (tedit 5C50F55E)
    (at 95.504 58.42)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference VDD2_FILT0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_red (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /VDD_2_FILT))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_red.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_red (layer F.Cu) (tedit 5C50F55E)
    (at 70.104 50.8)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference VDD1 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_red (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(B_VDD1-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_red.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 50.8 74.676)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 51.054 57.15)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(MODE_DRV0-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 51.054 53.848)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(EN_DRV0-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 51.054 50.546)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(EN_OSC0-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 51.054 60.452)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 15 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_red (layer F.Cu) (tedit 5C50F55E)
    (at 108.204 50.8)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference HW0 (at -0.508 2.54) (layer F.SilkS))
    (fp_text value Testpoint_red (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 19 "Net-(B_HW0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_red.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_black (layer F.Cu) (tedit 5C50F492)
    (at 82.804 30.62 270)
    (fp_text reference B_GND1 (at 13.322 0) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_black (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -7.65 0 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${VC_3D_DIR}/Banana_socket_black_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_black (layer F.Cu) (tedit 5C50F523)
    (at 121.158 88.392)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference GND2 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_black (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_black.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:Standoff_hole (layer F.Cu) (tedit 5C50F511)
    (at 36.068 21.336)
    (fp_text reference J1 (at 4.572 0.254) (layer F.SilkS))
    (fp_text value Standoff_hole (at 0 -4.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/Standoff_6_32.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 49.160545)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference EN_DRV0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 "Net-(EN_DRV0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 106.426)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference EN_CP3 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 "Net-(EN_CP3-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 100.69945)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference EN_CP2 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 7 "Net-(EN_CP2-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 60.613635)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference SEL_CLK0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 15 "Net-(R6-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_blue (layer F.Cu) (tedit 5C50F530)
    (at 121.158 81.24825)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference CLK_MUX0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_blue (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 30 "Net-(CLK_MUX0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_blue.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_blue (layer F.Cu) (tedit 5C50F530)
    (at 121.158 61.722)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference VOUT1 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_blue (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad24)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_blue.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_blue (layer F.Cu) (tedit 5C50F530)
    (at 121.158 74.9935)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference VOUT3 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_blue (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad22)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_blue.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_blue (layer F.Cu) (tedit 5C50F530)
    (at 121.158 68.73875)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference VOUT2 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_blue (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad23)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_blue.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_black (layer F.Cu) (tedit 5C50F523)
    (at 82.804 50.8)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference GND1 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_black (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_black.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_red (layer F.Cu) (tedit 5C50F4CE)
    (at 95.504 30.62 270)
    (fp_text reference B_VDD2 (at 13.576 0.254) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_red (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(B_VDD2-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(B_VDD2-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_red_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_red (layer F.Cu) (tedit 5C50F4CE)
    (at 70.104 30.62 270)
    (fp_text reference B_VDD1 (at 13.068 -0.254) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_red (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(B_VDD1-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(B_VDD1-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_red_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 50.8 83.693)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 13 "Net-(R9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 50.8 98.552)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(EN_CP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 50.8 78.994)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 1.65) (layer B.SilkS))
    (fp_text value Res_10Mohm_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 12 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 90.17 46.482 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value Res_1ohm_SMD_805 (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(B_VDD2-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 /VDD_2_FILT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 75.438 46.482 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value Res_1ohm_SMD_805 (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(B_VDD1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 /VDD_FILT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 89.293018 58.363263 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value Cap_0.1uF_SMD_805 (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 /VDD_2_FILT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 89.293018 51.115263 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value Cap_22pF_SMD_805 (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 /VDD_2_FILT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 89.293018 54.612263 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value Cap_1uF_SMD_805 (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 /VDD_2_FILT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 76.544357 51.115263)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 1.65) (layer B.SilkS))
    (fp_text value Cap_22pF_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 /VDD_FILT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 76.544357 54.612263)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.65) (layer B.SilkS))
    (fp_text value Cap_1uF_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 /VDD_FILT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 76.544357 58.363263)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.65) (layer B.SilkS))
    (fp_text value Cap_0.1uF_SMD_805 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 /VDD_FILT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 94.972905)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference EN_CP1 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 14 "Net-(EN_CP1-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 54.88709)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference MODE_DRV0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 "Net-(MODE_DRV0-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 77.79327)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference SEL_FRQ1 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 "Net-(R8-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_orange (layer F.Cu) (tedit 5C50F54E)
    (at 56.896 72.066725)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference SEL_FRQ2 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_orange (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_orange.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_red (layer F.Cu) (tedit 5C50F55E)
    (at 95.504 50.8)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference VDD2 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_red (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 8 "Net-(B_VDD2-Pad1)"))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_red.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:Standoff_hole (layer F.Cu) (tedit 5C50F511)
    (at 36.068 140.716)
    (fp_text reference J4 (at 0 -4.064) (layer F.SilkS))
    (fp_text value Standoff_hole (at 0 -4.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/Standoff_6_32.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:Standoff_hole (layer F.Cu) (tedit 5C50F511)
    (at 134.874 140.716)
    (fp_text reference J3 (at 0 -4.064) (layer F.SilkS))
    (fp_text value Standoff_hole (at 0 -4.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/Standoff_6_32.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:Banana_socket_4mm_571_red (layer F.Cu) (tedit 5C50F4CE)
    (at 108.204 30.62 270)
    (fp_text reference B_HW0 (at 13.576 0) (layer F.SilkS))
    (fp_text value Banana_socket_4mm_red (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text user DELTRON (at 0.635 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.65 0 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(B_HW0-Pad1)"))
    (pad 1 thru_hole circle (at -7.65 0 270) (size 2.7 2.7) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(B_HW0-Pad1)"))
    (model ${VC_3D_DIR}/Banana_socket_red_4mm.step
      (offset (xyz -7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 0000_VC_Library:Standoff_hole (layer F.Cu) (tedit 5C50F511)
    (at 134.874 21.336)
    (fp_text reference J2 (at -4.318 0) (layer F.SilkS))
    (fp_text value Standoff_hole (at 0 -4.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${VC_3D_DIR}/Standoff_6_32.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0000_VC_Library:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded_red (layer F.Cu) (tedit 5C50F55E)
    (at 70.104 58.42)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (fp_text reference VDD1_FILT0 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value Testpoint_red (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 /VDD_FILT))
    (model ${VC_3D_DIR}/TestPoint_Loop_D2_60mm_Drill0_9mm_Beaded_red.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Inputs (at 57.404 31.496) (layer F.SilkS))
  (gr_text PFET (at 107.696 108.966) (layer F.SilkS))
  (gr_text NFET (at 69.342 108.966) (layer F.SilkS))
  (gr_text "No\nConnects" (at 130.81 100.33) (layer F.SilkS))
  (gr_text Outputs (at 131.826 72.898) (layer F.SilkS))
  (gr_text Supplies (at 118.364 54.102) (layer F.SilkS))
  (gr_line (start 30.734 147.066) (end 30.734 16.51) (layer Edge.Cuts) (width 0.2))
  (gr_text "Board: MPW008 PCB 1\nDies: BA, BB, BD, BE\nDesigner: Vincent Cheung\nSupport: David Molinero\nDate: Jan 29 2019\n\n(•_•)\n( •_•)>⌐■-■\n(⌐■_■)\n\n   __o      \n _ \\<_ \n(_)/(_)" (at 116.84 36.068) (layer F.SilkS))
  (gr_line (start 30.734 16.51) (end 138.938 16.51) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 138.938 16.51) (end 138.938 146.812) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 138.938 146.812) (end 30.734 147.066) (layer Edge.Cuts) (width 0.2))
)
