(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 174)
    (tracks 1734)
    (zones 0)
    (modules 30)
    (nets 76)
  )
  (page A4)
  (title_block
    (title "Z80-512K: RC2014 Compatible CPU and Memory Module")
    (date 2021-01-15)
    (rev 1.1)
    (company "Designed by Sergey Kiselev")
    (comment 2 "Licensed under CERN-OHL-S: https://cern-ohl.web.cern.ch")
    (comment 3 "Documentation and design files: https://github.com/skiselev/Z80-512K")
    (comment 4 "Z80-512K is an open source hardware project")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1.5)
    (trace_clearance 0.15)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 /VBAT)
  (net 2 GND)
  (net 3 VCC)
  (net 4 /VRAM)
  (net 5 /A15)
  (net 6 /A14)
  (net 7 /A13)
  (net 8 /A12)
  (net 9 /A11)
  (net 10 /A10)
  (net 11 /A9)
  (net 12 /A8)
  (net 13 /A7)
  (net 14 /A6)
  (net 15 /A5)
  (net 16 /A4)
  (net 17 /A3)
  (net 18 /A2)
  (net 19 /A1)
  (net 20 /A0)
  (net 21 /~M1)
  (net 22 /~RESET)
  (net 23 /CPU_CLK)
  (net 24 /~INT)
  (net 25 /~MREQ)
  (net 26 /~WR)
  (net 27 /~RD)
  (net 28 /~IORQ)
  (net 29 /D0)
  (net 30 /D1)
  (net 31 /D2)
  (net 32 /D3)
  (net 33 /D4)
  (net 34 /D5)
  (net 35 /D6)
  (net 36 /D7)
  (net 37 /~RFSH)
  (net 38 /~BUSACK)
  (net 39 /~HALT)
  (net 40 /~BUSREQ)
  (net 41 /~WAIT)
  (net 42 /~NMI)
  (net 43 /TXDA)
  (net 44 /RXDA)
  (net 45 /USR1)
  (net 46 /MA17)
  (net 47 /MA14)
  (net 48 /MA16)
  (net 49 /MA15)
  (net 50 /MA18)
  (net 51 "Net-(RV1-Pad2)")
  (net 52 /~ROM_CS)
  (net 53 /~RAM_CS)
  (net 54 /~RAM_CSI)
  (net 55 "Net-(X1-Pad1)")
  (net 56 /UART_CLK)
  (net 57 /TCK)
  (net 58 /TDO)
  (net 59 /TMS)
  (net 60 /TDI)
  (net 61 "Net-(U5-Pad5)")
  (net 62 "Net-(U5-Pad6)")
  (net 63 "Net-(U5-Pad7)")
  (net 64 "Net-(U5-Pad8)")
  (net 65 "Net-(U5-Pad14)")
  (net 66 "Net-(U5-Pad16)")
  (net 67 /WDOG)
  (net 68 /USR2)
  (net 69 /USR3)
  (net 70 "Net-(J2-Pad6)")
  (net 71 "Net-(J2-Pad7)")
  (net 72 "Net-(J2-Pad8)")
  (net 73 "Net-(J4-Pad4)")
  (net 74 "Net-(R5-Pad2)")
  (net 75 "Net-(R6-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CPU_CLK)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /MA14)
    (add_net /MA15)
    (add_net /MA16)
    (add_net /MA17)
    (add_net /MA18)
    (add_net /RXDA)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /TXDA)
    (add_net /UART_CLK)
    (add_net /USR1)
    (add_net /USR2)
    (add_net /USR3)
    (add_net /WDOG)
    (add_net /~BUSACK)
    (add_net /~BUSREQ)
    (add_net /~HALT)
    (add_net /~INT)
    (add_net /~IORQ)
    (add_net /~M1)
    (add_net /~MREQ)
    (add_net /~NMI)
    (add_net /~RAM_CS)
    (add_net /~RAM_CSI)
    (add_net /~RD)
    (add_net /~RESET)
    (add_net /~RFSH)
    (add_net /~ROM_CS)
    (add_net /~WAIT)
    (add_net /~WR)
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(U5-Pad14)")
    (add_net "Net-(U5-Pad16)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(X1-Pad1)")
  )
  (net_class Power ""
    (clearance 0.15)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /VBAT)
    (add_net /VRAM)
    (add_net GND)
    (add_net VCC)
  )
  (module Symbol:KiCad-Logo2_5mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 204.47 111.4425 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 5.08) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_5mm_SilkScreen (at 0 -5.08) (layer B.Fab) hide)
  )
  (module My_Components:Conn_Pin_Header_10x1_2.54mm_Right_Angle (layer F.Cu) (tedit 6001D70D)
    (at 179.07 124.46)
    (descr "Pin Header, 10x1, 2.54mm pitch")
    (tags "CONN 10x1")
    (fp_text reference J4 (at 5.715 5.08) (layer F.SilkS) hide)
    (fp_text value RC2014_EXT (at 6.0325 6.985) (layer F.SilkS) hide)
    (pad 10 thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /~NMI))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /~WAIT))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /~BUSREQ))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /~HALT))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /~BUSACK))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /UART_CLK))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J4-Pad4)"))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /~RFSH))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 1 thru_hole rect (at -11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_39x1_2.54mm_Right_Angle (layer F.Cu) (tedit 6001D63B)
    (at 175.26 127)
    (descr "Pin Header, 39x1, 2.54mm pitch")
    (tags "CONN 39x1")
    (fp_text reference J3 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value RC2014_BUS (at 0 4.445) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -48.26 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A15))
    (pad 2 thru_hole circle (at -45.72 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A14))
    (pad 3 thru_hole circle (at -43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A13))
    (pad 4 thru_hole circle (at -40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A12))
    (pad 5 thru_hole circle (at -38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A11))
    (pad 6 thru_hole circle (at -35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A10))
    (pad 7 thru_hole circle (at -33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A9))
    (pad 8 thru_hole circle (at -30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A8))
    (pad 9 thru_hole circle (at -27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A7))
    (pad 10 thru_hole circle (at -25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A6))
    (pad 11 thru_hole circle (at -22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A5))
    (pad 12 thru_hole circle (at -20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A4))
    (pad 13 thru_hole circle (at -17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A3))
    (pad 14 thru_hole circle (at -15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A2))
    (pad 15 thru_hole circle (at -12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A1))
    (pad 16 thru_hole circle (at -10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A0))
    (pad 17 thru_hole circle (at -7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 18 thru_hole circle (at -5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 19 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /~M1))
    (pad 20 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /~RESET))
    (pad 21 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /CPU_CLK))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /~INT))
    (pad 23 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /~MREQ))
    (pad 24 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /~WR))
    (pad 25 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /~RD))
    (pad 26 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /~IORQ))
    (pad 27 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D0))
    (pad 28 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D1))
    (pad 29 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D2))
    (pad 30 thru_hole circle (at 25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D3))
    (pad 31 thru_hole circle (at 27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D4))
    (pad 32 thru_hole circle (at 30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D5))
    (pad 33 thru_hole circle (at 33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D6))
    (pad 34 thru_hole circle (at 35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /D7))
    (pad 35 thru_hole circle (at 38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /TXDA))
    (pad 36 thru_hole circle (at 40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /RXDA))
    (pad 37 thru_hole circle (at 43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /USR1))
    (pad 38 thru_hole circle (at 45.72 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /USR2))
    (pad 39 thru_hole circle (at 48.26 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 /USR3))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_5x2_2.54mm (layer F.Cu) (tedit 6001D907)
    (at 214.63 81.28)
    (descr "Pin Header, 13x2, 2.54mm pitch")
    (tags "CONN PIN HEADER 13x2")
    (fp_text reference J2 (at -8.255 -0.9525) (layer F.SilkS))
    (fp_text value JTAG (at -8.255 0.9525) (layer F.SilkS))
    (pad 10 thru_hole circle (at 5.08 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at 5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /TDI))
    (pad 8 thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J2-Pad8)"))
    (pad 7 thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J2-Pad7)"))
    (pad 6 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J2-Pad6)"))
    (pad 5 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /TMS))
    (pad 4 thru_hole circle (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 3 thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 /TDO))
    (pad 2 thru_hole circle (at -5.08 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 /TCK))
    (model pin_array/pins_array_13x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Socket_DIP16_300 (layer F.Cu) (tedit 600144EA)
    (at 153.67 88.9 90)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U5 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value ADM693A (at 2.54 0 90) (layer F.SilkS))
    (pad 16 thru_hole circle (at -8.89 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(U5-Pad16)"))
    (pad 15 thru_hole circle (at -6.35 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /~RESET))
    (pad 14 thru_hole circle (at -3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(U5-Pad14)"))
    (pad 13 thru_hole circle (at -1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~RAM_CSI))
    (pad 12 thru_hole circle (at 1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~RAM_CS))
    (pad 11 thru_hole circle (at 3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /WDOG))
    (pad 10 thru_hole circle (at 6.35 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /~NMI))
    (pad 9 thru_hole circle (at 8.89 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(RV1-Pad2)"))
    (pad 8 thru_hole circle (at 8.89 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(U5-Pad8)"))
    (pad 7 thru_hole circle (at 6.35 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(U5-Pad7)"))
    (pad 6 thru_hole circle (at 3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(U5-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(U5-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at -3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 2 thru_hole circle (at -6.35 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VRAM))
    (pad 1 thru_hole rect (at -8.89 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VBAT))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_PLCC44_TH (layer F.Cu) (tedit 60014443)
    (at 171.45 90.17)
    (descr "PLCC44 Socket, Through Hole")
    (tags "PLCC PLCC44")
    (fp_text reference U4 (at -12.7 10.795) (layer F.SilkS))
    (fp_text value ATF1504AS (at 9.2075 12.2555) (layer F.SilkS))
    (pad 44 thru_hole circle (at 1.27 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /~M1))
    (pad 43 thru_hole circle (at 3.81 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /CPU_CLK))
    (pad 42 thru_hole circle (at 3.81 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 41 thru_hole circle (at 6.35 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /UART_CLK))
    (pad 40 thru_hole circle (at 6.35 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /~WR))
    (pad 39 thru_hole circle (at 8.89 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /~IORQ))
    (pad 38 thru_hole circle (at 6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 /TDO))
    (pad 37 thru_hole circle (at 8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A14))
    (pad 36 thru_hole circle (at 6.35 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /~RD))
    (pad 35 thru_hole circle (at 8.89 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 34 thru_hole circle (at 6.35 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A15))
    (pad 33 thru_hole circle (at 8.89 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /WDOG))
    (pad 32 thru_hole circle (at 6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 /TCK))
    (pad 31 thru_hole circle (at 8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A1))
    (pad 30 thru_hole circle (at 6.35 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 29 thru_hole circle (at 8.89 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A0))
    (pad 28 thru_hole circle (at 6.35 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /MA18))
    (pad 27 thru_hole circle (at 3.81 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /MA17))
    (pad 26 thru_hole circle (at 3.81 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D5))
    (pad 25 thru_hole circle (at 1.27 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D4))
    (pad 24 thru_hole circle (at 1.27 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D3))
    (pad 23 thru_hole circle (at -1.27 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 22 thru_hole circle (at -1.27 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole circle (at -3.81 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /MA16))
    (pad 20 thru_hole circle (at -3.81 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /MA15))
    (pad 19 thru_hole circle (at -6.35 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /MA14))
    (pad 18 thru_hole circle (at -6.35 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D2))
    (pad 17 thru_hole circle (at -8.89 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D1))
    (pad 16 thru_hole circle (at -6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D0))
    (pad 15 thru_hole circle (at -8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 14 thru_hole circle (at -6.35 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A7))
    (pad 13 thru_hole circle (at -8.89 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 /TMS))
    (pad 12 thru_hole circle (at -6.35 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A6))
    (pad 11 thru_hole circle (at -8.89 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A5))
    (pad 10 thru_hole circle (at -6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at -8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A4))
    (pad 8 thru_hole circle (at -6.35 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A3))
    (pad 7 thru_hole circle (at -8.89 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /TDI))
    (pad 6 thru_hole circle (at -6.35 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A2))
    (pad 5 thru_hole circle (at -3.81 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~ROM_CS))
    (pad 4 thru_hole circle (at -3.81 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~RAM_CSI))
    (pad 3 thru_hole circle (at -1.27 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 2 thru_hole circle (at -1.27 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /~MREQ))
    (pad 1 thru_hole rect (at 1.27 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /~RESET))
  )
  (module My_Components:Socket_DIP32_600 (layer F.Cu) (tedit 6001434A)
    (at 204.47 93.98)
    (descr "32 pins DIL package, round pads")
    (tags "DIP DIL DIP32 DIL32")
    (fp_text reference U2 (at -11.43 -0.9525 180) (layer F.SilkS))
    (fp_text value SST39SF040 (at -11.1125 0.635) (layer F.SilkS))
    (pad 32 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 31 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /~WR))
    (pad 30 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /MA17))
    (pad 29 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /MA14))
    (pad 28 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A13))
    (pad 27 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A8))
    (pad 26 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A9))
    (pad 25 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A11))
    (pad 24 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /~RD))
    (pad 23 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A10))
    (pad 22 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~ROM_CS))
    (pad 21 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /D7))
    (pad 20 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D6))
    (pad 19 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D5))
    (pad 18 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D4))
    (pad 17 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D3))
    (pad 16 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D2))
    (pad 14 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D1))
    (pad 13 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D0))
    (pad 12 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A0))
    (pad 11 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A1))
    (pad 10 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A2))
    (pad 9 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A3))
    (pad 8 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A4))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A5))
    (pad 6 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A6))
    (pad 5 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A7))
    (pad 4 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A12))
    (pad 3 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /MA15))
    (pad 2 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /MA16))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /MA18))
    (model dil/dil_32-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Socket_DIP32_600 (layer F.Cu) (tedit 6001434A)
    (at 204.47 111.76)
    (descr "32 pins DIL package, round pads")
    (tags "DIP DIL DIP32 DIL32")
    (fp_text reference U3 (at -11.43 -0.9525) (layer F.SilkS))
    (fp_text value AS6C4008 (at -11.43 1.778) (layer F.SilkS))
    (pad 32 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VRAM))
    (pad 31 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /MA15))
    (pad 30 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /MA17))
    (pad 29 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /~WR))
    (pad 28 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A13))
    (pad 27 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A8))
    (pad 26 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A9))
    (pad 25 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A11))
    (pad 24 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /~RD))
    (pad 23 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A10))
    (pad 22 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~RAM_CS))
    (pad 21 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /D7))
    (pad 20 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D6))
    (pad 19 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D5))
    (pad 18 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D4))
    (pad 17 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D3))
    (pad 16 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D2))
    (pad 14 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D1))
    (pad 13 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D0))
    (pad 12 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A0))
    (pad 11 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A1))
    (pad 10 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A2))
    (pad 9 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A3))
    (pad 8 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A4))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A5))
    (pad 6 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A6))
    (pad 5 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A7))
    (pad 4 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A12))
    (pad 3 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /MA14))
    (pad 2 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /MA16))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /MA18))
    (model dil/dil_32-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Socket_DIP40_600 (layer F.Cu) (tedit 6001422F)
    (at 151.13 111.76)
    (descr "40 pins DIL package, round pads")
    (tags "DIP DIL DIP40 DIL40")
    (fp_text reference U1 (at -16.51 -1.5875) (layer F.SilkS))
    (fp_text value Z84C00 (at -16.51 0.9525) (layer F.SilkS))
    (pad 40 thru_hole circle (at -24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A10))
    (pad 39 thru_hole circle (at -21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A9))
    (pad 38 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A8))
    (pad 37 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A7))
    (pad 36 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A6))
    (pad 35 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A5))
    (pad 34 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A4))
    (pad 33 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A3))
    (pad 32 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A2))
    (pad 31 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A1))
    (pad 30 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A0))
    (pad 29 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 28 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /~RFSH))
    (pad 27 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /~M1))
    (pad 26 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /~RESET))
    (pad 25 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /~BUSREQ))
    (pad 24 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /~WAIT))
    (pad 23 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /~BUSACK))
    (pad 22 thru_hole circle (at 21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /~WR))
    (pad 21 thru_hole circle (at 24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /~RD))
    (pad 20 thru_hole circle (at 24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /~IORQ))
    (pad 19 thru_hole circle (at 21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /~MREQ))
    (pad 18 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /~HALT))
    (pad 17 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /~NMI))
    (pad 16 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /~INT))
    (pad 15 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D1))
    (pad 14 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D0))
    (pad 13 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /D7))
    (pad 12 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D2))
    (pad 11 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 10 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D6))
    (pad 9 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D5))
    (pad 8 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D3))
    (pad 7 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D4))
    (pad 6 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /CPU_CLK))
    (pad 5 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A15))
    (pad 4 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A14))
    (pad 3 thru_hole circle (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A13))
    (pad 2 thru_hole circle (at -21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A12))
    (pad 1 thru_hole rect (at -24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A11))
    (model dil/dil_40-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:OSC_Half_Can_DIP8 (layer F.Cu) (tedit 6001377F)
    (at 141.605 95.885)
    (descr "DIP8 package for half can OSC")
    (tags "OSC DIP")
    (fp_text reference X1 (at -8.89 -5.08 270) (layer F.SilkS))
    (fp_text value 7.3728MHz (at -7.3025 -5.08 90) (layer F.SilkS))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /CPU_CLK))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(X1-Pad1)"))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Friction_Lock_2P_2.54mm (layer F.Cu) (tedit 600136C1)
    (at 180.34 119.38)
    (descr "Connector, Friction Lock, 2 Positions, 2.54mm Pitch")
    (tags "CONN FRICTION LOCK 2P")
    (fp_text reference J1 (at 0 -5.715) (layer F.SilkS))
    (fp_text value VBAT (at 0 -4.1275) (layer F.SilkS))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VBAT))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_SIL9 (layer F.Cu) (tedit 60013625)
    (at 200.66 121.92)
    (descr "Footprint, SIL-9")
    (tags "CONN SIL-9")
    (fp_text reference RN1 (at -2.54 2.2225) (layer F.SilkS))
    (fp_text value 4.7k (at 2.54 2.2225) (layer F.SilkS))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /D7))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D6))
    (pad 7 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D5))
    (pad 6 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D4))
    (pad 5 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D3))
    (pad 4 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D2))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D1))
    (pad 2 thru_hole circle (at -7.62 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D0))
    (pad 1 thru_hole rect (at -10.16 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
  )
  (module My_Components:Conn_SIL6 (layer F.Cu) (tedit 600135FA)
    (at 168.91 121.92)
    (descr "Footprint, SIL-6")
    (tags "CONN SIL-6")
    (fp_text reference RN2 (at -7.3025 2.54) (layer F.SilkS))
    (fp_text value 4.7k (at -3.81 2.54) (layer F.SilkS))
    (pad 6 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /~WAIT))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /~BUSREQ))
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /~RESET))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /~NMI))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /~INT))
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 6001348F)
    (at 187.96 81.28)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C6 (at -4.2545 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.0635 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 6001348F)
    (at 187.96 83.82)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C2 (at -4.2545 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.0635 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 6001348F)
    (at 139.065 87.63)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C7 (at -2.54 -1.905 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 6001348F)
    (at 153.67 100.965 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C5 (at 4.445 0 90) (layer F.SilkS))
    (fp_text value 100nF (at -0.0635 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 6001348F)
    (at 149.86 121.92 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C1 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 100nF (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 6001348F)
    (at 181.61 106.68 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C3 (at -4.7625 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.0635 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VRAM))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 600133A0)
    (at 179.07 106.68 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C4 (at 4.7625 0 90) (layer F.SilkS))
    (fp_text value 100nF (at -0.0635 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 56D1B4CB)
    (at 130.2258 95.631)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.8) (layer F.Fab))
    (fp_text value 3.2mm (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 201.93 82.55 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 1.397 -1.27 270) (layer F.SilkS))
    (fp_text value 10k (at -1.905 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 57 /TCK))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 199.39 82.55 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 1.397 -1.27 270) (layer F.SilkS))
    (fp_text value 10k (at -1.905 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 /TDO))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 196.85 82.55 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 1.397 -1.27 270) (layer F.SilkS))
    (fp_text value 10k (at -1.905 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 59 /TMS))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 194.31 82.55 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 1.397 -1.27 270) (layer F.SilkS))
    (fp_text value 10k (at -1.905 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 /TDI))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 146.685 87.63 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 1.397 -1.2065 270) (layer F.SilkS))
    (fp_text value 10k (at 1.4605 1.27 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 74 "Net-(R5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 144.145 87.63 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 3.175 -2.54) (layer F.SilkS))
    (fp_text value 29.4k (at 1.905 -2.54) (layer F.SilkS))
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3266W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 141.605 82.55 180)
    (descr "Potentiometer, vertical, Bourns 3266W, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer vertical Bourns 3266W")
    (fp_text reference RV1 (at 1.905 -0.635 90) (layer F.SilkS))
    (fp_text value 2k (at 1.905 1.905 90) (layer F.SilkS))
    (fp_text user %R (at -3.175 1.23) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(R6-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 157.48 122.2375 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C8 (at 1.5875 4.1275 180) (layer F.SilkS))
    (fp_text value 47uF (at 2.8575 4.1275 180) (layer F.SilkS))
    (fp_text user %R (at 1 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 216.2175 94.9325 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference LOGO1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0.75 0) (layer B.Fab) hide)
  )
  (gr_text "Design files and documentation:\ngithub.com/skiselev/Z80-512K" (at 212.09 93.0275) (layer B.SilkS))
  (gr_text "Licensed under CERN-OHL-S:\nhttps://cern-ohl.web.cern.ch" (at 212.09 97.155) (layer B.SilkS))
  (gr_text GND (at 207.3275 80.01) (layer B.SilkS))
  (gr_text VCC (at 207.3275 82.55) (layer B.SilkS))
  (gr_text GND (at 221.9325 82.55) (layer B.SilkS))
  (gr_text TCK (at 209.55 84.1375) (layer B.SilkS))
  (gr_text TDO (at 212.09 84.1375) (layer B.SilkS))
  (gr_text TMS (at 214.63 84.1375) (layer B.SilkS))
  (gr_text TDI (at 219.71 84.1375) (layer B.SilkS))
  (gr_text ! (at 173.0375 111.125) (layer B.SilkS))
  (gr_text "Connect 3V battery to J1 for battery-backed SRAM\nPlace a jumper over J1 if battery backup is not required" (at 170.815 110.8075) (layer B.SilkS))
  (gr_text JLCJLCJLCJLC (at 134.9375 105.7275) (layer F.SilkS))
  (gr_text GND (at 167.64 117.475) (layer B.SilkS))
  (gr_text VCC (at 170.18 117.475) (layer B.SilkS))
  (gr_text ~RFSH (at 172.72 115.57) (layer B.SilkS))
  (gr_text M1 (at 172.72 117.475) (layer B.SilkS))
  (gr_text ~RESET (at 177.8 117.475) (layer B.SilkS))
  (gr_text ~CLK2 (at 177.8 121.285) (layer B.SilkS))
  (gr_text ~CLK1 (at 177.8 122.8725) (layer B.SilkS))
  (gr_text ~INT (at 180.34 122.8725) (layer B.SilkS))
  (gr_text ~BACK (at 180.34 121.285) (layer B.SilkS))
  (gr_text ~MREQ (at 182.88 122.8725) (layer B.SilkS))
  (gr_text ~HALT (at 182.88 121.285) (layer B.SilkS))
  (gr_text ~WR (at 185.42 122.8725) (layer B.SilkS))
  (gr_text ~BREQ (at 185.42 121.285) (layer B.SilkS))
  (gr_text ~WAIT (at 187.96 121.285) (layer B.SilkS))
  (gr_text ~RD (at 187.96 122.8725) (layer B.SilkS))
  (gr_text A3 (at 160.02 123.5075) (layer B.SilkS))
  (gr_text ~NMI (at 190.5 115.57) (layer B.SilkS))
  (gr_text ~IORQ (at 190.5 117.475) (layer B.SilkS))
  (gr_text A15 (at 127 125.4125) (layer B.SilkS))
  (gr_text A14 (at 129.54 125.4125) (layer B.SilkS))
  (gr_text A13 (at 132.08 125.4125) (layer B.SilkS))
  (gr_text A12 (at 134.62 125.4125) (layer B.SilkS))
  (gr_text A11 (at 137.16 125.4125) (layer B.SilkS))
  (gr_text A10 (at 139.7 125.4125) (layer B.SilkS))
  (gr_text A9 (at 142.24 125.4125) (layer B.SilkS))
  (gr_text A8 (at 144.78 125.4125) (layer B.SilkS))
  (gr_text A7 (at 147.32 125.4125) (layer B.SilkS))
  (gr_text A6 (at 149.86 125.4125) (layer B.SilkS))
  (gr_text A5 (at 152.4 125.4125) (layer B.SilkS))
  (gr_text A4 (at 154.94 125.4125) (layer B.SilkS))
  (gr_text A2 (at 160.02 125.4125) (layer B.SilkS))
  (gr_text A1 (at 162.56 125.4125) (layer B.SilkS))
  (gr_text A0 (at 165.1 125.4125) (layer B.SilkS))
  (gr_text USR3 (at 220.98 123.5075) (layer B.SilkS))
  (gr_text USR2 (at 220.98 125.4125) (layer B.SilkS))
  (gr_text USR1 (at 218.44 125.4125) (layer B.SilkS))
  (gr_text RXDA (at 215.9 125.4125) (layer B.SilkS))
  (gr_text TXDA (at 213.36 125.4125) (layer B.SilkS))
  (gr_text D0 (at 193.04 125.4125) (layer B.SilkS))
  (gr_text D1 (at 195.58 125.4125) (layer B.SilkS))
  (gr_text D2 (at 198.12 125.4125) (layer B.SilkS))
  (gr_text D3 (at 200.66 125.4125) (layer B.SilkS))
  (gr_text D4 (at 203.2 125.4125) (layer B.SilkS))
  (gr_text D5 (at 205.74 125.4125) (layer B.SilkS))
  (gr_text D6 (at 208.28 125.4125) (layer B.SilkS))
  (gr_text D7 (at 210.82 125.4125) (layer B.SilkS))
  (gr_text 1 (at 127 124.46) (layer F.SilkS))
  (gr_text - (at 182.245 115.2525) (layer F.SilkS))
  (gr_text + (at 178.435 115.2525) (layer F.SilkS))
  (gr_text "Z80-512K - Version 1.1\nCopyright (C) 2020, 2021 Sergey Kiselev" (at 203.835 88.9) (layer B.SilkS))
  (gr_text "Z80-512K - Version 1.1\n(C) 2020, 2021 Sergey Kiselev" (at 128.905 123.5075) (layer F.SilkS))
  (gr_text www.malinov.com (at 217.17 124.46) (layer F.SilkS))
  (gr_arc (start 126.2126 94.3229) (end 125.1966 94.3229) (angle 45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 219.2026 83.9924) (end 224.3026 83.9924) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 223.2866 127.7366) (end 223.2866 128.7526) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 126.2126 127.7366) (end 125.1966 127.7366) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.49418 93.60448) (end 139.90868 79.18998) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 140.6271 79.9084) (end 140.6271 78.8924) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.6271 78.8924) (end 219.2026 78.8924) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.1966 127.7366) (end 125.1966 94.3229) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 223.2866 128.7526) (end 126.2126 128.7526) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 224.3026 83.9924) (end 224.3026 127.7366) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.25 128.75) (xy 125.25 128.75) (xy 125.25 93.75) (xy 140.25 78.75) (xy 224.25 78.75)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.25 128.75) (xy 125.25 128.75) (xy 125.25 93.75) (xy 140.25 78.75) (xy 224.25 78.75)
      )
    )
  )
)
