<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.1">
<drawing>
<board>
<plain>
<wire x1="30.566309375" y1="37.612009375" x2="25.155840625" y2="34.783140625" width="0.2" layer="20" curve="0.695764"/>
<wire x1="14.844159375" y1="34.783140625" x2="25.155840625" y2="34.783140625" width="0.2" layer="20" curve="55.901534"/>
<wire x1="14.844159375" y1="34.783140625" x2="9.433690625" y2="37.612009375" width="0.2" layer="20" curve="0.695764"/>
<wire x1="9.433690625" y1="37.612009375" x2="6.2779" y2="39.05466875" width="0.2" layer="20" curve="5.375248"/>
<wire x1="6.2779" y1="39.05466875" x2="0.94533125" y2="33.7221" width="0.2" layer="20" curve="133.759363"/>
<wire x1="0.94533125" y1="33.7221" x2="2.387990625" y2="30.566309375" width="0.2" layer="20" curve="5.375248"/>
<wire x1="2.387990625" y1="30.566309375" x2="5.216859375" y2="25.155840625" width="0.2" layer="20" curve="0.695764"/>
<wire x1="5.216859375" y1="14.844159375" x2="5.216859375" y2="25.155840625" width="0.2" layer="20" curve="55.901534"/>
<wire x1="5.216859375" y1="14.844159375" x2="2.387990625" y2="9.433690625" width="0.2" layer="20" curve="0.695764"/>
<wire x1="2.387990625" y1="9.433690625" x2="0.94533125" y2="6.2779" width="0.2" layer="20" curve="5.375248"/>
<wire x1="0.94533125" y1="6.2779" x2="6.2779" y2="0.94533125" width="0.2" layer="20" curve="133.759363"/>
<wire x1="6.2779" y1="0.94533125" x2="9.433690625" y2="2.387990625" width="0.2" layer="20" curve="5.375248"/>
<wire x1="9.433690625" y1="2.387990625" x2="14.844159375" y2="5.216859375" width="0.2" layer="20" curve="0.695764"/>
<wire x1="25.155840625" y1="5.216859375" x2="14.844159375" y2="5.216859375" width="0.2" layer="20" curve="55.901534"/>
<wire x1="25.155840625" y1="5.216859375" x2="30.566309375" y2="2.387990625" width="0.2" layer="20" curve="0.695764"/>
<wire x1="30.566309375" y1="2.387990625" x2="33.7221" y2="0.94533125" width="0.2" layer="20" curve="5.375248"/>
<wire x1="33.7221" y1="0.94533125" x2="39.05466875" y2="6.2779" width="0.2" layer="20" curve="133.759363"/>
<wire x1="39.05466875" y1="6.2779" x2="37.612009375" y2="9.433690625" width="0.2" layer="20" curve="5.375248"/>
<wire x1="37.612009375" y1="9.433690625" x2="34.783140625" y2="14.844159375" width="0.2" layer="20" curve="0.695764"/>
<wire x1="34.783140625" y1="25.155840625" x2="34.783140625" y2="14.844159375" width="0.2" layer="20" curve="55.901534"/>
<wire x1="34.783140625" y1="25.155840625" x2="37.612009375" y2="30.566309375" width="0.2" layer="20" curve="0.695764"/>
<wire x1="37.612009375" y1="30.566309375" x2="39.05466875" y2="33.7221" width="0.2" layer="20" curve="5.375248"/>
<wire x1="39.05466875" y1="33.7221" x2="33.7221" y2="39.05466875" width="0.2" layer="20" curve="133.759363"/>
<wire x1="33.7221" y1="39.05466875" x2="30.566309375" y2="37.612009375" width="0.2" layer="20" curve="5.375248"/>
<hole x="4.75" y="35.25" drill="3"/>
<hole x="30" y="30" drill="3"/>
<hole x="10" y="30" drill="3"/>
<hole x="35.25" y="35.25" drill="3"/>
<hole x="4.75" y="4.75" drill="3"/>
<hole x="10" y="10" drill="3"/>
<hole x="30" y="10" drill="3"/>
<hole x="35.25" y="4.75" drill="3"/>
</plain>
<libraries>
<library name="myFootprints">
<packages>
<package name="POSITIVE-ESC-PAD">
</package>
<package name="POSITIVE-BATTERY-PAD">
</package>
<package name="LEMON">
</package>
<package name="POSITIVE-AUX_PAD">
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-252">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="myFootprints" package="POSITIVE-ESC-PAD" value="POSITIVE-ESC-PAD"/>
<element name="U$4" library="myFootprints" package="POSITIVE-ESC-PAD" value="POSITIVE-ESC-PAD"/>
<element name="U$5" library="myFootprints" package="POSITIVE-ESC-PAD" value="POSITIVE-ESC-PAD"/>
<element name="U$6" library="myFootprints" package="POSITIVE-ESC-PAD" value="POSITIVE-ESC-PAD"/>
<element name="U$13" library="myFootprints" package="POSITIVE-ESC-PAD" value="POSITIVE-ESC-PAD"/>
<element name="U$17" library="myFootprints" package="POSITIVE-ESC-PAD" value="POSITIVE-ESC-PAD"/>
<element name="U$18" library="myFootprints" package="POSITIVE-ESC-PAD" value="POSITIVE-ESC-PAD"/>
<element name="U$19" library="myFootprints" package="POSITIVE-ESC-PAD" value="POSITIVE-ESC-PAD"/>
<element name="U$1" library="myFootprints" package="POSITIVE-BATTERY-PAD" value="POSITIVE-BATTERY-PAD"/>
<element name="78XX" library="SparkFun-IC-Power" package="TO-252" value="+12v">
<attribute name="PROD_ID" value="VREG-12370"/>
</element>
<element name="U$7" library="myFootprints" package="LEMON" value=""/>
<element name="U$8" library="myFootprints" package="POSITIVE-AUX_PAD" value="POSITIVE-AUX-PAD"/>
<element name="U$9" library="myFootprints" package="POSITIVE-AUX_PAD" value="POSITIVE-AUX-PAD"/>
<element name="U$2" library="myFootprints" package="POSITIVE-BATTERY-PAD" value="POSITIVE-BATTERY-PAD"/>
</elements>
<signals>
<signal name="VIN">
<contactref element="U$3" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="78XX" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="U$13" pad="P$1"/>
<contactref element="U$17" pad="P$1"/>
<contactref element="U$18" pad="P$1"/>
<contactref element="U$19" pad="P$1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="78XX" pad="3"/>
<contactref element="U$9" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="78XX" pad="2"/>
<contactref element="U$8" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
