<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.75" x2="6.4" y2="1.75" width="0" layer="20"/>
<wire x1="6.4" y1="10.13" x2="0" y2="10.13" width="0" layer="20"/>
<wire x1="0" y1="10.13" x2="0" y2="1.75" width="0" layer="20"/>
<wire x1="33.1" y1="11.88" x2="33.1" y2="8.15" width="0" layer="20"/>
<wire x1="33.1" y1="3.55" x2="33.1" y2="0" width="0" layer="20"/>
<wire x1="33.1" y1="11.88" x2="17.65" y2="11.88" width="0" layer="20"/>
<wire x1="9.25" y1="11.88" x2="6.4" y2="11.88" width="0" layer="20"/>
<wire x1="6.4" y1="11.88" x2="6.4" y2="10.13" width="0" layer="20"/>
<wire x1="33.1" y1="0" x2="6.4" y2="0" width="0" layer="20"/>
<wire x1="6.4" y1="0" x2="6.4" y2="1.75" width="0" layer="20"/>
<wire x1="18.08" y1="7.9" x2="18.08" y2="4" width="0.65" layer="46"/>
<wire x1="19.1" y1="10.04" x2="27.13" y2="10.04" width="0" layer="20"/>
<wire x1="27.13" y1="10.04" x2="27.13" y2="1.84" width="0" layer="20"/>
<wire x1="27.13" y1="1.84" x2="19.1" y2="1.84" width="0" layer="20"/>
<wire x1="19.1" y1="1.84" x2="19.1" y2="2.54" width="0" layer="20"/>
<wire x1="19.1" y1="9.34" x2="19.1" y2="10.04" width="0" layer="20"/>
<wire x1="19.1" y1="9.34" x2="17.72" y2="9.34" width="0" layer="20"/>
<wire x1="17.98" y1="8.54" x2="17.98" y2="3.34" width="0" layer="20"/>
<wire x1="17.72" y1="2.54" x2="19.1" y2="2.54" width="0" layer="20"/>
<wire x1="17.72" y1="2.54" x2="17.72" y2="3.34" width="0" layer="20"/>
<wire x1="17.72" y1="3.34" x2="17.98" y2="3.34" width="0" layer="20"/>
<wire x1="17.78" y1="9.35" x2="17.72" y2="9.34" width="0" layer="20"/>
<wire x1="17.72" y1="9.34" x2="17.72" y2="8.54" width="0" layer="20"/>
<wire x1="17.72" y1="8.54" x2="17.98" y2="8.54" width="0" layer="20"/>
<hole x="9.85" y="12.23" drill="0.7"/>
<hole x="10.85" y="12.23" drill="0.7"/>
<hole x="11.85" y="12.23" drill="0.7"/>
<hole x="12.85" y="12.23" drill="0.7"/>
<hole x="13.85" y="12.23" drill="0.7"/>
<hole x="14.85" y="12.23" drill="0.7"/>
<hole x="15.85" y="12.23" drill="0.7"/>
<hole x="16.85" y="12.23" drill="0.7"/>
<wire x1="9.25" y1="12.58" x2="9.25" y2="11.88" width="0" layer="20"/>
<wire x1="17.65" y1="12.58" x2="17.65" y2="11.88" width="0" layer="20"/>
<hole x="33.45" y="4.35" drill="0.7"/>
<hole x="33.45" y="5.35" drill="0.7"/>
<hole x="33.45" y="6.35" drill="0.7"/>
<hole x="33.45" y="7.35" drill="0.7"/>
<wire x1="33.1" y1="8.15" x2="33.8" y2="8.15" width="0" layer="20"/>
<wire x1="33.1" y1="3.55" x2="33.8" y2="3.55" width="0" layer="20"/>
<wire x1="0" y1="14.33" x2="6.4" y2="14.33" width="0" layer="20"/>
<wire x1="6.4" y1="22.71" x2="0" y2="22.71" width="0" layer="20"/>
<wire x1="0" y1="22.71" x2="0" y2="14.33" width="0" layer="20"/>
<wire x1="33.1" y1="24.46" x2="33.1" y2="20.73" width="0" layer="20"/>
<wire x1="33.1" y1="16.13" x2="33.1" y2="12.58" width="0" layer="20"/>
<wire x1="33.1" y1="24.46" x2="17.65" y2="24.46" width="0" layer="20"/>
<wire x1="9.25" y1="24.46" x2="6.4" y2="24.46" width="0" layer="20"/>
<wire x1="6.4" y1="24.46" x2="6.4" y2="22.71" width="0" layer="20"/>
<wire x1="6.4" y1="12.58" x2="6.4" y2="14.33" width="0" layer="20"/>
<wire x1="18.08" y1="20.48" x2="18.08" y2="16.58" width="0.65" layer="46"/>
<wire x1="19.1" y1="22.62" x2="27.13" y2="22.62" width="0" layer="20"/>
<wire x1="27.13" y1="22.62" x2="27.13" y2="14.42" width="0" layer="20"/>
<wire x1="27.13" y1="14.42" x2="19.1" y2="14.42" width="0" layer="20"/>
<wire x1="19.1" y1="14.42" x2="19.1" y2="15.12" width="0" layer="20"/>
<wire x1="19.1" y1="21.92" x2="19.1" y2="22.62" width="0" layer="20"/>
<wire x1="19.1" y1="21.92" x2="17.72" y2="21.92" width="0" layer="20"/>
<wire x1="17.98" y1="21.12" x2="17.98" y2="15.92" width="0" layer="20"/>
<wire x1="17.72" y1="15.12" x2="19.1" y2="15.12" width="0" layer="20"/>
<wire x1="17.72" y1="15.12" x2="17.72" y2="15.92" width="0" layer="20"/>
<wire x1="17.72" y1="15.92" x2="17.98" y2="15.92" width="0" layer="20"/>
<wire x1="17.78" y1="21.93" x2="17.72" y2="21.92" width="0" layer="20"/>
<wire x1="17.72" y1="21.92" x2="17.72" y2="21.12" width="0" layer="20"/>
<wire x1="17.72" y1="21.12" x2="17.98" y2="21.12" width="0" layer="20"/>
<hole x="9.85" y="24.81" drill="0.7"/>
<hole x="10.85" y="24.81" drill="0.7"/>
<hole x="11.85" y="24.81" drill="0.7"/>
<hole x="12.85" y="24.81" drill="0.7"/>
<hole x="13.85" y="24.81" drill="0.7"/>
<hole x="14.85" y="24.81" drill="0.7"/>
<hole x="15.85" y="24.81" drill="0.7"/>
<hole x="16.85" y="24.81" drill="0.7"/>
<wire x1="9.25" y1="25.16" x2="9.25" y2="24.46" width="0" layer="20"/>
<wire x1="17.65" y1="25.16" x2="17.65" y2="24.46" width="0" layer="20"/>
<hole x="33.45" y="16.93" drill="0.7"/>
<hole x="33.45" y="17.93" drill="0.7"/>
<hole x="33.45" y="18.93" drill="0.7"/>
<hole x="33.45" y="19.93" drill="0.7"/>
<wire x1="33.1" y1="20.73" x2="33.8" y2="20.73" width="0" layer="20"/>
<wire x1="33.1" y1="16.13" x2="33.8" y2="16.13" width="0" layer="20"/>
<wire x1="33.1" y1="12.58" x2="17.65" y2="12.58" width="0" layer="20"/>
<wire x1="9.25" y1="12.58" x2="6.4" y2="12.58" width="0" layer="20"/>
<wire x1="33.8" y1="1.75" x2="40.2" y2="1.75" width="0" layer="20"/>
<wire x1="40.2" y1="10.13" x2="33.8" y2="10.13" width="0" layer="20"/>
<wire x1="66.9" y1="11.88" x2="66.9" y2="8.15" width="0" layer="20"/>
<wire x1="66.9" y1="3.55" x2="66.9" y2="0" width="0" layer="20"/>
<wire x1="66.9" y1="11.88" x2="51.45" y2="11.88" width="0" layer="20"/>
<wire x1="43.05" y1="11.88" x2="40.2" y2="11.88" width="0" layer="20"/>
<wire x1="40.2" y1="11.88" x2="40.2" y2="10.13" width="0" layer="20"/>
<wire x1="66.9" y1="0" x2="40.2" y2="0" width="0" layer="20"/>
<wire x1="40.2" y1="0" x2="40.2" y2="1.75" width="0" layer="20"/>
<wire x1="51.88" y1="7.9" x2="51.88" y2="4" width="0.65" layer="46"/>
<wire x1="52.9" y1="10.04" x2="60.93" y2="10.04" width="0" layer="20"/>
<wire x1="60.93" y1="10.04" x2="60.93" y2="1.84" width="0" layer="20"/>
<wire x1="60.93" y1="1.84" x2="52.9" y2="1.84" width="0" layer="20"/>
<wire x1="52.9" y1="1.84" x2="52.9" y2="2.54" width="0" layer="20"/>
<wire x1="52.9" y1="9.34" x2="52.9" y2="10.04" width="0" layer="20"/>
<wire x1="52.9" y1="9.34" x2="51.52" y2="9.34" width="0" layer="20"/>
<wire x1="51.78" y1="8.54" x2="51.78" y2="3.34" width="0" layer="20"/>
<wire x1="51.52" y1="2.54" x2="52.9" y2="2.54" width="0" layer="20"/>
<wire x1="51.52" y1="2.54" x2="51.52" y2="3.34" width="0" layer="20"/>
<wire x1="51.52" y1="3.34" x2="51.78" y2="3.34" width="0" layer="20"/>
<wire x1="51.58" y1="9.35" x2="51.52" y2="9.34" width="0" layer="20"/>
<wire x1="51.52" y1="9.34" x2="51.52" y2="8.54" width="0" layer="20"/>
<wire x1="51.52" y1="8.54" x2="51.78" y2="8.54" width="0" layer="20"/>
<hole x="43.65" y="12.23" drill="0.7"/>
<hole x="44.65" y="12.23" drill="0.7"/>
<hole x="45.65" y="12.23" drill="0.7"/>
<hole x="46.65" y="12.23" drill="0.7"/>
<hole x="47.65" y="12.23" drill="0.7"/>
<hole x="48.65" y="12.23" drill="0.7"/>
<hole x="49.65" y="12.23" drill="0.7"/>
<hole x="50.65" y="12.23" drill="0.7"/>
<wire x1="43.05" y1="12.58" x2="43.05" y2="11.88" width="0" layer="20"/>
<wire x1="51.45" y1="12.58" x2="51.45" y2="11.88" width="0" layer="20"/>
<hole x="67.25" y="4.35" drill="0.7"/>
<hole x="67.25" y="5.35" drill="0.7"/>
<hole x="67.25" y="6.35" drill="0.7"/>
<hole x="67.25" y="7.35" drill="0.7"/>
<wire x1="66.9" y1="8.15" x2="67.6" y2="8.15" width="0" layer="20"/>
<wire x1="66.9" y1="3.55" x2="67.6" y2="3.55" width="0" layer="20"/>
<wire x1="33.8" y1="14.33" x2="40.2" y2="14.33" width="0" layer="20"/>
<wire x1="40.2" y1="22.71" x2="33.8" y2="22.71" width="0" layer="20"/>
<wire x1="66.9" y1="24.46" x2="66.9" y2="20.73" width="0" layer="20"/>
<wire x1="66.9" y1="16.13" x2="66.9" y2="12.58" width="0" layer="20"/>
<wire x1="66.9" y1="24.46" x2="51.45" y2="24.46" width="0" layer="20"/>
<wire x1="43.05" y1="24.46" x2="40.2" y2="24.46" width="0" layer="20"/>
<wire x1="40.2" y1="24.46" x2="40.2" y2="22.71" width="0" layer="20"/>
<wire x1="40.2" y1="12.58" x2="40.2" y2="14.33" width="0" layer="20"/>
<wire x1="51.88" y1="20.48" x2="51.88" y2="16.58" width="0.65" layer="46"/>
<wire x1="52.9" y1="22.62" x2="60.93" y2="22.62" width="0" layer="20"/>
<wire x1="60.93" y1="22.62" x2="60.93" y2="14.42" width="0" layer="20"/>
<wire x1="60.93" y1="14.42" x2="52.9" y2="14.42" width="0" layer="20"/>
<wire x1="52.9" y1="14.42" x2="52.9" y2="15.12" width="0" layer="20"/>
<wire x1="52.9" y1="21.92" x2="52.9" y2="22.62" width="0" layer="20"/>
<wire x1="52.9" y1="21.92" x2="51.52" y2="21.92" width="0" layer="20"/>
<wire x1="51.78" y1="21.12" x2="51.78" y2="15.92" width="0" layer="20"/>
<wire x1="51.52" y1="15.12" x2="52.9" y2="15.12" width="0" layer="20"/>
<wire x1="51.52" y1="15.12" x2="51.52" y2="15.92" width="0" layer="20"/>
<wire x1="51.52" y1="15.92" x2="51.78" y2="15.92" width="0" layer="20"/>
<wire x1="51.58" y1="21.93" x2="51.52" y2="21.92" width="0" layer="20"/>
<wire x1="51.52" y1="21.92" x2="51.52" y2="21.12" width="0" layer="20"/>
<wire x1="51.52" y1="21.12" x2="51.78" y2="21.12" width="0" layer="20"/>
<hole x="43.65" y="24.81" drill="0.7"/>
<hole x="44.65" y="24.81" drill="0.7"/>
<hole x="45.65" y="24.81" drill="0.7"/>
<hole x="46.65" y="24.81" drill="0.7"/>
<hole x="47.65" y="24.81" drill="0.7"/>
<hole x="48.65" y="24.81" drill="0.7"/>
<hole x="49.65" y="24.81" drill="0.7"/>
<hole x="50.65" y="24.81" drill="0.7"/>
<wire x1="43.05" y1="25.16" x2="43.05" y2="24.46" width="0" layer="20"/>
<wire x1="51.45" y1="25.16" x2="51.45" y2="24.46" width="0" layer="20"/>
<hole x="67.25" y="16.93" drill="0.7"/>
<hole x="67.25" y="17.93" drill="0.7"/>
<hole x="67.25" y="18.93" drill="0.7"/>
<hole x="67.25" y="19.93" drill="0.7"/>
<wire x1="66.9" y1="20.73" x2="67.6" y2="20.73" width="0" layer="20"/>
<wire x1="66.9" y1="16.13" x2="67.6" y2="16.13" width="0" layer="20"/>
<wire x1="66.9" y1="12.58" x2="51.45" y2="12.58" width="0" layer="20"/>
<wire x1="43.05" y1="12.58" x2="40.2" y2="12.58" width="0" layer="20"/>
<wire x1="33.8" y1="10.13" x2="33.8" y2="8.15" width="0" layer="20"/>
<wire x1="33.8" y1="3.55" x2="33.8" y2="1.75" width="0" layer="20"/>
<wire x1="33.8" y1="22.71" x2="33.8" y2="20.73" width="0" layer="20"/>
<wire x1="33.8" y1="16.13" x2="33.8" y2="14.33" width="0" layer="20"/>
<wire x1="67.6" y1="1.75" x2="74" y2="1.75" width="0" layer="20"/>
<wire x1="74" y1="10.13" x2="67.6" y2="10.13" width="0" layer="20"/>
<wire x1="100.7" y1="11.88" x2="100.7" y2="3.55" width="0" layer="20"/>
<wire x1="100.7" y1="3.55" x2="100.7" y2="0" width="0" layer="20"/>
<wire x1="100.7" y1="11.88" x2="85.25" y2="11.88" width="0" layer="20"/>
<wire x1="76.85" y1="11.88" x2="74" y2="11.88" width="0" layer="20"/>
<wire x1="74" y1="11.88" x2="74" y2="10.13" width="0" layer="20"/>
<wire x1="100.7" y1="0" x2="74" y2="0" width="0" layer="20"/>
<wire x1="74" y1="0" x2="74" y2="1.75" width="0" layer="20"/>
<wire x1="85.68" y1="7.9" x2="85.68" y2="4" width="0.65" layer="46"/>
<wire x1="86.7" y1="10.04" x2="94.73" y2="10.04" width="0" layer="20"/>
<wire x1="94.73" y1="10.04" x2="94.73" y2="1.84" width="0" layer="20"/>
<wire x1="94.73" y1="1.84" x2="86.7" y2="1.84" width="0" layer="20"/>
<wire x1="86.7" y1="1.84" x2="86.7" y2="2.54" width="0" layer="20"/>
<wire x1="86.7" y1="9.34" x2="86.7" y2="10.04" width="0" layer="20"/>
<wire x1="86.7" y1="9.34" x2="85.32" y2="9.34" width="0" layer="20"/>
<wire x1="85.58" y1="8.54" x2="85.58" y2="3.34" width="0" layer="20"/>
<wire x1="85.32" y1="2.54" x2="86.7" y2="2.54" width="0" layer="20"/>
<wire x1="85.32" y1="2.54" x2="85.32" y2="3.34" width="0" layer="20"/>
<wire x1="85.32" y1="3.34" x2="85.58" y2="3.34" width="0" layer="20"/>
<wire x1="85.38" y1="9.35" x2="85.32" y2="9.34" width="0" layer="20"/>
<wire x1="85.32" y1="9.34" x2="85.32" y2="8.54" width="0" layer="20"/>
<wire x1="85.32" y1="8.54" x2="85.58" y2="8.54" width="0" layer="20"/>
<hole x="77.45" y="12.23" drill="0.7"/>
<hole x="78.45" y="12.23" drill="0.7"/>
<hole x="79.45" y="12.23" drill="0.7"/>
<hole x="80.45" y="12.23" drill="0.7"/>
<hole x="81.45" y="12.23" drill="0.7"/>
<hole x="82.45" y="12.23" drill="0.7"/>
<hole x="83.45" y="12.23" drill="0.7"/>
<hole x="84.45" y="12.23" drill="0.7"/>
<wire x1="76.85" y1="12.58" x2="76.85" y2="11.88" width="0" layer="20"/>
<wire x1="85.25" y1="12.58" x2="85.25" y2="11.88" width="0" layer="20"/>
<wire x1="67.6" y1="14.33" x2="74" y2="14.33" width="0" layer="20"/>
<wire x1="74" y1="22.71" x2="67.6" y2="22.71" width="0" layer="20"/>
<wire x1="100.7" y1="24.46" x2="100.7" y2="20.73" width="0" layer="20"/>
<wire x1="100.7" y1="20.73" x2="100.7" y2="12.58" width="0" layer="20"/>
<wire x1="100.7" y1="24.46" x2="85.25" y2="24.46" width="0" layer="20"/>
<wire x1="76.85" y1="24.46" x2="74" y2="24.46" width="0" layer="20"/>
<wire x1="74" y1="24.46" x2="74" y2="22.71" width="0" layer="20"/>
<wire x1="74" y1="12.58" x2="74" y2="14.33" width="0" layer="20"/>
<wire x1="85.68" y1="20.48" x2="85.68" y2="16.58" width="0.65" layer="46"/>
<wire x1="86.7" y1="22.62" x2="94.73" y2="22.62" width="0" layer="20"/>
<wire x1="94.73" y1="22.62" x2="94.73" y2="14.42" width="0" layer="20"/>
<wire x1="94.73" y1="14.42" x2="86.7" y2="14.42" width="0" layer="20"/>
<wire x1="86.7" y1="14.42" x2="86.7" y2="15.12" width="0" layer="20"/>
<wire x1="86.7" y1="21.92" x2="86.7" y2="22.62" width="0" layer="20"/>
<wire x1="86.7" y1="21.92" x2="85.32" y2="21.92" width="0" layer="20"/>
<wire x1="85.58" y1="21.12" x2="85.58" y2="15.92" width="0" layer="20"/>
<wire x1="85.32" y1="15.12" x2="86.7" y2="15.12" width="0" layer="20"/>
<wire x1="85.32" y1="15.12" x2="85.32" y2="15.92" width="0" layer="20"/>
<wire x1="85.32" y1="15.92" x2="85.58" y2="15.92" width="0" layer="20"/>
<wire x1="85.38" y1="21.93" x2="85.32" y2="21.92" width="0" layer="20"/>
<wire x1="85.32" y1="21.92" x2="85.32" y2="21.12" width="0" layer="20"/>
<wire x1="85.32" y1="21.12" x2="85.58" y2="21.12" width="0" layer="20"/>
<hole x="77.45" y="24.81" drill="0.7"/>
<hole x="78.45" y="24.81" drill="0.7"/>
<hole x="79.45" y="24.81" drill="0.7"/>
<hole x="80.45" y="24.81" drill="0.7"/>
<hole x="81.45" y="24.81" drill="0.7"/>
<hole x="82.45" y="24.81" drill="0.7"/>
<hole x="83.45" y="24.81" drill="0.7"/>
<hole x="84.45" y="24.81" drill="0.7"/>
<wire x1="76.85" y1="25.16" x2="76.85" y2="24.46" width="0" layer="20"/>
<wire x1="85.25" y1="25.16" x2="85.25" y2="24.46" width="0" layer="20"/>
<wire x1="100.7" y1="12.58" x2="85.25" y2="12.58" width="0" layer="20"/>
<wire x1="76.85" y1="12.58" x2="74" y2="12.58" width="0" layer="20"/>
<wire x1="67.6" y1="10.13" x2="67.6" y2="8.15" width="0" layer="20"/>
<wire x1="67.6" y1="3.55" x2="67.6" y2="1.75" width="0" layer="20"/>
<wire x1="67.6" y1="22.71" x2="67.6" y2="20.73" width="0" layer="20"/>
<wire x1="67.6" y1="16.13" x2="67.6" y2="14.33" width="0" layer="20"/>
<wire x1="0" y1="26.91" x2="6.4" y2="26.91" width="0" layer="20"/>
<wire x1="6.4" y1="35.29" x2="0" y2="35.29" width="0" layer="20"/>
<wire x1="0" y1="35.29" x2="0" y2="26.91" width="0" layer="20"/>
<wire x1="33.1" y1="37.04" x2="33.1" y2="33.31" width="0" layer="20"/>
<wire x1="33.1" y1="28.71" x2="33.1" y2="25.16" width="0" layer="20"/>
<wire x1="33.1" y1="37.04" x2="17.65" y2="37.04" width="0" layer="20"/>
<wire x1="9.25" y1="37.04" x2="6.4" y2="37.04" width="0" layer="20"/>
<wire x1="6.4" y1="37.04" x2="6.4" y2="35.29" width="0" layer="20"/>
<wire x1="6.4" y1="25.16" x2="6.4" y2="26.91" width="0" layer="20"/>
<wire x1="18.08" y1="33.06" x2="18.08" y2="29.16" width="0.65" layer="46"/>
<wire x1="19.1" y1="35.2" x2="27.13" y2="35.2" width="0" layer="20"/>
<wire x1="27.13" y1="35.2" x2="27.13" y2="27" width="0" layer="20"/>
<wire x1="27.13" y1="27" x2="19.1" y2="27" width="0" layer="20"/>
<wire x1="19.1" y1="27" x2="19.1" y2="27.7" width="0" layer="20"/>
<wire x1="19.1" y1="34.5" x2="19.1" y2="35.2" width="0" layer="20"/>
<wire x1="19.1" y1="34.5" x2="17.72" y2="34.5" width="0" layer="20"/>
<wire x1="17.98" y1="33.7" x2="17.98" y2="28.5" width="0" layer="20"/>
<wire x1="17.72" y1="27.7" x2="19.1" y2="27.7" width="0" layer="20"/>
<wire x1="17.72" y1="27.7" x2="17.72" y2="28.5" width="0" layer="20"/>
<wire x1="17.72" y1="28.5" x2="17.98" y2="28.5" width="0" layer="20"/>
<wire x1="17.78" y1="34.51" x2="17.72" y2="34.5" width="0" layer="20"/>
<wire x1="17.72" y1="34.5" x2="17.72" y2="33.7" width="0" layer="20"/>
<wire x1="17.72" y1="33.7" x2="17.98" y2="33.7" width="0" layer="20"/>
<hole x="9.85" y="37.39" drill="0.7"/>
<hole x="10.85" y="37.39" drill="0.7"/>
<hole x="11.85" y="37.39" drill="0.7"/>
<hole x="12.85" y="37.39" drill="0.7"/>
<hole x="13.85" y="37.39" drill="0.7"/>
<hole x="14.85" y="37.39" drill="0.7"/>
<hole x="15.85" y="37.39" drill="0.7"/>
<hole x="16.85" y="37.39" drill="0.7"/>
<wire x1="9.25" y1="37.74" x2="9.25" y2="37.04" width="0" layer="20"/>
<wire x1="17.65" y1="37.74" x2="17.65" y2="37.04" width="0" layer="20"/>
<hole x="33.45" y="29.51" drill="0.7"/>
<hole x="33.45" y="30.51" drill="0.7"/>
<hole x="33.45" y="31.51" drill="0.7"/>
<hole x="33.45" y="32.51" drill="0.7"/>
<wire x1="33.1" y1="33.31" x2="33.8" y2="33.31" width="0" layer="20"/>
<wire x1="33.1" y1="28.71" x2="33.8" y2="28.71" width="0" layer="20"/>
<wire x1="0" y1="39.49" x2="6.4" y2="39.49" width="0" layer="20"/>
<wire x1="6.4" y1="47.87" x2="0" y2="47.87" width="0" layer="20"/>
<wire x1="0" y1="47.87" x2="0" y2="39.49" width="0" layer="20"/>
<wire x1="33.1" y1="49.62" x2="33.1" y2="45.89" width="0" layer="20"/>
<wire x1="33.1" y1="41.29" x2="33.1" y2="37.74" width="0" layer="20"/>
<wire x1="33.1" y1="49.62" x2="17.65" y2="49.62" width="0" layer="20"/>
<wire x1="9.25" y1="49.62" x2="6.4" y2="49.62" width="0" layer="20"/>
<wire x1="6.4" y1="49.62" x2="6.4" y2="47.87" width="0" layer="20"/>
<wire x1="6.4" y1="37.74" x2="6.4" y2="39.49" width="0" layer="20"/>
<wire x1="18.08" y1="45.64" x2="18.08" y2="41.74" width="0.65" layer="46"/>
<wire x1="19.1" y1="47.78" x2="27.13" y2="47.78" width="0" layer="20"/>
<wire x1="27.13" y1="47.78" x2="27.13" y2="39.58" width="0" layer="20"/>
<wire x1="27.13" y1="39.58" x2="19.1" y2="39.58" width="0" layer="20"/>
<wire x1="19.1" y1="39.58" x2="19.1" y2="40.28" width="0" layer="20"/>
<wire x1="19.1" y1="47.08" x2="19.1" y2="47.78" width="0" layer="20"/>
<wire x1="19.1" y1="47.08" x2="17.72" y2="47.08" width="0" layer="20"/>
<wire x1="17.98" y1="46.28" x2="17.98" y2="41.08" width="0" layer="20"/>
<wire x1="17.72" y1="40.28" x2="19.1" y2="40.28" width="0" layer="20"/>
<wire x1="17.72" y1="40.28" x2="17.72" y2="41.08" width="0" layer="20"/>
<wire x1="17.72" y1="41.08" x2="17.98" y2="41.08" width="0" layer="20"/>
<wire x1="17.78" y1="47.09" x2="17.72" y2="47.08" width="0" layer="20"/>
<wire x1="17.72" y1="47.08" x2="17.72" y2="46.28" width="0" layer="20"/>
<wire x1="17.72" y1="46.28" x2="17.98" y2="46.28" width="0" layer="20"/>
<hole x="9.85" y="49.97" drill="0.7"/>
<hole x="10.85" y="49.97" drill="0.7"/>
<hole x="11.85" y="49.97" drill="0.7"/>
<hole x="12.85" y="49.97" drill="0.7"/>
<hole x="13.85" y="49.97" drill="0.7"/>
<hole x="14.85" y="49.97" drill="0.7"/>
<hole x="15.85" y="49.97" drill="0.7"/>
<hole x="16.85" y="49.97" drill="0.7"/>
<wire x1="9.25" y1="50.32" x2="9.25" y2="49.62" width="0" layer="20"/>
<wire x1="17.65" y1="50.32" x2="17.65" y2="49.62" width="0" layer="20"/>
<hole x="33.45" y="42.09" drill="0.7"/>
<hole x="33.45" y="43.09" drill="0.7"/>
<hole x="33.45" y="44.09" drill="0.7"/>
<hole x="33.45" y="45.09" drill="0.7"/>
<wire x1="33.1" y1="45.89" x2="33.8" y2="45.89" width="0" layer="20"/>
<wire x1="33.1" y1="41.29" x2="33.8" y2="41.29" width="0" layer="20"/>
<wire x1="33.1" y1="37.74" x2="17.65" y2="37.74" width="0" layer="20"/>
<wire x1="9.25" y1="37.74" x2="6.4" y2="37.74" width="0" layer="20"/>
<wire x1="33.8" y1="26.91" x2="40.2" y2="26.91" width="0" layer="20"/>
<wire x1="40.2" y1="35.29" x2="33.8" y2="35.29" width="0" layer="20"/>
<wire x1="66.9" y1="37.04" x2="66.9" y2="33.31" width="0" layer="20"/>
<wire x1="66.9" y1="28.71" x2="66.9" y2="25.16" width="0" layer="20"/>
<wire x1="66.9" y1="37.04" x2="51.45" y2="37.04" width="0" layer="20"/>
<wire x1="43.05" y1="37.04" x2="40.2" y2="37.04" width="0" layer="20"/>
<wire x1="40.2" y1="37.04" x2="40.2" y2="35.29" width="0" layer="20"/>
<wire x1="40.2" y1="25.16" x2="40.2" y2="26.91" width="0" layer="20"/>
<wire x1="51.88" y1="33.06" x2="51.88" y2="29.16" width="0.65" layer="46"/>
<wire x1="52.9" y1="35.2" x2="60.93" y2="35.2" width="0" layer="20"/>
<wire x1="60.93" y1="35.2" x2="60.93" y2="27" width="0" layer="20"/>
<wire x1="60.93" y1="27" x2="52.9" y2="27" width="0" layer="20"/>
<wire x1="52.9" y1="27" x2="52.9" y2="27.7" width="0" layer="20"/>
<wire x1="52.9" y1="34.5" x2="52.9" y2="35.2" width="0" layer="20"/>
<wire x1="52.9" y1="34.5" x2="51.52" y2="34.5" width="0" layer="20"/>
<wire x1="51.78" y1="33.7" x2="51.78" y2="28.5" width="0" layer="20"/>
<wire x1="51.52" y1="27.7" x2="52.9" y2="27.7" width="0" layer="20"/>
<wire x1="51.52" y1="27.7" x2="51.52" y2="28.5" width="0" layer="20"/>
<wire x1="51.52" y1="28.5" x2="51.78" y2="28.5" width="0" layer="20"/>
<wire x1="51.58" y1="34.51" x2="51.52" y2="34.5" width="0" layer="20"/>
<wire x1="51.52" y1="34.5" x2="51.52" y2="33.7" width="0" layer="20"/>
<wire x1="51.52" y1="33.7" x2="51.78" y2="33.7" width="0" layer="20"/>
<hole x="43.65" y="37.39" drill="0.7"/>
<hole x="44.65" y="37.39" drill="0.7"/>
<hole x="45.65" y="37.39" drill="0.7"/>
<hole x="46.65" y="37.39" drill="0.7"/>
<hole x="47.65" y="37.39" drill="0.7"/>
<hole x="48.65" y="37.39" drill="0.7"/>
<hole x="49.65" y="37.39" drill="0.7"/>
<hole x="50.65" y="37.39" drill="0.7"/>
<wire x1="43.05" y1="37.74" x2="43.05" y2="37.04" width="0" layer="20"/>
<wire x1="51.45" y1="37.74" x2="51.45" y2="37.04" width="0" layer="20"/>
<hole x="67.25" y="29.51" drill="0.7"/>
<hole x="67.25" y="30.51" drill="0.7"/>
<hole x="67.25" y="31.51" drill="0.7"/>
<hole x="67.25" y="32.51" drill="0.7"/>
<wire x1="66.9" y1="33.31" x2="67.6" y2="33.31" width="0" layer="20"/>
<wire x1="66.9" y1="28.71" x2="67.6" y2="28.71" width="0" layer="20"/>
<wire x1="33.8" y1="39.49" x2="40.2" y2="39.49" width="0" layer="20"/>
<wire x1="40.2" y1="47.87" x2="33.8" y2="47.87" width="0" layer="20"/>
<wire x1="66.9" y1="49.62" x2="66.9" y2="45.89" width="0" layer="20"/>
<wire x1="66.9" y1="41.29" x2="66.9" y2="37.74" width="0" layer="20"/>
<wire x1="66.9" y1="49.62" x2="51.45" y2="49.62" width="0" layer="20"/>
<wire x1="43.05" y1="49.62" x2="40.2" y2="49.62" width="0" layer="20"/>
<wire x1="40.2" y1="49.62" x2="40.2" y2="47.87" width="0" layer="20"/>
<wire x1="40.2" y1="37.74" x2="40.2" y2="39.49" width="0" layer="20"/>
<wire x1="51.88" y1="45.64" x2="51.88" y2="41.74" width="0.65" layer="46"/>
<wire x1="52.9" y1="47.78" x2="60.93" y2="47.78" width="0" layer="20"/>
<wire x1="60.93" y1="47.78" x2="60.93" y2="39.58" width="0" layer="20"/>
<wire x1="60.93" y1="39.58" x2="52.9" y2="39.58" width="0" layer="20"/>
<wire x1="52.9" y1="39.58" x2="52.9" y2="40.28" width="0" layer="20"/>
<wire x1="52.9" y1="47.08" x2="52.9" y2="47.78" width="0" layer="20"/>
<wire x1="52.9" y1="47.08" x2="51.52" y2="47.08" width="0" layer="20"/>
<wire x1="51.78" y1="46.28" x2="51.78" y2="41.08" width="0" layer="20"/>
<wire x1="51.52" y1="40.28" x2="52.9" y2="40.28" width="0" layer="20"/>
<wire x1="51.52" y1="40.28" x2="51.52" y2="41.08" width="0" layer="20"/>
<wire x1="51.52" y1="41.08" x2="51.78" y2="41.08" width="0" layer="20"/>
<wire x1="51.58" y1="47.09" x2="51.52" y2="47.08" width="0" layer="20"/>
<wire x1="51.52" y1="47.08" x2="51.52" y2="46.28" width="0" layer="20"/>
<wire x1="51.52" y1="46.28" x2="51.78" y2="46.28" width="0" layer="20"/>
<hole x="43.65" y="49.97" drill="0.7"/>
<hole x="44.65" y="49.97" drill="0.7"/>
<hole x="45.65" y="49.97" drill="0.7"/>
<hole x="46.65" y="49.97" drill="0.7"/>
<hole x="47.65" y="49.97" drill="0.7"/>
<hole x="48.65" y="49.97" drill="0.7"/>
<hole x="49.65" y="49.97" drill="0.7"/>
<hole x="50.65" y="49.97" drill="0.7"/>
<wire x1="43.05" y1="50.32" x2="43.05" y2="49.62" width="0" layer="20"/>
<wire x1="51.45" y1="50.32" x2="51.45" y2="49.62" width="0" layer="20"/>
<hole x="67.25" y="42.09" drill="0.7"/>
<hole x="67.25" y="43.09" drill="0.7"/>
<hole x="67.25" y="44.09" drill="0.7"/>
<hole x="67.25" y="45.09" drill="0.7"/>
<wire x1="66.9" y1="45.89" x2="67.6" y2="45.89" width="0" layer="20"/>
<wire x1="66.9" y1="41.29" x2="67.6" y2="41.29" width="0" layer="20"/>
<wire x1="66.9" y1="37.74" x2="51.45" y2="37.74" width="0" layer="20"/>
<wire x1="43.05" y1="37.74" x2="40.2" y2="37.74" width="0" layer="20"/>
<wire x1="33.8" y1="35.29" x2="33.8" y2="33.31" width="0" layer="20"/>
<wire x1="33.8" y1="28.71" x2="33.8" y2="26.91" width="0" layer="20"/>
<wire x1="33.8" y1="47.87" x2="33.8" y2="45.89" width="0" layer="20"/>
<wire x1="33.8" y1="41.29" x2="33.8" y2="39.49" width="0" layer="20"/>
<wire x1="67.6" y1="26.91" x2="74" y2="26.91" width="0" layer="20"/>
<wire x1="74" y1="35.29" x2="67.6" y2="35.29" width="0" layer="20"/>
<wire x1="100.7" y1="37.04" x2="100.7" y2="28.71" width="0" layer="20"/>
<wire x1="100.7" y1="28.71" x2="100.7" y2="25.16" width="0" layer="20"/>
<wire x1="100.7" y1="37.04" x2="85.25" y2="37.04" width="0" layer="20"/>
<wire x1="76.85" y1="37.04" x2="74" y2="37.04" width="0" layer="20"/>
<wire x1="74" y1="37.04" x2="74" y2="35.29" width="0" layer="20"/>
<wire x1="74" y1="25.16" x2="74" y2="26.91" width="0" layer="20"/>
<wire x1="85.68" y1="33.06" x2="85.68" y2="29.16" width="0.65" layer="46"/>
<wire x1="86.7" y1="35.2" x2="94.73" y2="35.2" width="0" layer="20"/>
<wire x1="94.73" y1="35.2" x2="94.73" y2="27" width="0" layer="20"/>
<wire x1="94.73" y1="27" x2="86.7" y2="27" width="0" layer="20"/>
<wire x1="86.7" y1="27" x2="86.7" y2="27.7" width="0" layer="20"/>
<wire x1="86.7" y1="34.5" x2="86.7" y2="35.2" width="0" layer="20"/>
<wire x1="86.7" y1="34.5" x2="85.32" y2="34.5" width="0" layer="20"/>
<wire x1="85.58" y1="33.7" x2="85.58" y2="28.5" width="0" layer="20"/>
<wire x1="85.32" y1="27.7" x2="86.7" y2="27.7" width="0" layer="20"/>
<wire x1="85.32" y1="27.7" x2="85.32" y2="28.5" width="0" layer="20"/>
<wire x1="85.32" y1="28.5" x2="85.58" y2="28.5" width="0" layer="20"/>
<wire x1="85.38" y1="34.51" x2="85.32" y2="34.5" width="0" layer="20"/>
<wire x1="85.32" y1="34.5" x2="85.32" y2="33.7" width="0" layer="20"/>
<wire x1="85.32" y1="33.7" x2="85.58" y2="33.7" width="0" layer="20"/>
<hole x="77.45" y="37.39" drill="0.7"/>
<hole x="78.45" y="37.39" drill="0.7"/>
<hole x="79.45" y="37.39" drill="0.7"/>
<hole x="80.45" y="37.39" drill="0.7"/>
<hole x="81.45" y="37.39" drill="0.7"/>
<hole x="82.45" y="37.39" drill="0.7"/>
<hole x="83.45" y="37.39" drill="0.7"/>
<hole x="84.45" y="37.39" drill="0.7"/>
<wire x1="76.85" y1="37.74" x2="76.85" y2="37.04" width="0" layer="20"/>
<wire x1="85.25" y1="37.74" x2="85.25" y2="37.04" width="0" layer="20"/>
<wire x1="67.6" y1="39.49" x2="74" y2="39.49" width="0" layer="20"/>
<wire x1="74" y1="47.87" x2="67.6" y2="47.87" width="0" layer="20"/>
<wire x1="100.7" y1="49.62" x2="100.7" y2="45.89" width="0" layer="20"/>
<wire x1="100.7" y1="45.89" x2="100.7" y2="37.74" width="0" layer="20"/>
<wire x1="100.7" y1="49.62" x2="85.25" y2="49.62" width="0" layer="20"/>
<wire x1="76.85" y1="49.62" x2="74" y2="49.62" width="0" layer="20"/>
<wire x1="74" y1="49.62" x2="74" y2="47.87" width="0" layer="20"/>
<wire x1="74" y1="37.74" x2="74" y2="39.49" width="0" layer="20"/>
<wire x1="85.68" y1="45.64" x2="85.68" y2="41.74" width="0.65" layer="46"/>
<wire x1="86.7" y1="47.78" x2="94.73" y2="47.78" width="0" layer="20"/>
<wire x1="94.73" y1="47.78" x2="94.73" y2="39.58" width="0" layer="20"/>
<wire x1="94.73" y1="39.58" x2="86.7" y2="39.58" width="0" layer="20"/>
<wire x1="86.7" y1="39.58" x2="86.7" y2="40.28" width="0" layer="20"/>
<wire x1="86.7" y1="47.08" x2="86.7" y2="47.78" width="0" layer="20"/>
<wire x1="86.7" y1="47.08" x2="85.32" y2="47.08" width="0" layer="20"/>
<wire x1="85.58" y1="46.28" x2="85.58" y2="41.08" width="0" layer="20"/>
<wire x1="85.32" y1="40.28" x2="86.7" y2="40.28" width="0" layer="20"/>
<wire x1="85.32" y1="40.28" x2="85.32" y2="41.08" width="0" layer="20"/>
<wire x1="85.32" y1="41.08" x2="85.58" y2="41.08" width="0" layer="20"/>
<wire x1="85.38" y1="47.09" x2="85.32" y2="47.08" width="0" layer="20"/>
<wire x1="85.32" y1="47.08" x2="85.32" y2="46.28" width="0" layer="20"/>
<wire x1="85.32" y1="46.28" x2="85.58" y2="46.28" width="0" layer="20"/>
<hole x="77.45" y="49.97" drill="0.7"/>
<hole x="78.45" y="49.97" drill="0.7"/>
<hole x="79.45" y="49.97" drill="0.7"/>
<hole x="80.45" y="49.97" drill="0.7"/>
<hole x="81.45" y="49.97" drill="0.7"/>
<hole x="82.45" y="49.97" drill="0.7"/>
<hole x="83.45" y="49.97" drill="0.7"/>
<hole x="84.45" y="49.97" drill="0.7"/>
<wire x1="76.85" y1="50.32" x2="76.85" y2="49.62" width="0" layer="20"/>
<wire x1="85.25" y1="50.32" x2="85.25" y2="49.62" width="0" layer="20"/>
<wire x1="100.7" y1="37.74" x2="85.25" y2="37.74" width="0" layer="20"/>
<wire x1="76.85" y1="37.74" x2="74" y2="37.74" width="0" layer="20"/>
<wire x1="67.6" y1="35.29" x2="67.6" y2="33.31" width="0" layer="20"/>
<wire x1="67.6" y1="28.71" x2="67.6" y2="26.91" width="0" layer="20"/>
<wire x1="67.6" y1="47.87" x2="67.6" y2="45.89" width="0" layer="20"/>
<wire x1="67.6" y1="41.29" x2="67.6" y2="39.49" width="0" layer="20"/>
<wire x1="33.1" y1="25.16" x2="17.65" y2="25.16" width="0" layer="20"/>
<wire x1="9.25" y1="25.16" x2="6.4" y2="25.16" width="0" layer="20"/>
<wire x1="66.9" y1="25.16" x2="51.45" y2="25.16" width="0" layer="20"/>
<wire x1="43.05" y1="25.16" x2="40.2" y2="25.16" width="0" layer="20"/>
<wire x1="100.7" y1="25.16" x2="85.25" y2="25.16" width="0" layer="20"/>
<wire x1="76.85" y1="25.16" x2="74" y2="25.16" width="0" layer="20"/>
<wire x1="0" y1="52.07" x2="6.4" y2="52.07" width="0" layer="20"/>
<wire x1="6.4" y1="60.45" x2="0" y2="60.45" width="0" layer="20"/>
<wire x1="0" y1="60.45" x2="0" y2="52.07" width="0" layer="20"/>
<wire x1="33.1" y1="62.2" x2="33.1" y2="58.47" width="0" layer="20"/>
<wire x1="33.1" y1="53.87" x2="33.1" y2="50.32" width="0" layer="20"/>
<wire x1="33.1" y1="62.2" x2="17.65" y2="62.2" width="0" layer="20"/>
<wire x1="9.25" y1="62.2" x2="6.4" y2="62.2" width="0" layer="20"/>
<wire x1="6.4" y1="62.2" x2="6.4" y2="60.45" width="0" layer="20"/>
<wire x1="6.4" y1="50.32" x2="6.4" y2="52.07" width="0" layer="20"/>
<wire x1="18.08" y1="58.22" x2="18.08" y2="54.32" width="0.65" layer="46"/>
<wire x1="19.1" y1="60.36" x2="27.13" y2="60.36" width="0" layer="20"/>
<wire x1="27.13" y1="60.36" x2="27.13" y2="52.16" width="0" layer="20"/>
<wire x1="27.13" y1="52.16" x2="19.1" y2="52.16" width="0" layer="20"/>
<wire x1="19.1" y1="52.16" x2="19.1" y2="52.86" width="0" layer="20"/>
<wire x1="19.1" y1="59.66" x2="19.1" y2="60.36" width="0" layer="20"/>
<wire x1="19.1" y1="59.66" x2="17.72" y2="59.66" width="0" layer="20"/>
<wire x1="17.98" y1="58.86" x2="17.98" y2="53.66" width="0" layer="20"/>
<wire x1="17.72" y1="52.86" x2="19.1" y2="52.86" width="0" layer="20"/>
<wire x1="17.72" y1="52.86" x2="17.72" y2="53.66" width="0" layer="20"/>
<wire x1="17.72" y1="53.66" x2="17.98" y2="53.66" width="0" layer="20"/>
<wire x1="17.78" y1="59.67" x2="17.72" y2="59.66" width="0" layer="20"/>
<wire x1="17.72" y1="59.66" x2="17.72" y2="58.86" width="0" layer="20"/>
<wire x1="17.72" y1="58.86" x2="17.98" y2="58.86" width="0" layer="20"/>
<hole x="9.85" y="62.55" drill="0.7"/>
<hole x="10.85" y="62.55" drill="0.7"/>
<hole x="11.85" y="62.55" drill="0.7"/>
<hole x="12.85" y="62.55" drill="0.7"/>
<hole x="13.85" y="62.55" drill="0.7"/>
<hole x="14.85" y="62.55" drill="0.7"/>
<hole x="15.85" y="62.55" drill="0.7"/>
<hole x="16.85" y="62.55" drill="0.7"/>
<wire x1="9.25" y1="62.9" x2="9.25" y2="62.2" width="0" layer="20"/>
<wire x1="17.65" y1="62.9" x2="17.65" y2="62.2" width="0" layer="20"/>
<hole x="33.45" y="54.67" drill="0.7"/>
<hole x="33.45" y="55.67" drill="0.7"/>
<hole x="33.45" y="56.67" drill="0.7"/>
<hole x="33.45" y="57.67" drill="0.7"/>
<wire x1="33.1" y1="58.47" x2="33.8" y2="58.47" width="0" layer="20"/>
<wire x1="33.1" y1="53.87" x2="33.8" y2="53.87" width="0" layer="20"/>
<wire x1="0" y1="64.65" x2="6.4" y2="64.65" width="0" layer="20"/>
<wire x1="6.4" y1="73.03" x2="0" y2="73.03" width="0" layer="20"/>
<wire x1="0" y1="73.03" x2="0" y2="64.65" width="0" layer="20"/>
<wire x1="33.1" y1="74.78" x2="33.1" y2="71.05" width="0" layer="20"/>
<wire x1="33.1" y1="66.45" x2="33.1" y2="62.9" width="0" layer="20"/>
<wire x1="33.1" y1="74.78" x2="17.65" y2="74.78" width="0" layer="20"/>
<wire x1="9.25" y1="74.78" x2="6.4" y2="74.78" width="0" layer="20"/>
<wire x1="6.4" y1="74.78" x2="6.4" y2="73.03" width="0" layer="20"/>
<wire x1="6.4" y1="62.9" x2="6.4" y2="64.65" width="0" layer="20"/>
<wire x1="18.08" y1="70.8" x2="18.08" y2="66.9" width="0.65" layer="46"/>
<wire x1="19.1" y1="72.94" x2="27.13" y2="72.94" width="0" layer="20"/>
<wire x1="27.13" y1="72.94" x2="27.13" y2="64.74" width="0" layer="20"/>
<wire x1="27.13" y1="64.74" x2="19.1" y2="64.74" width="0" layer="20"/>
<wire x1="19.1" y1="64.74" x2="19.1" y2="65.44" width="0" layer="20"/>
<wire x1="19.1" y1="72.24" x2="19.1" y2="72.94" width="0" layer="20"/>
<wire x1="19.1" y1="72.24" x2="17.72" y2="72.24" width="0" layer="20"/>
<wire x1="17.98" y1="71.44" x2="17.98" y2="66.24" width="0" layer="20"/>
<wire x1="17.72" y1="65.44" x2="19.1" y2="65.44" width="0" layer="20"/>
<wire x1="17.72" y1="65.44" x2="17.72" y2="66.24" width="0" layer="20"/>
<wire x1="17.72" y1="66.24" x2="17.98" y2="66.24" width="0" layer="20"/>
<wire x1="17.78" y1="72.25" x2="17.72" y2="72.24" width="0" layer="20"/>
<wire x1="17.72" y1="72.24" x2="17.72" y2="71.44" width="0" layer="20"/>
<wire x1="17.72" y1="71.44" x2="17.98" y2="71.44" width="0" layer="20"/>
<hole x="9.85" y="75.13" drill="0.7"/>
<hole x="10.85" y="75.13" drill="0.7"/>
<hole x="11.85" y="75.13" drill="0.7"/>
<hole x="12.85" y="75.13" drill="0.7"/>
<hole x="13.85" y="75.13" drill="0.7"/>
<hole x="14.85" y="75.13" drill="0.7"/>
<hole x="15.85" y="75.13" drill="0.7"/>
<hole x="16.85" y="75.13" drill="0.7"/>
<wire x1="9.25" y1="75.48" x2="9.25" y2="74.78" width="0" layer="20"/>
<wire x1="17.65" y1="75.48" x2="17.65" y2="74.78" width="0" layer="20"/>
<hole x="33.45" y="67.25" drill="0.7"/>
<hole x="33.45" y="68.25" drill="0.7"/>
<hole x="33.45" y="69.25" drill="0.7"/>
<hole x="33.45" y="70.25" drill="0.7"/>
<wire x1="33.1" y1="71.05" x2="33.8" y2="71.05" width="0" layer="20"/>
<wire x1="33.1" y1="66.45" x2="33.8" y2="66.45" width="0" layer="20"/>
<wire x1="33.1" y1="62.9" x2="17.65" y2="62.9" width="0" layer="20"/>
<wire x1="9.25" y1="62.9" x2="6.4" y2="62.9" width="0" layer="20"/>
<wire x1="33.8" y1="52.07" x2="40.2" y2="52.07" width="0" layer="20"/>
<wire x1="40.2" y1="60.45" x2="33.8" y2="60.45" width="0" layer="20"/>
<wire x1="66.9" y1="62.2" x2="66.9" y2="58.47" width="0" layer="20"/>
<wire x1="66.9" y1="53.87" x2="66.9" y2="50.32" width="0" layer="20"/>
<wire x1="66.9" y1="62.2" x2="51.45" y2="62.2" width="0" layer="20"/>
<wire x1="43.05" y1="62.2" x2="40.2" y2="62.2" width="0" layer="20"/>
<wire x1="40.2" y1="62.2" x2="40.2" y2="60.45" width="0" layer="20"/>
<wire x1="40.2" y1="50.32" x2="40.2" y2="52.07" width="0" layer="20"/>
<wire x1="51.88" y1="58.22" x2="51.88" y2="54.32" width="0.65" layer="46"/>
<wire x1="52.9" y1="60.36" x2="60.93" y2="60.36" width="0" layer="20"/>
<wire x1="60.93" y1="60.36" x2="60.93" y2="52.16" width="0" layer="20"/>
<wire x1="60.93" y1="52.16" x2="52.9" y2="52.16" width="0" layer="20"/>
<wire x1="52.9" y1="52.16" x2="52.9" y2="52.86" width="0" layer="20"/>
<wire x1="52.9" y1="59.66" x2="52.9" y2="60.36" width="0" layer="20"/>
<wire x1="52.9" y1="59.66" x2="51.52" y2="59.66" width="0" layer="20"/>
<wire x1="51.78" y1="58.86" x2="51.78" y2="53.66" width="0" layer="20"/>
<wire x1="51.52" y1="52.86" x2="52.9" y2="52.86" width="0" layer="20"/>
<wire x1="51.52" y1="52.86" x2="51.52" y2="53.66" width="0" layer="20"/>
<wire x1="51.52" y1="53.66" x2="51.78" y2="53.66" width="0" layer="20"/>
<wire x1="51.58" y1="59.67" x2="51.52" y2="59.66" width="0" layer="20"/>
<wire x1="51.52" y1="59.66" x2="51.52" y2="58.86" width="0" layer="20"/>
<wire x1="51.52" y1="58.86" x2="51.78" y2="58.86" width="0" layer="20"/>
<hole x="43.65" y="62.55" drill="0.7"/>
<hole x="44.65" y="62.55" drill="0.7"/>
<hole x="45.65" y="62.55" drill="0.7"/>
<hole x="46.65" y="62.55" drill="0.7"/>
<hole x="47.65" y="62.55" drill="0.7"/>
<hole x="48.65" y="62.55" drill="0.7"/>
<hole x="49.65" y="62.55" drill="0.7"/>
<hole x="50.65" y="62.55" drill="0.7"/>
<wire x1="43.05" y1="62.9" x2="43.05" y2="62.2" width="0" layer="20"/>
<wire x1="51.45" y1="62.9" x2="51.45" y2="62.2" width="0" layer="20"/>
<hole x="67.25" y="54.67" drill="0.7"/>
<hole x="67.25" y="55.67" drill="0.7"/>
<hole x="67.25" y="56.67" drill="0.7"/>
<hole x="67.25" y="57.67" drill="0.7"/>
<wire x1="66.9" y1="58.47" x2="67.6" y2="58.47" width="0" layer="20"/>
<wire x1="66.9" y1="53.87" x2="67.6" y2="53.87" width="0" layer="20"/>
<wire x1="33.8" y1="64.65" x2="40.2" y2="64.65" width="0" layer="20"/>
<wire x1="40.2" y1="73.03" x2="33.8" y2="73.03" width="0" layer="20"/>
<wire x1="66.9" y1="74.78" x2="66.9" y2="71.05" width="0" layer="20"/>
<wire x1="66.9" y1="66.45" x2="66.9" y2="62.9" width="0" layer="20"/>
<wire x1="66.9" y1="74.78" x2="51.45" y2="74.78" width="0" layer="20"/>
<wire x1="43.05" y1="74.78" x2="40.2" y2="74.78" width="0" layer="20"/>
<wire x1="40.2" y1="74.78" x2="40.2" y2="73.03" width="0" layer="20"/>
<wire x1="40.2" y1="62.9" x2="40.2" y2="64.65" width="0" layer="20"/>
<wire x1="51.88" y1="70.8" x2="51.88" y2="66.9" width="0.65" layer="46"/>
<wire x1="52.9" y1="72.94" x2="60.93" y2="72.94" width="0" layer="20"/>
<wire x1="60.93" y1="72.94" x2="60.93" y2="64.74" width="0" layer="20"/>
<wire x1="60.93" y1="64.74" x2="52.9" y2="64.74" width="0" layer="20"/>
<wire x1="52.9" y1="64.74" x2="52.9" y2="65.44" width="0" layer="20"/>
<wire x1="52.9" y1="72.24" x2="52.9" y2="72.94" width="0" layer="20"/>
<wire x1="52.9" y1="72.24" x2="51.52" y2="72.24" width="0" layer="20"/>
<wire x1="51.78" y1="71.44" x2="51.78" y2="66.24" width="0" layer="20"/>
<wire x1="51.52" y1="65.44" x2="52.9" y2="65.44" width="0" layer="20"/>
<wire x1="51.52" y1="65.44" x2="51.52" y2="66.24" width="0" layer="20"/>
<wire x1="51.52" y1="66.24" x2="51.78" y2="66.24" width="0" layer="20"/>
<wire x1="51.58" y1="72.25" x2="51.52" y2="72.24" width="0" layer="20"/>
<wire x1="51.52" y1="72.24" x2="51.52" y2="71.44" width="0" layer="20"/>
<wire x1="51.52" y1="71.44" x2="51.78" y2="71.44" width="0" layer="20"/>
<hole x="43.65" y="75.13" drill="0.7"/>
<hole x="44.65" y="75.13" drill="0.7"/>
<hole x="45.65" y="75.13" drill="0.7"/>
<hole x="46.65" y="75.13" drill="0.7"/>
<hole x="47.65" y="75.13" drill="0.7"/>
<hole x="48.65" y="75.13" drill="0.7"/>
<hole x="49.65" y="75.13" drill="0.7"/>
<hole x="50.65" y="75.13" drill="0.7"/>
<wire x1="43.05" y1="75.48" x2="43.05" y2="74.78" width="0" layer="20"/>
<wire x1="51.45" y1="75.48" x2="51.45" y2="74.78" width="0" layer="20"/>
<hole x="67.25" y="67.25" drill="0.7"/>
<hole x="67.25" y="68.25" drill="0.7"/>
<hole x="67.25" y="69.25" drill="0.7"/>
<hole x="67.25" y="70.25" drill="0.7"/>
<wire x1="66.9" y1="71.05" x2="67.6" y2="71.05" width="0" layer="20"/>
<wire x1="66.9" y1="66.45" x2="67.6" y2="66.45" width="0" layer="20"/>
<wire x1="66.9" y1="62.9" x2="51.45" y2="62.9" width="0" layer="20"/>
<wire x1="43.05" y1="62.9" x2="40.2" y2="62.9" width="0" layer="20"/>
<wire x1="33.8" y1="60.45" x2="33.8" y2="58.47" width="0" layer="20"/>
<wire x1="33.8" y1="53.87" x2="33.8" y2="52.07" width="0" layer="20"/>
<wire x1="33.8" y1="73.03" x2="33.8" y2="71.05" width="0" layer="20"/>
<wire x1="33.8" y1="66.45" x2="33.8" y2="64.65" width="0" layer="20"/>
<wire x1="67.6" y1="52.07" x2="74" y2="52.07" width="0" layer="20"/>
<wire x1="74" y1="60.45" x2="67.6" y2="60.45" width="0" layer="20"/>
<wire x1="100.7" y1="62.2" x2="100.7" y2="53.87" width="0" layer="20"/>
<wire x1="100.7" y1="53.87" x2="100.7" y2="50.32" width="0" layer="20"/>
<wire x1="100.7" y1="62.2" x2="85.25" y2="62.2" width="0" layer="20"/>
<wire x1="76.85" y1="62.2" x2="74" y2="62.2" width="0" layer="20"/>
<wire x1="74" y1="62.2" x2="74" y2="60.45" width="0" layer="20"/>
<wire x1="74" y1="50.32" x2="74" y2="52.07" width="0" layer="20"/>
<wire x1="85.68" y1="58.22" x2="85.68" y2="54.32" width="0.65" layer="46"/>
<wire x1="86.7" y1="60.36" x2="94.73" y2="60.36" width="0" layer="20"/>
<wire x1="94.73" y1="60.36" x2="94.73" y2="52.16" width="0" layer="20"/>
<wire x1="94.73" y1="52.16" x2="86.7" y2="52.16" width="0" layer="20"/>
<wire x1="86.7" y1="52.16" x2="86.7" y2="52.86" width="0" layer="20"/>
<wire x1="86.7" y1="59.66" x2="86.7" y2="60.36" width="0" layer="20"/>
<wire x1="86.7" y1="59.66" x2="85.32" y2="59.66" width="0" layer="20"/>
<wire x1="85.58" y1="58.86" x2="85.58" y2="53.66" width="0" layer="20"/>
<wire x1="85.32" y1="52.86" x2="86.7" y2="52.86" width="0" layer="20"/>
<wire x1="85.32" y1="52.86" x2="85.32" y2="53.66" width="0" layer="20"/>
<wire x1="85.32" y1="53.66" x2="85.58" y2="53.66" width="0" layer="20"/>
<wire x1="85.38" y1="59.67" x2="85.32" y2="59.66" width="0" layer="20"/>
<wire x1="85.32" y1="59.66" x2="85.32" y2="58.86" width="0" layer="20"/>
<wire x1="85.32" y1="58.86" x2="85.58" y2="58.86" width="0" layer="20"/>
<hole x="77.45" y="62.55" drill="0.7"/>
<hole x="78.45" y="62.55" drill="0.7"/>
<hole x="79.45" y="62.55" drill="0.7"/>
<hole x="80.45" y="62.55" drill="0.7"/>
<hole x="81.45" y="62.55" drill="0.7"/>
<hole x="82.45" y="62.55" drill="0.7"/>
<hole x="83.45" y="62.55" drill="0.7"/>
<hole x="84.45" y="62.55" drill="0.7"/>
<wire x1="76.85" y1="62.9" x2="76.85" y2="62.2" width="0" layer="20"/>
<wire x1="85.25" y1="62.9" x2="85.25" y2="62.2" width="0" layer="20"/>
<wire x1="67.6" y1="64.65" x2="74" y2="64.65" width="0" layer="20"/>
<wire x1="74" y1="73.03" x2="67.6" y2="73.03" width="0" layer="20"/>
<wire x1="100.7" y1="74.78" x2="100.7" y2="71.05" width="0" layer="20"/>
<wire x1="100.7" y1="71.05" x2="100.7" y2="62.9" width="0" layer="20"/>
<wire x1="100.7" y1="74.78" x2="85.25" y2="74.78" width="0" layer="20"/>
<wire x1="76.85" y1="74.78" x2="74" y2="74.78" width="0" layer="20"/>
<wire x1="74" y1="74.78" x2="74" y2="73.03" width="0" layer="20"/>
<wire x1="74" y1="62.9" x2="74" y2="64.65" width="0" layer="20"/>
<wire x1="85.68" y1="70.8" x2="85.68" y2="66.9" width="0.65" layer="46"/>
<wire x1="86.7" y1="72.94" x2="94.73" y2="72.94" width="0" layer="20"/>
<wire x1="94.73" y1="72.94" x2="94.73" y2="64.74" width="0" layer="20"/>
<wire x1="94.73" y1="64.74" x2="86.7" y2="64.74" width="0" layer="20"/>
<wire x1="86.7" y1="64.74" x2="86.7" y2="65.44" width="0" layer="20"/>
<wire x1="86.7" y1="72.24" x2="86.7" y2="72.94" width="0" layer="20"/>
<wire x1="86.7" y1="72.24" x2="85.32" y2="72.24" width="0" layer="20"/>
<wire x1="85.58" y1="71.44" x2="85.58" y2="66.24" width="0" layer="20"/>
<wire x1="85.32" y1="65.44" x2="86.7" y2="65.44" width="0" layer="20"/>
<wire x1="85.32" y1="65.44" x2="85.32" y2="66.24" width="0" layer="20"/>
<wire x1="85.32" y1="66.24" x2="85.58" y2="66.24" width="0" layer="20"/>
<wire x1="85.38" y1="72.25" x2="85.32" y2="72.24" width="0" layer="20"/>
<wire x1="85.32" y1="72.24" x2="85.32" y2="71.44" width="0" layer="20"/>
<wire x1="85.32" y1="71.44" x2="85.58" y2="71.44" width="0" layer="20"/>
<hole x="77.45" y="75.13" drill="0.7"/>
<hole x="78.45" y="75.13" drill="0.7"/>
<hole x="79.45" y="75.13" drill="0.7"/>
<hole x="80.45" y="75.13" drill="0.7"/>
<hole x="81.45" y="75.13" drill="0.7"/>
<hole x="82.45" y="75.13" drill="0.7"/>
<hole x="83.45" y="75.13" drill="0.7"/>
<hole x="84.45" y="75.13" drill="0.7"/>
<wire x1="76.85" y1="75.48" x2="76.85" y2="74.78" width="0" layer="20"/>
<wire x1="85.25" y1="75.48" x2="85.25" y2="74.78" width="0" layer="20"/>
<wire x1="100.7" y1="62.9" x2="85.25" y2="62.9" width="0" layer="20"/>
<wire x1="76.85" y1="62.9" x2="74" y2="62.9" width="0" layer="20"/>
<wire x1="67.6" y1="60.45" x2="67.6" y2="58.47" width="0" layer="20"/>
<wire x1="67.6" y1="53.87" x2="67.6" y2="52.07" width="0" layer="20"/>
<wire x1="67.6" y1="73.03" x2="67.6" y2="71.05" width="0" layer="20"/>
<wire x1="67.6" y1="66.45" x2="67.6" y2="64.65" width="0" layer="20"/>
<wire x1="0" y1="77.23" x2="6.4" y2="77.23" width="0" layer="20"/>
<wire x1="6.4" y1="85.61" x2="0" y2="85.61" width="0" layer="20"/>
<wire x1="0" y1="85.61" x2="0" y2="77.23" width="0" layer="20"/>
<wire x1="33.1" y1="87.36" x2="33.1" y2="83.63" width="0" layer="20"/>
<wire x1="33.1" y1="79.03" x2="33.1" y2="75.48" width="0" layer="20"/>
<wire x1="33.1" y1="87.36" x2="17.65" y2="87.36" width="0" layer="20"/>
<wire x1="9.25" y1="87.36" x2="6.4" y2="87.36" width="0" layer="20"/>
<wire x1="6.4" y1="87.36" x2="6.4" y2="85.61" width="0" layer="20"/>
<wire x1="6.4" y1="75.48" x2="6.4" y2="77.23" width="0" layer="20"/>
<wire x1="18.08" y1="83.38" x2="18.08" y2="79.48" width="0.65" layer="46"/>
<wire x1="19.1" y1="85.52" x2="27.13" y2="85.52" width="0" layer="20"/>
<wire x1="27.13" y1="85.52" x2="27.13" y2="77.32" width="0" layer="20"/>
<wire x1="27.13" y1="77.32" x2="19.1" y2="77.32" width="0" layer="20"/>
<wire x1="19.1" y1="77.32" x2="19.1" y2="78.02" width="0" layer="20"/>
<wire x1="19.1" y1="84.82" x2="19.1" y2="85.52" width="0" layer="20"/>
<wire x1="19.1" y1="84.82" x2="17.72" y2="84.82" width="0" layer="20"/>
<wire x1="17.98" y1="84.02" x2="17.98" y2="78.82" width="0" layer="20"/>
<wire x1="17.72" y1="78.02" x2="19.1" y2="78.02" width="0" layer="20"/>
<wire x1="17.72" y1="78.02" x2="17.72" y2="78.82" width="0" layer="20"/>
<wire x1="17.72" y1="78.82" x2="17.98" y2="78.82" width="0" layer="20"/>
<wire x1="17.78" y1="84.83" x2="17.72" y2="84.82" width="0" layer="20"/>
<wire x1="17.72" y1="84.82" x2="17.72" y2="84.02" width="0" layer="20"/>
<wire x1="17.72" y1="84.02" x2="17.98" y2="84.02" width="0" layer="20"/>
<hole x="9.85" y="87.71" drill="0.7"/>
<hole x="10.85" y="87.71" drill="0.7"/>
<hole x="11.85" y="87.71" drill="0.7"/>
<hole x="12.85" y="87.71" drill="0.7"/>
<hole x="13.85" y="87.71" drill="0.7"/>
<hole x="14.85" y="87.71" drill="0.7"/>
<hole x="15.85" y="87.71" drill="0.7"/>
<hole x="16.85" y="87.71" drill="0.7"/>
<wire x1="9.25" y1="88.06" x2="9.25" y2="87.36" width="0" layer="20"/>
<wire x1="17.65" y1="88.06" x2="17.65" y2="87.36" width="0" layer="20"/>
<hole x="33.45" y="79.83" drill="0.7"/>
<hole x="33.45" y="80.83" drill="0.7"/>
<hole x="33.45" y="81.83" drill="0.7"/>
<hole x="33.45" y="82.83" drill="0.7"/>
<wire x1="33.1" y1="83.63" x2="33.8" y2="83.63" width="0" layer="20"/>
<wire x1="33.1" y1="79.03" x2="33.8" y2="79.03" width="0" layer="20"/>
<wire x1="0" y1="89.81" x2="6.4" y2="89.81" width="0" layer="20"/>
<wire x1="6.4" y1="98.19" x2="0" y2="98.19" width="0" layer="20"/>
<wire x1="0" y1="98.19" x2="0" y2="89.81" width="0" layer="20"/>
<wire x1="33.1" y1="99.94" x2="33.1" y2="96.21" width="0" layer="20"/>
<wire x1="33.1" y1="91.61" x2="33.1" y2="88.06" width="0" layer="20"/>
<wire x1="33.1" y1="99.94" x2="17.65" y2="99.94" width="0" layer="20"/>
<wire x1="17.65" y1="99.94" x2="6.4" y2="99.94" width="0" layer="20"/>
<wire x1="6.4" y1="99.94" x2="6.4" y2="98.19" width="0" layer="20"/>
<wire x1="6.4" y1="88.06" x2="6.4" y2="89.81" width="0" layer="20"/>
<wire x1="18.08" y1="95.96" x2="18.08" y2="92.06" width="0.65" layer="46"/>
<wire x1="19.1" y1="98.1" x2="27.13" y2="98.1" width="0" layer="20"/>
<wire x1="27.13" y1="98.1" x2="27.13" y2="89.9" width="0" layer="20"/>
<wire x1="27.13" y1="89.9" x2="19.1" y2="89.9" width="0" layer="20"/>
<wire x1="19.1" y1="89.9" x2="19.1" y2="90.6" width="0" layer="20"/>
<wire x1="19.1" y1="97.4" x2="19.1" y2="98.1" width="0" layer="20"/>
<wire x1="19.1" y1="97.4" x2="17.72" y2="97.4" width="0" layer="20"/>
<wire x1="17.98" y1="96.6" x2="17.98" y2="91.4" width="0" layer="20"/>
<wire x1="17.72" y1="90.6" x2="19.1" y2="90.6" width="0" layer="20"/>
<wire x1="17.72" y1="90.6" x2="17.72" y2="91.4" width="0" layer="20"/>
<wire x1="17.72" y1="91.4" x2="17.98" y2="91.4" width="0" layer="20"/>
<wire x1="17.78" y1="97.41" x2="17.72" y2="97.4" width="0" layer="20"/>
<wire x1="17.72" y1="97.4" x2="17.72" y2="96.6" width="0" layer="20"/>
<wire x1="17.72" y1="96.6" x2="17.98" y2="96.6" width="0" layer="20"/>
<hole x="33.45" y="92.41" drill="0.7"/>
<hole x="33.45" y="93.41" drill="0.7"/>
<hole x="33.45" y="94.41" drill="0.7"/>
<hole x="33.45" y="95.41" drill="0.7"/>
<wire x1="33.1" y1="96.21" x2="33.8" y2="96.21" width="0" layer="20"/>
<wire x1="33.1" y1="91.61" x2="33.8" y2="91.61" width="0" layer="20"/>
<wire x1="33.1" y1="88.06" x2="17.65" y2="88.06" width="0" layer="20"/>
<wire x1="9.25" y1="88.06" x2="6.4" y2="88.06" width="0" layer="20"/>
<wire x1="33.8" y1="77.23" x2="40.2" y2="77.23" width="0" layer="20"/>
<wire x1="40.2" y1="85.61" x2="33.8" y2="85.61" width="0" layer="20"/>
<wire x1="66.9" y1="87.36" x2="66.9" y2="83.63" width="0" layer="20"/>
<wire x1="66.9" y1="79.03" x2="66.9" y2="75.48" width="0" layer="20"/>
<wire x1="66.9" y1="87.36" x2="51.45" y2="87.36" width="0" layer="20"/>
<wire x1="43.05" y1="87.36" x2="40.2" y2="87.36" width="0" layer="20"/>
<wire x1="40.2" y1="87.36" x2="40.2" y2="85.61" width="0" layer="20"/>
<wire x1="40.2" y1="75.48" x2="40.2" y2="77.23" width="0" layer="20"/>
<wire x1="51.88" y1="83.38" x2="51.88" y2="79.48" width="0.65" layer="46"/>
<wire x1="52.9" y1="85.52" x2="60.93" y2="85.52" width="0" layer="20"/>
<wire x1="60.93" y1="85.52" x2="60.93" y2="77.32" width="0" layer="20"/>
<wire x1="60.93" y1="77.32" x2="52.9" y2="77.32" width="0" layer="20"/>
<wire x1="52.9" y1="77.32" x2="52.9" y2="78.02" width="0" layer="20"/>
<wire x1="52.9" y1="84.82" x2="52.9" y2="85.52" width="0" layer="20"/>
<wire x1="52.9" y1="84.82" x2="51.52" y2="84.82" width="0" layer="20"/>
<wire x1="51.78" y1="84.02" x2="51.78" y2="78.82" width="0" layer="20"/>
<wire x1="51.52" y1="78.02" x2="52.9" y2="78.02" width="0" layer="20"/>
<wire x1="51.52" y1="78.02" x2="51.52" y2="78.82" width="0" layer="20"/>
<wire x1="51.52" y1="78.82" x2="51.78" y2="78.82" width="0" layer="20"/>
<wire x1="51.58" y1="84.83" x2="51.52" y2="84.82" width="0" layer="20"/>
<wire x1="51.52" y1="84.82" x2="51.52" y2="84.02" width="0" layer="20"/>
<wire x1="51.52" y1="84.02" x2="51.78" y2="84.02" width="0" layer="20"/>
<hole x="43.65" y="87.71" drill="0.7"/>
<hole x="44.65" y="87.71" drill="0.7"/>
<hole x="45.65" y="87.71" drill="0.7"/>
<hole x="46.65" y="87.71" drill="0.7"/>
<hole x="47.65" y="87.71" drill="0.7"/>
<hole x="48.65" y="87.71" drill="0.7"/>
<hole x="49.65" y="87.71" drill="0.7"/>
<hole x="50.65" y="87.71" drill="0.7"/>
<wire x1="43.05" y1="88.06" x2="43.05" y2="87.36" width="0" layer="20"/>
<wire x1="51.45" y1="88.06" x2="51.45" y2="87.36" width="0" layer="20"/>
<hole x="67.25" y="79.83" drill="0.7"/>
<hole x="67.25" y="80.83" drill="0.7"/>
<hole x="67.25" y="81.83" drill="0.7"/>
<hole x="67.25" y="82.83" drill="0.7"/>
<wire x1="66.9" y1="83.63" x2="67.6" y2="83.63" width="0" layer="20"/>
<wire x1="66.9" y1="79.03" x2="67.6" y2="79.03" width="0" layer="20"/>
<wire x1="33.8" y1="89.81" x2="40.2" y2="89.81" width="0" layer="20"/>
<wire x1="40.2" y1="98.19" x2="33.8" y2="98.19" width="0" layer="20"/>
<wire x1="66.9" y1="99.94" x2="66.9" y2="96.21" width="0" layer="20"/>
<wire x1="66.9" y1="91.61" x2="66.9" y2="88.06" width="0" layer="20"/>
<wire x1="66.9" y1="99.94" x2="51.45" y2="99.94" width="0" layer="20"/>
<wire x1="51.45" y1="99.94" x2="40.2" y2="99.94" width="0" layer="20"/>
<wire x1="40.2" y1="99.94" x2="40.2" y2="98.19" width="0" layer="20"/>
<wire x1="40.2" y1="88.06" x2="40.2" y2="89.81" width="0" layer="20"/>
<wire x1="51.88" y1="95.96" x2="51.88" y2="92.06" width="0.65" layer="46"/>
<wire x1="52.9" y1="98.1" x2="60.93" y2="98.1" width="0" layer="20"/>
<wire x1="60.93" y1="98.1" x2="60.93" y2="89.9" width="0" layer="20"/>
<wire x1="60.93" y1="89.9" x2="52.9" y2="89.9" width="0" layer="20"/>
<wire x1="52.9" y1="89.9" x2="52.9" y2="90.6" width="0" layer="20"/>
<wire x1="52.9" y1="97.4" x2="52.9" y2="98.1" width="0" layer="20"/>
<wire x1="52.9" y1="97.4" x2="51.52" y2="97.4" width="0" layer="20"/>
<wire x1="51.78" y1="96.6" x2="51.78" y2="91.4" width="0" layer="20"/>
<wire x1="51.52" y1="90.6" x2="52.9" y2="90.6" width="0" layer="20"/>
<wire x1="51.52" y1="90.6" x2="51.52" y2="91.4" width="0" layer="20"/>
<wire x1="51.52" y1="91.4" x2="51.78" y2="91.4" width="0" layer="20"/>
<wire x1="51.58" y1="97.41" x2="51.52" y2="97.4" width="0" layer="20"/>
<wire x1="51.52" y1="97.4" x2="51.52" y2="96.6" width="0" layer="20"/>
<wire x1="51.52" y1="96.6" x2="51.78" y2="96.6" width="0" layer="20"/>
<hole x="67.25" y="92.41" drill="0.7"/>
<hole x="67.25" y="93.41" drill="0.7"/>
<hole x="67.25" y="94.41" drill="0.7"/>
<hole x="67.25" y="95.41" drill="0.7"/>
<wire x1="66.9" y1="96.21" x2="67.6" y2="96.21" width="0" layer="20"/>
<wire x1="66.9" y1="91.61" x2="67.6" y2="91.61" width="0" layer="20"/>
<wire x1="66.9" y1="88.06" x2="51.45" y2="88.06" width="0" layer="20"/>
<wire x1="43.05" y1="88.06" x2="40.2" y2="88.06" width="0" layer="20"/>
<wire x1="33.8" y1="85.61" x2="33.8" y2="83.63" width="0" layer="20"/>
<wire x1="33.8" y1="79.03" x2="33.8" y2="77.23" width="0" layer="20"/>
<wire x1="33.8" y1="98.19" x2="33.8" y2="96.21" width="0" layer="20"/>
<wire x1="33.8" y1="91.61" x2="33.8" y2="89.81" width="0" layer="20"/>
<wire x1="67.6" y1="77.23" x2="74" y2="77.23" width="0" layer="20"/>
<wire x1="74" y1="85.61" x2="67.6" y2="85.61" width="0" layer="20"/>
<wire x1="100.7" y1="87.36" x2="100.7" y2="79.03" width="0" layer="20"/>
<wire x1="100.7" y1="79.03" x2="100.7" y2="75.48" width="0" layer="20"/>
<wire x1="100.7" y1="87.36" x2="85.25" y2="87.36" width="0" layer="20"/>
<wire x1="76.85" y1="87.36" x2="74" y2="87.36" width="0" layer="20"/>
<wire x1="74" y1="87.36" x2="74" y2="85.61" width="0" layer="20"/>
<wire x1="74" y1="75.48" x2="74" y2="77.23" width="0" layer="20"/>
<wire x1="85.68" y1="83.38" x2="85.68" y2="79.48" width="0.65" layer="46"/>
<wire x1="86.7" y1="85.52" x2="94.73" y2="85.52" width="0" layer="20"/>
<wire x1="94.73" y1="85.52" x2="94.73" y2="77.32" width="0" layer="20"/>
<wire x1="94.73" y1="77.32" x2="86.7" y2="77.32" width="0" layer="20"/>
<wire x1="86.7" y1="77.32" x2="86.7" y2="78.02" width="0" layer="20"/>
<wire x1="86.7" y1="84.82" x2="86.7" y2="85.52" width="0" layer="20"/>
<wire x1="86.7" y1="84.82" x2="85.32" y2="84.82" width="0" layer="20"/>
<wire x1="85.58" y1="84.02" x2="85.58" y2="78.82" width="0" layer="20"/>
<wire x1="85.32" y1="78.02" x2="86.7" y2="78.02" width="0" layer="20"/>
<wire x1="85.32" y1="78.02" x2="85.32" y2="78.82" width="0" layer="20"/>
<wire x1="85.32" y1="78.82" x2="85.58" y2="78.82" width="0" layer="20"/>
<wire x1="85.38" y1="84.83" x2="85.32" y2="84.82" width="0" layer="20"/>
<wire x1="85.32" y1="84.82" x2="85.32" y2="84.02" width="0" layer="20"/>
<wire x1="85.32" y1="84.02" x2="85.58" y2="84.02" width="0" layer="20"/>
<hole x="77.45" y="87.71" drill="0.7"/>
<hole x="78.45" y="87.71" drill="0.7"/>
<hole x="79.45" y="87.71" drill="0.7"/>
<hole x="80.45" y="87.71" drill="0.7"/>
<hole x="81.45" y="87.71" drill="0.7"/>
<hole x="82.45" y="87.71" drill="0.7"/>
<hole x="83.45" y="87.71" drill="0.7"/>
<hole x="84.45" y="87.71" drill="0.7"/>
<wire x1="76.85" y1="88.06" x2="76.85" y2="87.36" width="0" layer="20"/>
<wire x1="85.25" y1="88.06" x2="85.25" y2="87.36" width="0" layer="20"/>
<wire x1="67.6" y1="89.81" x2="74" y2="89.81" width="0" layer="20"/>
<wire x1="74" y1="98.19" x2="67.6" y2="98.19" width="0" layer="20"/>
<wire x1="100.7" y1="99.94" x2="100.7" y2="96.21" width="0" layer="20"/>
<wire x1="100.7" y1="96.21" x2="100.7" y2="88.06" width="0" layer="20"/>
<wire x1="100.7" y1="99.94" x2="85.25" y2="99.94" width="0" layer="20"/>
<wire x1="85.25" y1="99.94" x2="74" y2="99.94" width="0" layer="20"/>
<wire x1="74" y1="99.94" x2="74" y2="98.19" width="0" layer="20"/>
<wire x1="74" y1="88.06" x2="74" y2="89.81" width="0" layer="20"/>
<wire x1="85.68" y1="95.96" x2="85.68" y2="92.06" width="0.65" layer="46"/>
<wire x1="86.7" y1="98.1" x2="94.73" y2="98.1" width="0" layer="20"/>
<wire x1="94.73" y1="98.1" x2="94.73" y2="89.9" width="0" layer="20"/>
<wire x1="94.73" y1="89.9" x2="86.7" y2="89.9" width="0" layer="20"/>
<wire x1="86.7" y1="89.9" x2="86.7" y2="90.6" width="0" layer="20"/>
<wire x1="86.7" y1="97.4" x2="86.7" y2="98.1" width="0" layer="20"/>
<wire x1="86.7" y1="97.4" x2="85.32" y2="97.4" width="0" layer="20"/>
<wire x1="85.58" y1="96.6" x2="85.58" y2="91.4" width="0" layer="20"/>
<wire x1="85.32" y1="90.6" x2="86.7" y2="90.6" width="0" layer="20"/>
<wire x1="85.32" y1="90.6" x2="85.32" y2="91.4" width="0" layer="20"/>
<wire x1="85.32" y1="91.4" x2="85.58" y2="91.4" width="0" layer="20"/>
<wire x1="85.38" y1="97.41" x2="85.32" y2="97.4" width="0" layer="20"/>
<wire x1="85.32" y1="97.4" x2="85.32" y2="96.6" width="0" layer="20"/>
<wire x1="85.32" y1="96.6" x2="85.58" y2="96.6" width="0" layer="20"/>
<wire x1="100.7" y1="88.06" x2="85.25" y2="88.06" width="0" layer="20"/>
<wire x1="76.85" y1="88.06" x2="74" y2="88.06" width="0" layer="20"/>
<wire x1="67.6" y1="85.61" x2="67.6" y2="83.63" width="0" layer="20"/>
<wire x1="67.6" y1="79.03" x2="67.6" y2="77.23" width="0" layer="20"/>
<wire x1="67.6" y1="98.19" x2="67.6" y2="96.21" width="0" layer="20"/>
<wire x1="67.6" y1="91.61" x2="67.6" y2="89.81" width="0" layer="20"/>
<wire x1="33.1" y1="75.48" x2="17.65" y2="75.48" width="0" layer="20"/>
<wire x1="9.25" y1="75.48" x2="6.4" y2="75.48" width="0" layer="20"/>
<wire x1="66.9" y1="75.48" x2="51.45" y2="75.48" width="0" layer="20"/>
<wire x1="43.05" y1="75.48" x2="40.2" y2="75.48" width="0" layer="20"/>
<wire x1="100.7" y1="75.48" x2="85.25" y2="75.48" width="0" layer="20"/>
<wire x1="76.85" y1="75.48" x2="74" y2="75.48" width="0" layer="20"/>
<wire x1="33.1" y1="50.32" x2="17.65" y2="50.32" width="0" layer="20"/>
<wire x1="9.25" y1="50.32" x2="6.4" y2="50.32" width="0" layer="20"/>
<wire x1="66.9" y1="50.32" x2="51.45" y2="50.32" width="0" layer="20"/>
<wire x1="43.05" y1="50.32" x2="40.2" y2="50.32" width="0" layer="20"/>
<wire x1="100.7" y1="50.32" x2="85.25" y2="50.32" width="0" layer="20"/>
<wire x1="76.85" y1="50.32" x2="74" y2="50.32" width="0" layer="20"/>
</plain>
<libraries>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ATMEGA16U2-MU">
<description>&lt;8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="QFN50P500X500X100-33N">
<description>&lt;b&gt;32M1-A&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="molex105444-0001">
<packages>
<package name="DX07P024AJ1">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="BMP280pressure">
<packages>
<package name="XDCR_BMP280">
</package>
</packages>
</library>
<library name="resistor_fit">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mytransistors-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="MYTO251AA">
<description>&lt;b&gt;I-Pak&lt;/b&gt; International Rectifier</description>
</package>
</packages>
</library>
<library name="testpadcustom">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="VIA1">
</package>
<package name="SHIT">
</package>
</packages>
</library>
<library name="crystal-geyer_V1_0">
<description>&lt;BR&gt;&lt;big&gt;&lt;b&gt;GEYER ELECTRONIC --- Your producer for quartz crystals and oscillators&lt;/B&gt;&lt;/big&gt;&lt;br&gt;&lt;Hr&gt;

Version 1.0, 07.06.2016
&lt;hr&gt;
&lt;BR&gt;&lt;BR&gt; 

&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;GEYER ELECTRONIC e.K.&lt;/b&gt;&lt;br&gt;


Lochhamer Schlag 5&lt;br&gt;
D-82166 Gräfelfing/München&lt;br&gt;
&lt;br&gt;
Tel:   +49 89 546868-0&lt;br&gt;
Fax: +49 89 546868-90 für Batterien und Ladetechnik&lt;br&gt;
Fax: +49 89 546868-91 für Quarzprodukte&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.geyer-electronic.de"&gt;http://www.geyer-electronic.de&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:info@geyer-electronic.de"&gt;info@geyer-electronic.de&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor Geyer-Electronic does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Copyright: Geyer-Electronic</description>
<packages>
<package name="3.2X2.5_KX-7">
<description>4 Pad</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="RCLAMP7522T.TNT">
<packages>
<package name="RCLAMP7522TTNT">
<description>&lt;b&gt;RCLAMP7522T.TNT-3&lt;/b&gt;&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="Rohm Semiconductor - 2SCR523MT2L">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="ROHM_SEMICONDUCTOR_2SCR523MT2L_0">
<description>Bipolar (BJT) Transistor NPN 50V 100mA 350MHz 150mW Surface Mount VMT3</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="resistor" package="C0603" value="1u"/>
<element name="C3" library="resistor" package="C0603" value="100n"/>
<element name="C4" library="resistor" package="C0603" value="22p"/>
<element name="C5" library="resistor" package="C0603" value="22p"/>
<element name="IC1" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J1" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP1" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+" library="resistor_fit" package="R0603" value="22"/>
<element name="R-" library="resistor_fit" package="R0603" value="22"/>
<element name="Q1" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC1" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC2" library="resistor_fit" package="R0603" value="5k"/>
<element name="U1" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q2" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA1" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP3" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D1" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q3" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C2" library="resistor" package="C0603" value="1u"/>
<element name="C6" library="resistor" package="C0603" value="100n"/>
<element name="C7" library="resistor" package="C0603" value="22p"/>
<element name="C8" library="resistor" package="C0603" value="22p"/>
<element name="IC2" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J2" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP2" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET1" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+1" library="resistor_fit" package="R0603" value="22"/>
<element name="R-1" library="resistor_fit" package="R0603" value="22"/>
<element name="Q4" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC3" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC4" library="resistor_fit" package="R0603" value="5k"/>
<element name="U2" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q5" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP1" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP1" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA2" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP4" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE1" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR1" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D2" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q6" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C9" library="resistor" package="C0603" value="1u"/>
<element name="C10" library="resistor" package="C0603" value="100n"/>
<element name="C11" library="resistor" package="C0603" value="22p"/>
<element name="C12" library="resistor" package="C0603" value="22p"/>
<element name="IC3" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J3" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP5" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET2" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+2" library="resistor_fit" package="R0603" value="22"/>
<element name="R-2" library="resistor_fit" package="R0603" value="22"/>
<element name="Q7" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC5" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC6" library="resistor_fit" package="R0603" value="5k"/>
<element name="U3" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q8" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP2" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP2" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA3" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP6" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE2" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR2" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D3" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q9" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C13" library="resistor" package="C0603" value="1u"/>
<element name="C14" library="resistor" package="C0603" value="100n"/>
<element name="C15" library="resistor" package="C0603" value="22p"/>
<element name="C16" library="resistor" package="C0603" value="22p"/>
<element name="IC4" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J4" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP7" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET3" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+3" library="resistor_fit" package="R0603" value="22"/>
<element name="R-3" library="resistor_fit" package="R0603" value="22"/>
<element name="Q10" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC7" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC8" library="resistor_fit" package="R0603" value="5k"/>
<element name="U4" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q11" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP3" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP3" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA4" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP8" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE3" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR3" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D4" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q12" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C17" library="resistor" package="C0603" value="1u"/>
<element name="C18" library="resistor" package="C0603" value="100n"/>
<element name="C19" library="resistor" package="C0603" value="22p"/>
<element name="C20" library="resistor" package="C0603" value="22p"/>
<element name="IC5" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J5" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP9" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET4" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+4" library="resistor_fit" package="R0603" value="22"/>
<element name="R-4" library="resistor_fit" package="R0603" value="22"/>
<element name="Q13" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC9" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC10" library="resistor_fit" package="R0603" value="5k"/>
<element name="U5" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q14" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP4" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP4" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA5" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP10" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE4" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR4" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D5" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q15" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C21" library="resistor" package="C0603" value="1u"/>
<element name="C22" library="resistor" package="C0603" value="100n"/>
<element name="C23" library="resistor" package="C0603" value="22p"/>
<element name="C24" library="resistor" package="C0603" value="22p"/>
<element name="IC6" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J6" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP11" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET5" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+5" library="resistor_fit" package="R0603" value="22"/>
<element name="R-5" library="resistor_fit" package="R0603" value="22"/>
<element name="Q16" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC11" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC12" library="resistor_fit" package="R0603" value="5k"/>
<element name="U6" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q17" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP5" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP5" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA6" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP12" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE5" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR5" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D6" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q18" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C25" library="resistor" package="C0603" value="1u"/>
<element name="C26" library="resistor" package="C0603" value="100n"/>
<element name="C27" library="resistor" package="C0603" value="22p"/>
<element name="C28" library="resistor" package="C0603" value="22p"/>
<element name="IC7" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J7" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP13" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET6" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+6" library="resistor_fit" package="R0603" value="22"/>
<element name="R-6" library="resistor_fit" package="R0603" value="22"/>
<element name="Q19" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC13" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC14" library="resistor_fit" package="R0603" value="5k"/>
<element name="U7" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q20" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP6" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP6" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA7" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP14" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE6" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR6" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D7" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q21" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C29" library="resistor" package="C0603" value="1u"/>
<element name="C30" library="resistor" package="C0603" value="100n"/>
<element name="C31" library="resistor" package="C0603" value="22p"/>
<element name="C32" library="resistor" package="C0603" value="22p"/>
<element name="IC8" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J8" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP15" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET7" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+7" library="resistor_fit" package="R0603" value="22"/>
<element name="R-7" library="resistor_fit" package="R0603" value="22"/>
<element name="Q22" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC15" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC16" library="resistor_fit" package="R0603" value="5k"/>
<element name="U8" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q23" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP7" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP7" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA8" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP16" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE7" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR7" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D8" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q24" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C33" library="resistor" package="C0603" value="1u"/>
<element name="C34" library="resistor" package="C0603" value="100n"/>
<element name="C35" library="resistor" package="C0603" value="22p"/>
<element name="C36" library="resistor" package="C0603" value="22p"/>
<element name="IC9" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J9" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP17" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET8" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+8" library="resistor_fit" package="R0603" value="22"/>
<element name="R-8" library="resistor_fit" package="R0603" value="22"/>
<element name="Q25" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC17" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC18" library="resistor_fit" package="R0603" value="5k"/>
<element name="U9" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q26" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP8" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP8" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA9" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP18" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE8" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR8" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D9" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q27" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C37" library="resistor" package="C0603" value="1u"/>
<element name="C38" library="resistor" package="C0603" value="100n"/>
<element name="C39" library="resistor" package="C0603" value="22p"/>
<element name="C40" library="resistor" package="C0603" value="22p"/>
<element name="IC10" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J10" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP19" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET9" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+9" library="resistor_fit" package="R0603" value="22"/>
<element name="R-9" library="resistor_fit" package="R0603" value="22"/>
<element name="Q28" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC19" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC20" library="resistor_fit" package="R0603" value="5k"/>
<element name="U10" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q29" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP9" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP9" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA10" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP20" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE9" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR9" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D10" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q30" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C41" library="resistor" package="C0603" value="1u"/>
<element name="C42" library="resistor" package="C0603" value="100n"/>
<element name="C43" library="resistor" package="C0603" value="22p"/>
<element name="C44" library="resistor" package="C0603" value="22p"/>
<element name="IC11" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J11" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP21" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET10" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+10" library="resistor_fit" package="R0603" value="22"/>
<element name="R-10" library="resistor_fit" package="R0603" value="22"/>
<element name="Q31" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC21" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC22" library="resistor_fit" package="R0603" value="5k"/>
<element name="U11" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q32" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP10" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP10" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA11" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP22" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE10" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR10" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D11" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q33" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C45" library="resistor" package="C0603" value="1u"/>
<element name="C46" library="resistor" package="C0603" value="100n"/>
<element name="C47" library="resistor" package="C0603" value="22p"/>
<element name="C48" library="resistor" package="C0603" value="22p"/>
<element name="IC12" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J12" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP23" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET11" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+11" library="resistor_fit" package="R0603" value="22"/>
<element name="R-11" library="resistor_fit" package="R0603" value="22"/>
<element name="Q34" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC23" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC24" library="resistor_fit" package="R0603" value="5k"/>
<element name="U12" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q35" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP11" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP11" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA12" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP24" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE11" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR11" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D12" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q36" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C49" library="resistor" package="C0603" value="1u"/>
<element name="C50" library="resistor" package="C0603" value="100n"/>
<element name="C51" library="resistor" package="C0603" value="22p"/>
<element name="C52" library="resistor" package="C0603" value="22p"/>
<element name="IC13" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J13" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP25" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET12" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+12" library="resistor_fit" package="R0603" value="22"/>
<element name="R-12" library="resistor_fit" package="R0603" value="22"/>
<element name="Q37" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC25" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC26" library="resistor_fit" package="R0603" value="5k"/>
<element name="U13" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q38" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP12" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP12" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA13" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP26" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE12" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR12" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D13" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q39" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C53" library="resistor" package="C0603" value="1u"/>
<element name="C54" library="resistor" package="C0603" value="100n"/>
<element name="C55" library="resistor" package="C0603" value="22p"/>
<element name="C56" library="resistor" package="C0603" value="22p"/>
<element name="IC14" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J14" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP27" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET13" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+13" library="resistor_fit" package="R0603" value="22"/>
<element name="R-13" library="resistor_fit" package="R0603" value="22"/>
<element name="Q40" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC27" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC28" library="resistor_fit" package="R0603" value="5k"/>
<element name="U14" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q41" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP13" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP13" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA14" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP28" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE13" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR13" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D14" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q42" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C57" library="resistor" package="C0603" value="1u"/>
<element name="C58" library="resistor" package="C0603" value="100n"/>
<element name="C59" library="resistor" package="C0603" value="22p"/>
<element name="C60" library="resistor" package="C0603" value="22p"/>
<element name="IC15" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J15" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP29" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET14" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+14" library="resistor_fit" package="R0603" value="22"/>
<element name="R-14" library="resistor_fit" package="R0603" value="22"/>
<element name="Q43" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC29" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC30" library="resistor_fit" package="R0603" value="5k"/>
<element name="U15" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q44" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP14" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP14" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA15" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP30" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE14" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR14" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D15" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q45" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C61" library="resistor" package="C0603" value="1u"/>
<element name="C62" library="resistor" package="C0603" value="100n"/>
<element name="C63" library="resistor" package="C0603" value="22p"/>
<element name="C64" library="resistor" package="C0603" value="22p"/>
<element name="IC16" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J16" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP31" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET15" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+15" library="resistor_fit" package="R0603" value="22"/>
<element name="R-15" library="resistor_fit" package="R0603" value="22"/>
<element name="Q46" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC31" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC32" library="resistor_fit" package="R0603" value="5k"/>
<element name="U16" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q47" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP15" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP15" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA16" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP32" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE15" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR15" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D16" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q48" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C65" library="resistor" package="C0603" value="1u"/>
<element name="C66" library="resistor" package="C0603" value="100n"/>
<element name="C67" library="resistor" package="C0603" value="22p"/>
<element name="C68" library="resistor" package="C0603" value="22p"/>
<element name="IC17" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J17" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP33" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET16" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+16" library="resistor_fit" package="R0603" value="22"/>
<element name="R-16" library="resistor_fit" package="R0603" value="22"/>
<element name="Q49" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC33" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC34" library="resistor_fit" package="R0603" value="5k"/>
<element name="U17" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q50" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP16" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP16" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA17" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP34" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE16" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR16" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D17" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q51" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C69" library="resistor" package="C0603" value="1u"/>
<element name="C70" library="resistor" package="C0603" value="100n"/>
<element name="C71" library="resistor" package="C0603" value="22p"/>
<element name="C72" library="resistor" package="C0603" value="22p"/>
<element name="IC18" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J18" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP35" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET17" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+17" library="resistor_fit" package="R0603" value="22"/>
<element name="R-17" library="resistor_fit" package="R0603" value="22"/>
<element name="Q52" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC35" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC36" library="resistor_fit" package="R0603" value="5k"/>
<element name="U18" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q53" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP17" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP17" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA18" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP36" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE17" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR17" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D18" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q54" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C73" library="resistor" package="C0603" value="1u"/>
<element name="C74" library="resistor" package="C0603" value="100n"/>
<element name="C75" library="resistor" package="C0603" value="22p"/>
<element name="C76" library="resistor" package="C0603" value="22p"/>
<element name="IC19" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J19" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP37" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET18" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+18" library="resistor_fit" package="R0603" value="22"/>
<element name="R-18" library="resistor_fit" package="R0603" value="22"/>
<element name="Q55" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC37" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC38" library="resistor_fit" package="R0603" value="5k"/>
<element name="U19" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q56" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP18" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP18" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA19" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP38" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE18" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR18" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D19" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q57" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C77" library="resistor" package="C0603" value="1u"/>
<element name="C78" library="resistor" package="C0603" value="100n"/>
<element name="C79" library="resistor" package="C0603" value="22p"/>
<element name="C80" library="resistor" package="C0603" value="22p"/>
<element name="IC20" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J20" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP39" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET19" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+19" library="resistor_fit" package="R0603" value="22"/>
<element name="R-19" library="resistor_fit" package="R0603" value="22"/>
<element name="Q58" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC39" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC40" library="resistor_fit" package="R0603" value="5k"/>
<element name="U20" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q59" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP19" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP19" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA20" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP40" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE19" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR19" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D20" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q60" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C81" library="resistor" package="C0603" value="1u"/>
<element name="C82" library="resistor" package="C0603" value="100n"/>
<element name="C83" library="resistor" package="C0603" value="22p"/>
<element name="C84" library="resistor" package="C0603" value="22p"/>
<element name="IC21" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J21" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP41" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET20" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+20" library="resistor_fit" package="R0603" value="22"/>
<element name="R-20" library="resistor_fit" package="R0603" value="22"/>
<element name="Q61" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC41" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC42" library="resistor_fit" package="R0603" value="5k"/>
<element name="U21" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q62" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP20" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP20" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA21" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP42" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE20" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR20" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D21" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q63" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C85" library="resistor" package="C0603" value="1u"/>
<element name="C86" library="resistor" package="C0603" value="100n"/>
<element name="C87" library="resistor" package="C0603" value="22p"/>
<element name="C88" library="resistor" package="C0603" value="22p"/>
<element name="IC22" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J22" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP43" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET21" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+21" library="resistor_fit" package="R0603" value="22"/>
<element name="R-21" library="resistor_fit" package="R0603" value="22"/>
<element name="Q64" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC43" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC44" library="resistor_fit" package="R0603" value="5k"/>
<element name="U22" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q65" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP21" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP21" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA22" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP44" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE21" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR21" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D22" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q66" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C89" library="resistor" package="C0603" value="1u"/>
<element name="C90" library="resistor" package="C0603" value="100n"/>
<element name="C91" library="resistor" package="C0603" value="22p"/>
<element name="C92" library="resistor" package="C0603" value="22p"/>
<element name="IC23" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J23" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP45" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET22" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+22" library="resistor_fit" package="R0603" value="22"/>
<element name="R-22" library="resistor_fit" package="R0603" value="22"/>
<element name="Q67" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC45" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC46" library="resistor_fit" package="R0603" value="5k"/>
<element name="U23" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q68" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP22" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP22" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA23" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP46" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE22" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR22" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D23" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q69" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C93" library="resistor" package="C0603" value="1u"/>
<element name="C94" library="resistor" package="C0603" value="100n"/>
<element name="C95" library="resistor" package="C0603" value="22p"/>
<element name="C96" library="resistor" package="C0603" value="22p"/>
<element name="IC24" library="ATMEGA16U2-MU" package="QFN50P500X500X100-33N" value="16U2-TRIMMED">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU AVR USB 8K FLASH AVR USB 16K FLASH"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA16U2-MU"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATMEGA16U2-MU"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATMEGA16U2-MU"/>
<attribute name="RS_PART_NUMBER" value="1717746"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1717746"/>
</element>
<element name="J24" library="molex105444-0001" package="DX07P024AJ1" value="DX07P024AJ1"/>
<element name="JP47" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET23" library="resistor_fit" package="R0603" value="10k"/>
<element name="R+23" library="resistor_fit" package="R0603" value="22"/>
<element name="R-23" library="resistor_fit" package="R0603" value="22"/>
<element name="Q70" library="crystal-geyer_V1_0" package="3.2X2.5_KX-7" value="">
<attribute name="VALUE"/>
</element>
<element name="CC47" library="resistor_fit" package="R0603" value="5k"/>
<element name="CC48" library="resistor_fit" package="R0603" value="5k"/>
<element name="U24" library="BMP280pressure" package="XDCR_BMP280" value="BMP280">
<attribute name="DESCRIPTION" value=" BMP280 Absolute Barometric Pressure Sensor for Battery Powered Devices 2 x 2.5mm "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="828-1064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bosch-sensortec/BMP280/828-1064-1-ND/6136315?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Bosch"/>
<attribute name="MP" value="BMP280"/>
<attribute name="PACKAGE" value="SMD-8 Bosch Tools"/>
</element>
<element name="Q71" library="mytransistors-fet" package="MYTO251AA" value="SPD30P06P"/>
<element name="BASEPULLUP23" library="resistor_fit" package="R0603" value="10k"/>
<element name="GATEPULLUP23" library="resistor_fit" package="R0603" value="1k"/>
<element name="VIA24" library="testpadcustom" package="VIA1" value="VIA1">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP48" library="testpadcustom" package="SHIT" value="SHIT"/>
<element name="VSENSE23" library="resistor_fit" package="R0603" value="1k"/>
<element name="CALIBRATOR23" library="rcl" package="C0805" value="20n">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D24" library="RCLAMP7522T.TNT" package="RCLAMP7522TTNT" value="RCLAMP7522T">
<attribute name="ARROW_PART_NUMBER" value="RCLAMP7522T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rclamp7522t.tnt/semtech"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes RAILCLAMP 0.6PF 5A"/>
<attribute name="HEIGHT" value="0.43mm"/>
<attribute name="MANUFACTURER_NAME" value="SEMTECH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PART_NUMBER" value="947-RCLAMP7522T.TNT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=947-RCLAMP7522T.TNT"/>
</element>
<element name="Q72" library="Rohm Semiconductor - 2SCR523MT2L" package="ROHM_SEMICONDUCTOR_2SCR523MT2L_0" value="ROHM_SEMICONDUCTOR_2SCR523MT2LROHM_SEMICONDUCTOR_2SCR523MT2L_0_0">
<attribute name="AUTOMOTIVE" value="Yes"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLLECTOR_BASE_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_BREAKDOWN_VOLTAGE" value="50V"/>
<attribute name="COLLECTOR_EMITTER_SATURATION_VOLTAGE" value="100mV"/>
<attribute name="COLLECTOR_EMITTER_VOLTAGE" value="50V"/>
<attribute name="DATASHEET" value="https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/bipolar/2scr523mt2l-e.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Discrete Semiconductors"/>
<attribute name="DEVICE_CLASS_L2" value="Transistors"/>
<attribute name="DEVICE_CLASS_L3" value="BJTs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="TRANS NPN 50V 0.1A VMT3"/>
<attribute name="DIGIKEY_PART_NUMBER" value="2SCR523MT2LCT-ND"/>
<attribute name="EMITTER_BASE_VOLTAGE" value="5V"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="HFE_MAX" value="560"/>
<attribute name="HFE_MIN" value="120"/>
<attribute name="HFE_TESTIC" value="1mA"/>
<attribute name="HFE_TESTVCE" value="6V"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_COLLECTOR_CURRENT" value="100mA"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Rohm Semiconductor"/>
<attribute name="MFG_PACKAGE_IDENT" value="VMT3"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="2b40339e3bedae09"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Bipolar Transistors - BJT NPN General Purpose Amplification Transistor"/>
<attribute name="MOUSER_PART_NUMBER" value="755-2SCR523MT2L"/>
<attribute name="MPN" value="2SCR523MT2L"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_ELEMENTS" value="1"/>
<attribute name="NUMBER_OF_NPN" value="1"/>
<attribute name="PACKAGE" value="VMT3"/>
<attribute name="POWER_DISSIPATION" value="150mW"/>
<attribute name="PREFIX" value="Q"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="UNITY_GAIN_FREQ" value="350MHz"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
</elements>
<signals>
<signal name="SCK">
<contactref element="IC1" pad="15"/>
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="16"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="17"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="24"/>
<contactref element="RESET" pad="1"/>
</signal>
<signal name="D-">
<contactref element="IC1" pad="30"/>
<contactref element="R-" pad="1"/>
</signal>
<signal name="D+">
<contactref element="IC1" pad="29"/>
<contactref element="R+" pad="1"/>
</signal>
<signal name="R-">
<contactref element="R-" pad="2"/>
<contactref element="J1" pad="A7"/>
<contactref element="D1" pad="4"/>
</signal>
<signal name="R+">
<contactref element="R+" pad="2"/>
<contactref element="J1" pad="A6"/>
<contactref element="D1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="28"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="A1"/>
<contactref element="J1" pad="A12"/>
<contactref element="J1" pad="B1"/>
<contactref element="J1" pad="B12"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="CC1" pad="2"/>
<contactref element="CC2" pad="2"/>
<contactref element="IC1" pad="33"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="Q2" pad="3"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="9"/>
<contactref element="D1" pad="5"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="C5" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$3">
</signal>
<signal name="CC2">
<contactref element="J1" pad="B5"/>
<contactref element="CC2" pad="1"/>
</signal>
<signal name="CS">
<contactref element="IC1" pad="14"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="DRAIN">
</signal>
<signal name="COMPARE">
<contactref element="VSENSE" pad="2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="VSENSE">
<contactref element="VSENSE" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="CHARGE">
<contactref element="CALIBRATOR" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="CGROUND">
<contactref element="CALIBRATOR" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$9">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="CC1">
<contactref element="J1" pad="A5"/>
<contactref element="CC1" pad="1"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$14">
</signal>
<signal name="5V">
<contactref element="VIA1" pad="VIA1"/>
<contactref element="JP3" pad="SHIT"/>
<contactref element="J1" pad="B4"/>
<contactref element="J1" pad="A9"/>
<contactref element="J1" pad="A4"/>
<contactref element="J1" pad="B9"/>
<contactref element="IC1" pad="31"/>
<contactref element="C3" pad="2"/>
<contactref element="GATEPULLUP" pad="2"/>
</signal>
<signal name="N$16">
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="27"/>
<contactref element="RESET" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="32"/>
<contactref element="JP1" pad="5"/>
<contactref element="BASEPULLUP" pad="2"/>
</signal>
<signal name="PWM">
<contactref element="BASEPULLUP" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="GATE">
<contactref element="GATEPULLUP" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="SCK1">
<contactref element="IC2" pad="15"/>
<contactref element="JP2" pad="4"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="MOSI1">
<contactref element="JP2" pad="3"/>
<contactref element="IC2" pad="16"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="MISO1">
<contactref element="JP2" pad="6"/>
<contactref element="IC2" pad="17"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="RESET1">
<contactref element="JP2" pad="2"/>
<contactref element="IC2" pad="24"/>
<contactref element="RESET1" pad="1"/>
</signal>
<signal name="D-1">
<contactref element="IC2" pad="30"/>
<contactref element="R-1" pad="1"/>
</signal>
<signal name="D+1">
<contactref element="IC2" pad="29"/>
<contactref element="R+1" pad="1"/>
</signal>
<signal name="R-1">
<contactref element="R-1" pad="2"/>
<contactref element="J2" pad="A7"/>
<contactref element="D2" pad="4"/>
</signal>
<signal name="R+1">
<contactref element="R+1" pad="2"/>
<contactref element="J2" pad="A6"/>
<contactref element="D2" pad="3"/>
</signal>
<signal name="GND1">
<contactref element="IC2" pad="28"/>
<contactref element="C2" pad="2"/>
<contactref element="J2" pad="A1"/>
<contactref element="J2" pad="A12"/>
<contactref element="J2" pad="B1"/>
<contactref element="J2" pad="B12"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="CC3" pad="2"/>
<contactref element="CC4" pad="2"/>
<contactref element="IC2" pad="33"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="7"/>
<contactref element="Q5" pad="3"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC2" pad="9"/>
<contactref element="D2" pad="5"/>
<contactref element="Q6" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="C8" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C7" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="N$7">
</signal>
<signal name="CC3">
<contactref element="J2" pad="B5"/>
<contactref element="CC4" pad="1"/>
</signal>
<signal name="CS1">
<contactref element="IC2" pad="14"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="DRAIN1">
</signal>
<signal name="COMPARE1">
<contactref element="VSENSE1" pad="2"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="VSENSE1">
<contactref element="VSENSE1" pad="1"/>
<contactref element="Q5" pad="2"/>
</signal>
<signal name="CHARGE1">
<contactref element="CALIBRATOR1" pad="1"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="CGROUND1">
<contactref element="CALIBRATOR1" pad="2"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="CC4">
<contactref element="J2" pad="A5"/>
<contactref element="CC3" pad="1"/>
</signal>
<signal name="N$15">
</signal>
<signal name="N$17">
</signal>
<signal name="5V1">
<contactref element="VIA2" pad="VIA1"/>
<contactref element="JP4" pad="SHIT"/>
<contactref element="J2" pad="B4"/>
<contactref element="J2" pad="A9"/>
<contactref element="J2" pad="A4"/>
<contactref element="J2" pad="B9"/>
<contactref element="IC2" pad="31"/>
<contactref element="C6" pad="2"/>
<contactref element="GATEPULLUP1" pad="2"/>
</signal>
<signal name="N$18">
</signal>
<signal name="VCC1">
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="27"/>
<contactref element="RESET1" pad="2"/>
<contactref element="D2" pad="1"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="32"/>
<contactref element="JP2" pad="5"/>
<contactref element="BASEPULLUP1" pad="2"/>
</signal>
<signal name="PWM1">
<contactref element="BASEPULLUP1" pad="1"/>
<contactref element="Q6" pad="1"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="GATE1">
<contactref element="GATEPULLUP1" pad="1"/>
<contactref element="Q6" pad="3"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="SCK2">
<contactref element="IC3" pad="15"/>
<contactref element="JP5" pad="4"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="MOSI2">
<contactref element="JP5" pad="3"/>
<contactref element="IC3" pad="16"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="MISO2">
<contactref element="JP5" pad="6"/>
<contactref element="IC3" pad="17"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="RESET2">
<contactref element="JP5" pad="2"/>
<contactref element="IC3" pad="24"/>
<contactref element="RESET2" pad="1"/>
</signal>
<signal name="D-2">
<contactref element="IC3" pad="30"/>
<contactref element="R-2" pad="1"/>
</signal>
<signal name="D+2">
<contactref element="IC3" pad="29"/>
<contactref element="R+2" pad="1"/>
</signal>
<signal name="R-2">
<contactref element="R-2" pad="2"/>
<contactref element="J3" pad="A7"/>
<contactref element="D3" pad="4"/>
</signal>
<signal name="R+2">
<contactref element="R+2" pad="2"/>
<contactref element="J3" pad="A6"/>
<contactref element="D3" pad="3"/>
</signal>
<signal name="GND2">
<contactref element="IC3" pad="28"/>
<contactref element="C9" pad="2"/>
<contactref element="J3" pad="A1"/>
<contactref element="J3" pad="A12"/>
<contactref element="J3" pad="B1"/>
<contactref element="J3" pad="B12"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="CC5" pad="2"/>
<contactref element="CC6" pad="2"/>
<contactref element="IC3" pad="33"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="7"/>
<contactref element="Q8" pad="3"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC3" pad="9"/>
<contactref element="D3" pad="5"/>
<contactref element="Q9" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="C12" pad="1"/>
<contactref element="Q7" pad="3"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="C11" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="Q7" pad="1"/>
</signal>
<signal name="N$21">
</signal>
<signal name="CC5">
<contactref element="J3" pad="B5"/>
<contactref element="CC6" pad="1"/>
</signal>
<signal name="CS2">
<contactref element="IC3" pad="14"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="DRAIN2">
</signal>
<signal name="COMPARE2">
<contactref element="VSENSE2" pad="2"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="VSENSE2">
<contactref element="VSENSE2" pad="1"/>
<contactref element="Q8" pad="2"/>
</signal>
<signal name="CHARGE2">
<contactref element="CALIBRATOR2" pad="1"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="CGROUND2">
<contactref element="CALIBRATOR2" pad="2"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="CC6">
<contactref element="J3" pad="A5"/>
<contactref element="CC5" pad="1"/>
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="5V2">
<contactref element="VIA3" pad="VIA1"/>
<contactref element="JP6" pad="SHIT"/>
<contactref element="J3" pad="B4"/>
<contactref element="J3" pad="A9"/>
<contactref element="J3" pad="A4"/>
<contactref element="J3" pad="B9"/>
<contactref element="IC3" pad="31"/>
<contactref element="C10" pad="2"/>
<contactref element="GATEPULLUP2" pad="2"/>
</signal>
<signal name="N$27">
</signal>
<signal name="VCC2">
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="6"/>
<contactref element="C9" pad="1"/>
<contactref element="IC3" pad="27"/>
<contactref element="RESET2" pad="2"/>
<contactref element="D3" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="32"/>
<contactref element="JP5" pad="5"/>
<contactref element="BASEPULLUP2" pad="2"/>
</signal>
<signal name="PWM2">
<contactref element="BASEPULLUP2" pad="1"/>
<contactref element="Q9" pad="1"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="GATE2">
<contactref element="GATEPULLUP2" pad="1"/>
<contactref element="Q9" pad="3"/>
<contactref element="Q8" pad="1"/>
</signal>
<signal name="SCK3">
<contactref element="IC4" pad="15"/>
<contactref element="JP7" pad="4"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="MOSI3">
<contactref element="JP7" pad="3"/>
<contactref element="IC4" pad="16"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="MISO3">
<contactref element="JP7" pad="6"/>
<contactref element="IC4" pad="17"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="RESET3">
<contactref element="JP7" pad="2"/>
<contactref element="IC4" pad="24"/>
<contactref element="RESET3" pad="1"/>
</signal>
<signal name="D-3">
<contactref element="IC4" pad="30"/>
<contactref element="R-3" pad="1"/>
</signal>
<signal name="D+3">
<contactref element="IC4" pad="29"/>
<contactref element="R+3" pad="1"/>
</signal>
<signal name="R-3">
<contactref element="R-3" pad="2"/>
<contactref element="J4" pad="A7"/>
<contactref element="D4" pad="4"/>
</signal>
<signal name="R+3">
<contactref element="R+3" pad="2"/>
<contactref element="J4" pad="A6"/>
<contactref element="D4" pad="3"/>
</signal>
<signal name="GND3">
<contactref element="IC4" pad="28"/>
<contactref element="C13" pad="2"/>
<contactref element="J4" pad="A1"/>
<contactref element="J4" pad="A12"/>
<contactref element="J4" pad="B1"/>
<contactref element="J4" pad="B12"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="C14" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="CC7" pad="2"/>
<contactref element="CC8" pad="2"/>
<contactref element="IC4" pad="33"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="7"/>
<contactref element="Q11" pad="3"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC4" pad="9"/>
<contactref element="D4" pad="5"/>
<contactref element="Q12" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="C16" pad="1"/>
<contactref element="Q10" pad="3"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="C15" pad="2"/>
<contactref element="IC4" pad="1"/>
<contactref element="Q10" pad="1"/>
</signal>
<signal name="N$30">
</signal>
<signal name="CC7">
<contactref element="J4" pad="B5"/>
<contactref element="CC8" pad="1"/>
</signal>
<signal name="CS3">
<contactref element="IC4" pad="14"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="DRAIN3">
</signal>
<signal name="COMPARE3">
<contactref element="VSENSE3" pad="2"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="VSENSE3">
<contactref element="VSENSE3" pad="1"/>
<contactref element="Q11" pad="2"/>
</signal>
<signal name="CHARGE3">
<contactref element="CALIBRATOR3" pad="1"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="CGROUND3">
<contactref element="CALIBRATOR3" pad="2"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
</signal>
<signal name="CC8">
<contactref element="J4" pad="A5"/>
<contactref element="CC7" pad="1"/>
</signal>
<signal name="N$34">
</signal>
<signal name="N$35">
</signal>
<signal name="5V3">
<contactref element="VIA4" pad="VIA1"/>
<contactref element="JP8" pad="SHIT"/>
<contactref element="J4" pad="B4"/>
<contactref element="J4" pad="A9"/>
<contactref element="J4" pad="A4"/>
<contactref element="J4" pad="B9"/>
<contactref element="IC4" pad="31"/>
<contactref element="C14" pad="2"/>
<contactref element="GATEPULLUP3" pad="2"/>
</signal>
<signal name="N$36">
</signal>
<signal name="VCC3">
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="6"/>
<contactref element="C13" pad="1"/>
<contactref element="IC4" pad="27"/>
<contactref element="RESET3" pad="2"/>
<contactref element="D4" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC4" pad="32"/>
<contactref element="JP7" pad="5"/>
<contactref element="BASEPULLUP3" pad="2"/>
</signal>
<signal name="PWM3">
<contactref element="BASEPULLUP3" pad="1"/>
<contactref element="Q12" pad="1"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="GATE3">
<contactref element="GATEPULLUP3" pad="1"/>
<contactref element="Q12" pad="3"/>
<contactref element="Q11" pad="1"/>
</signal>
<signal name="SCK4">
<contactref element="IC5" pad="15"/>
<contactref element="JP9" pad="4"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="MOSI4">
<contactref element="JP9" pad="3"/>
<contactref element="IC5" pad="16"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="MISO4">
<contactref element="JP9" pad="6"/>
<contactref element="IC5" pad="17"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="RESET4">
<contactref element="JP9" pad="2"/>
<contactref element="IC5" pad="24"/>
<contactref element="RESET4" pad="1"/>
</signal>
<signal name="D-4">
<contactref element="IC5" pad="30"/>
<contactref element="R-4" pad="1"/>
</signal>
<signal name="D+4">
<contactref element="IC5" pad="29"/>
<contactref element="R+4" pad="1"/>
</signal>
<signal name="R-4">
<contactref element="R-4" pad="2"/>
<contactref element="J5" pad="A7"/>
<contactref element="D5" pad="4"/>
</signal>
<signal name="R+4">
<contactref element="R+4" pad="2"/>
<contactref element="J5" pad="A6"/>
<contactref element="D5" pad="3"/>
</signal>
<signal name="GND4">
<contactref element="IC5" pad="28"/>
<contactref element="C17" pad="2"/>
<contactref element="J5" pad="A1"/>
<contactref element="J5" pad="A12"/>
<contactref element="J5" pad="B1"/>
<contactref element="J5" pad="B12"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="C18" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="CC9" pad="2"/>
<contactref element="CC10" pad="2"/>
<contactref element="IC5" pad="33"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="7"/>
<contactref element="Q14" pad="3"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC5" pad="9"/>
<contactref element="D5" pad="5"/>
<contactref element="Q15" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="C20" pad="1"/>
<contactref element="Q13" pad="3"/>
<contactref element="IC5" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="C19" pad="2"/>
<contactref element="IC5" pad="1"/>
<contactref element="Q13" pad="1"/>
</signal>
<signal name="N$39">
</signal>
<signal name="CC9">
<contactref element="J5" pad="B5"/>
<contactref element="CC10" pad="1"/>
</signal>
<signal name="CS4">
<contactref element="IC5" pad="14"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="DRAIN4">
</signal>
<signal name="COMPARE4">
<contactref element="VSENSE4" pad="2"/>
<contactref element="IC5" pad="7"/>
</signal>
<signal name="VSENSE4">
<contactref element="VSENSE4" pad="1"/>
<contactref element="Q14" pad="2"/>
</signal>
<signal name="CHARGE4">
<contactref element="CALIBRATOR4" pad="1"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC5" pad="8"/>
</signal>
<signal name="CGROUND4">
<contactref element="CALIBRATOR4" pad="2"/>
<contactref element="IC5" pad="5"/>
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="N$42">
</signal>
<signal name="CC10">
<contactref element="J5" pad="A5"/>
<contactref element="CC9" pad="1"/>
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="5V4">
<contactref element="VIA5" pad="VIA1"/>
<contactref element="JP10" pad="SHIT"/>
<contactref element="J5" pad="B4"/>
<contactref element="J5" pad="A9"/>
<contactref element="J5" pad="A4"/>
<contactref element="J5" pad="B9"/>
<contactref element="IC5" pad="31"/>
<contactref element="C18" pad="2"/>
<contactref element="GATEPULLUP4" pad="2"/>
</signal>
<signal name="N$45">
</signal>
<signal name="VCC4">
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="6"/>
<contactref element="C17" pad="1"/>
<contactref element="IC5" pad="27"/>
<contactref element="RESET4" pad="2"/>
<contactref element="D5" pad="1"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC5" pad="32"/>
<contactref element="JP9" pad="5"/>
<contactref element="BASEPULLUP4" pad="2"/>
</signal>
<signal name="PWM4">
<contactref element="BASEPULLUP4" pad="1"/>
<contactref element="Q15" pad="1"/>
<contactref element="IC5" pad="13"/>
</signal>
<signal name="GATE4">
<contactref element="GATEPULLUP4" pad="1"/>
<contactref element="Q15" pad="3"/>
<contactref element="Q14" pad="1"/>
</signal>
<signal name="SCK5">
<contactref element="IC6" pad="15"/>
<contactref element="JP11" pad="4"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="MOSI5">
<contactref element="JP11" pad="3"/>
<contactref element="IC6" pad="16"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="MISO5">
<contactref element="JP11" pad="6"/>
<contactref element="IC6" pad="17"/>
<contactref element="U6" pad="5"/>
</signal>
<signal name="RESET5">
<contactref element="JP11" pad="2"/>
<contactref element="IC6" pad="24"/>
<contactref element="RESET5" pad="1"/>
</signal>
<signal name="D-5">
<contactref element="IC6" pad="30"/>
<contactref element="R-5" pad="1"/>
</signal>
<signal name="D+5">
<contactref element="IC6" pad="29"/>
<contactref element="R+5" pad="1"/>
</signal>
<signal name="R-5">
<contactref element="R-5" pad="2"/>
<contactref element="J6" pad="A7"/>
<contactref element="D6" pad="4"/>
</signal>
<signal name="R+5">
<contactref element="R+5" pad="2"/>
<contactref element="J6" pad="A6"/>
<contactref element="D6" pad="3"/>
</signal>
<signal name="GND5">
<contactref element="IC6" pad="28"/>
<contactref element="C21" pad="2"/>
<contactref element="J6" pad="A1"/>
<contactref element="J6" pad="A12"/>
<contactref element="J6" pad="B1"/>
<contactref element="J6" pad="B12"/>
<contactref element="C23" pad="1"/>
<contactref element="C24" pad="2"/>
<contactref element="IC6" pad="3"/>
<contactref element="C22" pad="1"/>
<contactref element="JP11" pad="1"/>
<contactref element="CC11" pad="2"/>
<contactref element="CC12" pad="2"/>
<contactref element="IC6" pad="33"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="7"/>
<contactref element="Q17" pad="3"/>
<contactref element="IC6" pad="10"/>
<contactref element="IC6" pad="9"/>
<contactref element="D6" pad="5"/>
<contactref element="Q18" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="C24" pad="1"/>
<contactref element="Q16" pad="3"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="C23" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="Q16" pad="1"/>
</signal>
<signal name="N$48">
</signal>
<signal name="CC11">
<contactref element="J6" pad="B5"/>
<contactref element="CC12" pad="1"/>
</signal>
<signal name="CS5">
<contactref element="IC6" pad="14"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="DRAIN5">
</signal>
<signal name="COMPARE5">
<contactref element="VSENSE5" pad="2"/>
<contactref element="IC6" pad="7"/>
</signal>
<signal name="VSENSE5">
<contactref element="VSENSE5" pad="1"/>
<contactref element="Q17" pad="2"/>
</signal>
<signal name="CHARGE5">
<contactref element="CALIBRATOR5" pad="1"/>
<contactref element="IC6" pad="6"/>
<contactref element="IC6" pad="8"/>
</signal>
<signal name="CGROUND5">
<contactref element="CALIBRATOR5" pad="2"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="N$49">
</signal>
<signal name="N$50">
</signal>
<signal name="N$51">
</signal>
<signal name="CC12">
<contactref element="J6" pad="A5"/>
<contactref element="CC11" pad="1"/>
</signal>
<signal name="N$52">
</signal>
<signal name="N$53">
</signal>
<signal name="5V5">
<contactref element="VIA6" pad="VIA1"/>
<contactref element="JP12" pad="SHIT"/>
<contactref element="J6" pad="B4"/>
<contactref element="J6" pad="A9"/>
<contactref element="J6" pad="A4"/>
<contactref element="J6" pad="B9"/>
<contactref element="IC6" pad="31"/>
<contactref element="C22" pad="2"/>
<contactref element="GATEPULLUP5" pad="2"/>
</signal>
<signal name="N$54">
</signal>
<signal name="VCC5">
<contactref element="U6" pad="8"/>
<contactref element="U6" pad="6"/>
<contactref element="C21" pad="1"/>
<contactref element="IC6" pad="27"/>
<contactref element="RESET5" pad="2"/>
<contactref element="D6" pad="1"/>
<contactref element="IC6" pad="4"/>
<contactref element="IC6" pad="32"/>
<contactref element="JP11" pad="5"/>
<contactref element="BASEPULLUP5" pad="2"/>
</signal>
<signal name="PWM5">
<contactref element="BASEPULLUP5" pad="1"/>
<contactref element="Q18" pad="1"/>
<contactref element="IC6" pad="13"/>
</signal>
<signal name="GATE5">
<contactref element="GATEPULLUP5" pad="1"/>
<contactref element="Q18" pad="3"/>
<contactref element="Q17" pad="1"/>
</signal>
<signal name="SCK6">
<contactref element="IC7" pad="15"/>
<contactref element="JP13" pad="4"/>
<contactref element="U7" pad="4"/>
</signal>
<signal name="MOSI6">
<contactref element="JP13" pad="3"/>
<contactref element="IC7" pad="16"/>
<contactref element="U7" pad="3"/>
</signal>
<signal name="MISO6">
<contactref element="JP13" pad="6"/>
<contactref element="IC7" pad="17"/>
<contactref element="U7" pad="5"/>
</signal>
<signal name="RESET6">
<contactref element="JP13" pad="2"/>
<contactref element="IC7" pad="24"/>
<contactref element="RESET6" pad="1"/>
</signal>
<signal name="D-6">
<contactref element="IC7" pad="30"/>
<contactref element="R-6" pad="1"/>
</signal>
<signal name="D+6">
<contactref element="IC7" pad="29"/>
<contactref element="R+6" pad="1"/>
</signal>
<signal name="R-6">
<contactref element="R-6" pad="2"/>
<contactref element="J7" pad="A7"/>
<contactref element="D7" pad="4"/>
</signal>
<signal name="R+6">
<contactref element="R+6" pad="2"/>
<contactref element="J7" pad="A6"/>
<contactref element="D7" pad="3"/>
</signal>
<signal name="GND6">
<contactref element="IC7" pad="28"/>
<contactref element="C25" pad="2"/>
<contactref element="J7" pad="A1"/>
<contactref element="J7" pad="A12"/>
<contactref element="J7" pad="B1"/>
<contactref element="J7" pad="B12"/>
<contactref element="C27" pad="1"/>
<contactref element="C28" pad="2"/>
<contactref element="IC7" pad="3"/>
<contactref element="C26" pad="1"/>
<contactref element="JP13" pad="1"/>
<contactref element="CC13" pad="2"/>
<contactref element="CC14" pad="2"/>
<contactref element="IC7" pad="33"/>
<contactref element="U7" pad="1"/>
<contactref element="U7" pad="7"/>
<contactref element="Q20" pad="3"/>
<contactref element="IC7" pad="10"/>
<contactref element="IC7" pad="9"/>
<contactref element="D7" pad="5"/>
<contactref element="Q21" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="C28" pad="1"/>
<contactref element="Q19" pad="3"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="C27" pad="2"/>
<contactref element="IC7" pad="1"/>
<contactref element="Q19" pad="1"/>
</signal>
<signal name="N$57">
</signal>
<signal name="CC13">
<contactref element="J7" pad="B5"/>
<contactref element="CC14" pad="1"/>
</signal>
<signal name="CS6">
<contactref element="IC7" pad="14"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="DRAIN6">
</signal>
<signal name="COMPARE6">
<contactref element="VSENSE6" pad="2"/>
<contactref element="IC7" pad="7"/>
</signal>
<signal name="VSENSE6">
<contactref element="VSENSE6" pad="1"/>
<contactref element="Q20" pad="2"/>
</signal>
<signal name="CHARGE6">
<contactref element="CALIBRATOR6" pad="1"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="8"/>
</signal>
<signal name="CGROUND6">
<contactref element="CALIBRATOR6" pad="2"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="N$58">
</signal>
<signal name="N$59">
</signal>
<signal name="N$60">
</signal>
<signal name="CC14">
<contactref element="J7" pad="A5"/>
<contactref element="CC13" pad="1"/>
</signal>
<signal name="N$61">
</signal>
<signal name="N$62">
</signal>
<signal name="5V6">
<contactref element="VIA7" pad="VIA1"/>
<contactref element="JP14" pad="SHIT"/>
<contactref element="J7" pad="B4"/>
<contactref element="J7" pad="A9"/>
<contactref element="J7" pad="A4"/>
<contactref element="J7" pad="B9"/>
<contactref element="IC7" pad="31"/>
<contactref element="C26" pad="2"/>
<contactref element="GATEPULLUP6" pad="2"/>
</signal>
<signal name="N$63">
</signal>
<signal name="VCC6">
<contactref element="U7" pad="8"/>
<contactref element="U7" pad="6"/>
<contactref element="C25" pad="1"/>
<contactref element="IC7" pad="27"/>
<contactref element="RESET6" pad="2"/>
<contactref element="D7" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC7" pad="32"/>
<contactref element="JP13" pad="5"/>
<contactref element="BASEPULLUP6" pad="2"/>
</signal>
<signal name="PWM6">
<contactref element="BASEPULLUP6" pad="1"/>
<contactref element="Q21" pad="1"/>
<contactref element="IC7" pad="13"/>
</signal>
<signal name="GATE6">
<contactref element="GATEPULLUP6" pad="1"/>
<contactref element="Q21" pad="3"/>
<contactref element="Q20" pad="1"/>
</signal>
<signal name="SCK7">
<contactref element="IC8" pad="15"/>
<contactref element="JP15" pad="4"/>
<contactref element="U8" pad="4"/>
</signal>
<signal name="MOSI7">
<contactref element="JP15" pad="3"/>
<contactref element="IC8" pad="16"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="MISO7">
<contactref element="JP15" pad="6"/>
<contactref element="IC8" pad="17"/>
<contactref element="U8" pad="5"/>
</signal>
<signal name="RESET7">
<contactref element="JP15" pad="2"/>
<contactref element="IC8" pad="24"/>
<contactref element="RESET7" pad="1"/>
</signal>
<signal name="D-7">
<contactref element="IC8" pad="30"/>
<contactref element="R-7" pad="1"/>
</signal>
<signal name="D+7">
<contactref element="IC8" pad="29"/>
<contactref element="R+7" pad="1"/>
</signal>
<signal name="R-7">
<contactref element="R-7" pad="2"/>
<contactref element="J8" pad="A7"/>
<contactref element="D8" pad="4"/>
</signal>
<signal name="R+7">
<contactref element="R+7" pad="2"/>
<contactref element="J8" pad="A6"/>
<contactref element="D8" pad="3"/>
</signal>
<signal name="GND7">
<contactref element="IC8" pad="28"/>
<contactref element="C29" pad="2"/>
<contactref element="J8" pad="A1"/>
<contactref element="J8" pad="A12"/>
<contactref element="J8" pad="B1"/>
<contactref element="J8" pad="B12"/>
<contactref element="C31" pad="1"/>
<contactref element="C32" pad="2"/>
<contactref element="IC8" pad="3"/>
<contactref element="C30" pad="1"/>
<contactref element="JP15" pad="1"/>
<contactref element="CC15" pad="2"/>
<contactref element="CC16" pad="2"/>
<contactref element="IC8" pad="33"/>
<contactref element="U8" pad="1"/>
<contactref element="U8" pad="7"/>
<contactref element="Q23" pad="3"/>
<contactref element="IC8" pad="10"/>
<contactref element="IC8" pad="9"/>
<contactref element="D8" pad="5"/>
<contactref element="Q24" pad="2"/>
</signal>
<signal name="N$64">
<contactref element="C32" pad="1"/>
<contactref element="Q22" pad="3"/>
<contactref element="IC8" pad="2"/>
</signal>
<signal name="N$65">
<contactref element="C31" pad="2"/>
<contactref element="IC8" pad="1"/>
<contactref element="Q22" pad="1"/>
</signal>
<signal name="N$66">
</signal>
<signal name="CC15">
<contactref element="J8" pad="B5"/>
<contactref element="CC16" pad="1"/>
</signal>
<signal name="CS7">
<contactref element="IC8" pad="14"/>
<contactref element="U8" pad="2"/>
</signal>
<signal name="DRAIN7">
</signal>
<signal name="COMPARE7">
<contactref element="VSENSE7" pad="2"/>
<contactref element="IC8" pad="7"/>
</signal>
<signal name="VSENSE7">
<contactref element="VSENSE7" pad="1"/>
<contactref element="Q23" pad="2"/>
</signal>
<signal name="CHARGE7">
<contactref element="CALIBRATOR7" pad="1"/>
<contactref element="IC8" pad="6"/>
<contactref element="IC8" pad="8"/>
</signal>
<signal name="CGROUND7">
<contactref element="CALIBRATOR7" pad="2"/>
<contactref element="IC8" pad="5"/>
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="CC16">
<contactref element="J8" pad="A5"/>
<contactref element="CC15" pad="1"/>
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="5V7">
<contactref element="VIA8" pad="VIA1"/>
<contactref element="JP16" pad="SHIT"/>
<contactref element="J8" pad="B4"/>
<contactref element="J8" pad="A9"/>
<contactref element="J8" pad="A4"/>
<contactref element="J8" pad="B9"/>
<contactref element="IC8" pad="31"/>
<contactref element="C30" pad="2"/>
<contactref element="GATEPULLUP7" pad="2"/>
</signal>
<signal name="N$72">
</signal>
<signal name="VCC7">
<contactref element="U8" pad="8"/>
<contactref element="U8" pad="6"/>
<contactref element="C29" pad="1"/>
<contactref element="IC8" pad="27"/>
<contactref element="RESET7" pad="2"/>
<contactref element="D8" pad="1"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC8" pad="32"/>
<contactref element="JP15" pad="5"/>
<contactref element="BASEPULLUP7" pad="2"/>
</signal>
<signal name="PWM7">
<contactref element="BASEPULLUP7" pad="1"/>
<contactref element="Q24" pad="1"/>
<contactref element="IC8" pad="13"/>
</signal>
<signal name="GATE7">
<contactref element="GATEPULLUP7" pad="1"/>
<contactref element="Q24" pad="3"/>
<contactref element="Q23" pad="1"/>
</signal>
<signal name="SCK8">
<contactref element="IC9" pad="15"/>
<contactref element="JP17" pad="4"/>
<contactref element="U9" pad="4"/>
</signal>
<signal name="MOSI8">
<contactref element="JP17" pad="3"/>
<contactref element="IC9" pad="16"/>
<contactref element="U9" pad="3"/>
</signal>
<signal name="MISO8">
<contactref element="JP17" pad="6"/>
<contactref element="IC9" pad="17"/>
<contactref element="U9" pad="5"/>
</signal>
<signal name="RESET8">
<contactref element="JP17" pad="2"/>
<contactref element="IC9" pad="24"/>
<contactref element="RESET8" pad="1"/>
</signal>
<signal name="D-8">
<contactref element="IC9" pad="30"/>
<contactref element="R-8" pad="1"/>
</signal>
<signal name="D+8">
<contactref element="IC9" pad="29"/>
<contactref element="R+8" pad="1"/>
</signal>
<signal name="R-8">
<contactref element="R-8" pad="2"/>
<contactref element="J9" pad="A7"/>
<contactref element="D9" pad="4"/>
</signal>
<signal name="R+8">
<contactref element="R+8" pad="2"/>
<contactref element="J9" pad="A6"/>
<contactref element="D9" pad="3"/>
</signal>
<signal name="GND8">
<contactref element="IC9" pad="28"/>
<contactref element="C33" pad="2"/>
<contactref element="J9" pad="A1"/>
<contactref element="J9" pad="A12"/>
<contactref element="J9" pad="B1"/>
<contactref element="J9" pad="B12"/>
<contactref element="C35" pad="1"/>
<contactref element="C36" pad="2"/>
<contactref element="IC9" pad="3"/>
<contactref element="C34" pad="1"/>
<contactref element="JP17" pad="1"/>
<contactref element="CC17" pad="2"/>
<contactref element="CC18" pad="2"/>
<contactref element="IC9" pad="33"/>
<contactref element="U9" pad="1"/>
<contactref element="U9" pad="7"/>
<contactref element="Q26" pad="3"/>
<contactref element="IC9" pad="10"/>
<contactref element="IC9" pad="9"/>
<contactref element="D9" pad="5"/>
<contactref element="Q27" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="C36" pad="1"/>
<contactref element="Q25" pad="3"/>
<contactref element="IC9" pad="2"/>
</signal>
<signal name="N$74">
<contactref element="C35" pad="2"/>
<contactref element="IC9" pad="1"/>
<contactref element="Q25" pad="1"/>
</signal>
<signal name="N$75">
</signal>
<signal name="CC17">
<contactref element="J9" pad="B5"/>
<contactref element="CC18" pad="1"/>
</signal>
<signal name="CS8">
<contactref element="IC9" pad="14"/>
<contactref element="U9" pad="2"/>
</signal>
<signal name="DRAIN8">
</signal>
<signal name="COMPARE8">
<contactref element="VSENSE8" pad="2"/>
<contactref element="IC9" pad="7"/>
</signal>
<signal name="VSENSE8">
<contactref element="VSENSE8" pad="1"/>
<contactref element="Q26" pad="2"/>
</signal>
<signal name="CHARGE8">
<contactref element="CALIBRATOR8" pad="1"/>
<contactref element="IC9" pad="6"/>
<contactref element="IC9" pad="8"/>
</signal>
<signal name="CGROUND8">
<contactref element="CALIBRATOR8" pad="2"/>
<contactref element="IC9" pad="5"/>
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$78">
</signal>
<signal name="CC18">
<contactref element="J9" pad="A5"/>
<contactref element="CC17" pad="1"/>
</signal>
<signal name="N$79">
</signal>
<signal name="N$80">
</signal>
<signal name="5V8">
<contactref element="VIA9" pad="VIA1"/>
<contactref element="JP18" pad="SHIT"/>
<contactref element="J9" pad="B4"/>
<contactref element="J9" pad="A9"/>
<contactref element="J9" pad="A4"/>
<contactref element="J9" pad="B9"/>
<contactref element="IC9" pad="31"/>
<contactref element="C34" pad="2"/>
<contactref element="GATEPULLUP8" pad="2"/>
</signal>
<signal name="N$81">
</signal>
<signal name="VCC8">
<contactref element="U9" pad="8"/>
<contactref element="U9" pad="6"/>
<contactref element="C33" pad="1"/>
<contactref element="IC9" pad="27"/>
<contactref element="RESET8" pad="2"/>
<contactref element="D9" pad="1"/>
<contactref element="IC9" pad="4"/>
<contactref element="IC9" pad="32"/>
<contactref element="JP17" pad="5"/>
<contactref element="BASEPULLUP8" pad="2"/>
</signal>
<signal name="PWM8">
<contactref element="BASEPULLUP8" pad="1"/>
<contactref element="Q27" pad="1"/>
<contactref element="IC9" pad="13"/>
</signal>
<signal name="GATE8">
<contactref element="GATEPULLUP8" pad="1"/>
<contactref element="Q27" pad="3"/>
<contactref element="Q26" pad="1"/>
</signal>
<signal name="SCK9">
<contactref element="IC10" pad="15"/>
<contactref element="JP19" pad="4"/>
<contactref element="U10" pad="4"/>
</signal>
<signal name="MOSI9">
<contactref element="JP19" pad="3"/>
<contactref element="IC10" pad="16"/>
<contactref element="U10" pad="3"/>
</signal>
<signal name="MISO9">
<contactref element="JP19" pad="6"/>
<contactref element="IC10" pad="17"/>
<contactref element="U10" pad="5"/>
</signal>
<signal name="RESET9">
<contactref element="JP19" pad="2"/>
<contactref element="IC10" pad="24"/>
<contactref element="RESET9" pad="1"/>
</signal>
<signal name="D-9">
<contactref element="IC10" pad="30"/>
<contactref element="R-9" pad="1"/>
</signal>
<signal name="D+9">
<contactref element="IC10" pad="29"/>
<contactref element="R+9" pad="1"/>
</signal>
<signal name="R-9">
<contactref element="R-9" pad="2"/>
<contactref element="J10" pad="A7"/>
<contactref element="D10" pad="4"/>
</signal>
<signal name="R+9">
<contactref element="R+9" pad="2"/>
<contactref element="J10" pad="A6"/>
<contactref element="D10" pad="3"/>
</signal>
<signal name="GND9">
<contactref element="IC10" pad="28"/>
<contactref element="C37" pad="2"/>
<contactref element="J10" pad="A1"/>
<contactref element="J10" pad="A12"/>
<contactref element="J10" pad="B1"/>
<contactref element="J10" pad="B12"/>
<contactref element="C39" pad="1"/>
<contactref element="C40" pad="2"/>
<contactref element="IC10" pad="3"/>
<contactref element="C38" pad="1"/>
<contactref element="JP19" pad="1"/>
<contactref element="CC19" pad="2"/>
<contactref element="CC20" pad="2"/>
<contactref element="IC10" pad="33"/>
<contactref element="U10" pad="1"/>
<contactref element="U10" pad="7"/>
<contactref element="Q29" pad="3"/>
<contactref element="IC10" pad="10"/>
<contactref element="IC10" pad="9"/>
<contactref element="D10" pad="5"/>
<contactref element="Q30" pad="2"/>
</signal>
<signal name="N$82">
<contactref element="C40" pad="1"/>
<contactref element="Q28" pad="3"/>
<contactref element="IC10" pad="2"/>
</signal>
<signal name="N$83">
<contactref element="C39" pad="2"/>
<contactref element="IC10" pad="1"/>
<contactref element="Q28" pad="1"/>
</signal>
<signal name="N$84">
</signal>
<signal name="CC19">
<contactref element="J10" pad="B5"/>
<contactref element="CC20" pad="1"/>
</signal>
<signal name="CS9">
<contactref element="IC10" pad="14"/>
<contactref element="U10" pad="2"/>
</signal>
<signal name="DRAIN9">
</signal>
<signal name="COMPARE9">
<contactref element="VSENSE9" pad="2"/>
<contactref element="IC10" pad="7"/>
</signal>
<signal name="VSENSE9">
<contactref element="VSENSE9" pad="1"/>
<contactref element="Q29" pad="2"/>
</signal>
<signal name="CHARGE9">
<contactref element="CALIBRATOR9" pad="1"/>
<contactref element="IC10" pad="6"/>
<contactref element="IC10" pad="8"/>
</signal>
<signal name="CGROUND9">
<contactref element="CALIBRATOR9" pad="2"/>
<contactref element="IC10" pad="5"/>
</signal>
<signal name="N$85">
</signal>
<signal name="N$86">
</signal>
<signal name="N$87">
</signal>
<signal name="CC20">
<contactref element="J10" pad="A5"/>
<contactref element="CC19" pad="1"/>
</signal>
<signal name="N$88">
</signal>
<signal name="N$89">
</signal>
<signal name="5V9">
<contactref element="VIA10" pad="VIA1"/>
<contactref element="JP20" pad="SHIT"/>
<contactref element="J10" pad="B4"/>
<contactref element="J10" pad="A9"/>
<contactref element="J10" pad="A4"/>
<contactref element="J10" pad="B9"/>
<contactref element="IC10" pad="31"/>
<contactref element="C38" pad="2"/>
<contactref element="GATEPULLUP9" pad="2"/>
</signal>
<signal name="N$90">
</signal>
<signal name="VCC9">
<contactref element="U10" pad="8"/>
<contactref element="U10" pad="6"/>
<contactref element="C37" pad="1"/>
<contactref element="IC10" pad="27"/>
<contactref element="RESET9" pad="2"/>
<contactref element="D10" pad="1"/>
<contactref element="IC10" pad="4"/>
<contactref element="IC10" pad="32"/>
<contactref element="JP19" pad="5"/>
<contactref element="BASEPULLUP9" pad="2"/>
</signal>
<signal name="PWM9">
<contactref element="BASEPULLUP9" pad="1"/>
<contactref element="Q30" pad="1"/>
<contactref element="IC10" pad="13"/>
</signal>
<signal name="GATE9">
<contactref element="GATEPULLUP9" pad="1"/>
<contactref element="Q30" pad="3"/>
<contactref element="Q29" pad="1"/>
</signal>
<signal name="SCK10">
<contactref element="IC11" pad="15"/>
<contactref element="JP21" pad="4"/>
<contactref element="U11" pad="4"/>
</signal>
<signal name="MOSI10">
<contactref element="JP21" pad="3"/>
<contactref element="IC11" pad="16"/>
<contactref element="U11" pad="3"/>
</signal>
<signal name="MISO10">
<contactref element="JP21" pad="6"/>
<contactref element="IC11" pad="17"/>
<contactref element="U11" pad="5"/>
</signal>
<signal name="RESET10">
<contactref element="JP21" pad="2"/>
<contactref element="IC11" pad="24"/>
<contactref element="RESET10" pad="1"/>
</signal>
<signal name="D-10">
<contactref element="IC11" pad="30"/>
<contactref element="R-10" pad="1"/>
</signal>
<signal name="D+10">
<contactref element="IC11" pad="29"/>
<contactref element="R+10" pad="1"/>
</signal>
<signal name="R-10">
<contactref element="R-10" pad="2"/>
<contactref element="J11" pad="A7"/>
<contactref element="D11" pad="4"/>
</signal>
<signal name="R+10">
<contactref element="R+10" pad="2"/>
<contactref element="J11" pad="A6"/>
<contactref element="D11" pad="3"/>
</signal>
<signal name="GND10">
<contactref element="IC11" pad="28"/>
<contactref element="C41" pad="2"/>
<contactref element="J11" pad="A1"/>
<contactref element="J11" pad="A12"/>
<contactref element="J11" pad="B1"/>
<contactref element="J11" pad="B12"/>
<contactref element="C43" pad="1"/>
<contactref element="C44" pad="2"/>
<contactref element="IC11" pad="3"/>
<contactref element="C42" pad="1"/>
<contactref element="JP21" pad="1"/>
<contactref element="CC21" pad="2"/>
<contactref element="CC22" pad="2"/>
<contactref element="IC11" pad="33"/>
<contactref element="U11" pad="1"/>
<contactref element="U11" pad="7"/>
<contactref element="Q32" pad="3"/>
<contactref element="IC11" pad="10"/>
<contactref element="IC11" pad="9"/>
<contactref element="D11" pad="5"/>
<contactref element="Q33" pad="2"/>
</signal>
<signal name="N$91">
<contactref element="C44" pad="1"/>
<contactref element="Q31" pad="3"/>
<contactref element="IC11" pad="2"/>
</signal>
<signal name="N$92">
<contactref element="C43" pad="2"/>
<contactref element="IC11" pad="1"/>
<contactref element="Q31" pad="1"/>
</signal>
<signal name="N$93">
</signal>
<signal name="CC21">
<contactref element="J11" pad="B5"/>
<contactref element="CC22" pad="1"/>
</signal>
<signal name="CS10">
<contactref element="IC11" pad="14"/>
<contactref element="U11" pad="2"/>
</signal>
<signal name="DRAIN10">
</signal>
<signal name="COMPARE10">
<contactref element="VSENSE10" pad="2"/>
<contactref element="IC11" pad="7"/>
</signal>
<signal name="VSENSE10">
<contactref element="VSENSE10" pad="1"/>
<contactref element="Q32" pad="2"/>
</signal>
<signal name="CHARGE10">
<contactref element="CALIBRATOR10" pad="1"/>
<contactref element="IC11" pad="6"/>
<contactref element="IC11" pad="8"/>
</signal>
<signal name="CGROUND10">
<contactref element="CALIBRATOR10" pad="2"/>
<contactref element="IC11" pad="5"/>
</signal>
<signal name="N$94">
</signal>
<signal name="N$95">
</signal>
<signal name="N$96">
</signal>
<signal name="CC22">
<contactref element="J11" pad="A5"/>
<contactref element="CC21" pad="1"/>
</signal>
<signal name="N$97">
</signal>
<signal name="N$98">
</signal>
<signal name="5V10">
<contactref element="VIA11" pad="VIA1"/>
<contactref element="JP22" pad="SHIT"/>
<contactref element="J11" pad="B4"/>
<contactref element="J11" pad="A9"/>
<contactref element="J11" pad="A4"/>
<contactref element="J11" pad="B9"/>
<contactref element="IC11" pad="31"/>
<contactref element="C42" pad="2"/>
<contactref element="GATEPULLUP10" pad="2"/>
</signal>
<signal name="N$99">
</signal>
<signal name="VCC10">
<contactref element="U11" pad="8"/>
<contactref element="U11" pad="6"/>
<contactref element="C41" pad="1"/>
<contactref element="IC11" pad="27"/>
<contactref element="RESET10" pad="2"/>
<contactref element="D11" pad="1"/>
<contactref element="IC11" pad="4"/>
<contactref element="IC11" pad="32"/>
<contactref element="JP21" pad="5"/>
<contactref element="BASEPULLUP10" pad="2"/>
</signal>
<signal name="PWM10">
<contactref element="BASEPULLUP10" pad="1"/>
<contactref element="Q33" pad="1"/>
<contactref element="IC11" pad="13"/>
</signal>
<signal name="GATE10">
<contactref element="GATEPULLUP10" pad="1"/>
<contactref element="Q33" pad="3"/>
<contactref element="Q32" pad="1"/>
</signal>
<signal name="SCK11">
<contactref element="IC12" pad="15"/>
<contactref element="JP23" pad="4"/>
<contactref element="U12" pad="4"/>
</signal>
<signal name="MOSI11">
<contactref element="JP23" pad="3"/>
<contactref element="IC12" pad="16"/>
<contactref element="U12" pad="3"/>
</signal>
<signal name="MISO11">
<contactref element="JP23" pad="6"/>
<contactref element="IC12" pad="17"/>
<contactref element="U12" pad="5"/>
</signal>
<signal name="RESET11">
<contactref element="JP23" pad="2"/>
<contactref element="IC12" pad="24"/>
<contactref element="RESET11" pad="1"/>
</signal>
<signal name="D-11">
<contactref element="IC12" pad="30"/>
<contactref element="R-11" pad="1"/>
</signal>
<signal name="D+11">
<contactref element="IC12" pad="29"/>
<contactref element="R+11" pad="1"/>
</signal>
<signal name="R-11">
<contactref element="R-11" pad="2"/>
<contactref element="J12" pad="A7"/>
<contactref element="D12" pad="4"/>
</signal>
<signal name="R+11">
<contactref element="R+11" pad="2"/>
<contactref element="J12" pad="A6"/>
<contactref element="D12" pad="3"/>
</signal>
<signal name="GND11">
<contactref element="IC12" pad="28"/>
<contactref element="C45" pad="2"/>
<contactref element="J12" pad="A1"/>
<contactref element="J12" pad="A12"/>
<contactref element="J12" pad="B1"/>
<contactref element="J12" pad="B12"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="2"/>
<contactref element="IC12" pad="3"/>
<contactref element="C46" pad="1"/>
<contactref element="JP23" pad="1"/>
<contactref element="CC23" pad="2"/>
<contactref element="CC24" pad="2"/>
<contactref element="IC12" pad="33"/>
<contactref element="U12" pad="1"/>
<contactref element="U12" pad="7"/>
<contactref element="Q35" pad="3"/>
<contactref element="IC12" pad="10"/>
<contactref element="IC12" pad="9"/>
<contactref element="D12" pad="5"/>
<contactref element="Q36" pad="2"/>
</signal>
<signal name="N$100">
<contactref element="C48" pad="1"/>
<contactref element="Q34" pad="3"/>
<contactref element="IC12" pad="2"/>
</signal>
<signal name="N$101">
<contactref element="C47" pad="2"/>
<contactref element="IC12" pad="1"/>
<contactref element="Q34" pad="1"/>
</signal>
<signal name="N$102">
</signal>
<signal name="CC23">
<contactref element="J12" pad="B5"/>
<contactref element="CC24" pad="1"/>
</signal>
<signal name="CS11">
<contactref element="IC12" pad="14"/>
<contactref element="U12" pad="2"/>
</signal>
<signal name="DRAIN11">
</signal>
<signal name="COMPARE11">
<contactref element="VSENSE11" pad="2"/>
<contactref element="IC12" pad="7"/>
</signal>
<signal name="VSENSE11">
<contactref element="VSENSE11" pad="1"/>
<contactref element="Q35" pad="2"/>
</signal>
<signal name="CHARGE11">
<contactref element="CALIBRATOR11" pad="1"/>
<contactref element="IC12" pad="6"/>
<contactref element="IC12" pad="8"/>
</signal>
<signal name="CGROUND11">
<contactref element="CALIBRATOR11" pad="2"/>
<contactref element="IC12" pad="5"/>
</signal>
<signal name="N$103">
</signal>
<signal name="N$104">
</signal>
<signal name="N$105">
</signal>
<signal name="CC24">
<contactref element="J12" pad="A5"/>
<contactref element="CC23" pad="1"/>
</signal>
<signal name="N$106">
</signal>
<signal name="N$107">
</signal>
<signal name="5V11">
<contactref element="VIA12" pad="VIA1"/>
<contactref element="JP24" pad="SHIT"/>
<contactref element="J12" pad="B4"/>
<contactref element="J12" pad="A9"/>
<contactref element="J12" pad="A4"/>
<contactref element="J12" pad="B9"/>
<contactref element="IC12" pad="31"/>
<contactref element="C46" pad="2"/>
<contactref element="GATEPULLUP11" pad="2"/>
</signal>
<signal name="N$108">
</signal>
<signal name="VCC11">
<contactref element="U12" pad="8"/>
<contactref element="U12" pad="6"/>
<contactref element="C45" pad="1"/>
<contactref element="IC12" pad="27"/>
<contactref element="RESET11" pad="2"/>
<contactref element="D12" pad="1"/>
<contactref element="IC12" pad="4"/>
<contactref element="IC12" pad="32"/>
<contactref element="JP23" pad="5"/>
<contactref element="BASEPULLUP11" pad="2"/>
</signal>
<signal name="PWM11">
<contactref element="BASEPULLUP11" pad="1"/>
<contactref element="Q36" pad="1"/>
<contactref element="IC12" pad="13"/>
</signal>
<signal name="GATE11">
<contactref element="GATEPULLUP11" pad="1"/>
<contactref element="Q36" pad="3"/>
<contactref element="Q35" pad="1"/>
</signal>
<signal name="SCK12">
<contactref element="IC13" pad="15"/>
<contactref element="JP25" pad="4"/>
<contactref element="U13" pad="4"/>
</signal>
<signal name="MOSI12">
<contactref element="JP25" pad="3"/>
<contactref element="IC13" pad="16"/>
<contactref element="U13" pad="3"/>
</signal>
<signal name="MISO12">
<contactref element="JP25" pad="6"/>
<contactref element="IC13" pad="17"/>
<contactref element="U13" pad="5"/>
</signal>
<signal name="RESET12">
<contactref element="JP25" pad="2"/>
<contactref element="IC13" pad="24"/>
<contactref element="RESET12" pad="1"/>
</signal>
<signal name="D-12">
<contactref element="IC13" pad="30"/>
<contactref element="R-12" pad="1"/>
</signal>
<signal name="D+12">
<contactref element="IC13" pad="29"/>
<contactref element="R+12" pad="1"/>
</signal>
<signal name="R-12">
<contactref element="R-12" pad="2"/>
<contactref element="J13" pad="A7"/>
<contactref element="D13" pad="4"/>
</signal>
<signal name="R+12">
<contactref element="R+12" pad="2"/>
<contactref element="J13" pad="A6"/>
<contactref element="D13" pad="3"/>
</signal>
<signal name="GND12">
<contactref element="IC13" pad="28"/>
<contactref element="C49" pad="2"/>
<contactref element="J13" pad="A1"/>
<contactref element="J13" pad="A12"/>
<contactref element="J13" pad="B1"/>
<contactref element="J13" pad="B12"/>
<contactref element="C51" pad="1"/>
<contactref element="C52" pad="2"/>
<contactref element="IC13" pad="3"/>
<contactref element="C50" pad="1"/>
<contactref element="JP25" pad="1"/>
<contactref element="CC25" pad="2"/>
<contactref element="CC26" pad="2"/>
<contactref element="IC13" pad="33"/>
<contactref element="U13" pad="1"/>
<contactref element="U13" pad="7"/>
<contactref element="Q38" pad="3"/>
<contactref element="IC13" pad="10"/>
<contactref element="IC13" pad="9"/>
<contactref element="D13" pad="5"/>
<contactref element="Q39" pad="2"/>
</signal>
<signal name="N$109">
<contactref element="C52" pad="1"/>
<contactref element="Q37" pad="3"/>
<contactref element="IC13" pad="2"/>
</signal>
<signal name="N$110">
<contactref element="C51" pad="2"/>
<contactref element="IC13" pad="1"/>
<contactref element="Q37" pad="1"/>
</signal>
<signal name="N$111">
</signal>
<signal name="CC25">
<contactref element="J13" pad="B5"/>
<contactref element="CC26" pad="1"/>
</signal>
<signal name="CS12">
<contactref element="IC13" pad="14"/>
<contactref element="U13" pad="2"/>
</signal>
<signal name="DRAIN12">
</signal>
<signal name="COMPARE12">
<contactref element="VSENSE12" pad="2"/>
<contactref element="IC13" pad="7"/>
</signal>
<signal name="VSENSE12">
<contactref element="VSENSE12" pad="1"/>
<contactref element="Q38" pad="2"/>
</signal>
<signal name="CHARGE12">
<contactref element="CALIBRATOR12" pad="1"/>
<contactref element="IC13" pad="6"/>
<contactref element="IC13" pad="8"/>
</signal>
<signal name="CGROUND12">
<contactref element="CALIBRATOR12" pad="2"/>
<contactref element="IC13" pad="5"/>
</signal>
<signal name="N$112">
</signal>
<signal name="N$113">
</signal>
<signal name="N$114">
</signal>
<signal name="CC26">
<contactref element="J13" pad="A5"/>
<contactref element="CC25" pad="1"/>
</signal>
<signal name="N$115">
</signal>
<signal name="N$116">
</signal>
<signal name="5V12">
<contactref element="VIA13" pad="VIA1"/>
<contactref element="JP26" pad="SHIT"/>
<contactref element="J13" pad="B4"/>
<contactref element="J13" pad="A9"/>
<contactref element="J13" pad="A4"/>
<contactref element="J13" pad="B9"/>
<contactref element="IC13" pad="31"/>
<contactref element="C50" pad="2"/>
<contactref element="GATEPULLUP12" pad="2"/>
</signal>
<signal name="N$117">
</signal>
<signal name="VCC12">
<contactref element="U13" pad="8"/>
<contactref element="U13" pad="6"/>
<contactref element="C49" pad="1"/>
<contactref element="IC13" pad="27"/>
<contactref element="RESET12" pad="2"/>
<contactref element="D13" pad="1"/>
<contactref element="IC13" pad="4"/>
<contactref element="IC13" pad="32"/>
<contactref element="JP25" pad="5"/>
<contactref element="BASEPULLUP12" pad="2"/>
</signal>
<signal name="PWM12">
<contactref element="BASEPULLUP12" pad="1"/>
<contactref element="Q39" pad="1"/>
<contactref element="IC13" pad="13"/>
</signal>
<signal name="GATE12">
<contactref element="GATEPULLUP12" pad="1"/>
<contactref element="Q39" pad="3"/>
<contactref element="Q38" pad="1"/>
</signal>
<signal name="SCK13">
<contactref element="IC14" pad="15"/>
<contactref element="JP27" pad="4"/>
<contactref element="U14" pad="4"/>
</signal>
<signal name="MOSI13">
<contactref element="JP27" pad="3"/>
<contactref element="IC14" pad="16"/>
<contactref element="U14" pad="3"/>
</signal>
<signal name="MISO13">
<contactref element="JP27" pad="6"/>
<contactref element="IC14" pad="17"/>
<contactref element="U14" pad="5"/>
</signal>
<signal name="RESET13">
<contactref element="JP27" pad="2"/>
<contactref element="IC14" pad="24"/>
<contactref element="RESET13" pad="1"/>
</signal>
<signal name="D-13">
<contactref element="IC14" pad="30"/>
<contactref element="R-13" pad="1"/>
</signal>
<signal name="D+13">
<contactref element="IC14" pad="29"/>
<contactref element="R+13" pad="1"/>
</signal>
<signal name="R-13">
<contactref element="R-13" pad="2"/>
<contactref element="J14" pad="A7"/>
<contactref element="D14" pad="4"/>
</signal>
<signal name="R+13">
<contactref element="R+13" pad="2"/>
<contactref element="J14" pad="A6"/>
<contactref element="D14" pad="3"/>
</signal>
<signal name="GND13">
<contactref element="IC14" pad="28"/>
<contactref element="C53" pad="2"/>
<contactref element="J14" pad="A1"/>
<contactref element="J14" pad="A12"/>
<contactref element="J14" pad="B1"/>
<contactref element="J14" pad="B12"/>
<contactref element="C55" pad="1"/>
<contactref element="C56" pad="2"/>
<contactref element="IC14" pad="3"/>
<contactref element="C54" pad="1"/>
<contactref element="JP27" pad="1"/>
<contactref element="CC27" pad="2"/>
<contactref element="CC28" pad="2"/>
<contactref element="IC14" pad="33"/>
<contactref element="U14" pad="1"/>
<contactref element="U14" pad="7"/>
<contactref element="Q41" pad="3"/>
<contactref element="IC14" pad="10"/>
<contactref element="IC14" pad="9"/>
<contactref element="D14" pad="5"/>
<contactref element="Q42" pad="2"/>
</signal>
<signal name="N$118">
<contactref element="C56" pad="1"/>
<contactref element="Q40" pad="3"/>
<contactref element="IC14" pad="2"/>
</signal>
<signal name="N$119">
<contactref element="C55" pad="2"/>
<contactref element="IC14" pad="1"/>
<contactref element="Q40" pad="1"/>
</signal>
<signal name="N$120">
</signal>
<signal name="CC27">
<contactref element="J14" pad="B5"/>
<contactref element="CC28" pad="1"/>
</signal>
<signal name="CS13">
<contactref element="IC14" pad="14"/>
<contactref element="U14" pad="2"/>
</signal>
<signal name="DRAIN13">
</signal>
<signal name="COMPARE13">
<contactref element="VSENSE13" pad="2"/>
<contactref element="IC14" pad="7"/>
</signal>
<signal name="VSENSE13">
<contactref element="VSENSE13" pad="1"/>
<contactref element="Q41" pad="2"/>
</signal>
<signal name="CHARGE13">
<contactref element="CALIBRATOR13" pad="1"/>
<contactref element="IC14" pad="6"/>
<contactref element="IC14" pad="8"/>
</signal>
<signal name="CGROUND13">
<contactref element="CALIBRATOR13" pad="2"/>
<contactref element="IC14" pad="5"/>
</signal>
<signal name="N$121">
</signal>
<signal name="N$122">
</signal>
<signal name="N$123">
</signal>
<signal name="CC28">
<contactref element="J14" pad="A5"/>
<contactref element="CC27" pad="1"/>
</signal>
<signal name="N$124">
</signal>
<signal name="N$125">
</signal>
<signal name="5V13">
<contactref element="VIA14" pad="VIA1"/>
<contactref element="JP28" pad="SHIT"/>
<contactref element="J14" pad="B4"/>
<contactref element="J14" pad="A9"/>
<contactref element="J14" pad="A4"/>
<contactref element="J14" pad="B9"/>
<contactref element="IC14" pad="31"/>
<contactref element="C54" pad="2"/>
<contactref element="GATEPULLUP13" pad="2"/>
</signal>
<signal name="N$126">
</signal>
<signal name="VCC13">
<contactref element="U14" pad="8"/>
<contactref element="U14" pad="6"/>
<contactref element="C53" pad="1"/>
<contactref element="IC14" pad="27"/>
<contactref element="RESET13" pad="2"/>
<contactref element="D14" pad="1"/>
<contactref element="IC14" pad="4"/>
<contactref element="IC14" pad="32"/>
<contactref element="JP27" pad="5"/>
<contactref element="BASEPULLUP13" pad="2"/>
</signal>
<signal name="PWM13">
<contactref element="BASEPULLUP13" pad="1"/>
<contactref element="Q42" pad="1"/>
<contactref element="IC14" pad="13"/>
</signal>
<signal name="GATE13">
<contactref element="GATEPULLUP13" pad="1"/>
<contactref element="Q42" pad="3"/>
<contactref element="Q41" pad="1"/>
</signal>
<signal name="SCK14">
<contactref element="IC15" pad="15"/>
<contactref element="JP29" pad="4"/>
<contactref element="U15" pad="4"/>
</signal>
<signal name="MOSI14">
<contactref element="JP29" pad="3"/>
<contactref element="IC15" pad="16"/>
<contactref element="U15" pad="3"/>
</signal>
<signal name="MISO14">
<contactref element="JP29" pad="6"/>
<contactref element="IC15" pad="17"/>
<contactref element="U15" pad="5"/>
</signal>
<signal name="RESET14">
<contactref element="JP29" pad="2"/>
<contactref element="IC15" pad="24"/>
<contactref element="RESET14" pad="1"/>
</signal>
<signal name="D-14">
<contactref element="IC15" pad="30"/>
<contactref element="R-14" pad="1"/>
</signal>
<signal name="D+14">
<contactref element="IC15" pad="29"/>
<contactref element="R+14" pad="1"/>
</signal>
<signal name="R-14">
<contactref element="R-14" pad="2"/>
<contactref element="J15" pad="A7"/>
<contactref element="D15" pad="4"/>
</signal>
<signal name="R+14">
<contactref element="R+14" pad="2"/>
<contactref element="J15" pad="A6"/>
<contactref element="D15" pad="3"/>
</signal>
<signal name="GND14">
<contactref element="IC15" pad="28"/>
<contactref element="C57" pad="2"/>
<contactref element="J15" pad="A1"/>
<contactref element="J15" pad="A12"/>
<contactref element="J15" pad="B1"/>
<contactref element="J15" pad="B12"/>
<contactref element="C59" pad="1"/>
<contactref element="C60" pad="2"/>
<contactref element="IC15" pad="3"/>
<contactref element="C58" pad="1"/>
<contactref element="JP29" pad="1"/>
<contactref element="CC29" pad="2"/>
<contactref element="CC30" pad="2"/>
<contactref element="IC15" pad="33"/>
<contactref element="U15" pad="1"/>
<contactref element="U15" pad="7"/>
<contactref element="Q44" pad="3"/>
<contactref element="IC15" pad="10"/>
<contactref element="IC15" pad="9"/>
<contactref element="D15" pad="5"/>
<contactref element="Q45" pad="2"/>
</signal>
<signal name="N$127">
<contactref element="C60" pad="1"/>
<contactref element="Q43" pad="3"/>
<contactref element="IC15" pad="2"/>
</signal>
<signal name="N$128">
<contactref element="C59" pad="2"/>
<contactref element="IC15" pad="1"/>
<contactref element="Q43" pad="1"/>
</signal>
<signal name="N$129">
</signal>
<signal name="CC29">
<contactref element="J15" pad="B5"/>
<contactref element="CC30" pad="1"/>
</signal>
<signal name="CS14">
<contactref element="IC15" pad="14"/>
<contactref element="U15" pad="2"/>
</signal>
<signal name="DRAIN14">
</signal>
<signal name="COMPARE14">
<contactref element="VSENSE14" pad="2"/>
<contactref element="IC15" pad="7"/>
</signal>
<signal name="VSENSE14">
<contactref element="VSENSE14" pad="1"/>
<contactref element="Q44" pad="2"/>
</signal>
<signal name="CHARGE14">
<contactref element="CALIBRATOR14" pad="1"/>
<contactref element="IC15" pad="6"/>
<contactref element="IC15" pad="8"/>
</signal>
<signal name="CGROUND14">
<contactref element="CALIBRATOR14" pad="2"/>
<contactref element="IC15" pad="5"/>
</signal>
<signal name="N$130">
</signal>
<signal name="N$131">
</signal>
<signal name="N$132">
</signal>
<signal name="CC30">
<contactref element="J15" pad="A5"/>
<contactref element="CC29" pad="1"/>
</signal>
<signal name="N$133">
</signal>
<signal name="N$134">
</signal>
<signal name="5V14">
<contactref element="VIA15" pad="VIA1"/>
<contactref element="JP30" pad="SHIT"/>
<contactref element="J15" pad="B4"/>
<contactref element="J15" pad="A9"/>
<contactref element="J15" pad="A4"/>
<contactref element="J15" pad="B9"/>
<contactref element="IC15" pad="31"/>
<contactref element="C58" pad="2"/>
<contactref element="GATEPULLUP14" pad="2"/>
</signal>
<signal name="N$135">
</signal>
<signal name="VCC14">
<contactref element="U15" pad="8"/>
<contactref element="U15" pad="6"/>
<contactref element="C57" pad="1"/>
<contactref element="IC15" pad="27"/>
<contactref element="RESET14" pad="2"/>
<contactref element="D15" pad="1"/>
<contactref element="IC15" pad="4"/>
<contactref element="IC15" pad="32"/>
<contactref element="JP29" pad="5"/>
<contactref element="BASEPULLUP14" pad="2"/>
</signal>
<signal name="PWM14">
<contactref element="BASEPULLUP14" pad="1"/>
<contactref element="Q45" pad="1"/>
<contactref element="IC15" pad="13"/>
</signal>
<signal name="GATE14">
<contactref element="GATEPULLUP14" pad="1"/>
<contactref element="Q45" pad="3"/>
<contactref element="Q44" pad="1"/>
</signal>
<signal name="SCK15">
<contactref element="IC16" pad="15"/>
<contactref element="JP31" pad="4"/>
<contactref element="U16" pad="4"/>
</signal>
<signal name="MOSI15">
<contactref element="JP31" pad="3"/>
<contactref element="IC16" pad="16"/>
<contactref element="U16" pad="3"/>
</signal>
<signal name="MISO15">
<contactref element="JP31" pad="6"/>
<contactref element="IC16" pad="17"/>
<contactref element="U16" pad="5"/>
</signal>
<signal name="RESET15">
<contactref element="JP31" pad="2"/>
<contactref element="IC16" pad="24"/>
<contactref element="RESET15" pad="1"/>
</signal>
<signal name="D-15">
<contactref element="IC16" pad="30"/>
<contactref element="R-15" pad="1"/>
</signal>
<signal name="D+15">
<contactref element="IC16" pad="29"/>
<contactref element="R+15" pad="1"/>
</signal>
<signal name="R-15">
<contactref element="R-15" pad="2"/>
<contactref element="J16" pad="A7"/>
<contactref element="D16" pad="4"/>
</signal>
<signal name="R+15">
<contactref element="R+15" pad="2"/>
<contactref element="J16" pad="A6"/>
<contactref element="D16" pad="3"/>
</signal>
<signal name="GND15">
<contactref element="IC16" pad="28"/>
<contactref element="C61" pad="2"/>
<contactref element="J16" pad="A1"/>
<contactref element="J16" pad="A12"/>
<contactref element="J16" pad="B1"/>
<contactref element="J16" pad="B12"/>
<contactref element="C63" pad="1"/>
<contactref element="C64" pad="2"/>
<contactref element="IC16" pad="3"/>
<contactref element="C62" pad="1"/>
<contactref element="JP31" pad="1"/>
<contactref element="CC31" pad="2"/>
<contactref element="CC32" pad="2"/>
<contactref element="IC16" pad="33"/>
<contactref element="U16" pad="1"/>
<contactref element="U16" pad="7"/>
<contactref element="Q47" pad="3"/>
<contactref element="IC16" pad="10"/>
<contactref element="IC16" pad="9"/>
<contactref element="D16" pad="5"/>
<contactref element="Q48" pad="2"/>
</signal>
<signal name="N$136">
<contactref element="C64" pad="1"/>
<contactref element="Q46" pad="3"/>
<contactref element="IC16" pad="2"/>
</signal>
<signal name="N$137">
<contactref element="C63" pad="2"/>
<contactref element="IC16" pad="1"/>
<contactref element="Q46" pad="1"/>
</signal>
<signal name="N$138">
</signal>
<signal name="CC31">
<contactref element="J16" pad="B5"/>
<contactref element="CC32" pad="1"/>
</signal>
<signal name="CS15">
<contactref element="IC16" pad="14"/>
<contactref element="U16" pad="2"/>
</signal>
<signal name="DRAIN15">
</signal>
<signal name="COMPARE15">
<contactref element="VSENSE15" pad="2"/>
<contactref element="IC16" pad="7"/>
</signal>
<signal name="VSENSE15">
<contactref element="VSENSE15" pad="1"/>
<contactref element="Q47" pad="2"/>
</signal>
<signal name="CHARGE15">
<contactref element="CALIBRATOR15" pad="1"/>
<contactref element="IC16" pad="6"/>
<contactref element="IC16" pad="8"/>
</signal>
<signal name="CGROUND15">
<contactref element="CALIBRATOR15" pad="2"/>
<contactref element="IC16" pad="5"/>
</signal>
<signal name="N$139">
</signal>
<signal name="N$140">
</signal>
<signal name="N$141">
</signal>
<signal name="CC32">
<contactref element="J16" pad="A5"/>
<contactref element="CC31" pad="1"/>
</signal>
<signal name="N$142">
</signal>
<signal name="N$143">
</signal>
<signal name="5V15">
<contactref element="VIA16" pad="VIA1"/>
<contactref element="JP32" pad="SHIT"/>
<contactref element="J16" pad="B4"/>
<contactref element="J16" pad="A9"/>
<contactref element="J16" pad="A4"/>
<contactref element="J16" pad="B9"/>
<contactref element="IC16" pad="31"/>
<contactref element="C62" pad="2"/>
<contactref element="GATEPULLUP15" pad="2"/>
</signal>
<signal name="N$144">
</signal>
<signal name="VCC15">
<contactref element="U16" pad="8"/>
<contactref element="U16" pad="6"/>
<contactref element="C61" pad="1"/>
<contactref element="IC16" pad="27"/>
<contactref element="RESET15" pad="2"/>
<contactref element="D16" pad="1"/>
<contactref element="IC16" pad="4"/>
<contactref element="IC16" pad="32"/>
<contactref element="JP31" pad="5"/>
<contactref element="BASEPULLUP15" pad="2"/>
</signal>
<signal name="PWM15">
<contactref element="BASEPULLUP15" pad="1"/>
<contactref element="Q48" pad="1"/>
<contactref element="IC16" pad="13"/>
</signal>
<signal name="GATE15">
<contactref element="GATEPULLUP15" pad="1"/>
<contactref element="Q48" pad="3"/>
<contactref element="Q47" pad="1"/>
</signal>
<signal name="SCK16">
<contactref element="IC17" pad="15"/>
<contactref element="JP33" pad="4"/>
<contactref element="U17" pad="4"/>
</signal>
<signal name="MOSI16">
<contactref element="JP33" pad="3"/>
<contactref element="IC17" pad="16"/>
<contactref element="U17" pad="3"/>
</signal>
<signal name="MISO16">
<contactref element="JP33" pad="6"/>
<contactref element="IC17" pad="17"/>
<contactref element="U17" pad="5"/>
</signal>
<signal name="RESET16">
<contactref element="JP33" pad="2"/>
<contactref element="IC17" pad="24"/>
<contactref element="RESET16" pad="1"/>
</signal>
<signal name="D-16">
<contactref element="IC17" pad="30"/>
<contactref element="R-16" pad="1"/>
</signal>
<signal name="D+16">
<contactref element="IC17" pad="29"/>
<contactref element="R+16" pad="1"/>
</signal>
<signal name="R-16">
<contactref element="R-16" pad="2"/>
<contactref element="J17" pad="A7"/>
<contactref element="D17" pad="4"/>
</signal>
<signal name="R+16">
<contactref element="R+16" pad="2"/>
<contactref element="J17" pad="A6"/>
<contactref element="D17" pad="3"/>
</signal>
<signal name="GND16">
<contactref element="IC17" pad="28"/>
<contactref element="C65" pad="2"/>
<contactref element="J17" pad="A1"/>
<contactref element="J17" pad="A12"/>
<contactref element="J17" pad="B1"/>
<contactref element="J17" pad="B12"/>
<contactref element="C67" pad="1"/>
<contactref element="C68" pad="2"/>
<contactref element="IC17" pad="3"/>
<contactref element="C66" pad="1"/>
<contactref element="JP33" pad="1"/>
<contactref element="CC33" pad="2"/>
<contactref element="CC34" pad="2"/>
<contactref element="IC17" pad="33"/>
<contactref element="U17" pad="1"/>
<contactref element="U17" pad="7"/>
<contactref element="Q50" pad="3"/>
<contactref element="IC17" pad="10"/>
<contactref element="IC17" pad="9"/>
<contactref element="D17" pad="5"/>
<contactref element="Q51" pad="2"/>
</signal>
<signal name="N$145">
<contactref element="C68" pad="1"/>
<contactref element="Q49" pad="3"/>
<contactref element="IC17" pad="2"/>
</signal>
<signal name="N$146">
<contactref element="C67" pad="2"/>
<contactref element="IC17" pad="1"/>
<contactref element="Q49" pad="1"/>
</signal>
<signal name="N$147">
</signal>
<signal name="CC33">
<contactref element="J17" pad="B5"/>
<contactref element="CC34" pad="1"/>
</signal>
<signal name="CS16">
<contactref element="IC17" pad="14"/>
<contactref element="U17" pad="2"/>
</signal>
<signal name="DRAIN16">
</signal>
<signal name="COMPARE16">
<contactref element="VSENSE16" pad="2"/>
<contactref element="IC17" pad="7"/>
</signal>
<signal name="VSENSE16">
<contactref element="VSENSE16" pad="1"/>
<contactref element="Q50" pad="2"/>
</signal>
<signal name="CHARGE16">
<contactref element="CALIBRATOR16" pad="1"/>
<contactref element="IC17" pad="6"/>
<contactref element="IC17" pad="8"/>
</signal>
<signal name="CGROUND16">
<contactref element="CALIBRATOR16" pad="2"/>
<contactref element="IC17" pad="5"/>
</signal>
<signal name="N$148">
</signal>
<signal name="N$149">
</signal>
<signal name="N$150">
</signal>
<signal name="CC34">
<contactref element="J17" pad="A5"/>
<contactref element="CC33" pad="1"/>
</signal>
<signal name="N$151">
</signal>
<signal name="N$152">
</signal>
<signal name="5V16">
<contactref element="VIA17" pad="VIA1"/>
<contactref element="JP34" pad="SHIT"/>
<contactref element="J17" pad="B4"/>
<contactref element="J17" pad="A9"/>
<contactref element="J17" pad="A4"/>
<contactref element="J17" pad="B9"/>
<contactref element="IC17" pad="31"/>
<contactref element="C66" pad="2"/>
<contactref element="GATEPULLUP16" pad="2"/>
</signal>
<signal name="N$153">
</signal>
<signal name="VCC16">
<contactref element="U17" pad="8"/>
<contactref element="U17" pad="6"/>
<contactref element="C65" pad="1"/>
<contactref element="IC17" pad="27"/>
<contactref element="RESET16" pad="2"/>
<contactref element="D17" pad="1"/>
<contactref element="IC17" pad="4"/>
<contactref element="IC17" pad="32"/>
<contactref element="JP33" pad="5"/>
<contactref element="BASEPULLUP16" pad="2"/>
</signal>
<signal name="PWM16">
<contactref element="BASEPULLUP16" pad="1"/>
<contactref element="Q51" pad="1"/>
<contactref element="IC17" pad="13"/>
</signal>
<signal name="GATE16">
<contactref element="GATEPULLUP16" pad="1"/>
<contactref element="Q51" pad="3"/>
<contactref element="Q50" pad="1"/>
</signal>
<signal name="SCK17">
<contactref element="IC18" pad="15"/>
<contactref element="JP35" pad="4"/>
<contactref element="U18" pad="4"/>
</signal>
<signal name="MOSI17">
<contactref element="JP35" pad="3"/>
<contactref element="IC18" pad="16"/>
<contactref element="U18" pad="3"/>
</signal>
<signal name="MISO17">
<contactref element="JP35" pad="6"/>
<contactref element="IC18" pad="17"/>
<contactref element="U18" pad="5"/>
</signal>
<signal name="RESET17">
<contactref element="JP35" pad="2"/>
<contactref element="IC18" pad="24"/>
<contactref element="RESET17" pad="1"/>
</signal>
<signal name="D-17">
<contactref element="IC18" pad="30"/>
<contactref element="R-17" pad="1"/>
</signal>
<signal name="D+17">
<contactref element="IC18" pad="29"/>
<contactref element="R+17" pad="1"/>
</signal>
<signal name="R-17">
<contactref element="R-17" pad="2"/>
<contactref element="J18" pad="A7"/>
<contactref element="D18" pad="4"/>
</signal>
<signal name="R+17">
<contactref element="R+17" pad="2"/>
<contactref element="J18" pad="A6"/>
<contactref element="D18" pad="3"/>
</signal>
<signal name="GND17">
<contactref element="IC18" pad="28"/>
<contactref element="C69" pad="2"/>
<contactref element="J18" pad="A1"/>
<contactref element="J18" pad="A12"/>
<contactref element="J18" pad="B1"/>
<contactref element="J18" pad="B12"/>
<contactref element="C71" pad="1"/>
<contactref element="C72" pad="2"/>
<contactref element="IC18" pad="3"/>
<contactref element="C70" pad="1"/>
<contactref element="JP35" pad="1"/>
<contactref element="CC35" pad="2"/>
<contactref element="CC36" pad="2"/>
<contactref element="IC18" pad="33"/>
<contactref element="U18" pad="1"/>
<contactref element="U18" pad="7"/>
<contactref element="Q53" pad="3"/>
<contactref element="IC18" pad="10"/>
<contactref element="IC18" pad="9"/>
<contactref element="D18" pad="5"/>
<contactref element="Q54" pad="2"/>
</signal>
<signal name="N$154">
<contactref element="C72" pad="1"/>
<contactref element="Q52" pad="3"/>
<contactref element="IC18" pad="2"/>
</signal>
<signal name="N$155">
<contactref element="C71" pad="2"/>
<contactref element="IC18" pad="1"/>
<contactref element="Q52" pad="1"/>
</signal>
<signal name="N$156">
</signal>
<signal name="CC35">
<contactref element="J18" pad="B5"/>
<contactref element="CC36" pad="1"/>
</signal>
<signal name="CS17">
<contactref element="IC18" pad="14"/>
<contactref element="U18" pad="2"/>
</signal>
<signal name="DRAIN17">
</signal>
<signal name="COMPARE17">
<contactref element="VSENSE17" pad="2"/>
<contactref element="IC18" pad="7"/>
</signal>
<signal name="VSENSE17">
<contactref element="VSENSE17" pad="1"/>
<contactref element="Q53" pad="2"/>
</signal>
<signal name="CHARGE17">
<contactref element="CALIBRATOR17" pad="1"/>
<contactref element="IC18" pad="6"/>
<contactref element="IC18" pad="8"/>
</signal>
<signal name="CGROUND17">
<contactref element="CALIBRATOR17" pad="2"/>
<contactref element="IC18" pad="5"/>
</signal>
<signal name="N$157">
</signal>
<signal name="N$158">
</signal>
<signal name="N$159">
</signal>
<signal name="CC36">
<contactref element="J18" pad="A5"/>
<contactref element="CC35" pad="1"/>
</signal>
<signal name="N$160">
</signal>
<signal name="N$161">
</signal>
<signal name="5V17">
<contactref element="VIA18" pad="VIA1"/>
<contactref element="JP36" pad="SHIT"/>
<contactref element="J18" pad="B4"/>
<contactref element="J18" pad="A9"/>
<contactref element="J18" pad="A4"/>
<contactref element="J18" pad="B9"/>
<contactref element="IC18" pad="31"/>
<contactref element="C70" pad="2"/>
<contactref element="GATEPULLUP17" pad="2"/>
</signal>
<signal name="N$162">
</signal>
<signal name="VCC17">
<contactref element="U18" pad="8"/>
<contactref element="U18" pad="6"/>
<contactref element="C69" pad="1"/>
<contactref element="IC18" pad="27"/>
<contactref element="RESET17" pad="2"/>
<contactref element="D18" pad="1"/>
<contactref element="IC18" pad="4"/>
<contactref element="IC18" pad="32"/>
<contactref element="JP35" pad="5"/>
<contactref element="BASEPULLUP17" pad="2"/>
</signal>
<signal name="PWM17">
<contactref element="BASEPULLUP17" pad="1"/>
<contactref element="Q54" pad="1"/>
<contactref element="IC18" pad="13"/>
</signal>
<signal name="GATE17">
<contactref element="GATEPULLUP17" pad="1"/>
<contactref element="Q54" pad="3"/>
<contactref element="Q53" pad="1"/>
</signal>
<signal name="SCK18">
<contactref element="IC19" pad="15"/>
<contactref element="JP37" pad="4"/>
<contactref element="U19" pad="4"/>
</signal>
<signal name="MOSI18">
<contactref element="JP37" pad="3"/>
<contactref element="IC19" pad="16"/>
<contactref element="U19" pad="3"/>
</signal>
<signal name="MISO18">
<contactref element="JP37" pad="6"/>
<contactref element="IC19" pad="17"/>
<contactref element="U19" pad="5"/>
</signal>
<signal name="RESET18">
<contactref element="JP37" pad="2"/>
<contactref element="IC19" pad="24"/>
<contactref element="RESET18" pad="1"/>
</signal>
<signal name="D-18">
<contactref element="IC19" pad="30"/>
<contactref element="R-18" pad="1"/>
</signal>
<signal name="D+18">
<contactref element="IC19" pad="29"/>
<contactref element="R+18" pad="1"/>
</signal>
<signal name="R-18">
<contactref element="R-18" pad="2"/>
<contactref element="J19" pad="A7"/>
<contactref element="D19" pad="4"/>
</signal>
<signal name="R+18">
<contactref element="R+18" pad="2"/>
<contactref element="J19" pad="A6"/>
<contactref element="D19" pad="3"/>
</signal>
<signal name="GND18">
<contactref element="IC19" pad="28"/>
<contactref element="C73" pad="2"/>
<contactref element="J19" pad="A1"/>
<contactref element="J19" pad="A12"/>
<contactref element="J19" pad="B1"/>
<contactref element="J19" pad="B12"/>
<contactref element="C75" pad="1"/>
<contactref element="C76" pad="2"/>
<contactref element="IC19" pad="3"/>
<contactref element="C74" pad="1"/>
<contactref element="JP37" pad="1"/>
<contactref element="CC37" pad="2"/>
<contactref element="CC38" pad="2"/>
<contactref element="IC19" pad="33"/>
<contactref element="U19" pad="1"/>
<contactref element="U19" pad="7"/>
<contactref element="Q56" pad="3"/>
<contactref element="IC19" pad="10"/>
<contactref element="IC19" pad="9"/>
<contactref element="D19" pad="5"/>
<contactref element="Q57" pad="2"/>
</signal>
<signal name="N$163">
<contactref element="C76" pad="1"/>
<contactref element="Q55" pad="3"/>
<contactref element="IC19" pad="2"/>
</signal>
<signal name="N$164">
<contactref element="C75" pad="2"/>
<contactref element="IC19" pad="1"/>
<contactref element="Q55" pad="1"/>
</signal>
<signal name="N$165">
</signal>
<signal name="CC37">
<contactref element="J19" pad="B5"/>
<contactref element="CC38" pad="1"/>
</signal>
<signal name="CS18">
<contactref element="IC19" pad="14"/>
<contactref element="U19" pad="2"/>
</signal>
<signal name="DRAIN18">
</signal>
<signal name="COMPARE18">
<contactref element="VSENSE18" pad="2"/>
<contactref element="IC19" pad="7"/>
</signal>
<signal name="VSENSE18">
<contactref element="VSENSE18" pad="1"/>
<contactref element="Q56" pad="2"/>
</signal>
<signal name="CHARGE18">
<contactref element="CALIBRATOR18" pad="1"/>
<contactref element="IC19" pad="6"/>
<contactref element="IC19" pad="8"/>
</signal>
<signal name="CGROUND18">
<contactref element="CALIBRATOR18" pad="2"/>
<contactref element="IC19" pad="5"/>
</signal>
<signal name="N$166">
</signal>
<signal name="N$167">
</signal>
<signal name="N$168">
</signal>
<signal name="CC38">
<contactref element="J19" pad="A5"/>
<contactref element="CC37" pad="1"/>
</signal>
<signal name="N$169">
</signal>
<signal name="N$170">
</signal>
<signal name="5V18">
<contactref element="VIA19" pad="VIA1"/>
<contactref element="JP38" pad="SHIT"/>
<contactref element="J19" pad="B4"/>
<contactref element="J19" pad="A9"/>
<contactref element="J19" pad="A4"/>
<contactref element="J19" pad="B9"/>
<contactref element="IC19" pad="31"/>
<contactref element="C74" pad="2"/>
<contactref element="GATEPULLUP18" pad="2"/>
</signal>
<signal name="N$171">
</signal>
<signal name="VCC18">
<contactref element="U19" pad="8"/>
<contactref element="U19" pad="6"/>
<contactref element="C73" pad="1"/>
<contactref element="IC19" pad="27"/>
<contactref element="RESET18" pad="2"/>
<contactref element="D19" pad="1"/>
<contactref element="IC19" pad="4"/>
<contactref element="IC19" pad="32"/>
<contactref element="JP37" pad="5"/>
<contactref element="BASEPULLUP18" pad="2"/>
</signal>
<signal name="PWM18">
<contactref element="BASEPULLUP18" pad="1"/>
<contactref element="Q57" pad="1"/>
<contactref element="IC19" pad="13"/>
</signal>
<signal name="GATE18">
<contactref element="GATEPULLUP18" pad="1"/>
<contactref element="Q57" pad="3"/>
<contactref element="Q56" pad="1"/>
</signal>
<signal name="SCK19">
<contactref element="IC20" pad="15"/>
<contactref element="JP39" pad="4"/>
<contactref element="U20" pad="4"/>
</signal>
<signal name="MOSI19">
<contactref element="JP39" pad="3"/>
<contactref element="IC20" pad="16"/>
<contactref element="U20" pad="3"/>
</signal>
<signal name="MISO19">
<contactref element="JP39" pad="6"/>
<contactref element="IC20" pad="17"/>
<contactref element="U20" pad="5"/>
</signal>
<signal name="RESET19">
<contactref element="JP39" pad="2"/>
<contactref element="IC20" pad="24"/>
<contactref element="RESET19" pad="1"/>
</signal>
<signal name="D-19">
<contactref element="IC20" pad="30"/>
<contactref element="R-19" pad="1"/>
</signal>
<signal name="D+19">
<contactref element="IC20" pad="29"/>
<contactref element="R+19" pad="1"/>
</signal>
<signal name="R-19">
<contactref element="R-19" pad="2"/>
<contactref element="J20" pad="A7"/>
<contactref element="D20" pad="4"/>
</signal>
<signal name="R+19">
<contactref element="R+19" pad="2"/>
<contactref element="J20" pad="A6"/>
<contactref element="D20" pad="3"/>
</signal>
<signal name="GND19">
<contactref element="IC20" pad="28"/>
<contactref element="C77" pad="2"/>
<contactref element="J20" pad="A1"/>
<contactref element="J20" pad="A12"/>
<contactref element="J20" pad="B1"/>
<contactref element="J20" pad="B12"/>
<contactref element="C79" pad="1"/>
<contactref element="C80" pad="2"/>
<contactref element="IC20" pad="3"/>
<contactref element="C78" pad="1"/>
<contactref element="JP39" pad="1"/>
<contactref element="CC39" pad="2"/>
<contactref element="CC40" pad="2"/>
<contactref element="IC20" pad="33"/>
<contactref element="U20" pad="1"/>
<contactref element="U20" pad="7"/>
<contactref element="Q59" pad="3"/>
<contactref element="IC20" pad="10"/>
<contactref element="IC20" pad="9"/>
<contactref element="D20" pad="5"/>
<contactref element="Q60" pad="2"/>
</signal>
<signal name="N$172">
<contactref element="C80" pad="1"/>
<contactref element="Q58" pad="3"/>
<contactref element="IC20" pad="2"/>
</signal>
<signal name="N$173">
<contactref element="C79" pad="2"/>
<contactref element="IC20" pad="1"/>
<contactref element="Q58" pad="1"/>
</signal>
<signal name="N$174">
</signal>
<signal name="CC39">
<contactref element="J20" pad="B5"/>
<contactref element="CC40" pad="1"/>
</signal>
<signal name="CS19">
<contactref element="IC20" pad="14"/>
<contactref element="U20" pad="2"/>
</signal>
<signal name="DRAIN19">
</signal>
<signal name="COMPARE19">
<contactref element="VSENSE19" pad="2"/>
<contactref element="IC20" pad="7"/>
</signal>
<signal name="VSENSE19">
<contactref element="VSENSE19" pad="1"/>
<contactref element="Q59" pad="2"/>
</signal>
<signal name="CHARGE19">
<contactref element="CALIBRATOR19" pad="1"/>
<contactref element="IC20" pad="6"/>
<contactref element="IC20" pad="8"/>
</signal>
<signal name="CGROUND19">
<contactref element="CALIBRATOR19" pad="2"/>
<contactref element="IC20" pad="5"/>
</signal>
<signal name="N$175">
</signal>
<signal name="N$176">
</signal>
<signal name="N$177">
</signal>
<signal name="CC40">
<contactref element="J20" pad="A5"/>
<contactref element="CC39" pad="1"/>
</signal>
<signal name="N$178">
</signal>
<signal name="N$179">
</signal>
<signal name="5V19">
<contactref element="VIA20" pad="VIA1"/>
<contactref element="JP40" pad="SHIT"/>
<contactref element="J20" pad="B4"/>
<contactref element="J20" pad="A9"/>
<contactref element="J20" pad="A4"/>
<contactref element="J20" pad="B9"/>
<contactref element="IC20" pad="31"/>
<contactref element="C78" pad="2"/>
<contactref element="GATEPULLUP19" pad="2"/>
</signal>
<signal name="N$180">
</signal>
<signal name="VCC19">
<contactref element="U20" pad="8"/>
<contactref element="U20" pad="6"/>
<contactref element="C77" pad="1"/>
<contactref element="IC20" pad="27"/>
<contactref element="RESET19" pad="2"/>
<contactref element="D20" pad="1"/>
<contactref element="IC20" pad="4"/>
<contactref element="IC20" pad="32"/>
<contactref element="JP39" pad="5"/>
<contactref element="BASEPULLUP19" pad="2"/>
</signal>
<signal name="PWM19">
<contactref element="BASEPULLUP19" pad="1"/>
<contactref element="Q60" pad="1"/>
<contactref element="IC20" pad="13"/>
</signal>
<signal name="GATE19">
<contactref element="GATEPULLUP19" pad="1"/>
<contactref element="Q60" pad="3"/>
<contactref element="Q59" pad="1"/>
</signal>
<signal name="SCK20">
<contactref element="IC21" pad="15"/>
<contactref element="JP41" pad="4"/>
<contactref element="U21" pad="4"/>
</signal>
<signal name="MOSI20">
<contactref element="JP41" pad="3"/>
<contactref element="IC21" pad="16"/>
<contactref element="U21" pad="3"/>
</signal>
<signal name="MISO20">
<contactref element="JP41" pad="6"/>
<contactref element="IC21" pad="17"/>
<contactref element="U21" pad="5"/>
</signal>
<signal name="RESET20">
<contactref element="JP41" pad="2"/>
<contactref element="IC21" pad="24"/>
<contactref element="RESET20" pad="1"/>
</signal>
<signal name="D-20">
<contactref element="IC21" pad="30"/>
<contactref element="R-20" pad="1"/>
</signal>
<signal name="D+20">
<contactref element="IC21" pad="29"/>
<contactref element="R+20" pad="1"/>
</signal>
<signal name="R-20">
<contactref element="R-20" pad="2"/>
<contactref element="J21" pad="A7"/>
<contactref element="D21" pad="4"/>
</signal>
<signal name="R+20">
<contactref element="R+20" pad="2"/>
<contactref element="J21" pad="A6"/>
<contactref element="D21" pad="3"/>
</signal>
<signal name="GND20">
<contactref element="IC21" pad="28"/>
<contactref element="C81" pad="2"/>
<contactref element="J21" pad="A1"/>
<contactref element="J21" pad="A12"/>
<contactref element="J21" pad="B1"/>
<contactref element="J21" pad="B12"/>
<contactref element="C83" pad="1"/>
<contactref element="C84" pad="2"/>
<contactref element="IC21" pad="3"/>
<contactref element="C82" pad="1"/>
<contactref element="JP41" pad="1"/>
<contactref element="CC41" pad="2"/>
<contactref element="CC42" pad="2"/>
<contactref element="IC21" pad="33"/>
<contactref element="U21" pad="1"/>
<contactref element="U21" pad="7"/>
<contactref element="Q62" pad="3"/>
<contactref element="IC21" pad="10"/>
<contactref element="IC21" pad="9"/>
<contactref element="D21" pad="5"/>
<contactref element="Q63" pad="2"/>
</signal>
<signal name="N$181">
<contactref element="C84" pad="1"/>
<contactref element="Q61" pad="3"/>
<contactref element="IC21" pad="2"/>
</signal>
<signal name="N$182">
<contactref element="C83" pad="2"/>
<contactref element="IC21" pad="1"/>
<contactref element="Q61" pad="1"/>
</signal>
<signal name="N$183">
</signal>
<signal name="CC41">
<contactref element="J21" pad="B5"/>
<contactref element="CC42" pad="1"/>
</signal>
<signal name="CS20">
<contactref element="IC21" pad="14"/>
<contactref element="U21" pad="2"/>
</signal>
<signal name="DRAIN20">
</signal>
<signal name="COMPARE20">
<contactref element="VSENSE20" pad="2"/>
<contactref element="IC21" pad="7"/>
</signal>
<signal name="VSENSE20">
<contactref element="VSENSE20" pad="1"/>
<contactref element="Q62" pad="2"/>
</signal>
<signal name="CHARGE20">
<contactref element="CALIBRATOR20" pad="1"/>
<contactref element="IC21" pad="6"/>
<contactref element="IC21" pad="8"/>
</signal>
<signal name="CGROUND20">
<contactref element="CALIBRATOR20" pad="2"/>
<contactref element="IC21" pad="5"/>
</signal>
<signal name="N$184">
</signal>
<signal name="N$185">
</signal>
<signal name="N$186">
</signal>
<signal name="CC42">
<contactref element="J21" pad="A5"/>
<contactref element="CC41" pad="1"/>
</signal>
<signal name="N$187">
</signal>
<signal name="N$188">
</signal>
<signal name="5V20">
<contactref element="VIA21" pad="VIA1"/>
<contactref element="JP42" pad="SHIT"/>
<contactref element="J21" pad="B4"/>
<contactref element="J21" pad="A9"/>
<contactref element="J21" pad="A4"/>
<contactref element="J21" pad="B9"/>
<contactref element="IC21" pad="31"/>
<contactref element="C82" pad="2"/>
<contactref element="GATEPULLUP20" pad="2"/>
</signal>
<signal name="N$189">
</signal>
<signal name="VCC20">
<contactref element="U21" pad="8"/>
<contactref element="U21" pad="6"/>
<contactref element="C81" pad="1"/>
<contactref element="IC21" pad="27"/>
<contactref element="RESET20" pad="2"/>
<contactref element="D21" pad="1"/>
<contactref element="IC21" pad="4"/>
<contactref element="IC21" pad="32"/>
<contactref element="JP41" pad="5"/>
<contactref element="BASEPULLUP20" pad="2"/>
</signal>
<signal name="PWM20">
<contactref element="BASEPULLUP20" pad="1"/>
<contactref element="Q63" pad="1"/>
<contactref element="IC21" pad="13"/>
</signal>
<signal name="GATE20">
<contactref element="GATEPULLUP20" pad="1"/>
<contactref element="Q63" pad="3"/>
<contactref element="Q62" pad="1"/>
</signal>
<signal name="SCK21">
<contactref element="IC22" pad="15"/>
<contactref element="JP43" pad="4"/>
<contactref element="U22" pad="4"/>
</signal>
<signal name="MOSI21">
<contactref element="JP43" pad="3"/>
<contactref element="IC22" pad="16"/>
<contactref element="U22" pad="3"/>
</signal>
<signal name="MISO21">
<contactref element="JP43" pad="6"/>
<contactref element="IC22" pad="17"/>
<contactref element="U22" pad="5"/>
</signal>
<signal name="RESET21">
<contactref element="JP43" pad="2"/>
<contactref element="IC22" pad="24"/>
<contactref element="RESET21" pad="1"/>
</signal>
<signal name="D-21">
<contactref element="IC22" pad="30"/>
<contactref element="R-21" pad="1"/>
</signal>
<signal name="D+21">
<contactref element="IC22" pad="29"/>
<contactref element="R+21" pad="1"/>
</signal>
<signal name="R-21">
<contactref element="R-21" pad="2"/>
<contactref element="J22" pad="A7"/>
<contactref element="D22" pad="4"/>
</signal>
<signal name="R+21">
<contactref element="R+21" pad="2"/>
<contactref element="J22" pad="A6"/>
<contactref element="D22" pad="3"/>
</signal>
<signal name="GND21">
<contactref element="IC22" pad="28"/>
<contactref element="C85" pad="2"/>
<contactref element="J22" pad="A1"/>
<contactref element="J22" pad="A12"/>
<contactref element="J22" pad="B1"/>
<contactref element="J22" pad="B12"/>
<contactref element="C87" pad="1"/>
<contactref element="C88" pad="2"/>
<contactref element="IC22" pad="3"/>
<contactref element="C86" pad="1"/>
<contactref element="JP43" pad="1"/>
<contactref element="CC43" pad="2"/>
<contactref element="CC44" pad="2"/>
<contactref element="IC22" pad="33"/>
<contactref element="U22" pad="1"/>
<contactref element="U22" pad="7"/>
<contactref element="Q65" pad="3"/>
<contactref element="IC22" pad="10"/>
<contactref element="IC22" pad="9"/>
<contactref element="D22" pad="5"/>
<contactref element="Q66" pad="2"/>
</signal>
<signal name="N$190">
<contactref element="C88" pad="1"/>
<contactref element="Q64" pad="3"/>
<contactref element="IC22" pad="2"/>
</signal>
<signal name="N$191">
<contactref element="C87" pad="2"/>
<contactref element="IC22" pad="1"/>
<contactref element="Q64" pad="1"/>
</signal>
<signal name="N$192">
</signal>
<signal name="CC43">
<contactref element="J22" pad="B5"/>
<contactref element="CC44" pad="1"/>
</signal>
<signal name="CS21">
<contactref element="IC22" pad="14"/>
<contactref element="U22" pad="2"/>
</signal>
<signal name="DRAIN21">
</signal>
<signal name="COMPARE21">
<contactref element="VSENSE21" pad="2"/>
<contactref element="IC22" pad="7"/>
</signal>
<signal name="VSENSE21">
<contactref element="VSENSE21" pad="1"/>
<contactref element="Q65" pad="2"/>
</signal>
<signal name="CHARGE21">
<contactref element="CALIBRATOR21" pad="1"/>
<contactref element="IC22" pad="6"/>
<contactref element="IC22" pad="8"/>
</signal>
<signal name="CGROUND21">
<contactref element="CALIBRATOR21" pad="2"/>
<contactref element="IC22" pad="5"/>
</signal>
<signal name="N$193">
</signal>
<signal name="N$194">
</signal>
<signal name="N$195">
</signal>
<signal name="CC44">
<contactref element="J22" pad="A5"/>
<contactref element="CC43" pad="1"/>
</signal>
<signal name="N$196">
</signal>
<signal name="N$197">
</signal>
<signal name="5V21">
<contactref element="VIA22" pad="VIA1"/>
<contactref element="JP44" pad="SHIT"/>
<contactref element="J22" pad="B4"/>
<contactref element="J22" pad="A9"/>
<contactref element="J22" pad="A4"/>
<contactref element="J22" pad="B9"/>
<contactref element="IC22" pad="31"/>
<contactref element="C86" pad="2"/>
<contactref element="GATEPULLUP21" pad="2"/>
</signal>
<signal name="N$198">
</signal>
<signal name="VCC21">
<contactref element="U22" pad="8"/>
<contactref element="U22" pad="6"/>
<contactref element="C85" pad="1"/>
<contactref element="IC22" pad="27"/>
<contactref element="RESET21" pad="2"/>
<contactref element="D22" pad="1"/>
<contactref element="IC22" pad="4"/>
<contactref element="IC22" pad="32"/>
<contactref element="JP43" pad="5"/>
<contactref element="BASEPULLUP21" pad="2"/>
</signal>
<signal name="PWM21">
<contactref element="BASEPULLUP21" pad="1"/>
<contactref element="Q66" pad="1"/>
<contactref element="IC22" pad="13"/>
</signal>
<signal name="GATE21">
<contactref element="GATEPULLUP21" pad="1"/>
<contactref element="Q66" pad="3"/>
<contactref element="Q65" pad="1"/>
</signal>
<signal name="SCK22">
<contactref element="IC23" pad="15"/>
<contactref element="JP45" pad="4"/>
<contactref element="U23" pad="4"/>
</signal>
<signal name="MOSI22">
<contactref element="JP45" pad="3"/>
<contactref element="IC23" pad="16"/>
<contactref element="U23" pad="3"/>
</signal>
<signal name="MISO22">
<contactref element="JP45" pad="6"/>
<contactref element="IC23" pad="17"/>
<contactref element="U23" pad="5"/>
</signal>
<signal name="RESET22">
<contactref element="JP45" pad="2"/>
<contactref element="IC23" pad="24"/>
<contactref element="RESET22" pad="1"/>
</signal>
<signal name="D-22">
<contactref element="IC23" pad="30"/>
<contactref element="R-22" pad="1"/>
</signal>
<signal name="D+22">
<contactref element="IC23" pad="29"/>
<contactref element="R+22" pad="1"/>
</signal>
<signal name="R-22">
<contactref element="R-22" pad="2"/>
<contactref element="J23" pad="A7"/>
<contactref element="D23" pad="4"/>
</signal>
<signal name="R+22">
<contactref element="R+22" pad="2"/>
<contactref element="J23" pad="A6"/>
<contactref element="D23" pad="3"/>
</signal>
<signal name="GND22">
<contactref element="IC23" pad="28"/>
<contactref element="C89" pad="2"/>
<contactref element="J23" pad="A1"/>
<contactref element="J23" pad="A12"/>
<contactref element="J23" pad="B1"/>
<contactref element="J23" pad="B12"/>
<contactref element="C91" pad="1"/>
<contactref element="C92" pad="2"/>
<contactref element="IC23" pad="3"/>
<contactref element="C90" pad="1"/>
<contactref element="JP45" pad="1"/>
<contactref element="CC45" pad="2"/>
<contactref element="CC46" pad="2"/>
<contactref element="IC23" pad="33"/>
<contactref element="U23" pad="1"/>
<contactref element="U23" pad="7"/>
<contactref element="Q68" pad="3"/>
<contactref element="IC23" pad="10"/>
<contactref element="IC23" pad="9"/>
<contactref element="D23" pad="5"/>
<contactref element="Q69" pad="2"/>
</signal>
<signal name="N$199">
<contactref element="C92" pad="1"/>
<contactref element="Q67" pad="3"/>
<contactref element="IC23" pad="2"/>
</signal>
<signal name="N$200">
<contactref element="C91" pad="2"/>
<contactref element="IC23" pad="1"/>
<contactref element="Q67" pad="1"/>
</signal>
<signal name="N$201">
</signal>
<signal name="CC45">
<contactref element="J23" pad="B5"/>
<contactref element="CC46" pad="1"/>
</signal>
<signal name="CS22">
<contactref element="IC23" pad="14"/>
<contactref element="U23" pad="2"/>
</signal>
<signal name="DRAIN22">
</signal>
<signal name="COMPARE22">
<contactref element="VSENSE22" pad="2"/>
<contactref element="IC23" pad="7"/>
</signal>
<signal name="VSENSE22">
<contactref element="VSENSE22" pad="1"/>
<contactref element="Q68" pad="2"/>
</signal>
<signal name="CHARGE22">
<contactref element="CALIBRATOR22" pad="1"/>
<contactref element="IC23" pad="6"/>
<contactref element="IC23" pad="8"/>
</signal>
<signal name="CGROUND22">
<contactref element="CALIBRATOR22" pad="2"/>
<contactref element="IC23" pad="5"/>
</signal>
<signal name="N$202">
</signal>
<signal name="N$203">
</signal>
<signal name="N$204">
</signal>
<signal name="CC46">
<contactref element="J23" pad="A5"/>
<contactref element="CC45" pad="1"/>
</signal>
<signal name="N$205">
</signal>
<signal name="N$206">
</signal>
<signal name="5V22">
<contactref element="VIA23" pad="VIA1"/>
<contactref element="JP46" pad="SHIT"/>
<contactref element="J23" pad="B4"/>
<contactref element="J23" pad="A9"/>
<contactref element="J23" pad="A4"/>
<contactref element="J23" pad="B9"/>
<contactref element="IC23" pad="31"/>
<contactref element="C90" pad="2"/>
<contactref element="GATEPULLUP22" pad="2"/>
</signal>
<signal name="N$207">
</signal>
<signal name="VCC22">
<contactref element="U23" pad="8"/>
<contactref element="U23" pad="6"/>
<contactref element="C89" pad="1"/>
<contactref element="IC23" pad="27"/>
<contactref element="RESET22" pad="2"/>
<contactref element="D23" pad="1"/>
<contactref element="IC23" pad="4"/>
<contactref element="IC23" pad="32"/>
<contactref element="JP45" pad="5"/>
<contactref element="BASEPULLUP22" pad="2"/>
</signal>
<signal name="PWM22">
<contactref element="BASEPULLUP22" pad="1"/>
<contactref element="Q69" pad="1"/>
<contactref element="IC23" pad="13"/>
</signal>
<signal name="GATE22">
<contactref element="GATEPULLUP22" pad="1"/>
<contactref element="Q69" pad="3"/>
<contactref element="Q68" pad="1"/>
</signal>
<signal name="SCK23">
<contactref element="IC24" pad="15"/>
<contactref element="JP47" pad="4"/>
<contactref element="U24" pad="4"/>
</signal>
<signal name="MOSI23">
<contactref element="JP47" pad="3"/>
<contactref element="IC24" pad="16"/>
<contactref element="U24" pad="3"/>
</signal>
<signal name="MISO23">
<contactref element="JP47" pad="6"/>
<contactref element="IC24" pad="17"/>
<contactref element="U24" pad="5"/>
</signal>
<signal name="RESET23">
<contactref element="JP47" pad="2"/>
<contactref element="IC24" pad="24"/>
<contactref element="RESET23" pad="1"/>
</signal>
<signal name="D-23">
<contactref element="IC24" pad="30"/>
<contactref element="R-23" pad="1"/>
</signal>
<signal name="D+23">
<contactref element="IC24" pad="29"/>
<contactref element="R+23" pad="1"/>
</signal>
<signal name="R-23">
<contactref element="R-23" pad="2"/>
<contactref element="J24" pad="A7"/>
<contactref element="D24" pad="4"/>
</signal>
<signal name="R+23">
<contactref element="R+23" pad="2"/>
<contactref element="J24" pad="A6"/>
<contactref element="D24" pad="3"/>
</signal>
<signal name="GND23">
<contactref element="IC24" pad="28"/>
<contactref element="C93" pad="2"/>
<contactref element="J24" pad="A1"/>
<contactref element="J24" pad="A12"/>
<contactref element="J24" pad="B1"/>
<contactref element="J24" pad="B12"/>
<contactref element="C95" pad="1"/>
<contactref element="C96" pad="2"/>
<contactref element="IC24" pad="3"/>
<contactref element="C94" pad="1"/>
<contactref element="JP47" pad="1"/>
<contactref element="CC47" pad="2"/>
<contactref element="CC48" pad="2"/>
<contactref element="IC24" pad="33"/>
<contactref element="U24" pad="1"/>
<contactref element="U24" pad="7"/>
<contactref element="Q71" pad="3"/>
<contactref element="IC24" pad="10"/>
<contactref element="IC24" pad="9"/>
<contactref element="D24" pad="5"/>
<contactref element="Q72" pad="2"/>
</signal>
<signal name="N$208">
<contactref element="C96" pad="1"/>
<contactref element="Q70" pad="3"/>
<contactref element="IC24" pad="2"/>
</signal>
<signal name="N$209">
<contactref element="C95" pad="2"/>
<contactref element="IC24" pad="1"/>
<contactref element="Q70" pad="1"/>
</signal>
<signal name="N$210">
</signal>
<signal name="CC47">
<contactref element="J24" pad="B5"/>
<contactref element="CC48" pad="1"/>
</signal>
<signal name="CS23">
<contactref element="IC24" pad="14"/>
<contactref element="U24" pad="2"/>
</signal>
<signal name="DRAIN23">
</signal>
<signal name="COMPARE23">
<contactref element="VSENSE23" pad="2"/>
<contactref element="IC24" pad="7"/>
</signal>
<signal name="VSENSE23">
<contactref element="VSENSE23" pad="1"/>
<contactref element="Q71" pad="2"/>
</signal>
<signal name="CHARGE23">
<contactref element="CALIBRATOR23" pad="1"/>
<contactref element="IC24" pad="6"/>
<contactref element="IC24" pad="8"/>
</signal>
<signal name="CGROUND23">
<contactref element="CALIBRATOR23" pad="2"/>
<contactref element="IC24" pad="5"/>
</signal>
<signal name="N$211">
</signal>
<signal name="N$212">
</signal>
<signal name="N$213">
</signal>
<signal name="CC48">
<contactref element="J24" pad="A5"/>
<contactref element="CC47" pad="1"/>
</signal>
<signal name="N$214">
</signal>
<signal name="N$215">
</signal>
<signal name="5V23">
<contactref element="VIA24" pad="VIA1"/>
<contactref element="JP48" pad="SHIT"/>
<contactref element="J24" pad="B4"/>
<contactref element="J24" pad="A9"/>
<contactref element="J24" pad="A4"/>
<contactref element="J24" pad="B9"/>
<contactref element="IC24" pad="31"/>
<contactref element="C94" pad="2"/>
<contactref element="GATEPULLUP23" pad="2"/>
</signal>
<signal name="N$216">
</signal>
<signal name="VCC23">
<contactref element="U24" pad="8"/>
<contactref element="U24" pad="6"/>
<contactref element="C93" pad="1"/>
<contactref element="IC24" pad="27"/>
<contactref element="RESET23" pad="2"/>
<contactref element="D24" pad="1"/>
<contactref element="IC24" pad="4"/>
<contactref element="IC24" pad="32"/>
<contactref element="JP47" pad="5"/>
<contactref element="BASEPULLUP23" pad="2"/>
</signal>
<signal name="PWM23">
<contactref element="BASEPULLUP23" pad="1"/>
<contactref element="Q72" pad="1"/>
<contactref element="IC24" pad="13"/>
</signal>
<signal name="GATE23">
<contactref element="GATEPULLUP23" pad="1"/>
<contactref element="Q72" pad="3"/>
<contactref element="Q71" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
