(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 39)
    (no_connects 1)
    (area 101.15 104.6825 135.740096 123.465714)
    (thickness 1.6)
    (drawings 7)
    (tracks 200)
    (zones 0)
    (modules 11)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x00008_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ./))
  )
  (net 0 "")
  (net 1 SWDIO)
  (net 2 VDD)
  (net 3 SWDCLK)
  (net 4 GND)
  (net 5 RESET)
  (net 6 MOSI)
  (net 7 SCK)
  (net 8 MISO)
  (net 9 DFU)
  (net 10 CS_Baro)
  (net 11 CS_Flash)
  (net 12 VBATT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CS_Baro)
    (add_net CS_Flash)
    (add_net DFU)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net RESET)
    (add_net SCK)
    (add_net SWDCLK)
    (add_net SWDIO)
    (add_net VBATT)
    (add_net VDD)
  )
  (module lib:BL651 (layer F.Cu) (tedit 5C3AC5BF)
    (at 101.6 115.443 90)
    (fp_text reference U1 (at 0 10.5 90) (layer F.SilkS) hide)
    (fp_text value bl651 (at 0 9.5 90) (layer F.Fab))
    (pad 17 smd rect (at 3.75 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 3 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 2.25 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 1.5 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 0.75 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 22 smd rect (at 0 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 SCK))
    (pad 23 smd rect (at -0.75 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at -1.5 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at -2.25 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at -3 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 27 smd rect (at -3.75 13.9 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 28 smd rect (at -4.9 13.45 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -4.9 12.7 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at -4.9 11.95 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at -4.9 11.2 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at -4.9 10.45 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at -4.9 9.7 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at -4.9 8.95 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 CS_Baro))
    (pad 35 smd rect (at -4.9 8.2 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 MISO))
    (pad 36 smd rect (at -4.9 7.45 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at -4.9 6.7 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at -4.9 5.95 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at -4.9 5.2 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 4.9 2.2 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 4.9 2.95 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 4.9 3.7 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 4.9 4.45 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 4.9 5.2 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 SWDIO))
    (pad 6 smd rect (at 4.9 5.95 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 SWDCLK))
    (pad 7 smd rect (at 4.9 6.7 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 RESET))
    (pad 8 smd rect (at 4.9 7.45 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 4.9 8.2 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 4.9 8.95 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 DFU))
    (pad 11 smd rect (at 4.9 9.7 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 4.9 10.45 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 4.9 11.2 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 4.9 11.95 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 4.9 12.7 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 CS_Flash))
    (pad 16 smd rect (at 4.9 13.45 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C3AC651)
    (at 117.475 119.38 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:bt (layer F.Cu) (tedit 5C3AC5F3)
    (at 125.476 119.38 90)
    (fp_text reference SW2 (at -0.381 0 180) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at -1.6002 -2.624963 90) (size 0.999998 1.549908) (layers F.Cu F.Paste F.Mask)
      (net 9 DFU))
    (pad 2 smd rect (at -1.6002 2.624963 90) (size 0.999998 1.549908) (layers F.Cu F.Paste F.Mask)
      (net 9 DFU))
    (pad 1 smd rect (at 1.6002 -2.624963 90) (size 0.999998 1.549908) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 1.6002 2.624963 90) (size 0.999998 1.549908) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5C4D28A6)
    (at 123.698 115.824)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:SO8 (layer F.Cu) (tedit 5C4D289C)
    (at 120.015 110.871 180)
    (fp_text reference U3 (at -3.905 0 270) (layer F.SilkS) hide)
    (fp_text value EEPROM (at 0 0 180) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -2.65 180) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 1 smd rect (at -1.905 2.65 180) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 11 CS_Flash))
    (pad 7 smd rect (at -0.635 -2.65 180) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at -0.635 2.65 180) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 MISO))
    (pad 6 smd rect (at 0.635 -2.65 180) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 SCK))
    (pad 3 smd rect (at 0.635 2.65 180) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 5 smd rect (at 1.905 -2.65 180) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 4 smd rect (at 1.905 2.65 180) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module lib:5pad_test (layer F.Cu) (tedit 5C4D2922)
    (at 109.474 108.204)
    (solder_paste_margin -0.9525)
    (fp_text reference J1 (at 0 2.4065) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 -2.4065) (layer F.Fab))
    (pad 1 smd rect (at -5.08 0) (size 1.905 1.905) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -2.54 0) (size 1.905 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 SWDIO))
    (pad 3 smd rect (at 0 0) (size 1.905 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 SWDCLK))
    (pad 4 smd rect (at 2.54 0) (size 1.905 1.905) (layers F.Cu F.Paste F.Mask)
      (net 5 RESET))
    (pad 5 smd rect (at 5.08 0) (size 1.905 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
  )
  (module lib:BMP388 (layer F.Cu) (tedit 5C4D28B1)
    (at 120.142 118.11)
    (fp_text reference U2 (at 0.5 -2.074999) (layer F.SilkS) hide)
    (fp_text value BMP380 (at 0.25 2) (layer F.Fab))
    (pad 6 smd rect (at -0.25 0.7625) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 10 CS_Baro))
    (pad 7 smd rect (at 0.25 0.7625) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.25 -0.7625) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at -0.25 -0.7625) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 7 SCK))
    (pad 10 smd rect (at 0.7625 -0.5 270) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 3 smd rect (at -0.7625 -0.5 270) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 9 smd rect (at 0.7625 0 270) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -0.7625 0 270) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 8 smd rect (at 0.7625 0.5 270) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 5 smd rect (at -0.7625 0.5 270) (size 0.25 0.275) (layers F.Cu F.Paste F.Mask)
      (net 8 MISO))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5C4D2893)
    (at 124.079 110.871 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:1225_glider (layer B.Cu) (tedit 5C687986)
    (at 118.11 113.792 180)
    (fp_text reference BT1 (at 0.254 -3.556 180) (layer B.SilkS) hide)
    (fp_text value Battery_Cell (at -0.254 3.81 180) (layer B.Fab))
    (pad 1 smd rect (at -9.144 0 180) (size 2.54 6.604) (layers B.Cu B.Paste B.Mask)
      (net 12 VBATT))
    (pad 2 smd rect (at 0 0 180) (size 5.08 5.08) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 9.144 0 180) (size 2.54 6.604) (layers B.Cu B.Paste B.Mask)
      (net 12 VBATT))
  )
  (module lib:sw2 (layer F.Cu) (tedit 5C4D271B)
    (at 127.635 111.76 270)
    (fp_text reference SW1 (at 2.667 2.794 270) (layer F.SilkS) hide)
    (fp_text value SW_DPDT_x2 (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at -2.499995 -1.199997 270) (size 0.999998 1.599946) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.499995 1.199997 270) (size 0.999998 1.599946) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 5 smd rect (at 0 -1.199997 270) (size 0.999998 1.599946) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 1.199997 270) (size 0.999998 1.599946) (layers F.Cu F.Paste F.Mask)
      (net 12 VBATT))
    (pad 6 smd rect (at 2.499995 -1.199997 270) (size 0.999998 1.599946) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 2.499995 1.199997 270) (size 0.999998 1.599946) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at 3.40106 0 270) (size 0.9017 0.9017) (drill 0.9017) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.400044 0 270) (size 0.9017 0.9017) (drill 0.9017) (layers *.Cu *.Mask))
  )
  (module lib:mounting_slot (layer F.Cu) (tedit 5C68C11D)
    (at 130.302 119.126)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value mounting_slot (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 1.905 3.81) (drill oval 1.905 3.81) (layers *.Cu *.Mask))
  )
  (gr_text "Mini rev-0a" (at 130.81 111.125 90) (layer B.SilkS))
  (gr_text "OFF  ON" (at 130.81 112.395 90) (layer F.SilkS))
  (gr_line (start 102.87 106.68) (end 102.87 121.92) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 132.08 106.68) (end 102.87 106.68) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 132.08 121.92) (end 132.08 106.68) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 102.87 121.92) (end 132.08 121.92) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text flightsketch.com (at 105.0925 114.554 90) (layer B.SilkS))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.68 121.412) (xy 131.572 121.412) (xy 131.572 107.188) (xy 106.68 107.188)
      )
    )
  )
)
