(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 141)
    (zones 0)
    (modules 37)
    (nets 19)
  )
  (page A4)
  (title_block
    (title Voltage_Current_Source)
    (rev v01)
    (company FRIB)
    (comment 4 "Author: Mike Scherer")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.000762)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDREF)
  (net 2 "Net-(BT1-Pad1)")
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(R2-Pad2)")
  (net 10 "Net-(R12-Pad1)")
  (net 11 "Net-(R6-Pad1)")
  (net 12 "Net-(R13-Pad1)")
  (net 13 "Net-(R7-Pad1)")
  (net 14 "Net-(R8-Pad1)")
  (net 15 "Net-(R9-Pad1)")
  (net 16 "Net-(R10-Pad1)")
  (net 17 "Net-(RV5-Pad2)")
  (net 18 "Net-(RV6-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDREF)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(RV5-Pad2)")
    (add_net "Net-(RV6-Pad2)")
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 158.7 76.58)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 63.5 76.58)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 63.5 121.92)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 158.7 121.92)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.331 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Battery:BatteryHolder_Eagle_12BH611-GR (layer F.Cu) (tedit 5BFC95F9)
    (at 88.9 74.93 90)
    (descr https://eu.mouser.com/datasheet/2/209/EPD-200766-1274481.pdf)
    (tags "9V Battery Holder")
    (fp_text reference "9V Battery" (at -24.13 -24.13 90) (layer F.SilkS))
    (fp_text value 9V (at -24.13 11.43 270) (layer F.Fab))
    (fp_text user + (at -7 0 90) (layer F.Fab))
    (fp_text user - (at -7 -12.7 90) (layer F.Fab))
    (fp_text user %R (at -24.13 -6.35 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -12.7 90) (size 3 3) (drill 2.4) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 2.4) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad "" np_thru_hole circle (at -10.9 -17.45 90) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -38.9 -17.45 90) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -24.9 4.75 90) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Eagle_12BH611-GR.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 112.3045 101.854)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value .01uF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.4 (layer F.Cu) (tedit 5BCA39CF)
    (at 112.522 108.458)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic A5 / Nichicon, 4.0x5.4mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at 0 -3.2) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 115.162 114.6175)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value .001uF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GNDREF))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.4 (layer F.Cu) (tedit 5BCA39CF)
    (at 103.654 108.458)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic A5 / Nichicon, 4.0x5.4mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C4 (at 0 -3.2) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 GNDREF))
    (pad 1 smd roundrect (at -1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 107.443 84.201)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2) (layer F.SilkS))
    (fp_text value 1N5819 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 586419F0)
    (at 101.408 88.265 180)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D2 (at 0 -1.3) (layer F.SilkS))
    (fp_text value 1N914 (at 0 1.4) (layer F.Fab))
    (fp_text user %R (at 0 -1.3) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 113.538 77.47)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value K150 (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:RF_SMA_RightAngle_5-1814400-1 (layer F.Cu) (tedit 5A4BE44C)
    (at 175.768 110.998 270)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1814400&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference J1 (at 5.7785 0.127 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial_Power (at 0 6.27 90) (layer F.Fab))
    (fp_text user %R (at -5.207 1.27 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 2 thru_hole circle (at -2.54 -2.54 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 2 thru_hole circle (at 2.54 2.54 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
  )
  (module Resistor_SMD:R_0612_1632Metric_Pad1.18x3.40mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 110.744 89.2295 90)
    (descr "Resistor SMD 0612 (1632 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.vishay.com/docs/20019/rcwe.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -2.65 90) (layer F.SilkS))
    (fp_text value 560 (at 0 2.65 90) (layer F.Fab))
    (fp_text user %R (at -0.8375 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8375 0 90) (size 1.175 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.8375 0 90) (size 1.175 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0612_1632Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 101.473 93.6355 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 14.9K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 106.68 93.6355 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 24.9K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 "Net-(R2-Pad2)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 112.3045 97.028)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.222 109.728 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 221K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.2585 104.394 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 221K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.2585 99.314 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 53.6K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(R7-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.2585 93.726 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 26.1K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.2585 88.646 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 5.11K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(R9-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.2585 77.724 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 5.11K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 16 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.222 83.058 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 4.99K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 16 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.2585 114.808)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0.0905 1.905) (layer F.SilkS))
    (fp_text value 47K (at 0.0905 -1.778) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GNDREF))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.2585 120.269 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 390K (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 "Net-(R13-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296Y_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 138.684 102.489)
    (descr "Potentiometer, vertical, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296Y")
    (fp_text reference RV1 (at -2.54 -2.39) (layer F.SilkS))
    (fp_text value 1M (at -2.54 4.94) (layer F.Fab))
    (fp_text user %R (at -3.175 1.275) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296Y_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296Y_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 138.684 93.472)
    (descr "Potentiometer, vertical, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296Y")
    (fp_text reference RV2 (at -2.54 -2.39) (layer F.SilkS))
    (fp_text value 1M (at -2.54 4.94) (layer F.Fab))
    (fp_text user %R (at -3.175 1.275) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R8-Pad1)"))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296Y_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296Y_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 138.684 84.582)
    (descr "Potentiometer, vertical, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296Y")
    (fp_text reference RV3 (at -2.54 -2.39) (layer F.SilkS))
    (fp_text value 1M (at -2.54 4.94) (layer F.Fab))
    (fp_text user %R (at -3.175 1.275) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R9-Pad1)"))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296Y_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296Y_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 138.684 75.692)
    (descr "Potentiometer, vertical, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296Y")
    (fp_text reference RV4 (at -2.54 -2.39) (layer F.SilkS))
    (fp_text value 1M (at -2.54 4.94) (layer F.Fab))
    (fp_text user %R (at -3.175 1.275) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296Y_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296Y_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 138.684 111.379)
    (descr "Potentiometer, vertical, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296Y")
    (fp_text reference RV5 (at -2.54 -2.39) (layer F.SilkS))
    (fp_text value 100K (at -2.54 4.94) (layer F.Fab))
    (fp_text user %R (at -3.175 1.275) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R6-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(RV5-Pad2)"))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296Y_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296Y_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 138.684 120.269)
    (descr "Potentiometer, vertical, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296Y")
    (fp_text reference RV6 (at -2.54 -2.39) (layer F.SilkS))
    (fp_text value 100K (at -2.54 4.94) (layer F.Fab))
    (fp_text user %R (at -3.175 1.275) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(RV6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296Y_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOIC-8_W3.9mm (layer F.Cu) (tedit 5D28A544)
    (at 105.029 120.56 180)
    (attr smd)
    (fp_text reference U1 (at -0.0127 -4.9922) (layer F.SilkS))
    (fp_text value ADR4525BRZ-R7 (at 0.06604 4.80314) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.905 2.45 180) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.635 2.45 180) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1.905 2.45 180) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 5 smd rect (at 1.905 -2.45 180) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.635 -2.45 180) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 7 smd rect (at -0.635 -2.45 180) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -1.905 -2.45 180) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.635 2.45 180) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
  )
  (module digikey-footprints:TO-92-3_Formed_Leads (layer F.Cu) (tedit 5AF4B307)
    (at 102.362 100.33)
    (descr http://www.ti.com/lit/ds/symlink/tl431a.pdf)
    (fp_text reference VR1 (at 2.6 -3.35) (layer F.SilkS))
    (fp_text value LM431 (at 2.6 2.5) (layer F.Fab))
    (fp_text user %R (at 2.6 -1.25 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.6 0 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 3 thru_hole circle (at 5.2 0 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad2)"))
  )
  (module SW_Rocker_411001:SW_Rocker_411001 (layer F.Cu) (tedit 5E1F7807)
    (at 105.4862 77.1398 180)
    (fp_text reference SW1 (at 5.461 1.778 90) (layer F.SilkS))
    (fp_text value SW_SPDT (at -5.207 1.524 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 -2.54 180) (size 1.55 1.55) (drill 1.09) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.55 1.55) (drill 1.09) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 3 thru_hole circle (at -2.54 -2.54 180) (size 1.55 1.55) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad "" thru_hole circle (at -2.54 2.54 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.54 2.54 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask))
  )
  (module Mikes_lib:CPA_12 (layer F.Cu) (tedit 5E1E2C8D)
    (at 157.014816 98.298 270)
    (fp_text reference SW2 (at 0.0635 -14.054184 90) (layer F.SilkS))
    (fp_text value SW_Rotary12 (at 0 -1.989184 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 10.625184 2.847009 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 "Net-(RV6-Pad2)"))
    (pad 2 thru_hole oval (at 7.778174 7.778174 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 "Net-(RV5-Pad2)"))
    (pad 3 thru_hole oval (at 2.847009 10.625184 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 13 "Net-(R7-Pad1)"))
    (pad 4 thru_hole oval (at -2.847009 10.625184 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 14 "Net-(R8-Pad1)"))
    (pad 5 thru_hole oval (at -7.778174 7.778174 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(R9-Pad1)"))
    (pad 6 thru_hole oval (at -10.625184 2.847009 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 16 "Net-(R10-Pad1)"))
    (pad 7 thru_hole oval (at -10.625184 -2.847009 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -7.778174 -7.778174 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at -2.847009 -10.625184 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.847009 -10.625184 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 7.778174 -7.778174 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 10.625184 -2.847009 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad A thru_hole circle (at 2.72236 2.72236 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
  )
  (module LEMO-EPL.00.650.NLN:LEMO-EPL.00.650.NLN (layer F.Cu) (tedit 5E25D900)
    (at 176.022 86.36)
    (descr "LEMO CONNECTOR")
    (tags "LEMO CONNECTOR")
    (attr virtual)
    (fp_text reference J2 (at -0.0635 -5.461 270) (layer F.SilkS))
    (fp_text value Conn_Triaxial_Power (at -5.1435 -0.381 90) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 2.54 -2.54) (size 1.29794 1.29794) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 1 GNDREF))
    (pad 3 thru_hole circle (at 2.54 2.54) (size 1.29794 1.29794) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 1 GNDREF))
    (pad 3 thru_hole circle (at -2.54 2.54) (size 1.29794 1.29794) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 1 GNDREF))
    (pad 3 thru_hole circle (at -2.54 -2.54) (size 1.29794 1.29794) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.29794 1.29794) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.29794 1.29794) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 1 GNDREF))
  )
  (gr_text "uA Output" (at 175.8188 98.3615 90) (layer F.SilkS))
  (gr_text 1000uA (at 142.367 77.089 90) (layer F.SilkS))
  (gr_text 500uA (at 142.24 85.9282 90) (layer F.SilkS))
  (gr_text 100uA (at 142.367 94.6785 90) (layer F.SilkS))
  (gr_text 50uA (at 142.367 103.8098 90) (layer F.SilkS))
  (gr_line (start 97.409 117.348) (end 97.409 128.016) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.4585 128.016) (end 112.8395 128.016) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.4585 117.348) (end 112.4585 128.016) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.8395 128.016) (end 180 128) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.457 128.016) (end 109.347 128.016) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 60 128) (end 97.409 128.016) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.347 128.016) (end 109.347 117.348) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.347 117.348) (end 112.4585 117.348) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.457 117.348) (end 100.457 128.016) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.409 117.348) (end 100.457 117.348) (layer Edge.Cuts) (width 0.05))
  (gr_text 10uA (at 142.3035 112.7506 90) (layer F.SilkS))
  (gr_text 1uA (at 142.24 121.3485 90) (layer F.SilkS))
  (gr_line (start 60 70.5) (end 60 128) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180 70.5) (end 180 128) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 60 70.5) (end 180 70.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GNDREF) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.182 69.469) (xy 181.737 69.469) (xy 181.737 129.3495) (xy 59.182 129.3495)
      )
    )
  )
)
