<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="34.595" y1="0.9525" x2="34.595" y2="49.2025" width="0" layer="20"/>
<wire x1="34.595" y1="49.2025" x2="33.325" y2="50.4725" width="0" layer="20" curve="90"/>
<wire x1="33.325" y1="50.4725" x2="1.905" y2="50.4725" width="0" layer="20"/>
<wire x1="1.905" y1="50.4725" x2="0.635" y2="49.2025" width="0" layer="20" curve="90"/>
<wire x1="0.635" y1="49.2025" x2="0.635" y2="0.9525" width="0" layer="20"/>
<wire x1="0.635" y1="0.9525" x2="1.905" y2="-0.3175" width="0" layer="20" curve="90"/>
<wire x1="1.905" y1="-0.3175" x2="33.325" y2="-0.3175" width="0" layer="20"/>
<wire x1="33.325" y1="-0.3175" x2="34.595" y2="0.9525" width="0" layer="20" curve="90"/>
<text>D5</text>
<text>D6</text>
<text>6V</text>
<text>GND</text>
<text>D7</text>
<text>SIG</text>
<text>GND</text>
<text>5V</text>
<text>TX</text>
<text>RX</text>
<hole x="19.685" y="46.99" drill="3.2"/>
<hole x="3.175" y="27.305" drill="3.2"/>
<hole x="29.845" y="5.715" drill="3.2"/>
<text>GND</text>
<text>VIN</text>
<text>D12</text>
<hole x="17.4625" y="2.54" drill="1.651"/>
<hole x="21.2725" y="2.54" drill="1.651"/>
<hole x="17.4625" y="10.16" drill="1.651"/>
<hole x="21.2725" y="10.16" drill="1.651"/>
<text>Logo Mouse v6</text>
<text>logomouse.akrobotnerd.com</text>
<text>D-A5</text>
<text>D-A6</text>
<text>D-A7</text>
<text>E-D4</text>
<text>E-D3</text>
<text>E-D2</text>
<wire x1="18.415" y1="4.445" x2="18.415" y2="2.2225" width="0.1524" layer="20"/>
<wire x1="18.415" y1="2.2225" x2="17.78" y2="1.5875" width="0.1524" layer="20" curve="-90"/>
<wire x1="17.78" y1="1.5875" x2="17.145" y2="1.5875" width="0.1524" layer="20"/>
<wire x1="17.145" y1="1.5875" x2="16.51" y2="2.2225" width="0.1524" layer="20" curve="-90"/>
<wire x1="16.51" y1="2.2225" x2="16.51" y2="4.445" width="0.1524" layer="20"/>
<wire x1="16.51" y1="4.445" x2="17.145" y2="5.08" width="0.1524" layer="20" curve="-90"/>
<wire x1="17.145" y1="5.08" x2="17.78" y2="5.08" width="0.1524" layer="20"/>
<wire x1="17.78" y1="5.08" x2="18.415" y2="4.445" width="0.1524" layer="20" curve="-90"/>
<wire x1="20.32" y1="4.445" x2="20.32" y2="2.2225" width="0.1524" layer="20"/>
<wire x1="20.32" y1="2.2225" x2="20.955" y2="1.5875" width="0.1524" layer="20" curve="90"/>
<wire x1="20.955" y1="1.5875" x2="21.59" y2="1.5875" width="0.1524" layer="20"/>
<wire x1="21.59" y1="1.5875" x2="22.225" y2="2.2225" width="0.1524" layer="20" curve="90"/>
<wire x1="22.225" y1="2.2225" x2="22.225" y2="4.445" width="0.1524" layer="20"/>
<wire x1="22.225" y1="4.445" x2="21.59" y2="5.08" width="0.1524" layer="20" curve="90"/>
<wire x1="21.59" y1="5.08" x2="20.955" y2="5.08" width="0.1524" layer="20"/>
<wire x1="20.955" y1="5.08" x2="20.32" y2="4.445" width="0.1524" layer="20" curve="90"/>
<wire x1="16.51" y1="12.065" x2="16.51" y2="9.8425" width="0.1524" layer="20"/>
<wire x1="16.51" y1="9.8425" x2="17.145" y2="9.2075" width="0.1524" layer="20" curve="90"/>
<wire x1="17.145" y1="9.2075" x2="17.78" y2="9.2075" width="0.1524" layer="20"/>
<wire x1="17.78" y1="9.2075" x2="18.415" y2="9.8425" width="0.1524" layer="20" curve="90"/>
<wire x1="18.415" y1="9.8425" x2="18.415" y2="12.065" width="0.1524" layer="20"/>
<wire x1="18.415" y1="12.065" x2="17.78" y2="12.7" width="0.1524" layer="20" curve="90"/>
<wire x1="17.78" y1="12.7" x2="17.145" y2="12.7" width="0.1524" layer="20"/>
<wire x1="17.145" y1="12.7" x2="16.51" y2="12.065" width="0.1524" layer="20" curve="90"/>
<wire x1="21.59" y1="12.7" x2="20.955" y2="12.7" width="0.1524" layer="20"/>
<wire x1="20.955" y1="12.7" x2="20.32" y2="12.065" width="0.1524" layer="20" curve="90"/>
<wire x1="20.32" y1="12.065" x2="20.32" y2="9.8425" width="0.1524" layer="20"/>
<wire x1="20.32" y1="9.8425" x2="20.955" y2="9.2075" width="0.1524" layer="20" curve="90"/>
<wire x1="20.955" y1="9.2075" x2="21.59" y2="9.2075" width="0.1524" layer="20"/>
<wire x1="21.59" y1="9.2075" x2="22.225" y2="9.8425" width="0.1524" layer="20" curve="90"/>
<wire x1="22.225" y1="9.8425" x2="22.225" y2="12.065" width="0.1524" layer="20"/>
<wire x1="22.225" y1="12.065" x2="21.59" y2="12.7" width="0.1524" layer="20" curve="90"/>
<text>+</text>
<text>_</text>
<text>10KΩ</text>
<text>10KΩ</text>
<text>10KΩ</text>
<text>100Ω</text>
<text>100Ω</text>
<text>100Ω</text>
<text>Buzzer: D8
Button: D9</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="DO41-7">
</package>
<package name="EG1218">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Backus">
<packages>
<package name="ARDUINONANO">
</package>
<package name="SERVO">
</package>
<package name="SCREWTERMINAL">
</package>
<package name="TACTILESWITCH">
</package>
<package name="BTMODULE">
</package>
<package name="LTE-302-REVERSE">
<description>&lt;h3&gt;IR Emitter/Detector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2.54mm&lt;/li&gt;
&lt;li&gt;Area: 2.25 x 4.4 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint&lt;/b&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/LTE-302.pdf"&gt; LTE-302&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LTE-302&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LTR-301-REVERSE">
<description>&lt;h3&gt;LTR-301 IR Phototransistor (Side-Receiving)&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/LTR-301.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 2&lt;/li&gt;
&lt;li&gt;Area: 4.4 x 0.75 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;LTR-301&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electromechanical Parts&lt;/h3&gt;
This library contains electromechanical devices, like motors, speakers,servos, and relays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-12MM">
<description>&lt;h3&gt;12mm Buzzer - PTH&lt;/h3&gt;
&lt;p&gt;This is a small 12mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/cem-1203-42-.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="adafruit" package="DO41-7" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="TO220V" value="7805TV"/>
<element name="U$1" library="Backus" package="ARDUINONANO" value="ARDUINONANO"/>
<element name="U$2" library="Backus" package="SERVO" value="SERVO"/>
<element name="U$3" library="Backus" package="SERVO" value="SERVO"/>
<element name="S1" library="adafruit" package="EG1218" value=""/>
<element name="U$4" library="Backus" package="SCREWTERMINAL" value="SCREWTERMINAL"/>
<element name="U$7" library="Backus" package="SERVO" value="SERVO"/>
<element name="U$8" library="Backus" package="TACTILESWITCH" value="TACTILESWITCH"/>
<element name="U$9" library="Backus" package="BTMODULE" value="BTMODULE"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE" value=" "/>
</element>
<element name="D2" library="Backus" package="LTE-302-REVERSE" value="LED-IR">
<attribute name="NAME"/>
</element>
<element name="D3" library="Backus" package="LTE-302-REVERSE" value="LED-IR"/>
<element name="D4" library="Backus" package="LTE-302-REVERSE" value="LED-IR"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE" value=" "/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE" value=" "/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE" value=" "/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE" value=" "/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE" value=" "/>
</element>
<element name="LS1" library="SparkFun-Electromechanical" package="BUZZER-12MM" value="BUZZER-PTH">
<attribute name="PROD_ID" value="COMP-08253"/>
<attribute name="SF_SKU" value="COM-07950"/>
</element>
<element name="Q4" library="Backus" package="LTR-301-REVERSE" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Backus" package="LTR-301-REVERSE" value="">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Backus" package="LTR-301-REVERSE" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3V3">
<contactref element="U$1" pad="P$29"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="P$2"/>
<contactref element="IC1" pad="3"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="U$7" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="S1" pad="S"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="S1" pad="P"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="P$3"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="P$17"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$7" pad="P$3"/>
<contactref element="U$8" pad="P$2"/>
<contactref element="U$9" pad="P$2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="LS1" pad="-"/>
</signal>
<signal name="D6">
<contactref element="U$1" pad="P$9"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="D5">
<contactref element="U$3" pad="P$1"/>
<contactref element="U$1" pad="P$8"/>
</signal>
<signal name="VIN">
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="1"/>
<contactref element="U$1" pad="P$16"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="P$18"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="P$19"/>
<contactref element="U$9" pad="P$1"/>
<contactref element="Q4" pad="C"/>
<contactref element="Q1" pad="C"/>
<contactref element="Q2" pad="C"/>
</signal>
<signal name="A7">
<contactref element="U$1" pad="P$20"/>
<contactref element="R4" pad="P$1"/>
<contactref element="Q4" pad="E"/>
</signal>
<signal name="A6">
<contactref element="U$1" pad="P$21"/>
<contactref element="R5" pad="P$1"/>
<contactref element="Q1" pad="E"/>
</signal>
<signal name="A5">
<contactref element="U$1" pad="P$22"/>
<contactref element="R6" pad="P$1"/>
<contactref element="Q2" pad="E"/>
</signal>
<signal name="A4">
<contactref element="U$1" pad="P$23"/>
</signal>
<signal name="A3">
<contactref element="U$1" pad="P$24"/>
</signal>
<signal name="A2">
<contactref element="U$1" pad="P$25"/>
</signal>
<signal name="A1">
<contactref element="U$1" pad="P$26"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="P$27"/>
</signal>
<signal name="REF">
<contactref element="U$1" pad="P$28"/>
</signal>
<signal name="D13">
<contactref element="U$1" pad="P$30"/>
</signal>
<signal name="TX1">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$9" pad="P$4"/>
</signal>
<signal name="RX0">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$9" pad="P$3"/>
</signal>
<signal name="RST2">
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="D2">
<contactref element="U$1" pad="P$5"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="D3">
<contactref element="U$1" pad="P$6"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="D4">
<contactref element="U$1" pad="P$7"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="D7">
<contactref element="U$1" pad="P$10"/>
<contactref element="U$7" pad="P$1"/>
</signal>
<signal name="D8">
<contactref element="U$1" pad="P$11"/>
<contactref element="LS1" pad="+"/>
</signal>
<signal name="D9">
<contactref element="U$1" pad="P$12"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="D10">
<contactref element="U$1" pad="P$13"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="C"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="P$2"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="P$2"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$15"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
