(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 239)
    (no_connects 49)
    (area 142.529999 70.899999 174.690001 103.100001)
    (thickness 0.8)
    (drawings 207)
    (tracks 1114)
    (zones 0)
    (modules 76)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.16)
    (user_trace_width 0.2)
    (user_trace_width 0.32)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1.2)
    (user_trace_width 0.2)
    (user_trace_width 0.32)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1.2)
    (user_trace_width 0.2)
    (user_trace_width 0.32)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1.2)
    (trace_clearance 0.16)
    (zone_clearance 0.15)
    (zone_45_only no)
    (trace_min 0.16)
    (segment_width 0.02)
    (edge_width 0.02)
    (via_size 0.36)
    (via_drill 0.26)
    (via_min_size 0.36)
    (via_min_drill 0.26)
    (user_via 0.4 0.26)
    (user_via 0.45 0.26)
    (user_via 0.5 0.3)
    (user_via 0.4 0.26)
    (user_via 0.45 0.26)
    (user_via 0.5 0.3)
    (user_via 0.4 0.26)
    (user_via 0.45 0.26)
    (user_via 0.5 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /M_A)
  (net 4 /M_B)
  (net 5 /M_C)
  (net 6 "Net-(Q1-Pad5)")
  (net 7 "Net-(Q1-Pad2)")
  (net 8 "Net-(Q2-Pad5)")
  (net 9 "Net-(Q2-Pad2)")
  (net 10 "Net-(Q3-Pad5)")
  (net 11 "Net-(Q3-Pad2)")
  (net 12 "Net-(R1-Pad1)")
  (net 13 "Net-(R4-Pad2)")
  (net 14 "Net-(R5-Pad2)")
  (net 15 "Net-(R6-Pad2)")
  (net 16 /C2CK)
  (net 17 /RC)
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.16)
    (via_dia 0.36)
    (via_drill 0.26)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /C2CK)
    (add_net /M_A)
    (add_net /M_B)
    (add_net /M_C)
    (add_net /RC)
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad5)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad5)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q3-Pad5)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
  )
  (net_class GND ""
    (clearance 0.16)
    (trace_width 0.34)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class VCC ""
    (clearance 0.16)
    (trace_width 0.34)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VCC)
  )
  (module KiCadCustomLibs:MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59EE00FC)
    (at 164.6 93)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_1.1mm_M1 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module KiCadCustomLibs:MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59EE00FC)
    (at 152.6 93)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_1.1mm_M1 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 173.762201 98.648277 315)
    (fp_text reference J1 (at 0 1.6 315) (layer F.SilkS) hide)
    (fp_text value A (at -0.1 -1.6 315) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 315) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 172.352201 100.058277 315)
    (fp_text reference J2 (at 0 1.6 315) (layer F.SilkS) hide)
    (fp_text value B (at -0.1 -1.6 315) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 315) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
  )
  (module KiCadCustomLibs:QFN20 (layer F.Cu) (tedit 59A7EE18)
    (at 167.642201 96.058277 270)
    (fp_text reference U1 (at -0.127 3.302 270) (layer F.SilkS) hide)
    (fp_text value EFM8BB21 (at 0.381 5.08 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.45 1.45 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (pad 16 smd rect (at -1.45 -1.45 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 0 0 270) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at -1.45 0.75) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (pad 14 smd rect (at -0.25 -1.45 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 15 smd rect (at -0.75 -1.45 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.25 -1.45 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad5)"))
    (pad 19 smd rect (at -1.45 0.25) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 18 smd rect (at -1.45 -0.25) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -1.45 -0.75) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /RC))
    (pad 12 smd rect (at 0.75 -1.45 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.45 -1.45 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)"))
    (pad 10 smd rect (at 1.45 -0.75) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad5)"))
    (pad 6 smd rect (at 1.45 1.45 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.45 0.75) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 1.45 -0.25) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q3-Pad2)"))
    (pad 8 smd rect (at 1.45 0.25) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q3-Pad5)"))
    (pad 5 smd rect (at 0.75 1.45 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /C2CK))
    (pad 4 smd rect (at 0.25 1.45 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -0.25 1.45 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 1.45 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E49F4C)
    (at 164.942201 96.708277 315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.2 315) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.25 315) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 315) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 315) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 315) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /C2CK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E4734E)
    (at 166.972199 98.858277 135)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.2 135) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.25 135) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 135) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 135) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 2 smd rect (at 0.45 0 135) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E4955F)
    (at 168.152199 97.258277 135)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.2 135) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 135) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 135) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /M_B))
    (pad 2 smd rect (at 0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E495AD)
    (at 168.5522 93.638278 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.2 180) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.249999 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A79)
    (at 167.4922 97.928276 315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 1.2 315) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 315) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 315) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /M_C))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A76)
    (at 169.002201 96.788277 315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 1.2 315) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.249999 315) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 315) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /M_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A0B)
    (at 169.672201 96.128277 315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 1.2 315) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.249999 315) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 315) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /M_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59D35907)
    (at 169.3022 100.558277 225)
    (fp_text reference Q3 (at -0.1 6.6 225) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 225) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 225) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 6 smd rect (at -0.38 0 225) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 6 smd rect (at -0.5 -0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 5 smd rect (at 0 -0.72 225) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q3-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 2 smd rect (at 0 0.72 225) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q3-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59D35907)
    (at 170.722201 99.138277 225)
    (fp_text reference Q2 (at -0.1 6.6 225) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 225) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 225) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 6 smd rect (at -0.38 0 225) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 6 smd rect (at -0.5 -0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 5 smd rect (at 0 -0.72 225) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 2 smd rect (at 0 0.72 225) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59E4697F)
    (at 172.132201 97.728277 225)
    (fp_text reference Q1 (at -0.1 6.6 225) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 225) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 225) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 6 smd rect (at -0.38 0 225) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 6 smd rect (at -0.5 -0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 5 smd rect (at 0 -0.72 225) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 2 smd rect (at 0 0.72 225) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 225) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59E4996B)
    (at 166.2922 95.958277 225)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 1.270001 225) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 -1.270001 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.270001 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 225) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 225) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59E49942)
    (at 166.9322 96.598276 225)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 1.270001 225) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.270001 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.270001 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 225) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 225) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 170.9322 101.478277 315)
    (fp_text reference J3 (at 0 1.6 315) (layer F.SilkS) hide)
    (fp_text value C (at -0.1 -1.6 315) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 315) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59EE000B)
    (at 166.092201 94.218277 225)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 225) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 225) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -0.75 0 225) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RC_PAD_TRIANGLE (layer F.Cu) (tedit 59EE004C)
    (at 167.782199 92.168277)
    (fp_text reference J4 (at 0 1.6) (layer F.SilkS) hide)
    (fp_text value RC (at -0.1 -1.6) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0) (size 0.8 0.8) (rect_delta 0 0.799 ) (layers F.Cu F.Paste F.Mask)
      (net 17 /RC))
  )
  (module KiCadCustomLibs:MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59EE00FC)
    (at 152.6 81)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_1.1mm_M1 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module RC_PAD_TRIANGLE (layer F.Cu) (tedit 59EE004C)
    (at 163.76 77.81 90)
    (fp_text reference J4 (at 0 1.6 90) (layer F.SilkS) hide)
    (fp_text value RC (at -0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 90) (size 0.8 0.8) (rect_delta 0 0.799 ) (layers F.Cu F.Paste F.Mask)
      (net 17 /RC))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59EE000B)
    (at 165.81 79.5 315)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 315) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5 315) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 315) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 315) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -0.75 0 315) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 173.07 74.66 45)
    (fp_text reference J3 (at 0 1.6 45) (layer F.SilkS) hide)
    (fp_text value C (at -0.1 -1.6 45) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 45) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59E49942)
    (at 168.19 78.66 315)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 1.270001 315) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.270001 315) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.270001 315) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 315) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 315) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59E4996B)
    (at 167.55 79.3 315)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 1.270001 315) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 -1.270001 315) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.270001 315) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 315) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 315) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59E4697F)
    (at 169.32 73.46 315)
    (fp_text reference Q1 (at -0.1 6.6 315) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 315) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 315) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 6 smd rect (at -0.38 0 315) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 6 smd rect (at -0.5 -0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 5 smd rect (at 0 -0.72 315) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 2 smd rect (at 0 0.72 315) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59D35907)
    (at 170.73 74.87 315)
    (fp_text reference Q2 (at -0.1 6.6 315) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 315) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 315) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 6 smd rect (at -0.38 0 315) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 6 smd rect (at -0.5 -0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 5 smd rect (at 0 -0.72 315) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 2 smd rect (at 0 0.72 315) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59D35907)
    (at 172.15 76.29 315)
    (fp_text reference Q3 (at -0.1 6.6 315) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 315) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 315) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 6 smd rect (at -0.38 0 315) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 6 smd rect (at -0.5 -0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 5 smd rect (at 0 -0.72 315) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q3-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 2 smd rect (at 0 0.72 315) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q3-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 315) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A0B)
    (at 167.72 75.92 45)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 1.2 45) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.249999 45) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 45) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 45) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 45) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /M_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A76)
    (at 168.38 76.59 45)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 1.2 45) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.249999 45) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 45) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 45) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 45) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /M_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A79)
    (at 169.52 78.1 45)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 1.2 45) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 45) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 45) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 45) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 45) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /M_C))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E495AD)
    (at 165.23 77.04 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.2 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.249999 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E4955F)
    (at 168.85 77.44 225)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.2 225) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 225) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /M_B))
    (pad 2 smd rect (at 0.45 0 225) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E4734E)
    (at 170.45 78.62 225)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.2 225) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.25 225) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 225) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 225) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 2 smd rect (at 0.45 0 225) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E49F4C)
    (at 168.3 80.65 45)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.2 45) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.25 45) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 45) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 45) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 45) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /C2CK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:QFN20 (layer F.Cu) (tedit 59A7EE18)
    (at 167.65 77.95)
    (fp_text reference U1 (at -0.127 3.302) (layer F.SilkS) hide)
    (fp_text value EFM8BB21 (at 0.381 5.08) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.45 1.45) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (pad 16 smd rect (at -1.45 -1.45) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 0 0) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at -1.45 0.75 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (pad 14 smd rect (at -0.25 -1.45) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 15 smd rect (at -0.75 -1.45) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.25 -1.45) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad5)"))
    (pad 19 smd rect (at -1.45 0.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 18 smd rect (at -1.45 -0.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -1.45 -0.75 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /RC))
    (pad 12 smd rect (at 0.75 -1.45) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.45 -1.45) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)"))
    (pad 10 smd rect (at 1.45 -0.75 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad5)"))
    (pad 6 smd rect (at 1.45 1.45) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.45 0.75 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 1.45 -0.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q3-Pad2)"))
    (pad 8 smd rect (at 1.45 0.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q3-Pad5)"))
    (pad 5 smd rect (at 0.75 1.45) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /C2CK))
    (pad 4 smd rect (at 0.25 1.45) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -0.25 1.45) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 1.45) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 171.65 73.24 45)
    (fp_text reference J2 (at 0 1.6 45) (layer F.SilkS) hide)
    (fp_text value B (at -0.1 -1.6 45) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 45) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 170.24 71.83 45)
    (fp_text reference J1 (at 0 1.6 45) (layer F.SilkS) hide)
    (fp_text value A (at -0.1 -1.6 45) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 45) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
  )
  (module KiCadCustomLibs:MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59EE00FC)
    (at 164.6 81)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_1.1mm_M1 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module RC_PAD_TRIANGLE (layer F.Cu) (tedit 59EE004C)
    (at 149.45 81.87 180)
    (fp_text reference J4 (at 0 1.6 180) (layer F.SilkS) hide)
    (fp_text value RC (at -0.1 -1.6 180) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 180) (size 0.8 0.8) (rect_delta 0 0.799 ) (layers F.Cu F.Paste F.Mask)
      (net 17 /RC))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59EE000B)
    (at 151.14 79.82 45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 45) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5 45) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 45) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -0.75 0 45) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 146.3 72.56 135)
    (fp_text reference J3 (at 0 1.6 135) (layer F.SilkS) hide)
    (fp_text value C (at -0.1 -1.6 135) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 135) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59E49942)
    (at 150.3 77.44 45)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 1.270001 45) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.270001 45) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.270001 45) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 45) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 45) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59E4996B)
    (at 150.94 78.08 45)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 1.270001 45) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 -1.270001 45) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.270001 45) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 45) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 45) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59E4697F)
    (at 145.1 76.31 45)
    (fp_text reference Q1 (at -0.1 6.6 45) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 45) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 45) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 6 smd rect (at -0.38 0 45) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 6 smd rect (at -0.5 -0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 5 smd rect (at 0 -0.72 45) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 2 smd rect (at 0 0.72 45) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59D35907)
    (at 146.51 74.9 45)
    (fp_text reference Q2 (at -0.1 6.6 45) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 45) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 45) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 6 smd rect (at -0.38 0 45) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 6 smd rect (at -0.5 -0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 5 smd rect (at 0 -0.72 45) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 2 smd rect (at 0 0.72 45) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59D35907)
    (at 147.93 73.48 45)
    (fp_text reference Q3 (at -0.1 6.6 45) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 45) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 45) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 6 smd rect (at -0.38 0 45) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 6 smd rect (at -0.5 -0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 5 smd rect (at 0 -0.72 45) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q3-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 2 smd rect (at 0 0.72 45) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q3-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 45) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A0B)
    (at 147.56 77.91 135)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 1.2 135) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.249999 135) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 135) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /M_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A76)
    (at 148.23 77.25 135)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 1.2 135) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.249999 135) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 135) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /M_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A79)
    (at 149.74 76.11 135)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 1.2 135) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 135) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 135) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /M_C))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E495AD)
    (at 148.68 80.4)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.2) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.249999) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E4955F)
    (at 149.08 76.78 315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.2 315) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 315) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 315) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /M_B))
    (pad 2 smd rect (at 0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E4734E)
    (at 150.26 75.18 315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.2 315) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.25 315) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 315) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 315) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 2 smd rect (at 0.45 0 315) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E49F4C)
    (at 152.29 77.33 135)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.2 135) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.25 135) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 135) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 135) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 135) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /C2CK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:QFN20 (layer F.Cu) (tedit 59A7EE18)
    (at 149.59 77.98 90)
    (fp_text reference U1 (at -0.127 3.302 90) (layer F.SilkS) hide)
    (fp_text value EFM8BB21 (at 0.381 5.08 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.45 1.45 90) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (pad 16 smd rect (at -1.45 -1.45 90) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 0 0 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at -1.45 0.75 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (pad 14 smd rect (at -0.25 -1.45 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 15 smd rect (at -0.75 -1.45 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.25 -1.45 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad5)"))
    (pad 19 smd rect (at -1.45 0.25 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 18 smd rect (at -1.45 -0.25 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -1.45 -0.75 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /RC))
    (pad 12 smd rect (at 0.75 -1.45 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.45 -1.45 90) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)"))
    (pad 10 smd rect (at 1.45 -0.75 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad5)"))
    (pad 6 smd rect (at 1.45 1.45 90) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.45 0.75 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 1.45 -0.25 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q3-Pad2)"))
    (pad 8 smd rect (at 1.45 0.25 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q3-Pad5)"))
    (pad 5 smd rect (at 0.75 1.45 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /C2CK))
    (pad 4 smd rect (at 0.25 1.45 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -0.25 1.45 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 1.45 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 144.88 73.98 135)
    (fp_text reference J2 (at 0 1.6 135) (layer F.SilkS) hide)
    (fp_text value B (at -0.1 -1.6 135) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 135) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 143.47 75.39 135)
    (fp_text reference J1 (at 0 1.6 135) (layer F.SilkS) hide)
    (fp_text value A (at -0.1 -1.6 135) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 135) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
  )
  (module RC_PAD_TRIANGLE (layer F.Cu) (tedit 59EE004C)
    (at 153.462505 96.180484 270)
    (fp_text reference J4 (at 0 1.6 270) (layer F.SilkS) hide)
    (fp_text value RC (at -0.1 -1.6 270) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 0 270) (size 0.8 0.8) (rect_delta 0 0.799 ) (layers F.Cu F.Paste F.Mask)
      (net 17 /RC))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59EE000B)
    (at 151.412505 94.490485 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 135) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5 135) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 144.152505 99.330484 225)
    (fp_text reference J3 (at 0 1.6 225) (layer F.SilkS) hide)
    (fp_text value C (at -0.1 -1.6 225) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 225) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59E49942)
    (at 149.032506 95.330484 135)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 1.270001 135) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.270001 135) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.270001 135) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 135) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 135) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59E4996B)
    (at 149.672505 94.690484 135)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 1.270001 135) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 -1.270001 135) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.270001 135) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 135) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 135) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59E4697F)
    (at 147.902505 100.530485 135)
    (fp_text reference Q1 (at -0.1 6.6 135) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 135) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 135) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 6 smd rect (at -0.38 0 135) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 6 smd rect (at -0.5 -0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 5 smd rect (at 0 -0.72 135) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 2 smd rect (at 0 0.72 135) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59D35907)
    (at 146.492505 99.120485 135)
    (fp_text reference Q2 (at -0.1 6.6 135) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 135) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 135) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 6 smd rect (at -0.38 0 135) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 6 smd rect (at -0.5 -0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 5 smd rect (at 0 -0.72 135) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
    (pad 2 smd rect (at 0 0.72 135) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:MicroFet-1.6 (layer F.Cu) (tedit 59D35907)
    (at 145.072505 97.700485 135)
    (fp_text reference Q3 (at -0.1 6.6 135) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 135) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.38 0 135) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 6 smd rect (at -0.38 0 135) (size 0.54 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 6 smd rect (at -0.5 -0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 5 smd rect (at 0 -0.72 135) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q3-Pad5)"))
    (pad 4 smd rect (at 0.5 -0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.5 0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 2 smd rect (at 0 0.72 135) (size 0.3 0.44) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q3-Pad2)"))
    (pad 1 smd rect (at -0.5 0.72 135) (size 0.33 0.44) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A0B)
    (at 149.502505 98.070485 225)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 1.2 225) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.249999 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 225) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 225) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /M_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A76)
    (at 148.842505 97.400485 225)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 1.2 225) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.249999 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 225) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 225) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /M_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E46A79)
    (at 147.702506 95.890484 225)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 1.2 225) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 225) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 225) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /M_C))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E495AD)
    (at 151.992504 96.950484 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.2 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.249999 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59E4955F)
    (at 148.372505 96.550484 45)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.2 45) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 45) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 45) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 45) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /M_B))
    (pad 2 smd rect (at 0.45 0 45) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E4734E)
    (at 146.772505 95.370484 45)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.2 45) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.25 45) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 45) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 45) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /M_C))
    (pad 2 smd rect (at 0.45 0 45) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59E49F4C)
    (at 148.922505 93.340485 225)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.2 225) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.25 225) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 225) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 225) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 225) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /C2CK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:QFN20 (layer F.Cu) (tedit 59A7EE18)
    (at 149.572505 96.040485 180)
    (fp_text reference U1 (at -0.127 3.302 180) (layer F.SilkS) hide)
    (fp_text value EFM8BB21 (at 0.381 5.08 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.45 1.45 180) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (pad 16 smd rect (at -1.45 -1.45 180) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 0 0 180) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at -1.45 0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (pad 14 smd rect (at -0.25 -1.45 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 15 smd rect (at -0.75 -1.45 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.25 -1.45 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad5)"))
    (pad 19 smd rect (at -1.45 0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 18 smd rect (at -1.45 -0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -1.45 -0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /RC))
    (pad 12 smd rect (at 0.75 -1.45 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.45 -1.45 180) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)"))
    (pad 10 smd rect (at 1.45 -0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad5)"))
    (pad 6 smd rect (at 1.45 1.45 180) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.45 0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 1.45 -0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q3-Pad2)"))
    (pad 8 smd rect (at 1.45 0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q3-Pad5)"))
    (pad 5 smd rect (at 0.75 1.45 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /C2CK))
    (pad 4 smd rect (at 0.25 1.45 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -0.25 1.45 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 1.45 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 145.572505 100.750485 225)
    (fp_text reference J2 (at 0 1.6 225) (layer F.SilkS) hide)
    (fp_text value B (at -0.1 -1.6 225) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 225) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /M_B))
  )
  (module KiCadCustomLibs:ESC_MOT_PAD_THIN (layer F.Cu) (tedit 59E48129)
    (at 146.982505 102.160485 225)
    (fp_text reference J1 (at 0 1.6 225) (layer F.SilkS) hide)
    (fp_text value A (at -0.1 -1.6 225) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 225) (size 1.1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /M_A))
  )
  (gr_text "uESC\n4in1" (at 158.7 87.3 90) (layer F.SilkS))
  (gr_text 1S (at 158.7 90.3) (layer F.SilkS))
  (gr_text + (at 159.45 91.55) (layer F.SilkS))
  (gr_text - (at 157.9 91.55) (layer F.SilkS))
  (gr_line (start 163.73 91.62) (end 161.86 90.76) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 160.88 90.76) (end 161.86 90.76) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 160.2 90.08) (end 160.88 90.76) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 160.2 90.08) (end 160.2 86.59) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 155.34 90.76) (end 156.32 90.76) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.47 91.62) (end 155.34 90.76) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 157 86.6) (end 157 90.08) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 157 90.08) (end 156.32 90.76) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 162.99 93.25) (end 161.49 92.56) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163 93.32) (end 162.99 93.25) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 160.2 86.59) (end 160.3 86.5) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.85 91.55) (end 163.73 91.62) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.11 91.44) (end 163.85 91.55) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.35 91.39) (end 164.11 91.44) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 155.72 92.56) (end 157 92.56) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 161.49 92.56) (end 160.2 92.56) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 160.2 93.9) (end 160.2 92.56) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 157 93.9) (end 160.2 93.9) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 157 92.56) (end 157 93.9) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 157 86.6) (end 156.9 86.5) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.28 91.52) (end 153.47 91.62) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.11 91.45) (end 153.28 91.52) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.91 91.4) (end 153.11 91.45) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.76 93) (end 155.72 92.56) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.22 93.25) (end 154.76 93) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.18 93.4) (end 154.22 93.25) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.28 96.19) (end 170.18 103.09) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164 95.47) (end 163.28 96.19) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 174.68 98.59) (end 170.18 103.09) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 167.78 91.69) (end 174.68 98.59) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 167.07 92.4) (end 167.78 91.69) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.52 91.37) (end 164.35 91.39) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.67 91.37) (end 164.52 91.37) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.85 91.39) (end 164.67 91.37) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165 91.42) (end 164.85 91.39) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.21 91.49) (end 165 91.42) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.32 91.54) (end 165.21 91.49) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.42 91.59) (end 165.32 91.54) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.58 91.7) (end 165.42 91.59) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.69 91.79) (end 165.58 91.7) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.79 91.89) (end 165.69 91.79) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.86 91.96) (end 165.79 91.89) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.94 92.07) (end 165.86 91.96) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 166.01 92.18) (end 165.94 92.07) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 166.06 92.28) (end 166.01 92.18) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 166.12 92.4) (end 166.06 92.28) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 167.07 92.4) (end 166.12 92.4) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164 94.52) (end 164 95.47) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.86 94.45) (end 164 94.52) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.69 94.35) (end 163.86 94.45) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.52 94.22) (end 163.69 94.35) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.4 94.1) (end 163.52 94.22) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.29 93.97) (end 163.4 94.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.23 93.88) (end 163.29 93.97) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.18 93.8) (end 163.23 93.88) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.1 93.65) (end 163.18 93.8) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.05 93.5) (end 163.1 93.65) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163 93.32) (end 163.05 93.5) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.14 93.53) (end 154.18 93.4) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.09 93.66) (end 154.14 93.53) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.04 93.76) (end 154.09 93.66) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.98 93.87) (end 154.04 93.76) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.84 94.05) (end 153.98 93.87) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.77 94.13) (end 153.84 94.05) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.67 94.23) (end 153.77 94.13) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.56 94.32) (end 153.67 94.23) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.45 94.39) (end 153.56 94.32) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.32 94.46) (end 153.45 94.39) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.2 94.52) (end 153.32 94.46) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.2 95.44) (end 153.2 94.52) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.77 91.38) (end 152.91 91.4) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.6 91.37) (end 152.77 91.38) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.42 91.38) (end 152.6 91.37) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.25 91.41) (end 152.42 91.38) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.13 91.44) (end 152.25 91.41) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.99 91.49) (end 152.13 91.44) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.78 91.59) (end 151.99 91.49) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.62 91.7) (end 151.78 91.59) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.53 91.77) (end 151.62 91.7) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.39 91.91) (end 151.53 91.77) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.25 92.09) (end 151.39 91.91) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.19 92.18) (end 151.25 92.09) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.11 92.34) (end 151.19 92.18) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.07 92.44) (end 151.11 92.34) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 150.2 92.44) (end 151.07 92.44) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.94 96.18) (end 147.04 103.08) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.2 95.44) (end 153.94 96.18) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 142.54 98.58) (end 147.04 103.08) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 149.44 91.68) (end 142.54 98.58) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 150.2 92.44) (end 149.44 91.68) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_text S (at 167.3122 93.088276 225) (layer F.SilkS))
  (gr_line (start 167.07 81.6) (end 167.78 82.31) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 166.12 81.6) (end 167.07 81.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 166.06 81.72) (end 166.12 81.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.99 81.85) (end 166.06 81.72) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.93 81.94) (end 165.99 81.85) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.83 82.07) (end 165.93 81.94) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.72 82.18) (end 165.83 82.07) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.61 82.28) (end 165.72 82.18) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.45 82.39) (end 165.61 82.28) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.3 82.47) (end 165.45 82.39) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 165.16 82.53) (end 165.3 82.47) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.99 82.58) (end 165.16 82.53) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.85 82.61) (end 164.99 82.58) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.69 82.63) (end 164.85 82.61) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.58 82.63) (end 164.69 82.63) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.44 82.62) (end 164.58 82.63) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.3 82.6) (end 164.44 82.62) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164.21 82.59) (end 164.3 82.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 160.3 86.5) (end 164.21 82.59) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.99 82.59) (end 156.9 86.5) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.92 82.6) (end 152.99 82.59) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.77 82.62) (end 152.92 82.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.56 82.63) (end 152.77 82.62) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.43 82.62) (end 152.56 82.63) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.24 82.59) (end 152.43 82.62) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.12 82.56) (end 152.24 82.59) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 152.04 82.53) (end 152.12 82.56) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.9 82.47) (end 152.04 82.53) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.78 82.41) (end 151.9 82.47) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.62 82.3) (end 151.78 82.41) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.51 82.21) (end 151.62 82.3) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.42 82.12) (end 151.51 82.21) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.31 82) (end 151.42 82.12) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.23 81.88) (end 151.31 82) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.12 81.68) (end 151.23 81.88) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 151.08 81.6) (end 151.12 81.68) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 150.2 81.6) (end 151.08 81.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 149.45 82.35) (end 150.2 81.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.2 78.6) (end 153.95 77.85) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164 78.53) (end 163.28 77.81) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 164 79.48) (end 164 78.53) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.84 79.56) (end 164 79.48) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.69 79.65) (end 163.84 79.56) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.5 79.8) (end 163.69 79.65) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.42 79.88) (end 163.5 79.8) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.29 80.03) (end 163.42 79.88) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.18 80.2) (end 163.29 80.03) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.12 80.32) (end 163.18 80.2) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.06 80.47) (end 163.12 80.32) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.01 80.65) (end 163.06 80.47) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 162.98 80.85) (end 163.01 80.65) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 162.97 81.03) (end 162.98 80.85) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 162.98 81.18) (end 162.97 81.03) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163 81.32) (end 162.98 81.18) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 163.01 81.39) (end 163 81.32) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 159.1 85.3) (end 163.01 81.39) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 158.1 85.3) (end 159.1 85.3) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.18 81.38) (end 158.1 85.3) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.2 81.3) (end 154.18 81.38) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.22 81.15) (end 154.2 81.3) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.23 80.99) (end 154.22 81.15) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.22 80.83) (end 154.23 80.99) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.19 80.65) (end 154.22 80.83) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.15 80.5) (end 154.19 80.65) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 154.09 80.35) (end 154.15 80.5) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.98 80.13) (end 154.09 80.35) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.9 80.02) (end 153.98 80.13) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.8 79.9) (end 153.9 80.02) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.71 79.81) (end 153.8 79.9) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.58 79.7) (end 153.71 79.81) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.45 79.61) (end 153.58 79.7) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.3 79.53) (end 153.45 79.61) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.2 79.48) (end 153.3 79.53) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 153.2 78.6) (end 153.2 79.48) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_text S (at 164.68 78.28 315) (layer F.SilkS))
  (gr_line (start 167.78 82.31) (end 174.68 75.41) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 170.18 70.91) (end 163.28 77.81) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 174.68 75.41) (end 170.18 70.91) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_text S (at 149.92 80.95 45) (layer F.SilkS))
  (gr_line (start 153.95 77.85) (end 147.05 70.95) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 142.55 75.45) (end 149.45 82.35) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 147.05 70.95) (end 142.55 75.45) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_text S (at 152.542506 95.710484 135) (layer F.SilkS))
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 164.36 82.61) (xy 164.42 81.11) (xy 166.33 79.52) (xy 168.75 81.86) (xy 168.2 82.71)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 162.14 81.51) (xy 163.89 81.25) (xy 165.93 79.55) (xy 164.5 77.68) (xy 161.53 80.68)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 166.08 79.13) (xy 164.95 80.27) (xy 164.19 81.05) (xy 164.14 82.68) (xy 160.4 86.59)
        (xy 160.408493 87.33734) (xy 160.6 87.34) (xy 160.6 90.030086) (xy 169.59 91.09) (xy 166.44 94.44)
        (xy 165.07 93.16) (xy 164.47 92.48) (xy 164.11 92.73) (xy 163.43 92.68) (xy 162.2 93.09)
        (xy 160.6 92.76375) (xy 160.6 94) (xy 158.77 93.99) (xy 156.65 94.78) (xy 153.37 97.01)
        (xy 151.16 94.81) (xy 152.77 93.17) (xy 153.21 93.08) (xy 154.02 91.3) (xy 156.929409 87.384989)
        (xy 148.54 81.87) (xy 150.91 79.5) (xy 152.41 81.04) (xy 153.08 81.39) (xy 154.32 81.47)
        (xy 158.489877 85.069844) (xy 158.49 85.04) (xy 163.61 76.65)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 154.64 78.24) (xy 154.78 81.08) (xy 158.94 84.64) (xy 158.944348 84.706431) (xy 162.18 81.76)
        (xy 163.91 81.49) (xy 166.41 79.38) (xy 168.66 81.56) (xy 167.81 82.41) (xy 167.05 81.64)
        (xy 167.06 87.3) (xy 160.501999 87.369766) (xy 160.515557 89.674622) (xy 163.21781 91.040208) (xy 164.42 93.54)
        (xy 164.783055 93.408982) (xy 166.07 94.74) (xy 163.3 97.46) (xy 160.527162 92.889598) (xy 160.55 94.1)
        (xy 158.85 94.1) (xy 158.85 92.178049) (xy 158.45 91.7) (xy 157.1 91.7) (xy 156.8 92)
        (xy 156.8 93.966667) (xy 155.17 92.88) (xy 152.53 92.86) (xy 151.03 94.33) (xy 148.78 92.19)
        (xy 148.78 91.36) (xy 156.23 89.62) (xy 156.37 86.95) (xy 156.861034 86.959512) (xy 153.12 82.86)
        (xy 153.06 81.18) (xy 151.12 79.3) (xy 153.41 77.06)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 153.48 77.17) (xy 151.26 79.42) (xy 152.89 81.18) (xy 154.58 81.27) (xy 154.4 78.09)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 148.42 82.03) (xy 150.88 79.56) (xy 152.82 81.43) (xy 152.87 83.12) (xy 151.21 84.63)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 153.68 91.5) (xy 153.11 92.81) (xy 152.48 92.89) (xy 151.24 94.17) (xy 148.817542 92.063196)
        (xy 149.760821 91.363443)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 158.44 92.11) (xy 158.44 94.212537) (xy 156.98 94.2) (xy 156.97 92.14) (xy 157.158858 91.92)
        (xy 158.05 91.92)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 154.76 93.17) (xy 152.83 93.17) (xy 151.23 94.77) (xy 152.87 96.41) (xy 154.97 94.31)
        (xy 155.24 94.31)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 162.67 93.11) (xy 163.51 92.87) (xy 165.01 93.68) (xy 166.11 94.75) (xy 163.75 96.91)
        (xy 162.86 95.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 163.62 91.17) (xy 164.36 92.8) (xy 165.32 93.37) (xy 166.45 94.4) (xy 168.87 91.87)
        (xy 167.9 91.31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 157 93.9) (xy 158.5 93.9) (xy 158.5 92.2) (xy 157 92.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 160.2 93.9) (xy 158.8 93.9) (xy 158.8 92.2) (xy 160.2 92.2)
      )
    )
  )
)
