(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 77)
    (no_connects 0)
    (area 89.666424 42.87 175.259 86.7)
    (thickness 1.6)
    (drawings 29)
    (tracks 376)
    (zones 0)
    (modules 34)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 IR_IN)
  (net 5 TEMP_READ)
  (net 6 LED_DR)
  (net 7 LED_DR_5)
  (net 8 "Net-(P4-Pad2)")
  (net 9 "Net-(P4-Pad4)")
  (net 10 "Net-(P4-Pad6)")
  (net 11 "Net-(P4-Pad8)")
  (net 12 RXD_UA_1)
  (net 13 TXD_UA_1)
  (net 14 "Net-(P6-Pad1)")
  (net 15 "Net-(P6-Pad2)")
  (net 16 "Net-(P6-Pad3)")
  (net 17 "Net-(P6-Pad4)")
  (net 18 "Net-(P6-Pad5)")
  (net 19 "Net-(P7-Pad1)")
  (net 20 "Net-(P7-Pad2)")
  (net 21 "Net-(P7-Pad3)")
  (net 22 "Net-(P7-Pad4)")
  (net 23 TEMT)
  (net 24 "Net-(R8-Pad1)")
  (net 25 "Net-(R9-Pad1)")
  (net 26 "Net-(R10-Pad2)")
  (net 27 "Net-(R11-Pad2)")
  (net 28 "Net-(R12-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net IR_IN)
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P6-Pad5)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net RXD_UA_1)
    (add_net TEMP_READ)
    (add_net TEMT)
    (add_net TXD_UA_1)
  )
  (net_class 3v ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net LED_DR)
  )
  (net_class 5v ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net LED_DR_5)
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 129.032 63.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0.032 -2.3965) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P7-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ESP8266:ESP-12E (layer F.Cu) (tedit 559F8D21)
    (at 109 74.5 90)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 0.078 16.4125 90) (layer F.SilkS))
    (fp_text value ESP-12E (at 8 1 90) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4 90) (layer F.CrtYd))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(R8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 23 TEMT))
    (pad 3 thru_hole oval (at 0 4 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(R9-Pad1)"))
    (pad 4 thru_hole oval (at 0 6 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P6-Pad5)"))
    (pad 5 thru_hole oval (at 0 8 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P6-Pad4)"))
    (pad 6 thru_hole oval (at 0 10 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 5 TEMP_READ))
    (pad 7 thru_hole oval (at 0 12 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P6-Pad3)"))
    (pad 8 thru_hole oval (at 0 14 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 9 smd oval (at 1.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P7-Pad4)"))
    (pad 10 smd oval (at 3.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P7-Pad3)"))
    (pad 11 smd oval (at 5.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P6-Pad1)"))
    (pad 12 smd oval (at 7.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P6-Pad2)"))
    (pad 13 smd oval (at 9.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P7-Pad2)"))
    (pad 14 smd oval (at 11.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P7-Pad1)"))
    (pad 15 thru_hole oval (at 14 14 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole oval (at 14 12 90) (size 2.5 1.1) (drill 0.65 (offset 0.6 0)) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(R10-Pad2)"))
    (pad 17 thru_hole oval (at 14 10 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R11-Pad2)"))
    (pad 18 thru_hole oval (at 14 8 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(R12-Pad2)"))
    (pad 19 thru_hole oval (at 14 6 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 4 IR_IN))
    (pad 20 thru_hole oval (at 14 4 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 6 LED_DR))
    (pad 21 thru_hole oval (at 14 2 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 13 TXD_UA_1))
    (pad 22 thru_hole oval (at 14 0 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 12 RXD_UA_1))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 155.702 73.803 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.4 0.0451 90) (layer F.SilkS))
    (fp_text value C (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 152.654 56.15 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.302 0 180) (layer F.SilkS))
    (fp_text value C (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 144.095 56.007 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -0.635 7.035 270) (layer F.SilkS))
    (fp_text value TL1838_PINHEADER (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 IR_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 147 60.7518 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value "Q_NPN_BEC (MMBT2222ALT1G, 1459098 on E14)" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_DR))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 7 LED_DR_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 143 60.75 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value "Q_NPN_BEC (MMBT2222ALT1G, 1459098 on E14)" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_DR))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 7 LED_DR_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 146 73.4 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.8635 0.1135 180) (layer F.SilkS))
    (fp_text value 25 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P4-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 143.25 73.4 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.9905 0.006 180) (layer F.SilkS))
    (fp_text value 25 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P4-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 66.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.8355 0.175) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 TEMP_READ))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 152.334 67.2871 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 2.1935 -1.4502 180) (layer F.SilkS))
    (fp_text value AP1117 (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 54F24281)
    (at 138.135 55.5715)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference P3 (at 1.7555 2.658) (layer F.SilkS))
    (fp_text value DS18B20_PINHEADER_TO92 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 5 TEMP_READ))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 139 60.75 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value "Q_NPN_BEC (MMBT2222ALT1G, 1459098 on E14)" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_DR))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 7 LED_DR_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 151 60.7518 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value "Q_NPN_BEC (MMBT2222ALT1G, 1459098 on E14)" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_DR))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 7 LED_DR_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 148.5 73.4 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -1.3395 2.0585 90) (layer F.SilkS))
    (fp_text value 25 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 140.75 73.4 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -1.403 -2.0025 90) (layer F.SilkS))
    (fp_text value 25 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P4-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 0)
    (at 148.5 65.5 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 1.3655 -2.5665 270) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 LED_DR_5))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 LED_DR_5))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 LED_DR_5))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P4-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 LED_DR_5))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 125.594 55.635 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -2.1045 3.2935 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 RXD_UA_1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 TXD_UA_1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 54EA0684)
    (at 126.374 79.365 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0.0735 -2.722 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P6-Pad5)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 134.47 55.889 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at -2.3585 0.8025 360) (layer F.SilkS))
    (fp_text value TEMP6000 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 TEMT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 64)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -0.3555 -4.31) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 69)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.772 0.0245) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 74 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 4.102 -0.295 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 61.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -3.899 -3.0795 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 134.15 71.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -4.026 0.3165 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer F.Cu) (tedit 555EF748)
    (at 152.273 73.47 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow")
    (tags "Tantal Capacitor Size-B EIA-3528 Reflow")
    (attr smd)
    (fp_text reference C1 (at -3.5035 0.0606 180) (layer F.SilkS))
    (fp_text value CP (at 0 2.7 90) (layer F.Fab))
    (pad 2 smd rect (at 1.46 0 90) (size 1.8 2.23) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.46 0 90) (size 1.8 2.23) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer F.Cu) (tedit 555EF748)
    (at 156.014 60.579)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow")
    (tags "Tantal Capacitor Size-B EIA-3528 Reflow")
    (attr smd)
    (fp_text reference C4 (at -3.614 1.4326) (layer F.SilkS))
    (fp_text value CP (at 0 2.7) (layer F.Fab))
    (pad 2 smd rect (at 1.46 0) (size 1.8 2.23) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.46 0) (size 1.8 2.23) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 58C555C3)
    (at 111.76 55.5625)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF04 (at 0.254 -5.7785) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 58C555BB)
    (at 111.76 79.502)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF03 (at 0 6.223) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 58C555B5)
    (at 156.845 79.502)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF02 (at 0.889 5.969) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 58C555A8)
    (at 156.845 55.499)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF01 (at 0.254 -7.112) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 555C8B1B)
    (at 135.128 79.248)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW1 (at 0.01011 0) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.01011 -0.00022) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 4.60243 0.00232) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 555C8B1B)
    (at 147.32 79.248)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW2 (at 0 0) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.01011 -0.00022) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.60243 0.00232) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R12-Pad2)"))
  )
  (module MyKiCadLibs:USB_Micro-B-OshPark (layer B.Cu) (tedit 57FEB7F7)
    (at 157.353 67.564 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P1 (at 0 3.45 270) (layer B.SilkS))
    (fp_text value USB_OTG (at 0 -4.8 270) (layer B.Fab))
    (pad 1 smd rect (at -1.3009 1.56254 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -0.6509 1.56254 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -0.0009 1.56254 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 0.6491 1.56254 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.2991 1.56254 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.5009 1.56254 180) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.4991 1.56254 180) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at -3.5009 -1.13746 180) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at 3.4991 -1.13746 180) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
  )
  (gr_text "IR In" (at 149.225 53.721) (layer F.SilkS))
  (dimension 52.07 (width 0.3) (layer Cmts.User)
    (gr_text "52.070 mm" (at 133.985 44.37) (layer Cmts.User))
    (feature1 (pts (xy 160.02 50.8) (xy 160.02 43.02)))
    (feature2 (pts (xy 107.95 50.8) (xy 107.95 43.02)))
    (crossbar (pts (xy 107.95 45.72) (xy 160.02 45.72)))
    (arrow1a (pts (xy 160.02 45.72) (xy 158.893496 46.306421)))
    (arrow1b (pts (xy 160.02 45.72) (xy 158.893496 45.133579)))
    (arrow2a (pts (xy 107.95 45.72) (xy 109.076504 46.306421)))
    (arrow2b (pts (xy 107.95 45.72) (xy 109.076504 45.133579)))
  )
  (dimension 29.845 (width 0.3) (layer Cmts.User)
    (gr_text "29.845 mm" (at 168.609 67.5005 90) (layer Cmts.User))
    (feature1 (pts (xy 162.56 52.578) (xy 169.959 52.578)))
    (feature2 (pts (xy 162.56 82.423) (xy 169.959 82.423)))
    (crossbar (pts (xy 167.259 82.423) (xy 167.259 52.578)))
    (arrow1a (pts (xy 167.259 52.578) (xy 167.845421 53.704504)))
    (arrow1b (pts (xy 167.259 52.578) (xy 166.672579 53.704504)))
    (arrow2a (pts (xy 167.259 82.423) (xy 167.845421 81.296496)))
    (arrow2b (pts (xy 167.259 82.423) (xy 166.672579 81.296496)))
  )
  (dimension 3.56506 (width 0.3) (layer F.Fab)
    (gr_text "3.565 mm" (at 95.602137 48.130938 85.91438322) (layer F.Fab))
    (feature1 (pts (xy 108.204 47.244) (xy 94.382568 46.256755)))
    (feature2 (pts (xy 107.95 50.8) (xy 94.128568 49.812755)))
    (crossbar (pts (xy 96.821706 50.005122) (xy 97.075706 46.449122)))
    (arrow1a (pts (xy 97.075706 46.449122) (xy 97.580376 47.614544)))
    (arrow1b (pts (xy 97.075706 46.449122) (xy 96.410515 47.530982)))
    (arrow2a (pts (xy 96.821706 50.005122) (xy 97.486897 48.923262)))
    (arrow2b (pts (xy 96.821706 50.005122) (xy 96.317036 48.8397)))
  )
  (gr_text ESP-12E (at 115.57 67.437) (layer F.SilkS))
  (gr_line (start 107.95 82.423) (end 107.95 52.578) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 82.423) (end 107.95 82.423) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 52.578) (end 160.02 82.423) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 52.578) (end 160.02 52.578) (layer Edge.Cuts) (width 0.15))
  (gr_text D16 (at 116.1415 81.4705) (layer F.SilkS))
  (gr_text D14 (at 118.745 81.4705) (layer F.SilkS))
  (gr_text D13 (at 121.285 81.4705) (layer F.SilkS))
  (gr_text D9 (at 126.365 81.4705) (layer F.SilkS))
  (gr_text D10 (at 123.8885 81.4705) (layer F.SilkS))
  (gr_text "IR OUT x 4" (at 144.7165 70.104) (layer F.SilkS))
  (gr_text SPI (at 127.0635 66.7385 90) (layer F.SilkS))
  (gr_text GPIO (at 127.381 76.3905) (layer F.SilkS))
  (gr_text GND (at 146.685 58.2295) (layer F.SilkS))
  (gr_text +3.3 (at 143.129 58.166) (layer F.SilkS))
  (gr_text GND (at 125.7935 58.039) (layer F.SilkS))
  (gr_text LIGHT (at 129.8575 53.7845) (layer F.SilkS))
  (gr_text GND (at 131.953 58.166) (layer F.SilkS))
  (gr_text +3.3 (at 135.382 58.293) (layer F.SilkS))
  (gr_text TX (at 122.9995 57.912) (layer F.SilkS))
  (gr_text RX (at 120.5865 57.8485) (layer F.SilkS))
  (gr_text TEMP (at 139.446 53.721) (layer F.SilkS))
  (gr_text PROG (at 147.32 81.28) (layer F.SilkS))
  (gr_text RESET (at 135.128 81.28) (layer F.SilkS))
  (gr_text "IRRemote - me@pjr.cc\nhttps://github.com/takigama\n" (at 141.605 73.152 5) (layer B.SilkS))
  (zone (net 7) (net_name LED_DR_5) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.16 60.96) (xy 137.16 66.802) (xy 150.368 66.802) (xy 150.368 63.5) (xy 152.4 63.5)
        (xy 152.4 60.96)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.4))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 52.578) (xy 107.95 82.423) (xy 160.02 82.423) (xy 160.02 52.578)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 76.2) (xy 139.7 76.2) (xy 139.7 69.85) (xy 151.13 69.85) (xy 151.13 67.056)
        (xy 153.416 67.056) (xy 153.416 64.77) (xy 160.02 64.77)
      )
    )
  )
)
