(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 36)
    (no_connects 0)
    (area 198.865857 148.581 222.480143 167.500001)
    (thickness 1.6)
    (drawings 18)
    (tracks 114)
    (zones 0)
    (modules 10)
    (nets 18)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.254)
    (trace_clearance 0.1)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.4)
    (user_via 0.6 0.4)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 AFilt)
  (net 3 VCC)
  (net 4 EXTI)
  (net 5 WDI)
  (net 6 nExtR)
  (net 7 VBat)
  (net 8 FOut/nIRQ)
  (net 9 ClkOut/nIRQ3)
  (net 10 PSW/nIRQ2)
  (net 11 nRST)
  (net 12 SCSel)
  (net 13 SMOSI)
  (net 14 SMISO)
  (net 15 SCLK)
  (net 16 XO)
  (net 17 XI)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net AFilt)
    (add_net ClkOut/nIRQ3)
    (add_net EXTI)
    (add_net FOut/nIRQ)
    (add_net GND)
    (add_net PSW/nIRQ2)
    (add_net SCLK)
    (add_net SCSel)
    (add_net SMISO)
    (add_net SMOSI)
    (add_net VBat)
    (add_net VCC)
    (add_net WDI)
    (add_net XI)
    (add_net XO)
    (add_net nExtR)
    (add_net nRST)
  )
  (module Pin_Header_Straight_1x07_Pitch2.54mm2 (layer F.Cu) (tedit 58F9855C)
    (at 218.4 165 270)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J1 (at -0.254 -3.048 360) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at -2.921 12.446 360) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VBat))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 EXTI))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 nExtR))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 WDI))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 ClkOut/nIRQ3))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 PSW/nIRQ2))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 nRST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 58F984C3)
    (at 203.2 152.4 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -3.302 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at 2.794 12.573 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SCSel))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 SMOSI))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 SCLK))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 SMISO))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 FOut/nIRQ))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B0D75D2)
    (at 205 157.8 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference CaFilt1 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 47pF (at 1.9 0.7 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 AFilt))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B0D75C9)
    (at 205 156.2 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference Cbyp1 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 1.8 1 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootprints:EpsonFC135 (layer F.Cu) (tedit 5B0ECD6D)
    (at 205.6 160.6 270)
    (fp_text reference ABS07-120 (at 2.4 -1.4 360) (layer F.SilkS))
    (fp_text value 32kHz (at 0 1.6 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.25 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 XI))
    (pad 2 smd rect (at -1.25 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 16 XO))
    (model SMD_Packages/SMD-0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.12 0.15 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootprints:QFN16thermalpasted (layer F.Cu) (tedit 5B0ECD65)
    (at 209.4 159 90)
    (fp_text reference AB1815 (at -2.6 -0.4 180) (layer F.SilkS))
    (fp_text value AB1815 (at 0.1905 -3.3655 90) (layer F.SilkS) hide)
    (pad 17 thru_hole rect (at -0.4 0.4 90) (size 0.8 0.8) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole rect (at -0.4 -0.4 90) (size 0.8 0.8) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole rect (at 0.4 0.4 90) (size 0.8 0.8) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 smd rect (at -0.4 -0.4 90) (size 0.68 0.68) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -0.4 0.4 90) (size 0.68 0.68) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 0.4 0.4 90) (size 0.68 0.68) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 thru_hole rect (at 0.0445 0.0055 90) (size 0.85 0.85) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole rect (at 0.4 -0.4 90) (size 0.8 0.8) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 smd oval (at -1.5494 -0.7493 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 11 nRST))
    (pad 2 smd oval (at -1.5494 -0.24892 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 5 WDI))
    (pad 3 smd oval (at -1.5494 0.24892 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 6 nExtR))
    (pad 4 smd oval (at -1.5494 0.7493 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 10 PSW/nIRQ2))
    (pad 5 smd oval (at -0.7493 1.5494 180) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 7 VBat))
    (pad 6 smd oval (at -0.24892 1.5494 180) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 14 SMISO))
    (pad 7 smd oval (at 0.24892 1.5494 180) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 15 SCLK))
    (pad 8 smd oval (at 0.7493 1.5494 180) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 9 ClkOut/nIRQ3))
    (pad 9 smd oval (at 1.5494 0.7493 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 13 SMOSI))
    (pad 10 smd oval (at 1.5494 0.24892 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 4 EXTI))
    (pad 11 smd oval (at 1.5494 -0.24892 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 8 FOut/nIRQ))
    (pad 12 smd oval (at 1.5494 -0.7493 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 12 SCSel))
    (pad 13 smd oval (at 0.7493 -1.5494 180) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 14 smd oval (at 0.24892 -1.5494 180) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 2 AFilt))
    (pad 15 smd oval (at -0.24892 -1.5494 180) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 16 XO))
    (pad 16 smd oval (at -0.7493 -1.5494 180) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 17 XI))
    (pad 17 smd rect (at 0.4 -0.4 90) (size 0.68 0.68) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module myFootprints:SolderJumperClosed (layer F.Cu) (tedit 5B0D78AA)
    (at 217.9 157.6 270)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference JVBat (at -1.6 0 360) (layer F.SilkS))
    (fp_text value VBat (at 1.524 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -0.635 270) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0 0.635 270) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 7 VBat))
  )
  (module myFootprints:SolderJumperClosed (layer F.Cu) (tedit 5B0D78AA)
    (at 215.9 160.2 270)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference JExtI (at -1.6 0 360) (layer F.SilkS))
    (fp_text value GS2 (at 1.524 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -0.635 270) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0.635 270) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 4 EXTI))
  )
  (module myFootprints:SolderJumperClosed (layer F.Cu) (tedit 5B0D78AA)
    (at 213.4 162.6 270)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference JnExtR (at -1.6 0 360) (layer F.SilkS))
    (fp_text value GS2 (at 1.524 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -0.635 270) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0.635 270) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 6 nExtR))
  )
  (module myFootprints:SolderJumperClosed (layer F.Cu) (tedit 5B0D90DC)
    (at 203.2 162.1)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference JWDI (at -0.5 -2.6 90) (layer F.SilkS))
    (fp_text value GS2 (at 1.524 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 5 WDI))
  )
  (gr_text <nRst (at 203.2 161.9 270) (layer B.SilkS))
  (gr_text <nIRQ2 (at 205.6 161.4 270) (layer B.SilkS))
  (gr_text <nIRQ3 (at 208.2 161.4 270) (layer B.SilkS))
  (gr_text >WDI (at 210.7 162.6 270) (layer B.SilkS))
  (gr_text >nExtR (at 213.4 161.8 270) (layer B.SilkS))
  (gr_text >ExtI (at 215.9 162.6 270) (layer B.SilkS))
  (gr_text VBat (at 218.4 162.3 270) (layer B.SilkS))
  (gr_text nIRQ> (at 218.6 155.6 270) (layer B.SilkS))
  (gr_text SMISO> (at 215.9 155.7 270) (layer B.SilkS))
  (gr_text SClk< (at 213.3 155.1 270) (layer B.SilkS))
  (gr_text SMOSI< (at 210.7 155.7 270) (layer B.SilkS))
  (gr_text SCSel< (at 208.2 155.5 270) (layer B.SilkS))
  (gr_text Vcc (at 205.6 153.6 270) (layer B.SilkS))
  (gr_text Gnd (at 203.2 153.5 270) (layer B.SilkS))
  (gr_line (start 201.676 166.624) (end 219.964 166.624) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 201.676 150.876) (end 201.676 166.624) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 219.964 150.876) (end 201.676 150.876) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 219.964 166.624) (end 219.964 150.876) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 220.5 167) (xy 201 167) (xy 201 150) (xy 220.5 150) (xy 220.5 167)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 221 167.5) (xy 200.5 167.5) (xy 200.5 149.5) (xy 221 149.5) (xy 221 167.5)
      )
    )
  )
)
