(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "core") (thickness 1.24) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "V2_GERBER/")
    )
  )
  (net 0 "")
  (net 1 "Blue in")
  (net 2 "Blue Out")
  (net 3 "Red in")
  (net 4 "Red Out")
  (net 5 "Green in")
  (net 6 "Green out")
  (net 7 "Luma")
  (net 8 "Net-(U1-VIDEO)")
  (net 9 "GND")
  (net 10 "Net-(U1-INT)")
  (net 11 "+5V")
  (net 12 "unconnected-(J1-Pin_7-Pad7)")
  (net 13 "unconnected-(J1-Pin_6-Pad6)")
  (net 14 "Right Audio")
  (net 15 "Left Audio")
  (net 16 "Net-(U1-CSYNC)")
  (net 17 "cSync")
  (net 18 "unconnected-(U1-O{slash}E-Pad7)")
  (net 19 "unconnected-(U1-BURST-Pad5)")
  (net 20 "unconnected-(U1-FRAME-Pad3)")
  (footprint "ICspretty:coaxPad" (layer "F.Cu")
    (at 136.45 57.5)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J14" (at 0 -6.7 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 4.6 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 1 5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 9 "GND") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 125.05 63.2 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.85 90) (layer "F.SilkS") hide)
    (fp_text value "220uf" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 5 "Green in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 6 "Green out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 135.75 63.25 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0.05 2.1 180) (layer "F.SilkS") hide)
    (fp_text value "220uf" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "Blue in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "Blue Out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICspretty:coaxPad" (layer "F.Cu")
    (at 128.45 57.5)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J10" (at 0 -6.7 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 4.6 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 1 5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 9 "GND") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "ICspretty:coaxPad" (layer "F.Cu")
    (at 132.45 57.5)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J12" (at 0 -6.7 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 4.6 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 1 5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 9 "GND") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 132.75 61.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -0.9 1.375) (layer "F.SilkS"))
    (fp_text value "680k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "Net-(U1-INT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 130.05 62.8 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 2.525 0.15 180) (layer "F.SilkS"))
    (fp_text value "100nf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U1-INT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICspretty:coaxPad" (layer "F.Cu")
    (at 134.45 57.5)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "B" (at -0.05 3.2 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 4.6 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 1 5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 2 "Blue Out") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "ICspretty:coaxPad" (layer "F.Cu")
    (at 126.45 57.5)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "G" (at -0.05 3.1 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 4.6 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 1 5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 6 "Green out") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 127.6 63.275 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0.25 2.25 180) (layer "F.SilkS") hide)
    (fp_text value "220uf" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "Red in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "Red Out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Ports:PSX_AV" (layer "F.Cu")
    (at 131.3 70 180)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x12, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -3.691 5.151) (layer "F.SilkS") hide)
    (fp_text value "PS1_AV_Multi-Out" (at 0.05 7) (layer "F.Fab"))
    (fp_text user "PCB EDGE" (at 0.05 -1) (layer "Dwgs.User"))
    (pad "1" smd rect (at -5.95 1.75 180) (size 1.5 3.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -4.868182 1.75 180) (size 1.5 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Left Audio") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -3.786364 1.75 180) (size 1.5 3.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at -2.704546 1.75 180) (size 1.5 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Right Audio") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -1.622728 1.75 180) (size 1.5 3.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "Luma") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at -0.54091 1.75 180) (size 1.5 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "unconnected-(J1-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.540908 1.75 180) (size 1.5 3.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "unconnected-(J1-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 1.622726 1.75 180) (size 1.5 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 2.704544 1.75 180) (size 1.5 3.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "Blue in") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 3.786362 1.75 180) (size 1.5 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+5V") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 4.86818 1.75 180) (size 1.5 3.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Red in") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 5.95 1.75 180) (size 1.5 3.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Green in") (pinfunction "Pin_12") (pintype "passive"))
  )
  (footprint "ICspretty:coaxPad" (layer "F.Cu")
    (at 130.45 57.5)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "R" (at 0 3.1 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 4.6 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 1 5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 4 "Red Out") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "ICspretty:coaxPad" (layer "B.Cu")
    (at 136.45 57.5 180)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J2" (at 0 6.7 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 -4.6 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.1 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1)
      (net 9 "GND") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "ICspretty:coaxPad" (layer "B.Cu")
    (at 132.45 57.5 180)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J4" (at 0 6.7 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 -4.6 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.1 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1)
      (net 14 "Right Audio") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "ICspretty:coaxPad" (layer "B.Cu")
    (at 126.45 57.5 180)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J8" (at 0 6.7 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 -4.6 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.1 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1)
      (net 9 "GND") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "ICspretty:coaxPad" (layer "B.Cu")
    (at 134.45 57.5 180)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J3" (at 0 6.7 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 -4.6 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.1 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1)
      (net 15 "Left Audio") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "ICspretty:coaxPad" (layer "B.Cu")
    (at 130.45 57.5 180)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J6" (at 0 6.7 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 -4.6 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.1 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1)
      (net 9 "GND") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Ports:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (at 132.7 63.25)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf)")
    (tags "SOIC 1.27")
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 4.775 1.4) (layer "B.SilkS"))
    (fp_text value "LM1881" (at 0 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -2.7 1.905) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "Net-(U1-CSYNC)") (pinfunction "CSYNC") (pintype "output"))
    (pad "2" smd rect (at -2.7 0.635) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "Net-(U1-VIDEO)") (pinfunction "VIDEO") (pintype "input"))
    (pad "3" smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "unconnected-(U1-FRAME-Pad3)") (pinfunction "FRAME") (pintype "output"))
    (pad "4" smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "unconnected-(U1-BURST-Pad5)") (pinfunction "BURST") (pintype "output"))
    (pad "6" smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(U1-INT)") (pinfunction "INT") (pintype "input"))
    (pad "7" smd rect (at 2.7 0.635) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "unconnected-(U1-O{slash}E-Pad7)") (pinfunction "O/E") (pintype "output"))
    (pad "8" smd rect (at 2.7 1.905) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 127.15 61.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.55 0.1) (layer "B.SilkS"))
    (fp_text value "470Ω" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(U1-CSYNC)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 17 "cSync") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICspretty:coaxPad" (layer "B.Cu")
    (at 128.45 57.5 180)
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J7" (at 0 6.7 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 -4.6 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.1 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1)
      (net 17 "cSync") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 127.95 64.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PS1 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at -0.15 -2.05 180) (layer "B.SilkS"))
    (fp_text value "100nf" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Luma") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U1-VIDEO)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 123.65 54.9) (end 138.9 70)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "C" (at 129.275 60.975) (layer "B.SilkS"))
  (gr_text "RL" (at 132.95 61.05) (layer "B.SilkS"))
  (gr_text "LL" (at 134.525 61) (layer "B.SilkS"))
  (zone (net 9) (net_name "GND") (layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 138.85 54.95)
        (xy 138.85 69.95)
        (xy 123.7 69.95)
        (xy 123.7 54.95)
      )
    )
  )
)
