(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 175)
    (no_connects 0)
    (area 115.748999 77.511 143.331001 119.693)
    (thickness 1.6)
    (drawings 9)
    (tracks 100)
    (zones 0)
    (modules 151)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.49)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.3 4.3)
    (pad_drill 2.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x310f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +12V)
  (net 5 +12VA)
  (net 6 "Net-(C8-Pad1)")
  (net 7 "Net-(C9-Pad1)")
  (net 8 "Net-(C10-Pad1)")
  (net 9 "Net-(C11-Pad1)")
  (net 10 "Net-(C11-Pad2)")
  (net 11 "Net-(C12-Pad1)")
  (net 12 "Net-(C12-Pad2)")
  (net 13 "Net-(R5-Pad2)")
  (net 14 "Net-(R7-Pad2)")
  (net 15 "Net-(R10-Pad1)")
  (net 16 "Net-(AT1-Pad1)")
  (net 17 "Net-(AT1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.49)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +12VA)
    (add_net GND)
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.49)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad2)")
  )
  (net_class Signal ""
    (clearance 0.2)
    (trace_width 0.49)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(AT1-Pad1)")
    (add_net "Net-(AT1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C9-Pad1)")
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 139.7 93.98)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 140.716 93.98)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 140.716 97.536)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 137.668 97.536)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 136.652 98.044)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 136.144 98.552)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 116.84 93.98)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 127 116.205)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.128 116.84)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 136.525 117.475)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 136.525 115.57)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 122.428 97.79)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.063 96.52)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.063 95.25)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 93.98)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.11 106.045)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.11 104.775)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.11 103.505)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.11 102.235)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.11 100.965)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.11 99.695)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.364 90.932)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.364 98.552)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.364 98.044)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 117.856 98.044)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 116.84 98.044)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 119.888 91.948)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 119.38 92.964)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 118.872 93.98)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 133.35 94.615)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 134.62 97.79)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 133.35 96.52)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 132.08 95.25)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 128.778 96.52)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.063 100.33)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 102.87)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 129.413 102.87)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 130.683 101.6)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 131.318 99.695)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 130.048 97.79)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 124.968 95.885)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 134.62 90.805)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.89 90.805)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.255 93.98)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.255 94.615)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.255 95.25)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.255 95.885)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.89 96.52)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.89 97.155)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 141.732 98.044)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 141.732 93.98)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 139.7 93.345)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 139.7 92.075)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 139.7 90.805)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 125.603 89.535)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 125.603 87.63)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 125.603 85.725)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.063 97.155)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.063 95.885)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.063 94.615)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 93.345)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 92.075)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 90.805)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 89.535)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 88.265)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.063 87.63)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 86.995)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 85.725)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 84.455)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.698 83.185)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 117.856 87.884)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 119.888 83.82)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 119.888 82.55)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 119.888 81.28)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 120.523 80.645)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 121.793 80.645)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 122.428 80.01)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 138.43 90.805)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 138.43 89.535)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 138.43 88.265)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 138.43 86.995)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 138.43 85.725)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 133.858 90.17)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 132.588 84.455)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 132.588 88.265)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 132.715 86.36)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 130.683 86.995)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 130.683 85.725)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 130.683 84.455)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 130.683 83.185)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 131.318 83.185)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 132.588 83.185)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 134.493 88.9)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 134.493 87.63)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 134.493 86.36)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 134.493 85.09)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 123.063 79.375)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 137.795 82.55)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 125.603 79.375)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 126.238 80.01)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 127.508 80.01)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 128.143 79.375)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 129.413 79.375)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 130.683 79.375)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 131.953 79.375)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 133.223 79.375)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 134.493 83.82)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 133.858 83.185)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 134.62 79.375)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 137.795 83.82)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 137.795 85.09)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 137.16 81.915)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 136.525 81.28)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.89 80.645)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 135.255 80.01)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 119.888 90.932)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:VIA-0.6mm (layer F.Cu) (tedit 59B2CDAB)
    (at 117.856 93.98)
    (fp_text reference " " (at 0.127 1.143) (layer F.SilkS) hide)
    (fp_text value " " (at 0 -0.889) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 59B2F72E)
    (at 139.192 106.172 90)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C1 (at 0.508 -2.54 90) (layer F.SilkS))
    (fp_text value 4.7u (at 0 -2.54 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59B2B9A9)
    (at 127 106.68 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 131.445 115.57 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 132.08 103.632 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59B2B965)
    (at 130.175 90.805 45)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 3.592102 0 45) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 45) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 45) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12VA))
    (pad 2 smd rect (at 1.25 0 45) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59B2B94E)
    (at 128.27 93.98 225)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.796051 225) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 225) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 225) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12VA))
    (pad 2 smd rect (at 1.25 0 225) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59B2B951)
    (at 127 92.075 225)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.796051 225) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 225) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 225) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12VA))
    (pad 2 smd rect (at 1.25 0 225) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59B2B984)
    (at 120.65 107.315 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 121.92 91.44 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(AT1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 121.92 83.82 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(AT1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 130.81 81.28)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59B2B8E7)
    (at 137.668 94.488 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value 10u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MELF_Handsoldering (layer F.Cu) (tedit 5905D89D)
    (at 139.192 112.776 270)
    (descr "Diode MELF Handsoldering")
    (tags "Diode MELF Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value BYD17D (at 0 2.25 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -3.4 0 270) (size 3.5 2.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 3.4 0 270) (size 3.5 2.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_1806_Handsoldering (layer F.Cu) (tedit 59B2B9C2)
    (at 134.62 102.87 270)
    (descr "Ferrite bead SMD 1806, hand soldering, see Murata BLM41P")
    (tags "ferrite bead 1806")
    (attr smd)
    (fp_text reference L1 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 2.3 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.4 0 270) (size 1.75 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +12VA))
    (pad 2 smd rect (at 2.4 0 270) (size 1.75 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1806.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 129.54 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 10.2K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 129.54 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 1.24K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 127 111.76 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 715 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59B1A839)
    (at 124.46 106.68 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 1.0K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 120.65 102.87 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 1.0K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 120.65 97.79 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 1.0K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59B1A8F9)
    (at 128.27 88.9 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 107 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +12VA))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59B2B909)
    (at 128.27 84.455 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 107 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59B2B933)
    (at 131.445 92.71)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 1.905) (layer F.SilkS))
    (fp_text value 107 (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +12VA))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59B2B8DA)
    (at 135.255 92.71)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 1.905) (layer F.SilkS))
    (fp_text value 107 (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 59B1A89F)
    (at 134.62 110.49 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value LM317LM (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6_Handsoldering (layer F.Cu) (tedit 59B1A6D6)
    (at 125.095 81.915 315)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (attr smd)
    (fp_text reference U2 (at 0 -2 315) (layer F.SilkS))
    (fp_text value GBH112 (at 0 2 495) (layer F.Fab))
    (fp_text user %R (at 0 0 495) (layer F.Fab))
    (pad 1 smd rect (at -1.33 -0.65 315) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.33 0 315) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.33 0.65 315) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (pad 4 smd rect (at 1.33 0.65 315) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.33 0 315) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1.33 -0.65 315) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6_Handsoldering (layer F.Cu) (tedit 59B1AAA3)
    (at 136.525 88.265 270)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (attr smd)
    (fp_text reference U3 (at 0 -2 270) (layer F.SilkS))
    (fp_text value GBH112 (at 0 2 450) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.33 -0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.33 0 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.33 0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad2)"))
    (pad 4 smd rect (at 1.33 0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.33 0 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1.33 -0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootPrint:PAT1220 (layer F.Cu) (tedit 59B19948)
    (at 120.015 87.63 270)
    (descr attenuator)
    (tags attenuator)
    (fp_text reference AT1 (at 0.254 1.905 270) (layer F.SilkS))
    (fp_text value "4dB Attenuator" (at 0.381 -2.54 270) (layer F.Fab))
    (pad 3 smd rect (at 0 0.254 270) (size 4.1 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.016 -1.143 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(AT1-Pad1)"))
    (pad 2 smd rect (at -1.016 -1.143 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(AT1-Pad2)"))
  )
  (module MyFootPrint:GND_Screw (layer F.Cu) (tedit 59B2FC45)
    (at 126.492 100.076)
    (fp_text reference " " (at -0.127 4.572) (layer F.SilkS))
    (fp_text value " " (at 0.508 -3.429) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 4.3 4.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:GND_Screw (layer F.Cu) (tedit 59B2FC6E)
    (at 121.412 113.792)
    (fp_text reference " " (at -0.127 4.572) (layer F.SilkS))
    (fp_text value GND_Screw (at 0.508 -3.429) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 4.3 4.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:GND_Screw (layer F.Cu) (tedit 59B2FC5C)
    (at 139.192 100.076)
    (fp_text reference " " (at -0.127 4.572) (layer F.SilkS))
    (fp_text value " " (at 0.508 -3.429) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 4.3 4.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module MyFootPrint:Input_Finger100mil (layer F.Cu) (tedit 59B2F7C7)
    (at 117.856 96.012)
    (fp_text reference In (at 0 -3.556) (layer F.SilkS))
    (fp_text value SMA (at 0.127 -1.905) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.54 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad1)"))
  )
  (module MyFootPrint:Input_Finger100mil (layer F.Cu) (tedit 59B2F77A)
    (at 140.716 96.012)
    (fp_text reference Out (at 0.508 -3.048) (layer F.SilkS))
    (fp_text value SMA (at 0.127 -1.905) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.54 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad2)"))
  )
  (module MyFootPrint:Input_Finger100mil (layer F.Cu) (tedit 59B2F73E)
    (at 140.716 109.22)
    (fp_text reference 15v-IN (at 1.016 -4.064 90) (layer F.SilkS))
    (fp_text value +15V (at -1.016 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.54 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (gr_line (start 115.824 119.38) (end 115.824 77.724) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.256 119.38) (end 115.824 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.256 77.724) (end 143.256 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.824 77.724) (end 143.256 77.724) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "GHz Amplifier V 0.1" (at 140.716 84.836 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.748 118.872) (xy 116.332 118.872) (xy 116.332 78.232) (xy 142.748 78.232)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.748 118.872) (xy 116.332 118.872) (xy 116.332 78.232) (xy 142.748 78.232)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.748 118.872) (xy 116.332 118.872) (xy 116.332 78.232) (xy 142.748 78.232)
      )
    )
  )
)
