(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Coil Voltages Board")
    (date "10/14/2022")
    (rev "v01")
    (company "NHMFL")
    (comment 1 "Sujana Uppalapati")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010a8_7fffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "Net-(R1-Pad2)")
  (net 2 "Net-(R3-Pad2)")
  (net 3 "Net-(R5-Pad2)")
  (net 4 "Net-(R7-Pad2)")
  (net 5 "Net-(R10-Pad1)")
  (net 6 "Net-(J2-Pad10)")
  (net 7 "Net-(R11-Pad2)")
  (net 8 "Net-(J2-Pad12)")
  (net 9 "Net-(R13-Pad2)")
  (net 10 "Net-(J2-Pad14)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 "Net-(J1-Pad6)")
  (net 14 "Net-(J1-Pad8)")
  (net 15 "unconnected-(J1-Pad1)")
  (net 16 "Net-(J1-Pad10)")
  (net 17 "unconnected-(J1-Pad3)")
  (net 18 "Net-(J1-Pad12)")
  (net 19 "unconnected-(J1-Pad5)")
  (net 20 "Net-(J1-Pad14)")
  (net 21 "unconnected-(J1-Pad7)")
  (net 22 "Net-(J1-Pad16)")
  (net 23 "unconnected-(J1-Pad9)")
  (net 24 "Net-(J2-Pad2)")
  (net 25 "unconnected-(J1-Pad11)")
  (net 26 "Net-(J2-Pad4)")
  (net 27 "unconnected-(J1-Pad13)")
  (net 28 "Net-(J2-Pad6)")
  (net 29 "unconnected-(J1-Pad15)")
  (net 30 "Net-(J2-Pad8)")
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 151.13 90.424 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -1.876 -0.1) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(J2-Pad6)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(J1-Pad12)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 105.41 119.38)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 6.35 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad14)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(R1-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 151.13 76.2 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at -1.876 -0.1) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(J2-Pad8)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J1-Pad10)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 129.54 33.528)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R14" (at 6.604 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(R13-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad14)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 129.54 47.498)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R12" (at 6.604 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(R11-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad12)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 129.54 62.357)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R10" (at 6.604 2.159) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(R10-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad10)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 182.88 31.75)
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad2" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 105.41 76.2)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 6.35 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad8)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(R7-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 182.88 129.54)
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad3" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 105.41 90.424)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 6.35 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad10)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(R5-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 151.13 105.41 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -1.876 0) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(J2-Pad4)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(J1-Pad14)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 105.41 62.357)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R9" (at 6.35 2.159) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad6)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(R10-Pad1)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 151.13 47.498 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at -1.976 -0.1) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J2-Pad12)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(J1-Pad6)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 129.54 76.2)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at 6.604 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(R7-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad8)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 129.54 105.41)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 6.604 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(R3-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad4)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 151.13 119.38 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at -1.776 0) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(J2-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(J1-Pad16)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 77.47 31.75)
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad1" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 77.47 129.54)
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad4" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 105.41 47.498)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R11" (at 6.35 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad4)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(R11-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "KiCAD Library_SU:MCV_16Pin_1803565" (layer "F.Cu")
    (tedit 615EFF57)
    (at 92.05 48.81 -90)
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -4.064 3.683 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "MCV_16Pin_1803565" (at 7.874 5.588 90) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 15 "unconnected-(J1-Pad1)") (pinfunction "1") (pintype "passive+no_connect"))
    (pad "2" thru_hole roundrect (at 3.81 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(J1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 7.62 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 17 "unconnected-(J1-Pad3)") (pinfunction "3") (pintype "passive+no_connect"))
    (pad "4" thru_hole roundrect (at 11.43 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J1-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole roundrect (at 15.24 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 19 "unconnected-(J1-Pad5)") (pinfunction "5") (pintype "passive+no_connect"))
    (pad "6" thru_hole roundrect (at 19.05 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole roundrect (at 22.86 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 21 "unconnected-(J1-Pad7)") (pinfunction "7") (pintype "passive+no_connect"))
    (pad "8" thru_hole roundrect (at 26.67 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(J1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole roundrect (at 30.48 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 23 "unconnected-(J1-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (pad "10" thru_hole roundrect (at 34.29 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(J1-Pad10)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole roundrect (at 38.1 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 25 "unconnected-(J1-Pad11)") (pinfunction "11") (pintype "passive+no_connect"))
    (pad "12" thru_hole roundrect (at 41.91 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J1-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole roundrect (at 45.72 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 27 "unconnected-(J1-Pad13)") (pinfunction "13") (pintype "passive+no_connect"))
    (pad "14" thru_hole roundrect (at 49.53 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(J1-Pad14)") (pinfunction "14") (pintype "passive"))
    (pad "15" thru_hole roundrect (at 53.34 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 29 "unconnected-(J1-Pad15)") (pinfunction "15") (pintype "passive+no_connect"))
    (pad "16" thru_hole roundrect (at 57.15 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(J1-Pad16)") (pinfunction "16") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_6-Pin_1803468.stp"
      (offset (xyz -2.5908 -3.4798 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 129.54 90.424)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 6.604 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(R5-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad6)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 105.41 33.528)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R13" (at 6.35 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(R13-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "KiCAD Library_SU:MCV_14Pin_1803549" (layer "F.Cu")
    (tedit 615EFF57)
    (at 168.425 103.472 90)
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -4.064 3.683 90) (layer "F.SilkS"))
    (fp_text value "MCV_14Pin_1803549" (at 7.874 5.588 90) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(J1-Pad16)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 3.81 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(J2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 7.62 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(J1-Pad14)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole roundrect (at 11.43 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(J2-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole roundrect (at 15.24 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J1-Pad12)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole roundrect (at 19.05 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(J2-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole roundrect (at 22.86 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(J1-Pad10)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole roundrect (at 26.67 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(J2-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole roundrect (at 30.48 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(J1-Pad8)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole roundrect (at 34.29 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J2-Pad10)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole roundrect (at 38.1 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J1-Pad6)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole roundrect (at 41.91 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J2-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole roundrect (at 45.72 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J1-Pad4)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole roundrect (at 49.53 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pad14)") (pinfunction "14") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_6-Pin_1803468.stp"
      (offset (xyz -2.5908 -3.4798 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 151.13 33.528 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at -1.976 0.1) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(J2-Pad14)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(J1-Pad4)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 129.54 119.38)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 6.604 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(R1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_PCB_Misc:Maglab_Logo" (layer "F.Cu")
    (tedit 5F3FD4DC)
    (at 138.525 134.23667)
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "111" (at 2.0574 3.13436) (layer "F.SilkS") hide)
    (fp_text value "MAGLAB_LOGO_1_2" (at 2.62382 1.36652) (layer "F.Fab") hide)
    (fp_text user "AGLAB" (at 11.176 -1.5875) (layer "F.SilkS"))
    (fp_text user "NATIONAL" (at 9.144 -4.2545) (layer "F.SilkS"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 151.13 62.357 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at -1.776 0) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J2-Pad10)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J1-Pad8)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_Thru:R_500" (layer "F.Cu")
    (tedit 5F0F2C1F)
    (at 105.41 105.41)
    (descr "Resistor, Thru Hole, 500mil Spacing")
    (tags "500")
    (property "Sheetfile" "Coil Voltages Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 6.35 2.286) (layer "F.SilkS"))
    (fp_text value "res_500" (at 6.477 2.413) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad12)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 12.7 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(R3-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (gr_rect (start 69.85 24.13) (end 190.5 137.16) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Scaled Coil B" (at 179.07 93.98) (layer "F.SilkS"))
  (gr_text "Coil Voltages Board (v01)\nS Uppalapati 2022" (at 121.92 132.08) (layer "F.SilkS"))
  (gr_text "Voltage Tap FG" (at 80.7974 60.325) (layer "F.SilkS"))
  (gr_text "Voltage Tap BC" (at 80.7974 90.805) (layer "F.SilkS"))
  (gr_text "Coil B Scaling Resistors" (at 123.952 102.87) (layer "F.SilkS"))
  (gr_text "Scaled Coil F" (at 179.07 63.5) (layer "F.SilkS"))
  (gr_text "Scaled Coil Voltages" (at 168.91 49.53) (layer "F.SilkS"))
  (gr_text "Coil F Scaling Resistors" (at 123.952 45.212) (layer "F.SilkS"))
  (gr_text "Voltage Tap G" (at 80.7974 52.705) (layer "F.SilkS"))
  (gr_text "Scaled Coil E" (at 179.07 71.12) (layer "F.SilkS"))
  (gr_text "Coil E Scaling Resistors" (at 123.952 59.69) (layer "F.SilkS"))
  (gr_text "Voltage Tap EF" (at 80.7974 67.945) (layer "F.SilkS"))
  (gr_text "Scaled Coil D" (at 179.07 78.74) (layer "F.SilkS"))
  (gr_text "Scaled Coil A" (at 179.07 101.6) (layer "F.SilkS"))
  (gr_text "Voltage Tap CD" (at 80.7974 83.185) (layer "F.SilkS"))
  (gr_text "Coil C Scaling Resistors" (at 123.952 87.884) (layer "F.SilkS"))
  (gr_text "Raw Coil Voltages" (at 91.44 110.49) (layer "F.SilkS"))
  (gr_text "Voltage Tap DE\n" (at 80.7974 75.565) (layer "F.SilkS"))
  (gr_text "1" (at 86.868 46.482 -90) (layer "F.SilkS"))
  (gr_text "Coil G Scaling Resistors" (at 123.952 30.988) (layer "F.SilkS"))
  (gr_text "Voltage Tap AB" (at 80.7974 98.5774) (layer "F.SilkS"))
  (gr_text "1" (at 173.736 105.791 90) (layer "F.SilkS"))
  (gr_text "Coil A Scaling Resistors" (at 123.952 116.84) (layer "F.SilkS"))
  (gr_text "Coil D Scaling Resistors" (at 123.952 73.914) (layer "F.SilkS"))
  (gr_text "Scaled Coil C" (at 179.07 86.36) (layer "F.SilkS"))
  (gr_text "Voltage Tap A" (at 80.7974 106.172) (layer "F.SilkS"))
  (gr_text "Scaled Coil G" (at 179.07 56.007) (layer "F.SilkS"))
)
