(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 47)
    (no_connects 0)
    (area 136.674999 69.424999 180.575001 88.575001)
    (thickness 1.6)
    (drawings 10)
    (tracks 84)
    (zones 0)
    (modules 26)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 136.75 88.5)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C4-Pad2)")
  (net 9 "Net-(C5-Pad1)")
  (net 10 "Net-(C5-Pad2)")
  (net 11 "Net-(C6-Pad1)")
  (net 12 "Net-(C6-Pad2)")
  (net 13 "Net-(C7-Pad1)")
  (net 14 "Net-(C7-Pad2)")
  (net 15 "Net-(C8-Pad1)")
  (net 16 "Net-(C8-Pad2)")
  (net 17 "Net-(J1-Pad10)")
  (net 18 "Net-(J1-Pad9)")
  (net 19 GND)
  (net 20 "Net-(J1-Pad7)")
  (net 21 "Net-(J1-Pad6)")
  (net 22 "Net-(J1-Pad4)")
  (net 23 "Net-(J1-Pad3)")
  (net 24 "Net-(J1-Pad1)")
  (net 25 "Net-(J1-Pad12)")
  (net 26 "Net-(J1-Pad13)")
  (net 27 "Net-(J1-Pad14)")
  (net 28 "Net-(J1-Pad15)")
  (net 29 "Net-(J1-Pad16)")
  (net 30 +5V)
  (net 31 "Net-(J1-Pad19)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad9)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D4687E)
    (at 170 75.25 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D46871)
    (at 164.5 76.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D46881)
    (at 170 77.75 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D46873)
    (at 164.5 79 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D46884)
    (at 170 80.25 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D46876)
    (at 164.5 81.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D46886)
    (at 170 82.75 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D46879)
    (at 164.5 84 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hdmi:hdmi_new (layer F.Cu) (tedit 58D46C6D)
    (at 144.5 79 270)
    (fp_text reference J1 (at 7.0064 -3.3688 360) (layer F.SilkS) hide)
    (fp_text value HDMI (at 0.25 3.556 270) (layer F.SilkS) hide)
    (pad 10 smd rect (at 0.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad10)"))
    (pad 9 smd rect (at 0.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad9)"))
    (pad 8 smd rect (at 1.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 7 smd rect (at 1.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at 2.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at 2.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 4 smd rect (at 3.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 3.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 4.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 1 smd rect (at 4.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J1-Pad1)"))
    (pad 11 smd rect (at -0.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 12 smd rect (at -0.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J1-Pad12)"))
    (pad 13 smd rect (at -1.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad13)"))
    (pad 14 smd rect (at -1.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad14)"))
    (pad 15 smd rect (at -2.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J1-Pad15)"))
    (pad 16 smd rect (at -2.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J1-Pad16)"))
    (pad 17 smd rect (at -3.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 18 smd rect (at -3.75 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 30 +5V))
    (pad 19 smd rect (at -4.25 -1.3 270) (size 0.3 2.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J1-Pad19)"))
    (pad 0 thru_hole circle (at -7.25 0 270) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 7.25 0 270) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at -7.85 4.9 270) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 7.85 4.9 270) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  )
  (module my-libs:10pinSolderpads (layer F.Cu) (tedit 58D457FA)
    (at 177 79 270)
    (fp_text reference P1 (at 0 0.15 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at -0.25 -0.5 270) (layer F.Fab) hide)
    (fp_text user 10 (at -7 2.9 360) (layer F.SilkS))
    (fp_text user 9 (at 5 3.75 270) (layer F.SilkS))
    (fp_text user 8 (at 3.75 3.75 270) (layer F.SilkS))
    (fp_text user 7 (at 2.5 3.75 270) (layer F.SilkS))
    (fp_text user 6 (at 1.25 3.75 270) (layer F.SilkS))
    (fp_text user 5 (at 0 3.75 270) (layer F.SilkS))
    (fp_text user 4 (at -1.25 3.75 270) (layer F.SilkS))
    (fp_text user 3 (at -2.5 3.75 270) (layer F.SilkS))
    (fp_text user 2 (at -3.75 3.75 270) (layer F.SilkS))
    (fp_text user 1 (at -5 3.75 270) (layer F.SilkS))
    (fp_text user 10 (at 7 2.9 360) (layer F.SilkS))
    (pad 1 smd oval (at -5 -1.35 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 30 +5V))
    (pad 2 smd oval (at -3.75 1.4 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd oval (at -2.5 -1.35 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd oval (at -1.25 1.4 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 5 smd oval (at 0 -1.35 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 6 smd oval (at 1.25 1.4 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 7 smd oval (at 2.5 -1.35 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 8 smd oval (at 3.75 1.4 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (pad 9 smd oval (at 5 -1.35 270) (size 1.524 2.524) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (pad 10 smd oval (at 7 0 90) (size 1.524 3.524) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 10 smd oval (at -7 0 90) (size 1.524 3.524) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D46863)
    (at 158.5 75.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value 47R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J1-Pad12)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D466DE)
    (at 152 76.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value 47R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad10)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D46891)
    (at 158.5 75.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 620R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J1-Pad12)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D46855)
    (at 152 76.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 620R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J1-Pad10)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D46866)
    (at 158.5 77.75 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value 47R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad9)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D46859)
    (at 152 79 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value 47R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D46894)
    (at 158.5 77.75 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 620R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad9)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D4689C)
    (at 152 79 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 620R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D46869)
    (at 158.5 80.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value 47R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D4685B)
    (at 152 81.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value 47R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D46897)
    (at 158.5 80.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 620R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D4689E)
    (at 152 81.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 620R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D4686C)
    (at 158.5 82.75 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value 47R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D46860)
    (at 152 84 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value 47R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C8-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D46899)
    (at 158.5 82.75 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 620R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D468A1)
    (at 152 84 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value 620R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 620R (at 155 72.5 180) (layer B.SilkS))
  (gr_text LVDS2TMDS (at 161 71.75) (layer F.SilkS))
  (gr_text " 6. D1-\n 7. D1+\n 8. D2-\n 9. D2+\n10. GND" (at 175.25 79 180) (layer B.SilkS))
  (gr_text " 1. 5V\n 2. Clk-  \n 3. Clk+\n 4. D0-\n 5. D0+" (at 161.75 79 180) (layer B.SilkS))
  (gr_text 100n (at 167.25 86.5) (layer F.SilkS))
  (gr_text 47R (at 155 86.5) (layer F.SilkS))
  (gr_line (start 136.75 88.5) (end 136.75 69.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.5 88.5) (end 136.75 88.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.5 69.5) (end 180.5 88.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.75 69.5) (end 180.5 69.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 19) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.25 70) (xy 137.25 88) (xy 180 88) (xy 180 70)
      )
    )
  )
  (zone (net 19) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.25 70) (xy 137.25 88) (xy 180 88) (xy 180 70)
      )
    )
  )
)
